Companies are to share their inputs on the excel spreadsheet in /tsg\_ran/WG1\_RL1/TSGR1\_106b-e/Inbox/drafts/8.1.2.4/RRC parameters/ herein.

## Inputs on version 00

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| ZTE | * One new RRC parameter should be introduced to enable UE identifying two QCL-TypeD properties for multiple overlapping CORESETs * The third row for simultaneousTCI-UpdateList1, simultaneousTCI-UpdateList2 is not needed as we have agreed the Rel-16 ones are reused |
| CATT | Agree with ZTE that if UE reports capability of monitoring two QCL-TypeD properties for multiple overlapping CORESETs, one new RRC parameter should be introduced to enable UE identifying two QCL-TypeD properties. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version xx

Please share your inputs, if any, in the following table

....