3GPP TSG-RAN WG2 Meeting #115-e ***R2-2108933***

Electronic Meeting, August 16 – 27, 2021

**Agenda item:** 6.3.1

**Source:** Qualcomm Incorporated

**Title:** Summary of [AT115-e][603][POS] AI 7.5 LTE Positioning and Rel-16 stage 2 CRs

**Document for:**  Discussion

# 1. Introduction

This document summarizes the following email discussion:

* [AT115-e][603][POS] AI 7.5 LTE Positioning and Rel-16 stage 2 CRs (Qualcomm)

 Scope:

* Handle the CR in R2-2107959 and determine conclusion.
* Handle the CR in R2-2107333 and determine conclusion
* Handle the CR in R2-2107958 and determine conclusion

 Intended outcome: Agreed CRs (without comebacks), report in R2-2108933

 Deadline: Tuesday 2021-08-24 0800 UTC

## 1.1 References

[1] [R2-2107959](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_115-e/Docs/R2-2107959.zip), "Correction on user-plane positioning support by SUPL", Samsung, Qualcomm Incorporated,
 CR Rel-16 36.305 16.3.0 0105 - F LCS\_LTE

[2] [R2-2107958](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_115-e/Docs/R2-2107958.zip), "Correction on user-plane positioning support by SUPL", Samsung, Qualcomm Incorporated,
 CR Rel-16 38.305 16.5.0 0078 - F NR\_pos-Core

[3] [R2-2107333](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_115-e/Docs/R2-2107333.zip), "Correction to NB-IoT positioning", Huawei, HiSilicon,
 CR Rel-16 38.305 16.5.0 0076 - F NR\_pos-Core

# 2. Correction on user-plane positioning support by SUPL [1],[2]

## 2.1 Background

Both CRs [1][2] clarify the "SUPL column" in Table 4.3.1-1 "Supported versions of UE positioning methods".

A new NOTE is proposed as follows (the equivalent NOTE is proposed for 36.305 [1]):

Table 4.3.1-1: Supported versions of UE positioning methods

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Method | UE-based | UE-assisted, LMF-based | NG-RAN node assisted | SUPL Note 8 |
| A-GNSS | Yes | Yes | No | Yes |
| OTDOA Note1, Note 2 | No | Yes | No | Yes |
| E-CID Note 4, Note 7  | No | Yes | Yes | Yes for E-UTRA |
| Sensor | Yes | Yes | No | No |
| WLAN | Yes | Yes | No | Yes  |
| Bluetooth | No | Yes | No | No |
| TBS Note 5 | Yes | Yes | No | Yes (MBS) |
| DL-TDOA | Yes | Yes | No | Yes |
| DL-AoD | Yes | Yes | No | Yes |
| Multi-RTT | No | Yes | Yes | Yes |
| NR E-CID  | No | Yes | Yes | Yes (DL NR E-CID) |
| UL-TDOA | No | No | Yes | Yes |
| UL-AoA | No | No | Yes | Yes |
| NOTE 1: This includes TBS positioning based on PRS signals.NOTE 2: In this version of the specification only OTDOA based on LTE signals is supported.NOTE 3: VoidNOTE 4: This includes Cell-ID for NR method when UE is served by gNB.NOTE 5: In this version of the specification only for TBS positioning based on MBS signals.NOTE 6: VoidNOTE 7: Enhanced Cell ID based on LTE signals.NOTE 8: This shows whether the positioning method is supported by SUPL ULP [16]. |

This is to avoid confusion with Annex B (36.305) or Annex A (38.305), as also discussed in [R2-2104512](http://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_113bis-e/Docs/R2-2104512.zip) from RAN2#113bis ("Report of [AT113b-e][602][POS] Positioning corrections for NR Rel-15 (Samsung)").

Additional changes are proposed to the informative Annex A (38.305) and Annex B (36.305):

38.305 [2]:

- *NRCellInformation* as defined in SUPL ULP is added.

- Comments on "NR signals are not supported" are deleted.

- Not needed copy of RRC *MeasResultListEUTRA* is deleted.

- SUPL ULP reference is updated to the latest version 2.0.6 (which includes the NR positioning support).

36.305 [1]:

 - *LteCellInformation* is corrected (as defined in SUPL ULP).

- Not needed copy of RRC *MeasResultListEUTRA* is deleted.

- SUPL ULP reference is updated to the latest version 2.0.6.

## 2.2 Discussion

**Question 1:** Do you agree with the CR to TS 38.305 in [R2-2107958](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_115-e/Docs/R2-2107958.zip), "Correction on user-plane positioning support by SUPL"?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2:** Do you agree with the CR to TS 36.305 in [R2-2107959](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_115-e/Docs/R2-2107959.zip), "Correction on user-plane positioning support by SUPL"?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3. Correction to NB-IoT positioning [3]

## 3.1 Background

TS 23.273 Rel-16 specifies "Low Power Periodic and Triggered 5GC-MT-LR Procedures" in clause 6.7 which allows a UE to provide LCS Event Reports in idle state using EDT for Control Plane with CIoT 5GS Optimization.

If the UE and NG-RAN node both support EDT, the UE sends an *RRCEarlyDataRequest* message to the NG-RAN node and includes a NAS control plane service request. Otherwise, the UE established an RRC connection with the NG-RAN node and sends the NAS control plane service request.

However, in the current Stage 2 TS 38.305 for the NB-IoT positioning procedures, there is no description that a UE can send an LCS Event Report to the network in CM\_IDLE without transition to RRC\_CONNECTED.

Therefore, the following changes are proposed in [3]:

1. Add a new clause for the previous description of NB-IOT positioning measurement in RRC\_IDLE state and measurement report in RRC\_CONNECTED, in Clause 7.1.3

2. Add a new clause for NB-IOT positioning measurement and event report in RRC\_IDLE with CP CIoT 5GC Optimization.

3. Reference to TS 36.300 is added.

For reference, the proposed procedure in [3] is repeated below (item #2 above).

--------------------------------------------------- Begin excerpt from [3] ------------------------------------------------------------

#### 7.1.3.y NB-IoT positioning measurement report in RRC\_IDLE state with Control Plane CIoT 5GC Optimization



Figure 7.1.3.2-1: UE positioning measurements and measurement report in RRC\_IDLE state with Control Plane CIoT 5GC Optimization.

1. Step 1-3 for NB-IOT positioning with measurement report in RRC\_CONENCTED are performed.
2. The LMF sends LCS Periodic-Triggered Invoke Request to the UE as in TS 23.273 [35] carrying location reqeust information received from the AMF. It may also include an LPP message to request the type of location measurement or location estimate in step 6. For E-CID positioning method, when NRSRP/NRSRQ measurements are requested the UE is requested to provide NRSRP/NRSRQ measurements for intra-frequency neighbour cells and for inter-frequency neighbour cells. The UE may use inter-frequency information in system information of the serving cell specified in TS 36.331 [13] to decide on which inter-frequency cells to measure.
3. If the request can be supported, the UE returns a LCS Periodic-Trigger Invoke Accept message to the LMF.
4. The UE may finish any other activities in progress (e.g., SMS or data transfer), and waits until the network releases or suspends the connection (after a certain period of inactivity). The UE will then receive an RRC connection release or suspend from the ng-eNB due to the expiration of the inactivity timer.
5. For a periodic or triggered location request in step 2 and 3 were successfully performed, the UE monitors for occurrence of the trigger or periodic event requested in step 2.
6. If the configured event is detected in step 5, the UE performs measurements according to the request in step 2.
7. If the UE and ng-eNB node both support Control Plane CIoT 5GC Optimization, the UE sends an *RRCEarlyDataRequest* message as in TS 36.300 [xx] to the ng-eNB and includes a NAS control plane service request as in TS 24.501 [29]. The NAS control plane service request includes an Event Report message as in Clause 7.3.4, including the measurement report or location estimate with the measurement performed in step 5.

--------------------------------------------------- End excerpt from [3] ------------------------------------------------------------

**Rapporteur's comments:**

- It is not clear why the CR is specific to NB-IoT. As part of negotiating 5G network behaviour during registration, a UE indicates in a Registration Request whether Control Plane CIoT 5GS Optimisation is supported for location event reporting. This indication may be passed to the LMF by the AMF at step 14 in clause 6.3.1 of TS 23.273 as specified in TS 29.572 (UeLcsCapability). Therefore, all UEs supporting Control Plane CIoT 5GS Optimisation and LCS Event Reporting can make use of the procedure.

- Steps 1-4 are confusing in this context, since the procedures before Step 5 comprise all the deferred MT-LR Initiation Procedures. A suggestion would be to collapse steps 1-4 into a single box with "Deferred 5GC-MT-LR Procedure for Periodic or Triggered Location Events in TS 23.273 Clause 6.3.1 Steps 1-23".

- It may make sense to add this procedure after clause 7.3.4 (Deferred MT-LR Event Reporting Support) in TS 38.305.

**Question 3:** Do you agree with the CR to TS 38.305 in [R2-2107333](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_115-e/Docs/R2-2107333.zip), "Correction to NB-IoT positioning"?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 4. Summary