**3GPP TSG RAN2 #117-e R2-22xx**

**Electronic Meeting, 21 Feb – 03 Mar 2022**

**Agenda Item:**  **9.3**

**Source: Qualcomm Inc. (rapporteur)**

**Title:** **Report on [AT117-e][204][LTE] CRs LTE-based 5G terrestrial broadcast (Qualcomm)**

**Document for: Discussion and decision**

### **1 Introduction**

This is the email discussion report of the following:

* [AT117-e][204][LTE] CRs LTE-based 5G terrestrial broadcast (Qualcomm)

 Scope: Review CRs for LTE-based 5G terrestrial broadcast. In case critical issues are found, those can be raised also online prior to the discussion deadline.

 Intended outcome: Agreeable CRs in [R2-2203633](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_117-e%5CR2-2203633.zip) (36.331) and [R2-2203634](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_117-e%5CR2-2203634.zip) (36.306) (to be submitted to RANP approval).

 Deadline: Deadline 4

**Deadline 4 (discussions for 2nd week Wed online):**

* **Comment deadline:** MondayW2, 1200 UTC (for collecting views)
* **Rapporteur proposals:** Tuesday W2, 1200 UTC (proposed resolution of issues)
* **Document deadline:** Tuesday W2, 1600 UTC (report or agreed CRs)

#### **1.1 Contact Information**

|  |  |  |
| --- | --- | --- |
| **Company** | **Contact Name** | **Email** |
| Qualcomm | Umesh Phuyal | uphuyal@qti.qualcomm.com |
| Lenovo | Hyung-Nam Choi | hchoi5@lenovo.com |
|  |  |  |
|  |  |  |
|  |  |  |

### **2 Discussion**

#### **2.1 Background**

RAN1 CRs for the WI were approved by RAN#94e in RP-212975. RAN1 concluded the RRC parameter in R1-2112975 and sent LS to RAN2 in R2-2200095. Further, RAN1 sent LS to RAN2 in R2-2200090/R1-2112900 regarding UE capabilities for the feature.

These CRs are to introduce the RRC parameter and UE capabilities to the RAN2 specifications.

#### **2.2 Discussion on CRs**

The CRs under discussion are

[R2-2202237](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_117-e/Docs/R2-2202237.zip) Introduction of new bands and bandwidth allocation for LTE-based 5G terrestrial broadcast Qualcomm Incorporated CR Rel-17 36.331 16.7.0 4750 1 B LTE\_terr\_bcast\_bands\_part1-Core R2-2200209

[R2-2202238](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_117-e/Docs/R2-2202238.zip) Introduction of new bands and bandwidth allocation for LTE-based 5G terrestrial broadcast Qualcomm Incorporated CR Rel-17 36.306 16.7.0 1836 - B LTE\_terr\_bcast\_bands\_part1-Core

**Table 1: Comments on RRC CR R2-2202237.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Support/No Support** | **Comments**  |
| Lenovo | Partly | MBSFN-AreaInfoList IE:* Is there a need to signal the value kHz15-r17 in subcarrierSpacingMBMS-r16? So far we understood the new BWs of 6/7/8 MHz are only applicable for 15kHz SCS.
* If there is no need to introduce 15 kHz SCS for MBMS then new MBSFN-AreaInfo-r17 IE can be defined reusing the fields of MBSFN-AreaInfo-r16 except of subcarrierSpacingMBMS-r16.

The capability signaling is still tbd in RAN1, so for the time being we prefer to leave out the capability part. |
| Qualcomm | Support | We are proponent of the CR.**In response to Lenovo’s questions/comments:****Regarding SCS:**According to our understanding, the new BWs are applicable for all SCS values (including but not limited to 15 kHz). After checking the WID and the RAN1 CRs again, I cannot find any restriction about the SCS for new PMCH BWs in terms of SCS. Note that 15kHz was not applicable for MBSFN-AreaInfo-r16 and hence currently there is no way to configure 15kHz using signalling for Rel-16 MBSFN Areas. So, only when included in Rel-17, the spare value would be set to indicate 15kHz SCS. This is further clarified in the field description by adding “Value kHz15-r17 is applicable only when the field is included in *mbsfn-AreaInfo-r17”*In this case, it would be equivalent to copy-paste everything from MBSFN-AreaInfo-r16 into MBSFN-AreaInfo-r17, change them to -r17 fields, change one spare in SCS to 15 kHz as done in the current CR, and add a new field pmch-Bandwidth-r17. The approach taken in the CR is to minimize changes with the same end result.**Regarding Capability:**RAN1 has already concluded that there will be new optional UE capabilities per band. What is still TBD in RAN1 is whether to have single bit for all new PMCH BWs, or multiple bits for different new supported PMCH BWs. So, the CR attempts to show related other changes such as the structure to include it in the MBMS supported band list etc. Depending on RAN1 conclusion the following would be 3 fields or one field, as captured by Editor’s note there.  -- Editor’s Note: Following assumes one capability bit for each new supported PMCH BW, which is still TBD in RAN1 and may need further update. pmch-Bandwidth-n40-r17 ENUMERATED {supported} OPTIONAL, pmch-Bandwidth-n35-r17 ENUMERATED {supported} OPTIONAL, pmch-Bandwidth-n30-r17 ENUMERATED {supported} OPTIONALIt is expected RAN1 will conclude this during ongoing meeting. If RAN1 confirms to have a single capability bit per band, then the above 3 fields would be merged into the following single field (and the top level OPTIONAL tag removed): pmch-Bandwidth-r17 ENUMERATED {supported} OPTIONALConsequently, in the field description, “40/ 35/ 30 PRBs” would change to “40, 35 and 30 PRBs”. With these in mind, we would be interested to know if there are other comments on the capability section. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary:**

**TBD**

**Table 2: Comments on 36.306 CR R2-2202238.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Support/No Support** | **Comments**  |
| Lenovo | No support | The capability signaling is still tbd in RAN1, so for the time being we prefer to leave out the capability part.  |
| Qualcomm | Support | Please see above.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary:**

**TBD**

#### **2.3 Other**

**Table 3: Anything else that is not covered by above questions? Please explain.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

### **3 Conclusion**

TBD

### **4 References**

[1] [R2-2202237](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_117-e/Docs/R2-2202237.zip) Introduction of new bands and bandwidth allocation for LTE-based 5G terrestrial broadcast Qualcomm Incorporated CR Rel-17 36.331 16.7.0 4750 1 B LTE\_terr\_bcast\_bands\_part1-Core R2-2200209

[2] [R2-2202238](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_117-e/Docs/R2-2202238.zip) Introduction of new bands and bandwidth allocation for LTE-based 5G terrestrial broadcast Qualcomm Incorporated CR Rel-17 36.306 16.7.0 1836 - B LTE\_terr\_bcast\_bands\_part1-Core