**3GPP TSG-RAN WG2#117-e Draft R2-2203639**

**Online, 21 February - 3 March 2022**

**Source:** Huawei, HiSilicon

**Title:** [AT117-e][222][DCCA] Actions at SCG activation and deactivation (Huawei)

**Agenda Item:** 8.2.2.2

**Document for:** Discussion and decision

# 1 Introduction

This document is a summary of:

* [AT117-e][222][DCCA] Actions at SCG activation and deactivation (Huawei)

 Scope: Discuss remaining critical open issues (MAC aspects, SCG deactivation UE preference) for actions at SCG de/activation that were not yet handled as part of [Pre117-e][220].

 Intended outcome: Discussion report in [R2-2203639](file:///C%3A%5CUsers%5Cterhentt%5CDocuments%5CTdocs%5CRAN2%5CRAN2_117-e%5CR2-2203638.zip).

 Deadline: Deadline 2

Company contact persons for this discussion are invited to fill one entry in the table below:

|  |  |
| --- | --- |
| Company | Contact details |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 2 Discussion

## 2.1 MAC actions at SCG deactivation / activation

### 2.1.1 Handling of Bj

This is about:

FFS if UE initializes Bj for each logical channel to zero upon SCG deactivation as a part of partial MAC reset. Should consider e.g. what to do with possible Bj increase while SCG is deactivated.

[23] [32][33] propose the Bj are initialized to zero upon SCG deactivation as part of partial MAC reset and are not increased while the SCG is deactivated.

[29] thinks LCP is not done when the SCG is deactivated, so the Bj are never incremented and if set to 0 at SCG deactivation they will remain to zero, while [39][40] think Bj will increase.

[39][40] propose initializing the Bj to zero upon SCG activation. [40] further considers that it is better not to initialize Bj to zero at SCG deactivation even if they are not initialized to zero at SCG activation.

So the possible options are:

1) Bj are initialized to zero and remain to zero while the SCG is deactivated

2) Bj are initialized to zero at SCG activation

3) Bj are not initialized to zero, neither at SCG deactivation nor at SCG deactivation

**Q1: Which option(s) do companies prefer?**

|  |  |  |
| --- | --- | --- |
| Company | Preference(s)  | Comments |
|  |  |  |

### 2.1.2 Explicitly signalled contention-free Random Access Resources

This is about

FFS if UE discards explicitly signalled contention-free Random Access Resources for 4-step RA type and 2-step RA type, if any, upon SCG deactivation as a part of partial MAC reset.

[39] thinks the "explicitly signalled contention-free Random Access Resources for 4-step RA type and 2-step RA type" is rach-ConfigBFR in BeamFailureRecoveryConfig.

Several other companies think that this refers to resources configured in rach-ConfigDedicated in reconfigurationWithSync.

In Rel-16, rach-ConfigDedicated is optional "Need N", i.e. this field is not stored and upon reception of a subsequent RRC message in which reconfigurationWithSync is included but this field is absent, the UE performs contention-based RACH.

The rapporteur would like to remind that RAN2 discussed the possibility to store, while the SCG is deactivated, dedicated RACH resources to be used for random access (when needed) at SCG activation and this was not agreed, so the rapporteur assumes this is not supported.

What is perhaps not sufficiently clear is that, if RACH is triggered by an SCG activation command that does not include an SN RRC message with reconfigurationWithSync, the UE shall perform contention-based random access.

This could be clarified e.g.

1) in the initiation of the random access procedure due to SCG activation while reconfigurationWithSync is not included (could be in 38.321 or in 38.331)

2) in 38.331 by indicating to discard the contents of rach-ConfigDedicated, if it was included, in the completion of a reconfiguration procedure in which the SCG is deactivated

The rapporteur thinks 2) might be simpler from specification perspective.

**Q2: Would companies like to clarify that if RACH is triggered by an SCG activation command that does not include an SN RRC message with reconfigurationWithSync, the UE shall perform contention-based random access? If yes, please indicate preference between 1) and 2) or other.**

|  |  |  |
| --- | --- | --- |
| Company | Yes (and choice) or No  | Comments |
|  |  |  |

**Q3: Assuming a clarification such as 1) and 2) is captured, do companies see the need to indicate in the partial MAC reset at SCG deactivation that the UE "discards explicitly signalled contention-free Random Access Resources for 4-step RA type and 2-step RA type, if any"?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No  | Comments |
|  |  |  |

## 2.2 SCG deactivation UE preference

RAN2 agreed previously to support an indication that the UE prefers the SCG is deactivated but did not agree any detail. There are a few proposals in this meeting for this, but they are not aligned.

[10] proposes something reusing the principles of UE preferences indicated in UE assistance information:

- the network configures the UE to provide a preference for SCG deactivation

- if this is configured, the UE can report a "preference for the SCG to be deactivated" or no such preference

- the UE can only report a preference if it has changed (i.e. change from "preference for the SCG to be deactivated" to no such preference, or vice-versa)

 - the UE cannot report a preference before a certain time after its last report

- the UE preference is valid as long as the RRC connection is not release

- the reporting does not depend whether an SCG is configured or not, and, if configured, it is activated or deactivated

[40] proposes the same except that:

- the preference is either "SCG activated" or "SCG deactivated"

- there is a cause value

- "SCG activated" with cause "uplinkData" is used instead of current uplink data indication for SCG bearer while the SCG is deactivated

However, that proposal does not consider the following scenario:

- the UE indicates a preference of "SCG activation" because there are uplink data for an SCG DRB

- the network activates the SCG and uplink data are transmitted

- as there is no more activity on SCG DRBs, the network deactivates the SCG

- there are uplink data but, since the UE preference is already "SCG activation", the UE cannot report it again

So this proposal is not feasible as it is.

[35] proposes:

- the network configures the UE to provide a preference for SCG deactivation

- if this is configured, the UE can report a preference "deactivated", "activated" or "released"

- the UE can report the preference even if it has not changed

- no prohibit timer

Since there is no time for any further study, the rapporteur suggests that the choice is limited between [10] and [35].

**Q4: Do companies want to specify in Rel-17 a new UE assistance information as summarized above for [10] or [35]?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/NoPreference between [10] and [35] | Comments |
|  |  |  |

# 3 Conclusion

# 4 References

[1] R2-2202248, How to model the PSCell in SCG deactivation?, OPPO

[2] R2-2202250, SCG deactivation indication when resuming from RRC\_INACTIVE due to MO data, OPPO

[3] R2-2202280 QoS flow remapping during SCG deactivation Fujitsu

[4] R2-2202575 Discussion on UE behavior with SCG deactivated Lenovo, Motorola Mobility

[5] R2-2202649 Discussion on UE behaviour when SCG is deactivated ZTE Corporation, Sanechips

[6] R2-2202679 Views on several issues Samsung Electronics

[7] R2-2202680 DC power sharing for deactivated SCG Samsung Electronics

[8] R2-2202705 UE behaviour while SCG is deactivated Qualcomm Incorporated

[9] R2-2202756 UE behavior while the SCG is deactivated InterDigital, Inc.

[10] R2-2202767 Deactivation of SCG LG Electronics Finland

[11] R2-2202795 Discussion on UE behaviour while SCG is deactivated vivo

[12] R2-2202919 TA timer and RLM/BFD while the SCG is deactivated MediaTek Inc.

[13] R2-2203097 Discussions on UE Behavior in Deactivated SCG CATT

[14] R2-2203176 Open Issues on UE Behavior NTT DOCOMO INC.

[15] R2-2203184 UE behaviour while SCG is deactivated Nokia, Nokia Shanghai Bell

[16] R2-2203375 Open issues on UE behaviours while the SCG is deactivated Huawei, HiSilicon

[17] R2-2203390 UE behaviour while SCG is deactivated Ericsson

[18] R2-2202247 L2 based SCG activation and SCG RRM OPPO

[19] R2-2202281 Proposal for releasing statusReportRequired for SCG bearers at SCG deactivation Fujitsu

[20] R2-2202282 Remaining issues on UL data arrival for SCG Fujitsu

[21] R2-2202351 Futher discussion on actions at SCG activation or deactivation Transsion Holdings

[22] R2-2202413 Discussion on activation and deactivation of SCG Spreadtrum Communications

[23] R2-2202576 MAC related issues upon SCG activation and deactivation Lenovo, Motorola Mobility

[24] R2-2202650 Activation of deactivated SCG ZTE Corporation, Sanechips

[25] R2-2202701 Actions at SCG activation and deactivation Qualcomm Incorporated

[26] R2-2202757 Deactivation of SCG InterDigital, Inc.

[27] R2-2202758 Activation of SCG InterDigital, Inc.

[28] R2-2202796 Discussion on actions at SCG activation and deactivation vivo

[29] R2-2202809 Remaining issues on SCG deactivation NEC

[30] R2-2203039 Remaining issues for MAC procedure in deactivated SCG SHARP Corporation

[31] R2-2203061 split bearer handling upon SCG deactivation Sharp

[32] R2-2203087 Open issues on SCG deactivation DENSO CORPORATION

[33] R2-2203092 Discussion on partial MAC reset upon SCG deactivation LG Electronics Inc.

[34] R2-2203098 Remaining Issues on Actions at SCG Activation and Deactivation CATT

[35] R2-2203099 Discussion on RRC Aspects of SCG Deactivation CATT

[36] R2-2203166 Discussion on data transmission to MN for split bearer LG Electronics Inc.

[37] R2-2203177 Open Issues on SCG Activation and Deactivation NTT DOCOMO INC.

[38] R2-2203185 UL data handling at SCG deactivation Nokia, Nokia Shanghai Bell

[39] R2-2203186 Actions at SCG activation and deactivation Nokia, Nokia Shanghai Bell

[40] R2-2203391 Actions at SCG activation and deactivation Ericsson

[41] R2-2203376 Handling of uplink split bearers and BWP when the SCG deactivated Huawei, HiSilicon