**3GPP TSG-RAN WG2 Meeting #117 R2-220xxxx**

**Electronic Meeting, February 21 – March 3, 2022**

**Agenda item:** 8.11.2.2

**Source:** InterDigital Inc.

**Title:** Email discussion Report on [AT117-e][630][POS] Remaining proposals on RRC\_INACTIVE (InterDigital)

**Document for:**  Discussion

# 1. Introduction

This document summarizes the following email discussion:

* [AT117-e][630][POS] Remaining proposals on RRC\_INACTIVE (InterDigital)

Scope:

* Discuss P8 and P10 of R2-2203524 and attempt to reach consensus.
* Check the LS in R2-2202166 and determine if there is impact to our specs.

Intended outcome: Report to Monday CB session

Deadline: Friday 2022-02-25 1200 UTC

**Deadline for initial comments (companies inputs/views):** Thursday 2022-02-24 1200 UTC;

**Deadline for further comments (mainly for further discussion on LS from RAN4):** Friday 2022-02-25 1200 UTC

Please provide the contact information in the following Table:

|  |  |  |
| --- | --- | --- |
| **Company** | **Point of contact** | **Email address** |
| vivo | Xiang Pan | panxiang@vivo.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 2. Discussion

The scope of this email discussion is to discuss the potential remaining issues related to positioning in RRC\_INACTIVE which are identified in the following documents:

* [1] R2-2203524, Email discussion Report on [Pre117-e][609][POS] Open issues on positioning in RRC\_INACTIVE (InterDigital)
* [2] R2-2202166, LS on DRX cycle used in PRS measurement in RRC\_INACTIVE state

## 2.1 TA Timer associated with SRSp

During the pre-meeting open issues discussion [1], vivo indicated the following open issue:

|  |  |  |
| --- | --- | --- |
| **Company** | **Open Issue** | **Comments** |
| vivo | Whether the inactivePosSRS-TAT will be restarted when a Timing Advance Command is received during SDT. | In the running CR, the inactivePosSRS-TAT can be restarted only when the configuration for inactivePosSRS-TAT is received. However, the CG-SDT TAT will be restarted when a Timing Advance Command MAC CE is received. We are wondering whether the solutions shall be aligned. |

Based on the comments from vivo, the following proposal was formulated in [1] for further discussion:

“**Proposal 8: TA Timer for SRS for positioning is restarted upon reception of TA command in RRC\_INACTIVE state”**

In a contribution from Oppo (R2-2202338 [3]), it was indicated that for positioning in RRC\_INACTIVE state, a TA command may also be received if an SDT procedure has been initiated. It was also mentioned in [3] that RAN2 has agreed that the SRSp configuration is considered as invalid if TA is not valid, and that since the TA is available upon reception TA command, it is straightforward to restart the SRS TA timer for SRS configuration maintenance.

The agreement made in SDT WI during RAN2#113e for restarting the TAT-SDT, which may be relevant for positioning, is as follows:

**Agreements**

1. TAT-SDT is started upon receiving the TAT-SDT configuration from gNB, i.e. RRCrelease message, and can be (re)started upon reception of TA command.

In this regard, the following is to be discussed:

**Question 1: Do companies agree to follow SDT solution that the TA timer associated with SRS for positioning (SRSp) is restarted upon reception of TA command in RRC INACTIVE?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| vivo | Yes | Prefer to align with CG-SDT as it’s beneficial to maintain the SRS. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 RRC message for providing SRSp configuration in RRC\_INACTIVE

During the pre-meeting open issues discussion [1], Oppo indicated the following open issue:

|  |  |  |
| --- | --- | --- |
| **Company** | **Open Issue** | **Comments** |
| OPPO | Whether SRS for positioning in RRC\_INACTIVE state can be configured through RRC reconfiguration message. | Currently, SRS configuration can be carried in either RRC reconfiguration message or RRC release message, and both of the RRC message types have not been excluded based on the agreements made in positioning session.  Meanwhile, SDT has made the restriction on the RRC message that supported during an SDT procedure, that is, no RRCReconfiguration and RRCReconfigurationComplete are allowed during SDT session.  As positioning in RRC\_INACTIVE relies on the SDT for positioning related message transmission, it is suggested to align positioning agreements with SDT, i.e. SRS for positioning in RRC\_INACTIVE state can only be configured through RRC release message. |

Based on the comments from Oppo, the following proposal was formulated in [1] for further discussion:

**“Proposal 10: SRS for positioning in RRC\_INACTIVE state can only be configured through RRC release message”**

In a contribution from Oppo (R2-2202338 [3]), it was also indicated that SRS for positioning in RRC\_INACTIVE state can be configured through the following ways as agreed in previous positioning meeting. It was mentioned in [3] that for SDT DL message, it is not clear which RRC message is used according to the agreements. Also in [3], it was indicated that currently SRS configuration can be carried in either RRC reconfiguration message or RRC release message, and both of the RRC message types have not been excluded based on the agreements made in positioning session.

The relevant positioning agreement made during RAN2#116-e is as follows:

Agreement:

Proposal 6: SRS for positioning in RRC\_INACTIVE state can be configured through the following ways:

- RRCRelease with SuspendConfig (13/13)

- SDT DL RRC message, i.e. Msg B / Msg 4 of RA-SDT (9/13)

During RAN2#116bis-e, the following agreement was made in SDT WI on the RRC message that is supported during an SDT procedure:

**Agreement**

RRCReconfiguration and RRCReconfigurationComplete are not supported during an SDT session

For clarifying the previous agreement above in positioning and whether to align the positioning agreement with SDT agreement, the following is to be discussed:

**Question 2: Do companies agree to follow SDT solution that SRS for positioning (SRSp) in RRC\_INACTIVE state can only be configured through RRC Release message (i.e. RRCReconfiguration and RRCReconfigurationComplete are not used for configuring SRSp)?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| vivo | Yes | Follow the restriction of SDT, and no need to enhance SDT at this stage. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 RAN4 LS: DRX cycle used in PRS measurement in RRC\_INACTIVE state

During RAN2#117-e, an LS (R4-2202686 [2]) was received from RAN4, indicating the following RAN4 agreement regarding UE requirements for NR positioning measurements performed while the UE is in RRC\_INACTIVE state:

|  |  |
| --- | --- |
| |  | | --- | | Agreement   * DRX cycle should be considered in the positioning measurement delay requirements in RRC\_INACTIVE state. |   RAN4 also observes that DRX cycle may be different in different cells. RAN4 is further discussing the impact of DRX cycle on positioning measurement delay requirements under cell reselection in RRC\_INACTIVE state.  RAN4 respectfully asks RAN2 and RAN3 to take into account the above agreements and observations, and to determine if there would be any impact on their specifications, including potential impact to signalling. |

In RAN2#117-e under AI 8.11.2.2 (RRC\_INACTIVE), there were no contributions submitted to describe the relationship between DRX cycle and positioning measurement delay requirements in RRC\_INACTIVE state or relevant solutions. The moderator would like to open the discussion to collect company inputs with the following question:

**Question 3: Do companies think that the agreement made in RAN4 described in R4-2202686 [2] has an impact on stage 2/stage 3 specification. If your answer is “yes”, please explain the details of specification impacts.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| vivo | Yes | The LMF shall send the QoS requirement (e.g., response time) to gNB, and gNB may decide whether release the UE to RRC\_INACTIVE based on the DRX cycle and delay requirement.  However, the above solution is in the RAN3 scope. If RAN3 will introduce the enhancement, RAN2 can further discuss whether there is stage 2 impact. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 4 Summary

The following is the summary containing the proposals derived from the discussion above:

**Potentially easy to agree**

**Need further discussion**

# 5 Reference

1. R2-2203524, Email discussion Report on [Pre117-e][609][POS] Open issues on positioning in RRC\_INACTIVE (InterDigital)
2. R2-2202166, LS on DRX cycle used in PRS measurement in RRC\_INACTIVE state
3. R2-2202338, Open issues on positioning in RRC\_INACTIVE state, Oppo, Feb 2022
4. R1-2202523, Feature Lead Summary#1 for E-mail Discussion [108-e-NR-ePos-06], Intel, Feb 2022
5. RAN2 chairman notes RAN2#114-e, May 2021
6. RAN2 chairman notes RAN2#116-e, Nov 2021
7. RAN2 chairman notes RAN2#116bis-e, Jan 2022