3GPP TSG-RAN WG2 #117-e Tdoc R2-220XXXX

Electronic meeting, Feb 21st – Mar 3rd, 2022

Agenda Item: 8.12.2.2.1

Source: Ericsson (Rapporteur)

Title: Email discussion report for [Pre117-e][105][RedCap] CP open issues

Document for: Discussion, Decision

# 1 Introduction

In RAN2#116bis-e, it was agreed to have post email discussions after the meeting to update the running CRs based on the agreements made during the meeting and to identify the remaining open issues. The open issues were then captured in a document with the intention to determine which issues are to be handled via Pre-RAN2#117 offline discussion(s) and which others are to be handled based on company contributions.

In this document, the discussion continues based on the list of open issues captured in [R2-2201887](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201887.zip) and [R2-2201889](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201889.zip) as the outcome of the related offline discussions after RAN2#116bis-e regarding TS 38.331 and TS 38.304, respectively.

Contact information

|  |  |
| --- | --- |
| Company | Contact person - email@address.com |
| OPPO | Haitao (lihaitao@oppo.com) |
| CATT | Xiangdong zhang (zhangxiangdong@catt.cn) |
| Nokia | Jussi-Pekka Koskinen (jussi-pekka.koskinen@nokia.com) |
| Apple | Naveen Palle (naveen.palle@apple.com) |
| Ericsson | Emre A. Yavuz (emre.yavuz@ericsson.com) |
|  |  |
|  |  |

# 2 Discussion

## 2.1 Identification, access and camping restrictions

In RAN2#116bis-e, UE behaviour for the following cases were discussed but no conclusion was made:

1. the cell does not indicate support for RedCap UEs
2. Red Cap UE is unable to acquire SIB1
3. *cellBarred* in MIB is set

For i. and ii. the following options have been proposed:

1. UE considers IFRI as “allowed”
2. UE follows the IFRI in MIB

**Q 2.1.1** Assuming that common UE behaviour is preferred for cases i. and ii. above, which option do you prefer? Please elaborate your reply and comment especially if you think that UE behaviour should be different for cases i. and ii.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option****(a or b)** | **Comments** |
| OPPO | a |  |
| CATT | a |  |
| Nokia | b | It seems obvious there is a reason for NW to set IFRI as “not allowed” |
| Apple | a | i and ii can be from different cases (for eg., NW deployment differences) and common UE behavior might not be the best for both i and ii, but we are ok to go with common approach, as ultimately it’s chipset vendor’s implementation when it comes to the cell search in such cases  |
| Ericsson | b | It is important that RedCap UEs follow the legacy behavior where possible. If a (legacy) cell indicates that the cell is barred and that intra-frequency reselection is not allowed, this must also be respected by RedCap UEs particularly since UEs that may end up operating in a non-best cell, may impact network performance severly. The same should apply when it is not possible for a RedCap UE to camp in a cell due to lack support for RedCap. Note that failing to acquire SIB1 could be a sign that the cell supports only EN-DC (NSA). So, also in this case the UE should not reselect to another cell on the same carrier unless it is allowed. |
|  |  |  |
|  |  |  |

**Summary – Q 2.1.1**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

For iii. above, i.e., *cellBarred* in MIB is set to barred, the following options have been proposed:

1. UE follows legacy IFRI in MIB
2. UE acquires SIB1 and follows the RedCap-specific IFRI provided in SIB1

**Q 2.1.2** Which option do you prefer for case iii. above? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option****(a or b)** | **Comments** |
| OPPO | b |  |
| CATT | b | That is the reason to define Redcap-specific IFRI. |
| Nokia | b first, then a | If SIB1 does not provide RedCap-specific IFRI or the UE cannot acquire SIB1, the legacy IFRI is followed. |
| Apple | b | Same comment as CATT |
| Ericsson | a | As explained above for the previous question, it is important that RedCap UEs follow the legacy behavior where possible. If MIB indicates that the cell is barred, regardless of whether SIB1 indicates support for RedCap, the RedCap UE, as others, is not allowed to camp in the cell and thus should follow the legacy IFRI in MIB. |
|  |  |  |
|  |  |  |

**Summary – Q 2.1.2**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

In RAN2#116bis-e the following working assumption was made:

|  |
| --- |
| **Working assumption**:System information can provide information on which frequencies accept RedCap UE access (e.g. by considering whether supporting RedCap). |

The proposal was supported by many companies, yet a working assumption was made since a few companies preferred support for providing information also on cell level and few others think that this is an optimization that adds complexity with no significant gain.

**Q 2.1.3** Do you agree that the working assumption can be confirmed? Please comment especially if you do not agree and elaborate about the signalling aspects of the solution you propose, i.e., how such information can be provided, in which SIB etc.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | See comments | We don’t think it is efficient to indicate RedCap’s access support per frequency. With this, if one neighbor cell within the frequency does not accept RedCap UE’s access, network has to set the whole frequency as not accepting RedCap UE’s access, which will prevent RedCap UE from reselecting to those RedCap-supporting neighbor cells. We think the RedCap-supporting information should be indicated via a cell list.  |
| CATT | Yes | In SIB4 |
| Nokia | Yes |  |
| Apple | Yes with comments | We tend to agree with Oppo for an “optional” cell-list as well (i.e., not limit to freq alone).Also, as discussed below, there can be other access limiting factors: HD-FDD operation, 1Rx/2Rx barring etc, and it’s better to have these in SIB3/4 for the Ncells. Maybe define an ASN.1 structure in SIB1 for redcap, and that can be reused in cell-list of SIB3/4. |
| Ericsson | No (and not per cell either) | We do not think this is essential functionality. It is an optimization, and gains are not significant given the increased SI overhead (also for legacy UEs) and complexity. Therefore, this should not be prioritized in Rel-17. Regarding the proposals about providing such information per cell rather than per frequency; this would increase the SI overhead and complexity further with still no significant gain. We do not think the scenario where one or some cells do not support RedCap on a certain frequency as opposed to the rest is a realistic deployment case. |
|  |  |  |
|  |  |  |

**Summary – Q 2.1.3**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

RAN2 has agreed to introduce means for the network to control UEs with, for example, 1 Rx branch to access the network in order to avoid any impact on the performance. It has been agreed in RAN1 that a capability bit on Half-duplex FDD operation type A for RedCap UEs is introduced, therefore a similar mechanism, which indicates that HD-FDD is supported in the serving cell, may need to be introduced especially considering that half-duplex (HD) in FDD bands is not supported in NR prior to the RedCap feature. Note that supporting HD-FDD in the network may require quite large implementation effort and thus it would be beneficial to have an indication for HD-FDD to facilitate early support of FD-FDD RedCap UEs.

**Q 2.1.4** Do you think that support for Half-Duplex FDD RedCap should be indicated in SIB1? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | No | HD-FDD operation is RRC connected state feature. We think this can handled by the UE capability and connection management, e.g. if NW does not support HD-FDD, it can send UE to idle state. |
| Nokia | No |  |
| Apple | Yes |  |
| Ericsson | Yes | It is essential that UEs that omit basic legacy functionality (e.g., full-duplex FDD operation) do not enter a legacy cell. The procedures captured in the running CR so far do not ensure that! |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.1.4**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

## 2.2 eDRX

In RAN2#115-e, the following was agreed:

“RAN2 considers the configuration as an invalid case, where INACTIVE eDRX cycle is configured but IDLE eDRX cycle is not configured. FFS whether to capture this restriction in RAN2 spec”

**Q 2.2.1** Do you think that the case for invalid configuration should be captured in the specs? Please elaborate your reply and, if you agree, provide your opinion on how and where it should be captured.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes | It can be captured in the field description of INACTIVE eDRX cycle in 38.331. |
| CATT | Yes | The restriction for configuration of inactive eDRX should be added in the spec, by adding in the field description of the INACTIVE eDRX cycle that it can only be configured when the idle eDRX is configured for the UE, otherwise it should be absent. |
| Nokia | Yes | This can be captured in Stage-2 |
| Apple | Yes | Same view as Oppo |
| Ericsson | Yes | One option can be to capture those in the form of a table. |
|  |  |  |
|  |  |  |

**Summary – Q 2.2.1**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

In RAN2#115-e, the following was agreed:

“RAN2 considers the configuration as invalid case, where INACTIVE eDRX cycle is longer than IDLE eDRX cycle. FFS whether to capture this restriction in RAN2 spec.”

**Q 2.2.2** Do you think that the case for invalid configuration should be captured in the specs? Please elaborate your reply and provide your opinion regarding how and where it should be captured.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes | It can be captured in the field description of INACTIVE eDRX cycle in 38.331. |
| CATT | Yes | Similar with the answer of 2.2.1, it can be specified in the field description of the INACTIVE eDRX cycle that its value should be no longer than the ldle eDRX cycle. |
| Nokia | Yes | Stage-2 |
| Apple | Yes | Same view as Oppo |
| Ericsson | Yes | Same suggestion as above. |
|  |  |  |
|  |  |  |

**Summary – Q 2.2.2**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

The following note is captured in subclause 5.2.2.2.2 on “SI change indication and PWS notification” in the running CR for TS 38.331:

“Editor’s Note: The details for modification period, eDRX acquisition period and which eDRX/DRX cycles are referred to below are subject to further changes once relevant agreements are made.”

The following options have been considered regarding which DRX cycle UE should consider for comparing with the modification period to decide if eDRX acquisition period is used.:

1. CN\_eDRX for both RRC\_IDLE and RRC\_INACTIVE (same as LTE)
2. CN\_eDRX for RRC\_IDLE, and RAN eDRX, if configured, for RRC\_INACTIVE, i.e., use CN\_eDRX if RAN eDRX is not configured.

**Q 2.2.3** Which option do you prefer? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option****(a or b)** | **Comments** |
| OPPO | b with modification | For UE in RRC INACTIVE, since UE would always monitor for RAN paging based on RAN eDRX if configured for RRC\_INACTIVE or RAN DRX if RAN eDRX is not configured, we think it would be better to use RAN eDRX (if RAN eDRX is configured) or RAN DRX (if RAN eDRX is not configured) to compare with the modification period.The proposed option b-bis:CN\_eDRX for RRC\_IDLE, and RAN eDRX, if configured, for RRC\_INACTIVE, i.e., use RAN DRX if RAN eDRX is not configured. |
| CATT | a | We think it is fine to align with LTE which is also the simplest solution. |
| Nokia | b | Agree with OPPO |
| Apple | a | We agreed to this already…? |
| Ericsson | a | We prefer to follow LTE to make the implementation simple and straightforward especially since this would make the SI change indication mechanism simpler, i.e., legacy mechanism can be used. |
|  |  |  |
|  |  |  |

**Summary – Q 2.2.3**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

The following note is captured in subclause 5.2.2.2.2 on “SI change indication and PWS notification” in the running CR for TS 38.331:

“Editor’s Note: The case for RRC\_INACTIVE is FFS”

**Q 2.2.4** Please provide your preference regarding the case for RRC\_INACTIVE considering the procedure in subclause 5.2.2.2.2.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Depending on the outcome of Q 2.2.3, the procedure text should be added for RRC\_INACTIVE case. |
| CATT | It depends on the answer of Q2.2.3, if option a is adopted, for RRC inactive state, if the idle eDRX cycle longer than the modification period and the *systemInfoModification-eDRX* bit of Short Message is set, UE shall apply the SI acquisition procedure.An example of the modification on the spec as following:1. if the UE is ~~in RRC\_IDLE,~~ configured with an eDRX cycle longer than the modification period and the *systemInfoModification-eDRX* bit of Short Message is set:

2> apply the SI acquisition procedure as defined in sub-clause 5.2.2.3 from the start of the next eDRX acquisition period boundary. |
| Apple | Same view as CATT |
| Ericsson | This depends on the outcome of Q.2.2.3. We prefer to use the same mechanism for both RRC\_IDLE and RRC\_INACTIVE and adopt the text from LTE in principle. |
|  |  |
|  |  |
|  |  |

**Summary – Q 2.2.4**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

The following note is captured as part of the ASN.1 coding for the *RRCRelease* message in the running CR for TS 38.331:

ExtendedPagingCycle-r17 ::= ENUMERATED {rf256, rf512, rf1024, spare1} -- Editor's note: TBD how many spare values are needed.

Only one spare value is available currently, but more may be required for forward compatibility.

**Q 2.2.5** Please provide your preference regarding the number of spare values needed and motivate why.

|  |  |  |
| --- | --- | --- |
| **Company** | **# of spare values** | **Comments** |
| OPPO | 1 | But no strong view. |
| CATT | Slightly prefer 1 in R-17 | Even considering the inactive eDRX cycle extension beyond 10.24, the maximum inactive eDRX cycle would also need to be discussed, so the number of the spare bits is not clear. Anyway, if extension is needed in the future, an ExtendedPagingCycle-r18 can be introduced. |
| Nokia | 1 | Should suffice as we can add a new IE in a later release if more values required. |
| Apple | No strong view, but ok with 1 for R17 |  |
| Ericsson | See the comment | We prefer to have a number of spare values enough for at least the include the possible values for idle mode. |
|  |  |  |
|  |  |  |

**Summary – Q 2.2.5**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

The following note is captured in subclause 7.x on “Paging in extended DRX” in the running TS 38.304 CR:

The PH for CN is the H-SFN satisfying the following equations:

H-SFN mod TeDRX\_CN= (UE\_ID\_H mod TeDRX\_CN), where

- UE\_ID\_H

- xx most significant bits of the Hashed ID.

Editor’s note: FFS how many bits we use above for UE\_ID\_H.

- TeDRX\_CN: UE-specific eDRX cycle in Hyper-frames, (TeDRX\_CN = 2, …, 1024 Hyper-frames) configured by upper layers.

**Q 2.2.6** Please indicate your preference regarding the number of most significant bits that should be used for UE\_ID\_H? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **# of bits** | **Comments** |
| OPPO | 12 | To align with NB-IoT. |
| CATT | 12 | In LTE the UE\_ID\_H is defined as follows:- UE\_ID\_H:- 10 most significant bits of the Hashed ID, if P-RNTI is monitored on PDCCH or MPDCCH- 12 most significant bits of the Hashed ID, if P-RNTI is monitored on NPDCCHAnd in LTE the range of the eDRX cycle is as follows:- T eDRX,H : eDRX cycle of the UE in Hyper-frames, (TeDRX,H =1, 2, …, 256 Hyper-frames) (for NB-IoT, TeDRX,H =2, …, 1024 Hyper-frames) and configured by upper layers.We can see the eDRX cycle can be up to 1024HSFN in LTE NB-IoT which aligns with NR, so 12 bits used for UE\_ID\_H can similarly be used for NR |
| Nokia | 12 | Same as LTE. |
| Apple | 12 | To align with LTE |
| Ericsson | 10 | Same as in LTE (Note that “same as LTE” would mean 10 not 12 and NPDCCH refers to NB-IoT not LTE) |
|  |  |  |
|  |  |  |

**Summary – Q 2.2.6**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

## 2.3 RRM relaxations

The following note was captured in the procedural part of the “Relaxed measurement criterion for a stationary UE” in the subclause 5.7.4.X in the running CR for TS 38.331:

5.7.4.X Relaxed measurement criterion for a stationary UE

The relaxed measurement criterion for a stationary UE is fulfilled when:

- (SrxlevRefStationaryConnected – Srxlev) < SSearchDeltaP-StationaryConnected,

Where:

- Srxlev = current Srxlev value of the PCell cell (dB).

- SrxlevRefStationaryConnected = reference Srxlev value of the PCell cell (dB), set as follows:

- After MAC of an MCG successfully completes a Random Access procedure after applying an *reconfigurationWithSync* in *spCellConfig* of an MCG, or

Editor's Note: The above bullet and how to capture the case if RRM relaxation is not configured at the time of handover is TBD.

- If (Srxlev – SrxlevRefStationaryConnected) > 0, or

- If the relaxed measurement criterion has not been met for TSearchDeltaP-StationaryConnected:

- The UE shall set the value of SrxlevRefStationaryConnected to the current Srxlev value of the serving cell.

**Q 2.3.1** Please provide your preference regarding the following bullet

“After MAC of an MCG successfully completes a Random Access procedure after applying an *reconfigurationWithSync* in *spCellConfig* of an MCG,”

and how to capture the case if RRM relaxation is not configured at the time of handover.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | We understand this relates to initiation of SrxlevRefStationaryConnected, but we think handover is not the only case which needs to be addressed. To us, following cases are relelvant:Case 1: configuration (first time) of RRM relaxationIn this case, initiation of SrxlevRefStationaryConnected shoud be specified.Case 2: handoverIn this case, handover command may not explicitly include RRM relaxation (e.g. delta configuation), but UE should still set the initial value of SrxlevRefStationaryConnected. |
| CATT | If the RRM relaxation is not configured for the UE by the target gNB for handover case, the UE shall not perform the evaluation of the Relaxed measurement criterion for a stationary UE, i.e. the UE shall not perform the procedural text of 5.7.4.X |
| Nokia | We agree with CATT |
| Ericsson |  |
|  |  |
|  |  |
|  |  |

**Summary – Q 2.3.1**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

The following note was captured in the subclause 5.2.4.9.0 on “Relaxed measurement rules” in the running CR for TS 38.304:

Editor's note: When the network configures both R16/R17 relaxation criteria and the UE fulfils both, it is TBD if the UE performs Rel-17 RRM relaxation method or it is up to UE implementation to select either Rel-16 or Rel-17 relaxation operation.

The following options have been considered when the network configures both R16/R17 relaxation criteria and the UE fulfils both:

1. UE performs Rel-17 RRM relaxation method
2. it is up to UE implementation to perform either Rel-16 or Rel-17 relaxation method

**Q 2.3.2** Which option do you prefer? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option****(a or b)** | **Comments** |
| OPPO | A | But b is also ok. |
| CATT |  | No strong view, both can work.Option a can bring more power saving, but option b can leave more flexibility for UE. |
| Nokia |  | Both works |
| Apple | B |  |
| Ericsson |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.3.2**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

Regarding the same case above, Rel-16 low mobility and Rel-17 stationary criteria are evaluated based on independent *Tsearch* periods, which may have different durations and therefore the evaluations can be out of synch. It has been observed that typically a UE considers one criterion fulfilled first while still waiting for the other to conclude. Based on the current text, the UE may simply proceed with the RRM relaxation actions related to the first criterion fulfilled. The UE may wait for the measurement period of the second criterion to conclude, but it is possible that the UE does not end up in a state where both criteria are fulfilled at the same time.

**Q 2.3.3** Do you agree with the assessment above? Please elaborate your reply and provide comments regarding how to capture the UE behaviour especially if you reply “Yes”.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes |  |
| CATT | Yes | One option is to make the stationary criterion has higher priority if configured by NW, i.e. UE should first check whether stationary criterion is fulfilled, it means the evaluation time shouldn’t less than the Tsearch for stationary criterion. If the stationary criterion is not fulfilled, UE should evaluate the low mobility criterion.Or it can be left to UE implementation. |
| Nokia | Yes |  |
| Apple | Yes | Can be left to UE impl, but expect that UE follows the specified procedure |
| Ericsson |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.3.3**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

## 2.4 NCD-SSB

For further discussion regarding the configuration of SSBs and the corresponding measurement objects, possible deployment and configuration variants should be considered. The rapporteur takes the variants listed in [R4-2201780](http://www.3gpp.org/ftp//tsg_ran/WG4_Radio/TSGR4_101-bis-e/Docs//R4-2201780.zip) as reference for this discussion.

*RedCap UE's BWP contains CD SSB*

When the network configures a RedCap to use the Cell-defining (CD) SSB, it can do so using BWP#0 or a dedicated BWP, e.g., BWP#1 in the example below. In this case, the CD-SSB can be used for all purposes including serving- and neighbour cell measurements. Hence, an NCD-SSB is not required and not configured for this UE.



**Figure 1.** **RedCap UE operating on dedicated BWP that contains the CD-SSB**

*RedCap UE’s BWP does not contain CD-SSB*

In this case the NW configures the NCD-SSB in UE’s dedicated BWP. There are two scenarios to consider:

1. All neighbour cells send SSBs on UE’s NCD-SSB frequency
2. Some neighbour cells do not send SSBs on UE’s NCD-SSB frequency

In scenario a)., RedCap UEs may measure serving- and neighbour cells on NCD-SSB frequency which requires no measurement gaps. UEs measure (neighbour) cells according to the configured Measurement Object (*MeasObj*).



**Figure 2. RedCap UE operating on dedicated BWP that does not contain the CD-SSB - all neighbour cells broadcast their SSB on the UE's NCD-SSB frequency**

The rapporteur observes two possible approaches for this scenario:

1. UE can follow the legacy principles, i.e., it would configure an MO on the NCD-SSB frequency (but no gaps) and associate necessary report configurations (e.g., A3, A2, ...).
2. instead of configuring a *MeasObj* on the NCD-SSB frequency explicitly, RAN2 could specify that a UE that is configured with a dedicated BWP that contains an NCD-SSB should perform serving- and neighbour cell measurements on the NCD-SSB instead of on the CD-SSB, i.e., the UE would re-interpret the *MeasObj* based on the given NCD-SSB configuration.

In case RAN2 follows the first approach, rapporteur thinks that the following should be considered: whether the network should also configure a MO on CD-SSB and, if not, whether the network should set the *servingCellMO* to the ID of the NCD-SSB.

In scenario b), where some neighbour cells do not send an SSB on UE’s NCD-SSB frequency, measurements should be done on the CD-SSB frequency, otherwise, the UE may end up in a neighbour cell without noticing it and without providing a corresponding measurement report to its serving gNB.



**Figure 3. RedCap UE operating on dedicated BWP that does not contain the CD-SSB - some neighbour cells do NOT broadcast their SSB on the UE's NCD-SSB frequency**

Even though it may be a rare case, rapporteur thinks that it would be better if the network configures the *MeasObj* and suitable measurement configurations on the CD-SSB frequency as shown in Figure 3 above. In this case configuring a *MeasObj* on the NCD-SSB frequency appears unnecessary for the sole purpose of performing serving cell measurements and all information about the NCD-SSB would be given in the serving cell configuration (either explicitly or inherited from the CD-SSB configuration).

In case RAN2 follows the 1st approach above, the rapporteur would like to ask companies the following two questions:

**Q 2.4.1** Do you think the network should configure a MO on the NCD-SSB if it wants the UE to perform neighbour cell measurements thereon (as in legacy)? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes |  |
| CATT | Yes | As in legacy |
| Nokia |  | Legacy principles can naturally be applied. |
| Apple | We do not see the need | As long as it is clear to the UE and the NW that the UE will have to use NCD-SSB for serving cell measurements, when in that BWP, then either explicit MO config (scenario 1) or UE internal translation of meas obj (scenario 2) serve the same purpose.For Ncell measurement, then the NW would know if the UE needs gaps or not (based on intra-freq or not) and in scenario b, the NW has to configure gaps to the UE.The key is that NW and the UE are both in sync, on which BWP the UE is operating in.We think it’s simpler to not explicitly configure MOs, rather just use scenario 2 (UE assumes that MO is now based on NCD-SSB)… But we are open to a less complicated approach. |
| Ericsson | Yes | This is the legacy behavior and allows supporting all relevant scenarios (e.g., measurements only on NCD-SSB without gaps; measurements on CD-SSB with gaps). |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.1**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

**Q 2.4.2** Do you think that the network should also configure MO on CD-SSB even if it does not expect the UE to perform neighbour measurements thereon? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO |  | We think this may be up to network’s implementation. |
| CATT | See my comments | If the NW doesn’t expect the UE to perform neighbor measurement on the CD-SSB, the NW doesn’t need to configure MO on CD-SSB.But currently, the field description about servingCellMO in the 38331is as following:*measObjectId* of the *MeasObjectNR* in *MeasConfig* which is associated to the serving cell. For this *MeasObjectNR*, the following relationship applies between this MeasObjectNR and *frequencyInfoDL* in *ServingCellConfigCommon* of the serving cell: if *ssbFrequency* is configured, its value is the same as the *absoluteFrequencySSB* and if *csi-rs-ResourceConfigMobility* is configured, the value of its *subcarrierSpacing* is present in one entry of the *scs-SpecificCarrierList*, *csi-RS-CellListMobility* includes an entry corresponding to the serving cell (with *cellId* equal to *physCellId* in *ServingCellConfigCommon*) and the frequency range indicated by the *csi-rs-MeasurementBW* of the entry in *csi-RS-CellListMobility* is included in the frequency range indicated by in the entry of the *scs-SpecificCarrierList*.If the NW wants to configure the servingCellMO to associate with the CD-SSB, the NW can configure a MO on CD-SSB.So it is up to NW to decide to configure MO on CD-SSB. |
| Nokia |  | Up to NW. |
| Ericsson | No | The NW could omit the MO on the CD-SSB if it does not want the UE to measure neighbor cells on that frequency. But of course the network may decide to configure it like any other MO on any other frequency. |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.2**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

**Q 2.4.3** Regarding the discussion on scenario b), do you think the network should configure a MO on the NCD-SSB frequency if it wants the UE to use it only for serving cell measurements? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes |  |
| CATT | No | In currently,UE and NW assume the measurement on the servingCellMO to be the measurement of the serving cell. If no further enhancement needed, MO on the NCD-SSB for serving cell measurements is not needed.In legacy, activated BWP may be a BWP which is not including CD-SSB, currently the servingCellMO is used for serving cell measurement. Of course it is up to NW implementation to decide whether to configure one MO to assoicate with the NCD-SSB or CSI-RS. |
| Nokia |  | Up to NW. |
| Ericsson | No | When configured with the NCD-SSB, UE has all required information to measure its serving cell’s SSB thereon. A general statement, as follows, seems sufficient: “A UE operating on a BWP for which a NCD-SSB is configured shall use it for all purposes for which it would otherwise have used the CD-SSB (sync, serving cell measurements, …)” |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.3**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

**Q 2.4.4** If you replied with “Yes” to the previous question, do you think that the network should refer to this MO explicitly from within the *ServingCell* configuration (similarly to servingCellMO)? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes |  |
| Ericsson | No | We tend to agree with other companies’ views raised in the previous meeting that such additional explicit cross-reference is technically not needed and complicates the configuration. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.4**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

*RedCap UE’s BWP contains neither CD-SSB nor NCD-SSB*

The network’s configuration should follow the previous case above, i.e., network will configure the *servingCellMO* to the MO on the CD-SSB.

**Q 2.4.5** Regarding scenario a); which approach do you prefer? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **1 or 2** | **Comments** |
| OPPO | Neither | Network should configure an MO on the CD-SSB frequency. |
| CATT | 1 | Follow the legacy |
| Nokia |  | Legacy principles. |
| Apple | 1 | Follow the legacy |
| Ericsson |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.5**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

*Non-overlapping BWPs*

If the UE supports DCI-based BWP-switching, the network could configure different NCD-SSB in different non-overlapping dedicated BWPs (only one NCD-SSB per BWP!) as depicted below.



Figure 4. RedCap UE configured with several non-overlapping BWPs
that contain different NCD-SSBs.

In this scenario the UE may always use the SSB in its currently active BWP. If all neighbour nodes are known to send the same SSBs, the UE may measure serving- and neighbour cells on the NCD-SSB frequency. To achieve that, the network should configure MOs and report configurations on each NCD-SSB frequency of the UE. However, the NW does not need to configure gaps.

Assuming that the NCD-SSB is configured in the *BWP-DownlinkDedicated* anyway, the rapporteur observes that RRC signalling offers the possibility to configure a UE with several NCD-SSB. Note that if this is not meant to be allowed, a restriction should be specified.

**Q 2.4.6** Do you think that such configuration should be allowed? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes | Several BWP-DownlinkDedicated containing NCD-SSB. |
| CATT | Yes | It is up to NW implementation to configure MO associated with different SSB. No restriction is needed. |
| Nokia | Yes | No need to restrict. |
| Apple | Yes | Should be allowed irrespective of the MO discussion. |
| Ericsson | Yes (probably) | As said above, configuring different NCD-SSBs in different BWPs (no more than one NCD-SSB per BWP!!) does not require changes in the ASN.1 structure. A UE that supports DCI-based BWP switching should also be able to acquire and use a different SSB when changing the BWP (as it does when switching from the initial BWP to the dedicated BWP with NCD-SSB). And it allows the network to spread the RedCap load on a wide carrier. However, if hidden challenges are identified we are also fine to restrict the configuration to at most one NCD-SSB per UE’s serving cell. |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.6**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

**Q 2.4.7** If it is allowed to configure several NCD-SSBs, Which MO should be set in *servingCellMO*? Any of the NCD-SSBs? Or the CD-SSB? Or none, since the UE can derive it anyway? Please elaborate your reply.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | The NCD-SSB contained in the current active BWP. |
| CATT | As legacy *servingCellMO* should associated with the MO configured with CD-SSB if the MO assoicated with SSB.*measObjectId* of the *MeasObjectNR* in *MeasConfig* which is associated to the serving cell. For this *MeasObjectNR*, the following relationship applies between this MeasObjectNR and *frequencyInfoDL* in *ServingCellConfigCommon* of the serving cell: if *ssbFrequency* is configured, its value is the same as the *absoluteFrequencySSB* and if *csi-rs-ResourceConfigMobility* is configured, the value of its *subcarrierSpacing* is present in one entry of the *scs-SpecificCarrierList*, *csi-RS-CellListMobility* includes an entry corresponding to the serving cell (with *cellId* equal to *physCellId* in *ServingCellConfigCommon*) and the frequency range indicated by the *csi-rs-MeasurementBW* of the entry in *csi-RS-CellListMobility* is included in the frequency range indicated by in the entry of the *scs-SpecificCarrierList*. |
| Nokia | Up to NW. |
| Apple | Scenario 2 from the first NCD-SSB question, the UE and NW remap the serving cell MO to the NCD-SSB, without explicit config. |
| Ericsson | There is no need to mandate one specific SSB. As discussed on Q 2.4.3 and 2.4.4 network may need to configure MOs on CD-SSB or NCD-SSB or both. Configuring at least one of them as *servingCellMO* (in the legacy field) should be sufficient. |
|  |  |
|  |  |

**Summary – Q 2.4.7**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

*Other aspects*

In RAN2#116bis-e the following working assumption was made:

|  |
| --- |
| **Working assumption**:The periodicity of NCD-SSB shall be not less than the periodicity of serving cell’s CD-SSB. |

**Q 2.4.8** Do you agree that the working assumption can be confirmed? Please comment especially if you do not agree.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes |  |
| CATT | Yes |  |
| Nokia | Yes |  |
| Apple | Yes, and | As expressed earlier, we like to keep the NCD-SSB and CD-SSB periodicity the same. Also helps with MO discussion ☺..  |
| Ericsson | Yes |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.8**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

**Q 2.4.9** Do you think it should be possible to use NCD-SSB to trigger the handover procedure? If so, in which field should it be indicated? How should *ServingCellConfigCommon*-> *absoluteFrequencySSB* be set in this case? Still to the CD-SSB?” Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | No | UE will read MIB in the target, for which NCD-SSB should not be indicated. |
| CATT |  | Triggering of handover is up to NW implementation.I think this question should be “whether it should be possibleto use measurement on the NCD-SSB as the serving cell measurement”. It depends on whether the *servingCellMO* canbe associated with the CD-SSB. |
| Nokia |  | NW can trigger HO based on any information. |
| Apple | Yes, and  | This can be another reason to remap the MO to NCD-SSB implicitly then explicit config. And also same view as CATT |
| Ericsson |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.9**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

**Q 2.4.10** Do you think a non-RedCap UE should be able to use NCD-SSB instead of CD-SSB with an optional capability? Please elaborate your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO |  | No strong view. For simplicity, we can focus on RedCap UEs in Rel-17. |
| CATT |  | It is allowed to configure MO to associated with NCD-SSB in current spec. |
| Nokia |  | It should already be allowed. |
| Apple |  | Not essential now. |
| Ericsson |  |  |
|  |  |  |
|  |  |  |

**Summary – Q 2.4.10**

TBD

Based on the observations above, the rapporteur proposes the following:

1. ???

# 3 Conclusion

Based on the discussion above rapporteur suggests a discussion on the following proposals:

[Proposal 1 ???](#_Toc93533244)

# References

1. [R2-2201886](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201886.zip) Running 331 CR for RedCap Ericsson
2. [R2-2201887](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201887.zip) Open issue list for 38.331 for RedCap Ericsson
3. [R2-2201888](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201888.zip) Running 304 CR for RedCap Ericsson
4. [R2-2201889](http://ftp.3gpp.org/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201889.zip) Open issue list for 38.304 for RedCap Ericsson
5. [R4-2201780](http://www.3gpp.org/ftp//tsg_ran/WG4_Radio/TSGR4_101-bis-e/Docs//R4-2201780.zip) Discussion on the use of NCD-SSB MediaTek