**3GPP TSG-RAN Meeting #118-e *draft-***

**Electronic Meeting, 9 - 20 May 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.306** | **CR** |  | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Clarification on the applicability of mixed numerology on UE capability *maxNumberCSI-RS-RRM-RS-SINR* |
|  |  |
| ***Source to WG:*** | Apple, Inc. |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_CSIRS\_L3meas |  | ***Date:*** | 2022-04-25 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In R4-2205655**,** RAN4 made the below agreement that for the case of mixed numerology: *the number of CSI-RS resources in any duration that equals to the length of a slot is no larger than UE capability maxNumberCSI-RS-RRM-RS-SINR*the number of CSI-RS resources in any duration that equals to the length of a slot is no larger than UE capability *maxNumberCSI-RS-RRM-RS-SINR*.* When there are mixed numerologies, the length of a slot is defined based on the smallest SCS

As per the LS R2-2204472, the definition of the UE capability *maxNumberCSI-RS-RRM-RS-SINR* needs to be clarified reflecting this. |
|  |  |
| ***Summary of change:*** | Clarify that for the case of mixed numerologies, the slot is defined based on the smallest SCS of all active BWPs across all carriers.**Impact Analysis**Impacted 5G architecture options:NR SA, NR-DC, (NG)EN-DC, NE-DCImpacted functionality:UE radio capabilityInter-operability:1. If the UE is implemented according to the CR and the NW is not, the definition of length of slot is not aligned and may result in overconfiguration of CSI resources by the network exceeding UE capability, which can potentially lead to a connection failure.
2. If the network is implemented according to the CR and the UE is not, there is no inter-operability issue.
 |
|  |  |
| ***Consequences if not approved:*** | TS 38.306 remains unclear on the time duration of a slot for the interpretation of *maxNumberCSI-RS-RRM-RS-SINR* when mixed numerologies are in use. |
|  |  |
| ***Clauses affected:*** | 4.2.9 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Unchaged sections are omitted>

### 4.2.9 *MeasAndMobParameters*

| Definitions for parameters | Per | M | FDD-TDD DIFF | FR1-FR2 DIFF |
| --- | --- | --- | --- | --- |
| ***cli-RSSI-Meas-r16***Indicates whether the UE can perform CLI RSSI measurements as specified in TS 38.215 [13] and supports periodical reporting and measurement event triggering as specified in TS 38.331 [9]. If the UE supports this feature, the UE needs to report *maxNumberCLI-RSSI-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measurement resources to be measured. | UE | No | TDD only | Yes |
| ***cli-SRS-RSRP-Meas-r16***Indicates whether the UE can perform SRS RSRP measurements as specified in TS 38.215 [13] and supports periodical reporting and measurement event triggering based on SRS-RSRP as specified in TS 38.331 [9]. If the UE supports this feature, the UE needs to report *maxNumberCLI-SRS-RSRP-r16* and *maxNumberPerSlotCLI-SRS-RSRP-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measurement resources to be measured. | UE | No | TDD only | Yes |
| ***concurrentMeasGap-r17***Indicates whether the UE supports the concurrent measurement gap as specified in TS 38.133 [5] including support of more than 1 per-UE measurement gap configurations. For UE capable of Rel-15 per-FR gap (*independentGapConfig*), this field indicates whether the UE supports more than 1 per-FR gap measurement gap configurations in an FR, or simultaneous 1 per UE measurement gap plus 1 per-FR measurement gap configurations in an FR, or more than 1 per-UE measurement gap configurations. | UE | No | No | No |
| ***condHandoverFDD-TDD-r16***Indicates whether the UE supports conditional handover between FDD and TDD cells. The parameter can only be set if *condHandover-r16* is set for at least one FDD band and one TDD band. The UE that indicates support of this feature shall also indicate support of *handoverFDD-TDD*. | UE | No | No | No |
| ***condHandoverFR1-FR2-r16***Indicates whether the UE supports conditional handover HO between FR1 and FR2. The parameter can only be set if *condHandover-r16* is set for at least one FR1 band and one FR2 band. The UE that indicates support of this feature shall also indicate support of *handoverFR1-FR2*. | UE | No | No | No |
| ***csi-RS-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of CSI-RS as specified in TS 38.213 [11] and TS 38.133 [5]. This parameter needs FR1 and FR2 differentiation. If the UE supports this feature, the UE needs to report *maxNumberResource-CSI-RS-RLM*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RS-RLM-r16* applies. | UE | Yes | No | Yes |
| ***csi-RSRP-AndRSRQ-MeasWithSSB***Indicates whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured with an associated SS/PBCH. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RS-RLM-r16* applies. | UE | No | No | Yes |
| ***csi-RSRP-AndRSRQ-MeasWithoutSSB***Indicates whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured for a cell that transmits SS/PBCH block and without an associated SS/PBCH block. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RSRP-AndRSRQ-MeasWithoutSSB-r16* applies. | UE | No | No | Yes |
| ***csi-SINR-Meas***Indicates whether the UE can perform CSI-SINR measurements based on configured CSI-RS resources as specified in TS 38.215 [13]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponding to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-SINR-Meas-r16* applies. | UE | No | No | Yes |
| ***eutra-AutonomousGaps-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when MR-DC is not configured.  | UE | No | No | No |
| ***eutra-AutonomousGaps-NEDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NE-DC is configured. | UE | No | No | No |
| ***eutra-AutonomousGaps-NRDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NR-DC is configured. | UE | No | No | No |
| ***eutra-CGI-Reporting***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. It is mandated if the UE supports EUTRA. It is optional for RedCap UEs. | UE | CY | No | No |
| ***eutra-CGI-Reporting-NEDC***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when theNE-DCis configured. | UE | No | No | No |
| ***eutra-CGI-Reporting-NRDC***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when theNR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. | UE | No | No | No |
| ***eventA-MeasAndReport***Indicates whether the UE supports NR measurements and events A triggered reporting as specified in TS 38.331 [9]. This field only applies to SN configured measurement when (NG)EN-DC is configured. For NR SA, MN and SN configured measurement when NR-DC is configured, and MN configured measurement when NE-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | No |
| ***eventB-MeasAndReport***Indicates whether the UE supports EUTRA measurement and event B triggered reporting as specified in TS 38.331 [9]. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***handoverLTE-5GC, handoverLTE-5GC-r17***Indicates whether the UE supports HO to EUTRA connected to 5GC. It is mandated if the UE supports EUTRA connected to 5GC. | UE | CY | Yes | Yes(Incl FR2-2 DIFF) |
| ***handoverFDD-TDD***Indicates whether the UE supports HO between FDD and TDD. It is mandated if the UE supports both FDD and TDD. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. UEs supporting this shall indicate support of *handoverInterF* for both FDD and TDD. | UE | Yes | No | No |
| ***handoverFR1-FR2***Indicates whether the UE supports HO between FR1 and FR2. Support is mandatory for the UE supporting both FR1 and FR2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. UEs supporting this shall indicate support of *handoverInterF* for both FR1 and FR2. | UE | Yes | No | No |
| ***handoverFR1-FR2-2-r17***Indicates whether the UE supports HO between FR1 and FR2-2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover) and PSCell change when (NG)EN-DC/NR-DC is configured. UEs supporting this shall indicate support of *handoverInterF* for both FR1 and FR2-2. | UE | No | No | No |
| ***handoverFR2-1-FR2-2-r17***Indicates whether the UE supports HO between FR2-1 and FR2-2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover) and PSCell change when (NG)EN-DC/NR-DC is configured. UEs supporting this shall indicate support of *handoverInterF* for both FR2-1 and FR2-2. | UE | No | No | No |
| ***handoverInterF, handoverInterF-r17***Indicates whether the UE supports inter-frequency HO. It indicates the support for inter-frequency HO from the corresponding duplex mode and from frequency range indicated to be supported as described in Annex B. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | Yes(Incl FR2-2 DIFF) |
| ***handoverLTE-EPC, handoverLTE-EPC-r17***Indicates whether the UE supports HO to EUTRA connected to EPC. It is mandated if the UE supports EUTRA connected to EPC. | UE | CY | Yes | Yes(Incl FR2-2 DIFF) |
| ***idleInactiveNR-MeasReport-r16, idleInactiveNR-MeasReport-r17***Indicates whether the UE supports configuration of NR SSB measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 [9]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes(Incl FR2-2 DIFF) |
| ***idleInactiveNR-MeasBeamReport-r16***Indicates whether the UE supports beam level measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding beam measurement results upon network request as specified in TS 38.331 [9]. A UE supports this feature shall also support *idleInactiveNR-MeasReport-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***idleInactiveEUTRA-MeasReport-r16***Indicates whether the UE supports configuration of E-UTRA measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 [9]. | UE | No | No | No |
| ***idleInactive-ValidityArea-r16***Indicates whether the UE supports configuration of a validity area for NR measurements in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.331 [9]. | UE | No | No | No |
| ***independentGapConfig***This field indicates whether the UE supports two independent measurement gap configurations for FR1 and FR2 specified in clause 9.1.2 of TS 38.133 [5]. The field also indicates whether the UE supports the FR2 inter-RAT measurement without gaps when (NG)EN-DC is not configured. | UE | No | No | No |
| ***independentGapConfigPRS-r17***Indicates whether the UE supports two independent measurement gap configurations for FR1 and FR2 for PRS measurement, as specified in clause 9.1.2 of TS 38.133 [5]. | UE | No | No | No |
| ***intraAndInterF-MeasAndReport***Indicates whether the UE supports NR intra-frequency and inter-frequency measurements and at least periodical reporting. This field only applies to SN configured measurement when (NG)EN-DC is configured. For NR SA, MN and SN configured measurement when NR-DC is configured, and MN configured measurement when NE-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | No |
| ***interFrequencyMeas-NoGap-r16***Indicates whether the UE can perform inter-frequency SSB based measurements without measurement gaps if the SSB is completely contained in the active BWP of the UE as specified in TS 38.133 [5]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of cells to be measured. | UE | No | No | Yes |
| ***periodicEUTRA-MeasAndReport***Indicates whether the UE supports periodic EUTRA measurement and reporting. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***maxNumberCLI-RSSI-r16***Defines the maximum number of CLI-RSSI measurement resources for CLI RSSI measurement. If the UE supports *cli-RSSI-Meas-r16*, the UE shall report this capability. | UE | CY | TDD only | No |
| ***maxNumberCLI-SRS-RSRP-r16***Defines the maximum number of SRS-RSRP measurement resources for SRS-RSRP measurement. If the UE supports *cli-SRS-RSRP-Meas-r16*, the UE shall report this capability.NOTE 1: A slot is based on minimum SCS among active BWPs across all CCs configured for SRS-RSRP measurement.NOTE 2: A SRS resource occasion that overlaps with the slot is counted as one measurement resource in the slot. | UE | CY | TDD only | No |
| ***increasedNumberofCSIRSPerMO-r16***Indicates support of up to 192 CSI-RS resource for L3 mobility configuration per measurement object configured with *associatedSSB*. | UE | No | No | Yes |
| ***maxNumberCSI-RS-RRM-RS-SINR***Defines the maximum number of CSI-RS resources for RRM and RS-SINR measurement across all measurement frequencies per slot. If UE supports any of *csi-RSRP-AndRSRQ-MeasWithSSB*, *csi-RSRP-AndRSRQ-MeasWithoutSSB*, and *csi-SINR-Meas*, UE shall report this capability.NOTE: A slot is based on minimum SCS among all measurement frequencies configured for RRM and RS-SINR measurement. | UE | CY | No | No |
| ***maxNumberPerSlotCLI-SRS-RSRP-r16***Defines the maximum number of SRS-RSRP measurement resources per slot for SRS-RSRP measurement. If the UE supports *cli-SRS-RSRP-Meas-r16*, the UE shall report this capability. | UE | CY | TDD only | No |
| ***maxNumberResource-CSI-RS-RLM***Defines the maximum number of CSI-RS resources within a slot per spCell for CSI-RS based RLM. If UE supports any of *csi-RS-RLM* and *ssb-AndCSI-RS-RLM*, UE shall report this capability. | UE | CY | No | Yes |
| ***ncsg-MeasGap-r17***Indicates whether the UE supports the NCSG measurement gap as specified in TS 38.133 [5]. | UE | No | No | No |
| ***ncsg-MeasGapEUTRAN-r17***Indicates whether the UE supports reporting of the NCSG measurement gap for E-UTRA target bands as specified in TS 38.331 [9]. | UE | No | No | No |
| ***nr-AutonomousGaps-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when MR-DC is not configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-ENDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when (NG)EN-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-NEDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NE-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-NRDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NR-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-CGI-Reporting***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. It is optional for RedCap UEs. | UE | Yes | No | No |
| ***nr-CGI-Reporting-ENDC***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the (NG)EN-DC is configured. | UE | Yes | No | No |
| ***reportAddNeighMeasForPeriodic-r16***Defines whether the UE supports periodic reporting of best neighbour cells per serving frequency, as defined in TS 38.331 [9]. It is optional for RedCap UEs. | UE | Yes | No | No |
| ***nr-CGI-Reporting-NEDC***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NE-DC is configured. | UE | Yes | No | No |
| ***nr-CGI-Reporting-NPN-r16***Defines whether the UE supports acquisition of NPN-relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR NPN cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9]. If UE supports NPN, UE shall report this capability. It is optional for RedCap UEs. | UE | CY | No | No |
| ***nr-CGI-Reporting-NRDC***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. | UE | Yes | No | No |
| ***nr-NeedForGap-Reporting-r16***Indicates whether the UE supports reporting the measurement gap requirement information for NR target in the UE response to a network configuration RRC message. | UE | No | No | No |
| ***pcellT312-r16***Indicates whether the UE supports T312 based fast failure recovery for PCell. | UE | No | No | No |
| ***preconfiguredUE-AutonomousMeasGap-r17***Indicates whether the UE supports the preconfigured measurement gap with UE-autonomous mechanism for activation and deactivation as specified in TS 38.133 [5].Editor's Note: current version assume procedure is specify in RAN4 spec. Change is needed according if it will specify in 331. | UE | No | No | No |
| ***preconfiguredNW-ControlledMeasGap-r17***Indicates whether the UE supports the preconfigured measurement gap with network-controlled mechanism for activation and deactivation as specified in TS 38.133 [5].Editor's Note: current version assume procedure is specify in RAN4 spec. Change is needed according if it will specify in 331. | UE | No | No | No |
| ***simultaneousRxDataSSB-DiffNumerology***Indicates whether the UE supports concurrent intra-frequency measurement on serving cell or neighbouring cell and PDCCH or PDSCH reception from the serving cell with a different numerology as defined in clause 8 and 9 of TS 38.133 [5]. | UE | No | No | Yes |
| ***simultaneousRxDataSSB-DiffNumerology-Inter-r16***Indicates whether the UE supports concurrent SSB based inter-frequency measurement without measurement gap on neighbouring cell and PDCCH or PDSCH reception from the serving cell with a different numerology as defined in clause 8 and 9 of TS 38.133 [5]. UE indicates support of this indicates support of *interFrequencyMeas-NoGap-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range where the SSB and PDCCH/PDSCH are received. | UE | No | No | Yes |
| ***sftd-MeasPSCell***Indicates whether the UE supports SFTD measurements between the PCell and a configured PSCell. If this capability is included in UE-MRDC-Capability, it indicates that the UE supports SFTD measurement between PCell and PSCell in (NG)EN-DC. If this capability is included in UE-NR-Capability, it indicates that the UE supports SFTD measurement between PCell and PSCell in NR-DC. | UE | No | Yes | No |
| ***sftd-MeasPSCell-NEDC***Indicates whether the UE supports SFTD measurement between the NR PCell and a configured E-UTRA PSCell in NE-DC. | UE | No | Yes | No |
| ***sftd-MeasNR-Cell***Indicates whether the SFTD measurement with and without measurement gaps between the EUTRA PCell and the NR cells is supported by the UE which is capable of EN-DC/NGEN-DC when EN-DC/NGEN-DC is not configured. The SFTD measurement without gaps can be used when the UE supports at least one EN-DC band combination consisting of the set of the current E-UTRA serving frequencies and the NR frequency where SFTD measurement is configured. In UE-NR-Capability, this field is not used, and UE does not include the field. | UE | No | Yes | No |
| ***sftd-MeasNR-Neigh***Indicates whether the inter-frequency SFTD measurement with and without measurement gaps between the NR PCell and inter-frequency NR neighbour cells is supported by the UE when MR-DC is not configured. The SFTD measurement without gaps can be used when the UE supports at least one DC or CA band combination consisting of the set of the current NR serving frequencies and the NR frequency where SFTD measurement is configured.  | UE | No | Yes | No |
| ***sftd-MeasNR-Neigh-DRX***Indicates whether the inter-frequency SFTD measurement using DRX off period between the NR PCell and the inter-frequency NR neighbour cells is supported by the UE when MR-DC is not configured. | UE | No | Yes | No |
| ***ssb-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of SS/PBCH block as specified in TS 38.213 [11] and TS 38.133 [5]. This field shall be set to *supported*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ssb-RLM-DynamicChAccess-r16* or *ssb-RLM-Semi-StaticChAccess-r16* applies. | UE | Yes | No | No |
| ***ssb-AndCSI-RS-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of SS/PBCH block and CSI-RS as specified in TS 38.213 [11] and TS 38.133 [5]. If the UE supports this feature, the UE needs to report *maxNumberResource-CSI-RS-RLM*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ssb-AndCSI-RS-RLM-r16* applies. | UE | No | No | No |
| ***ss-SINR-Meas***Indicates whether the UE can perform SS-SINR measurement as specified in TS 38.215 [13]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ss-SINR-Meas-r16* applies. | UE | No | No | Yes |
| ***supportedGapPattern***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA, for NR-DC, for NE-DC and for independent measurement gap configuration on FR2 in (NG)EN-DC. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3, as specified in TS 38.133 [5] and so on. The UE shall set the bits corresponding to the measurement gap pattern 13, 14, 17, 18 and 19 to 1 if the UE is an NR standalone capable UE that supports a band in FR2 or if the UE is an (NG)EN-DC capable UE that supports *independentGapConfig* and supports a band in FR2. | UE | CY | No | No |
| ***supportedGapPattern-r16***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA, for NR-DC for PRS measurement and NR/E-UTRA RRM measurement. The leading / leftmost bit (bit 0) corresponds to the gap pattern 24, the next bit corresponds to the gap pattern 25, as specified in TS 38.133 [5]. The applicability of the gap patterns 24 and 25 is defined in clause 9.1.2 of TS 38.133 [5]. A UE that indicates support of this capability shall indicate support of *NR-DL-PRS-ProcessingCapability-r16* defined in TS 37.355 [22]. | UE | No | No | No |
| ***supportedGapPattern-NRonly-r16***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA and NR-DC when the frequencies to be measured within this measurement gap are all NR frequencies. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3 and so on. The UE shall set the bits corresponding to the measurement gap pattern 2, 3 and 11 to 1. | UE | FD | No | No |
| ***supportedGapPattern-NRonly-NEDC-r16***Indicates whether the UE supports gap patterns 2, 3 and 11 in NE-DC when the frequencies to be measured within this measurement gap are all NR frequencies. | UE | No | No | No |

<End of changes>