3GPP TSG-RAN WG3 #107-e R3-201276

**E-meeting, 24th February – 6th March 2020**

Source: CATT

**Title:** **Summary on CB: # 106\_HO\_Timer\_handling**

Agenda Item: 9.3.8.1

Document for: Discussion and decision

# Introduction

This contribution summarizes discussions on the following CB:

**CB: # 106\_HO\_Timer\_handling**

**- check details**

**- make consistent with CHO handling (there timer handling is captured)**

**- further check against CHO handling in Rel-16**

 (CATT)

# Summary

After further check the NGAP baseline CR for Rel-16 mobility enhancement WI, the following paragraph is introduced

*Upon reception of the HANDOVER REQUEST ACKNOWLEDGE message, the source NG-RAN node shall stop the timer TXnRELOCprep and terminate the Handover Preparation procedure. If the procedure was initiated for an immediate handover, the source NG-RAN node shall start the timer TXnRELOCoverall. The source NG-RAN node is then defined to have a Prepared Handover for that Xn UE-associated signalling.*

*Editor’s note: the wording “immediate handover” for legacy HO (i.e. non-CHO) is FFS*

So, in Rel-16, the CR for mobility enhancement WI has already included this timer related description, Rel-16 CR dedicated for this issue is not needed.However,Rel-15 CR is still necessary which could use similar sentence, just remove the words highlight with yellow.

**It is proposed to agree the Rel-15 CR in R3-201275.**

Any comments, please add it here.