3GPP TSG-RAN WG3 Meeting #107-e**R3-200776**

24 – 28 February 2020

**Agenda item:** 19.5

**Source:** Qualcomm Incorporated

**Title:** (TP for NR\_POS BL CR for TS 38.473) F1AP changes to support Exchange of TRP Information

**Document for:** Discussion and Decision

1. Introduction

An LMF needs to be able to request information for TRPs hosted by an NG-RAN node. A running CR to LPP in TS

# 4. Text Proposal for the baseline CR

**>>>> FIRST CHANGE <<<<**

# 8 F1AP procedures

## 8.1 List of F1AP Elementary procedures

[Editor’s Notes: procedures and associated functions require further checking]

In the following tables, all EPs are divided into Class 1 and Class 2 EPs (see subclause 3.1 for explanation of the different classes):

Table 1: Class 1 procedures

|  |  |  |  |
| --- | --- | --- | --- |
| Elementary Procedure | Initiating Message | Successful Outcome | Unsuccessful Outcome |
| Response message | Response message |
| Reset | RESET | RESET ACKNOWLEDGE |  |
| F1 Setup | F1 SETUP REQUEST | F1 SETUP RESPONSE | F1 SETUP FAILURE |
| gNB-DU Configuration Update | GNB-DU CONFIGURATION UPDATE | GNB-DU CONFIGURATION UPDATE ACKNOWLEDGE | GNB-DU CONFIGURATION UPDATE FAILURE |
| gNB-CU Configuration Update | GNB-CU CONFIGURATION UPDATE | GNB-CU CONFIGURATION UPDATE ACKNOWLEDGE | GNB-CU CONFIGURATION UPDATE FAILURE |
| UE Context Setup | UE CONTEXT SETUP REQUEST | UE CONTEXT SETUP RESPONSE | UE CONTEXT SETUP FAILURE |
| UE Context Release (gNB-CU initiated) | UE CONTEXT RELEASE COMMAND | UE CONTEXT RELEASE COMPLETE |  |
| UE Context Modification (gNB-CU initiated) | UE CONTEXT MODIFICATION REQUEST | UE CONTEXT MODIFICATION RESPONSE | UE CONTEXT MODIFICATION FAILURE |
| UE Context Modification Required (gNB-DU initiated) | UE CONTEXT MODIFICATION REQUIRED | UE CONTEXT MODIFICATION CONFIRM | UE CONTEXT MODIFICATION REFUSE |
| Write-Replace Warning  | WRITE-REPLACE WARNING REQUEST | WRITE-REPLACE WARNING RESPONSE |  |
| PWS Cancel | PWS CANCEL REQUEST | PWS CANCEL RESPONSE |  |
| GNB-DU RESOURCE COORDINATION | GNB-DU RESOURCE COORDINATION REQUEST | GNB-DU RESOURCE COORDINATION RESPONSE |  |
| Positioning Information Exchange | POSITIONING INFORMATION REQUEST | POSITIONING INFORMATION RESPONSE | POSITIONING INFORMATION FAILURE |
| TRP Information Exchange | TRP INFORMATION REQUEST | TRP INFORMATION RESPONSE | TRP INFORMATION FAILURE |

Table 2: Class 2 procedures

|  |  |
| --- | --- |
| Elementary Procedure | Message |
| Error Indication | ERROR INDICATION |
| UE Context Release Request (gNB-DU initiated) | UE CONTEXT RELEASE REQUEST |
| Initial UL RRC Message Transfer | INITIAL UL RRC MESSAGE TRANSFER |
| DL RRC Message Transfer | DL RRC MESSAGE TRANSFER |
| UL RRC Message Transfer | UL RRC MESSAGE TRANSFER |
| UE Inactivity Notification  | UE INACTIVITY NOTIFICATION |
| System Information Delivery | SYSTEM INFORMATION DELIVERY COMMAND |
| Paging | PAGING |
| Notify | NOTIFY |
| PWS Restart Indication | PWS RESTART INDICATION |
| PWS Failure Indication | PWS FAILURE INDICATION |
| gNB-DU Status Indication | GNB-DU STATUS INDICATION |
| RRC Delivery Report | RRC DELIVERY REPORT |
| Network Access Rate Reduction | NETWORK ACCESS RATE REDUCTION |
| Positioning Assistance Information Control | POSITIONING ASSISTANCE INFORMATION CONTROL |
| Positioning Assistance Information Feedback | POSITIONING ASSISTANCE INFORMATION FEEDBACK |
| Positioning Measurement Report | POSITIONING MEASUREMENT REPORT |
| Positioning Measurement Termination | POSITIONING MEASUREMENT TERMINATION COMMAND |
| Positioning Measurement Failure Indication | POSITIONING MEASUREMENT FAILURE INDICATION |
| Positioning Measurement Modification | POSITIONING MEASUREMENT MODIFICATION |

**>>>> NEXT CHANGE <<<<**

## 8.x Positioning Procedures

### 8.x.a TRP Information Exchange

#### 8.x.a.1 General

The purpose of the TRP Information Exchange procedure is to allow the gNB-CU to request the gNB-DU to provide detailed information for some or all TRPs hosted by the gNB-DU.

#### 8.x.a.2 Successful Operation



Figure 8.x.a.2-1: TRP Information Exchange procedure, successful operation

The gNB-CU initiates the procedure by sending a TRP INFORMATION REQUEST message. The gNB-DU responds with a TRP INFORMATION RESPONSE message that contains the requested TRP information. If the gNB-CU includes one or more TRPs for the TRP List IE in the TRP INFORMATION REQUEST message, the gNB-DU includes information for all TRPs included for the TRP List IE in the TRP INFORMATION RESPONSE message. If the gNB-CU includes no TRPs for the TRP List IE in the TRP INFORMATION REQUEST message, the gNB-DU includes information for all TRPs hosted by the gNB-DU in the TRP INFORMATION RESPONSE message

#### 8.x.a.3 Unsuccessful Operation



Figure 8.x.a.3-1: TRP Information Exchange procedure, unsuccessful operation

If the gNB-DU cannot provide any of the requested information, the gNB-DU shall respond with a TRP INFORMATION FAILURE message.

**>>>> NEXT CHANGE <<<<**

### 9.2.x Messages for Positioning Procedures

#### 9.2.x.b TRP INFORMATION REQUEST

This message is sent by the gNB-CU to request information for one or more TRPs hosted by a gNB-DU.

Direction: gNB-CU → gNB-DU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| **TRP Information Type** |  | *1 .. <maxnoTRPInfoTypes>* |  |  | EACH | reject |
| >TRP Information Item | M |  | ENUMERATED (arfcn, FFS, …) |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoTRPs | Maximum no. of TRPs in a gNB-DU. Value is 256. |

[Editor’s Note: further details on the IEs are FFS / pending RAN2]

#### 9.2.x.c TRP INFORMATION RESPONSE

This message is sent by a gNB-DU to convey TRP information to the gNB-CU.

Direction: gNB-DU → gNB-CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| **TRP Information List** | M | *1 .. <maxnoTRPs>* |  |  |  |  |
| >TRP Information | M |  | 9.3.1.bb |  |  |  |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoTRPs | Maximum no. of TRPs in a gNB-DU. Value is 256 |

[Editor’s Note: further details on the IEs are FFS / pending RAN2]

#### 9.2.x.d TRP INFORMATION FAILURE

This message is sent by a gNB-DU to indicate that the requested TRP information cannot be provided to the gNB-CU.

Direction: gNB-DU → gNB-CU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.3 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

**>>>> NEXT CHANGE <<<<**

### 9.3.1.aa TRP ID

The *TRP ID* IE is used to identify a TRP uniquely within the gNB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| TRP Identifier | M |  | INTEGER(1..16384,…) | Identifies a TRP within the gNB  |

### 9.3.1.bb TRP Information

The *TRP Information* IE contains information for one TRP within the gNB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| TRP ID | M |  | TRP ID9.3.1.aa |  |
| **TRP Information Type** |  | *1 .. <maxnoTRPInfoTypes>* |  |  |
| >CHOICE TRP *Information Item* | M |  |  |  |
| >>NR ARFCN | M |  | INTEGER (0..3279165) | NR ARFCN |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoTRPInfoTypes | Maximum no of TRP information types that can be requested and reported with one message. Value is FFS. |

[Editor’s Note: further details on the IEs are FFS / pending RAN2]

**>>>> NEXT CHANGE <<<<**

### 9.4.3 Elementary Procedure Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-PDU-Descriptions (0)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 Criticality,

 ProcedureCode

FROM F1AP-CommonDataTypes

 Reset,

 ResetAcknowledge,

 F1SetupRequest,

 F1SetupResponse,

 F1SetupFailure,

 GNBDUConfigurationUpdate,

 GNBDUConfigurationUpdateAcknowledge,

 GNBDUConfigurationUpdateFailure,

 GNBCUConfigurationUpdate,

 GNBCUConfigurationUpdateAcknowledge,

 GNBCUConfigurationUpdateFailure,

 UEContextSetupRequest,

 UEContextSetupResponse,

 UEContextSetupFailure,

 UEContextReleaseCommand,

 UEContextReleaseComplete,

 UEContextModificationRequest,

 UEContextModificationResponse,

 UEContextModificationFailure,

 UEContextModificationRequired,

 UEContextModificationConfirm,

 ErrorIndication,

 UEContextReleaseRequest,

 DLRRCMessageTransfer,

 ULRRCMessageTransfer,

 GNBDUResourceCoordinationRequest,

 GNBDUResourceCoordinationResponse,

 PrivateMessage,

 UEInactivityNotification,

 InitialULRRCMessageTransfer,

 SystemInformationDeliveryCommand,

 Paging,

 Notify,

 WriteReplaceWarningRequest,

 WriteReplaceWarningResponse,

 PWSCancelRequest,

 PWSCancelResponse,

 PWSRestartIndication,

 PWSFailureIndication,

 GNBDUStatusIndication,

 RRCDeliveryReport,

 UEContextModificationRefuse,

 F1RemovalRequest,

 F1RemovalResponse,

 F1RemovalFailure,

 NetworkAccessRateReduction,

 TraceStart,

 DeactivateTrace,

 DUCURadioInformationTransfer,

 CUDURadioInformationTransfer,

 TRPInformationRequest,

 TRPInformationResponse,

 TRPInformationFailure

FROM F1AP-PDU-Contents

 id-Reset,

 id-F1Setup,

 id-gNBDUConfigurationUpdate,

 id-gNBCUConfigurationUpdate,

 id-UEContextSetup,

 id-UEContextRelease,

 id-UEContextModification,

 id-UEContextModificationRequired,

 id-ErrorIndication,

 id-UEContextReleaseRequest,

 id-DLRRCMessageTransfer,

 id-ULRRCMessageTransfer,

 id-GNBDUResourceCoordination,

 id-privateMessage,

 id-UEInactivityNotification,

 id-InitialULRRCMessageTransfer,

 id-SystemInformationDeliveryCommand,

 id-Paging,

 id-Notify,

 id-WriteReplaceWarning,

 id-PWSCancel,

 id-PWSRestartIndication,

 id-PWSFailureIndication,

 id-GNBDUStatusIndication,

 id-RRCDeliveryReport,

 id-F1Removal,

 id-NetworkAccessRateReduction,

 id-TraceStart,

 id-DeactivateTrace,

 id-DUCURadioInformationTransfer,

 id-CUDURadioInformationTransfer,

 id-tRPInformationExchange

**\*\* skip unchanged asn \*\***

F1AP-ELEMENTARY-PROCEDURES-CLASS-1 F1AP-ELEMENTARY-PROCEDURE ::= {

 reset |

 f1Setup |

 gNBDUConfigurationUpdate |

 gNBCUConfigurationUpdate |

 uEContextSetup |

 uEContextRelease |

 uEContextModification |

 uEContextModificationRequired |

 writeReplaceWarning |

 pWSCancel |

 gNBDUResourceCoordination |

 f1Removal |

 tRPInformationExchange,

 ...

}

**\*\* skip unchanged asn \*\***

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**\*\* skip unchanged asn \*\***

cUDURadioInformationTransfer F1AP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE CUDURadioInformationTransfer

 PROCEDURE CODE id-CUDURadioInformationTransfer

 CRITICALITY ignore

}

tRPInformationExchange F1AP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE TRPInformationRequest

 SUCCESSFUL OUTCOME TRPInformationResponse

 UNSUCCESSFUL OUTCOME TRPInformationFailure

 PROCEDURE CODE id-tROInformationExchange

 CRITICALITY reject

}

END

-- ASN1STOP

**>>>> NEXT CHANGE <<<<**

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for F1AP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 Candidate-SpCell-Item,

 Cause,

 Cells-Failed-to-be-Activated-List-Item,

 Cells-Status-Item,

 Cells-to-be-Activated-List-Item,

 Cells-to-be-Deactivated-List-Item,

 CellULConfigured,

 CriticalityDiagnostics,

 C-RNTI,

 CUtoDURRCInformation,

 DRB-Activity-Item,

 DRBID,

 DRBs-FailedToBeModified-Item,

 DRBs-FailedToBeSetup-Item,

 DRBs-FailedToBeSetupMod-Item,

 DRB-Notify-Item,

 DRBs-ModifiedConf-Item,

 DRBs-Modified-Item,

 DRBs-Required-ToBeModified-Item,

 DRBs-Required-ToBeReleased-Item,

 DRBs-Setup-Item,

 DRBs-SetupMod-Item,

 DRBs-ToBeModified-Item,

 DRBs-ToBeReleased-Item,

 DRBs-ToBeSetup-Item,

 DRBs-ToBeSetupMod-Item,

 DRXCycle,

 DRXConfigurationIndicator,

 DUtoCURRCInformation,

 EUTRANQoS,

 ExecuteDuplication,

 FullConfiguration,

 GNB-CU-UE-F1AP-ID,

 GNB-DU-UE-F1AP-ID,

 GNB-DU-ID,

 GNB-DU-Served-Cells-Item,

 GNB-DU-System-Information,

 GNB-CU-Name,

 GNB-DU-Name,

 InactivityMonitoringRequest,

 InactivityMonitoringResponse,

 LowerLayerPresenceStatusChange,

 NotificationControl,

 NRCGI,

 NRPCI,

 UEContextNotRetrievable,

 Potential-SpCell-Item,

 RAT-FrequencyPriorityInformation,

 ResourceCoordinationTransferContainer,

 RRCContainer,

 RRCContainer-RRCSetupComplete,

 RRCReconfigurationCompleteIndicator,

 SCellIndex,

 SCell-ToBeRemoved-Item,

 SCell-ToBeSetup-Item,

 SCell-ToBeSetupMod-Item,

 SCell-FailedtoSetup-Item,

 SCell-FailedtoSetupMod-Item,

 ServCellIndex,

 Served-Cell-Information,

 Served-Cells-To-Add-Item,

 Served-Cells-To-Delete-Item,

 Served-Cells-To-Modify-Item,

 ServingCellMO,

 SRBID,

 SRBs-FailedToBeSetup-Item,

 SRBs-FailedToBeSetupMod-Item,

 SRBs-Required-ToBeReleased-Item,

 SRBs-ToBeReleased-Item,

 SRBs-ToBeSetup-Item,

 SRBs-ToBeSetupMod-Item,

 SRBs-Modified-Item,

 SRBs-Setup-Item,

 SRBs-SetupMod-Item,

 TimeToWait,

 TransactionID,

 TransmissionActionIndicator,

 UE-associatedLogicalF1-ConnectionItem,

 DUtoCURRCContainer,

 PagingCell-Item,

 SItype-List,

 UEIdentityIndexValue,

 GNB-CU-TNL-Association-Setup-Item,

 GNB-CU-TNL-Association-Failed-To-Setup-Item,

 GNB-CU-TNL-Association-To-Add-Item,

 GNB-CU-TNL-Association-To-Remove-Item,

 GNB-CU-TNL-Association-To-Update-Item,

 MaskedIMEISV,

 PagingDRX,

 PagingPriority,

 PagingIdentity,

 Cells-to-be-Barred-Item,

 PWSSystemInformation,

 Broadcast-To-Be-Cancelled-Item,

 Cells-Broadcast-Cancelled-Item,

 NR-CGI-List-For-Restart-Item,

 PWS-Failed-NR-CGI-Item,

 RepetitionPeriod,

 NumberofBroadcastRequest,

 Cells-To-Be-Broadcast-Item,

 Cells-Broadcast-Completed-Item,

 Cancel-all-Warning-Messages-Indicator,

 EUTRA-NR-CellResourceCoordinationReq-Container,

 EUTRA-NR-CellResourceCoordinationReqAck-Container,

 RequestType,

 PLMN-Identity,

 RLCFailureIndication,

 UplinkTxDirectCurrentListInformation,

 SULAccessIndication,

 Protected-EUTRA-Resources-Item,

 GNB-DUConfigurationQuery,

 BitRate,

 RRC-Version,

 GNBDUOverloadInformation,

 RRCDeliveryStatusRequest,

 NeedforGap,

 RRCDeliveryStatus,

 ResourceCoordinationTransferInformation,

 Dedicated-SIDelivery-NeededUE-Item,

 Associated-SCell-Item,

 IgnoreResourceCoordinationContainer,

 PagingOrigin,

 UAC-Assistance-Info,

 RANUEID,

 GNB-DU-TNL-Association-To-Remove-Item,

 NotificationInformation,

 TraceActivation,

 TraceID,

 Neighbour-Cell-Information-Item,

 SymbolAllocInSlot,

 Slot-Configuration-Item,

 NumDLULSymbols,

 AdditionalRRMPriorityIndex,

 DUCURadioInformationType,

 CUDURadioInformationType,

 Transport-Layer-Addresses-Info,

 TRP-ID,

 TRP-List,

 TYPE TRP-Information-Type,

 TRP-Information-List

**\*\* skip unchanged asn \*\***

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CU-DU Radio Information Transfer ELEMENTARY PROCEDURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CU-DU Radio Information Transfer

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

CUDURadioInformationTransfer ::= SEQUENCE {

 protocolIEs ProtocolIE-Container {{ CUDURadioInformationTransferIEs}},

 ...

}

CUDURadioInformationTransferIEs F1AP-PROTOCOL-IES ::= {

 { ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

 { ID id-CUDURadioInformationType CRITICALITY ignore TYPE CUDURadioInformationType PRESENCE mandatory },

 ...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRP INFORMATION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TRPInformationRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container {{TRPInformationRequest-IEs}},

 ...

}

TRPInformationRequest-IEs F1AP-PROTOCOL-IES ::= {

 { ID id-tRP-List CRITICALITY ignore TYPE TRP-List PRESENCE optional}|

 { ID id-tRP-Information-Type-Group CRITICALITY reject TYPE TRP-Information-Type PRESENCE mandatory},

 ...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRP INFORMATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TRPInformationResponse ::= SEQUENCE {

 protocolIEs ProtocolIE-Container {{TRPInformationResponse-IEs}},

 ...

}

TRPInformationResponse-IEs F1AP-PROTOCOL-IES ::= {

 { ID id-tRP-Information-List CRITICALITY ignore TYPE TRP-Information-List PRESENCE mandatory}|

 { ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

 ...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- TRP INFORMATION FAILURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

TRPInformationFailure ::= SEQUENCE {

 protocolIEs ProtocolIE-Container {{TRPInformationFailure-IEs}},

 ...

}

TRPInformationFailure-IEs F1AP-PROTOCOL-IES ::= {

 { ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory}|

 { ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

 ...

}

END

-- ASN1STOP

**>>>> NEXT CHANGE <<<<**

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-gNB-CUSystemInformation,

 id-HandoverPreparationInformation,

 id-TAISliceSupportList,

 id-RANAC,

 id-BearerTypeChange,

 id-Cell-Direction,

 id-Cell-Type,

 id-CellGroupConfig,

 id-AvailablePLMNList,

 id-PDUSessionID,

 id-ULPDUSessionAggregateMaximumBitRate,

 id-DC-Based-Duplication-Configured,

 id-DC-Based-Duplication-Activation,

 id-Duplication-Activation,

 id-DLPDCPSNLength,

 id-ULPDCPSNLength,

 id-RLC-Status,

 id-MeasurementTimingConfiguration,

 id-DRB-Information,

 id-QoSFlowMappingIndication,

 id-ServingCellMO,

 id-RLCMode,

 id-ExtendedServedPLMNs-List,

 id-ExtendedAvailablePLMN-List,

 id-DRX-LongCycleStartOffset,

 id-SelectedBandCombinationIndex,

 id-SelectedFeatureSetEntryIndex,

 id-Ph-InfoSCG,

 id-latest-RRC-Version-Enhanced,

 id-RequestedBandCombinationIndex,

 id-RequestedFeatureSetEntryIndex,

 id-RequestedP-MaxFR2,

 id-DRX-Config,

 id-UEAssistanceInformation,

 id-PDCCH-BlindDetectionSCG,

 id-Requested-PDCCH-BlindDetectionSCG,

 id-BPLMN-ID-Info-List,

 id-NotificationInformation,

 id-TNLAssociationTransportLayerAddressgNBDU,

 id-portNumber,

 id-AdditionalSIBMessageList,

 id-IgnorePRACHConfiguration,

 id-CG-Config,

 id-Ph-InfoMCG,

 id-AggressorgNBSetID,

 id-VictimgNBSetID,

 id-MeasGapSharingConfig,

 id-systemInformationAreaID,

 id-areaScope,

 maxNRARFCN,

 maxnoofErrors,

 maxnoofBPLMNs,

 maxnoofBPLMNsNRminus1,

 maxnoofDLUPTNLInformation,

 maxnoofNrCellBands,

 maxnoofULUPTNLInformation,

 maxnoofQoSFlows,

 maxnoofSliceItems,

 maxnoofSIBTypes,

 maxnoofSITypes,

 maxCellineNB,

 maxnoofExtendedBPLMNs,

 maxnoofAdditionalSIBs,

 maxnoofUACPLMNs,

 maxnoofUACperPLMN,

 maxCellingNBDU,

 maxnoofTLAs,

 maxnoofGTPTLAs,

 maxnoTRPs,

 maxnoTRPInfoTypes

**\*\* skip unchanged asn \*\***

-- T

FiveGS-TAC ::= OCTET STRING (SIZE(3))

Configured-EPS-TAC ::= OCTET STRING (SIZE(2))

TDD-Info ::= SEQUENCE {

 nRFreqInfo NRFreqInfo,

 transmission-Bandwidth Transmission-Bandwidth,

 intendedTDD-DL-ULConfig IntendedTDD-DL-ULConfig OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { {TDD-Info-ExtIEs} } OPTIONAL,

 ...

}

TDD-Info-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TimeToWait ::= ENUMERATED {v1s, v2s, v5s, v10s, v20s, v60s, ...}

TNLAssociationUsage ::= ENUMERATED {

 ue,

 non-ue,

 both,

 ...

}

TraceActivation ::= SEQUENCE {

 traceID TraceID,

 interfacesToTrace InterfacesToTrace,

 traceDepth TraceDepth,

 traceCollectionEntityIPAddress TransportLayerAddress,

 iE-Extensions ProtocolExtensionContainer { {TraceActivation-ExtIEs} } OPTIONAL

}

TraceActivation-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TraceDepth ::= ENUMERATED {

 minimum,

 medium,

 maximum,

 minimumWithoutVendorSpecificExtension,

 mediumWithoutVendorSpecificExtension,

 maximumWithoutVendorSpecificExtension,

 ...

}

TraceID ::= OCTET STRING (SIZE(8))

TransportLayerAddress ::= BIT STRING (SIZE(1..160, ...))

TransactionID ::= INTEGER (0..255, ...)

Transmission-Bandwidth ::= SEQUENCE {

 nRSCS NRSCS,

 nRNRB NRNRB,

 iE-Extensions ProtocolExtensionContainer { { Transmission-Bandwidth-ExtIEs} } OPTIONAL,

 ...

}

Transmission-Bandwidth-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

Transport-UP-Layer-Addresses-Info-To-Add-List ::= SEQUENCE (SIZE(1.. maxnoofTLAs)) OF Transport-UP-Layer-Addresses-Info-To-Add-Item

Transport-UP-Layer-Addresses-Info-To-Add-Item ::= SEQUENCE {

 iP-SecTransportLayerAddress TransportLayerAddress,

 gTPTransportLayerAddressesToAdd GTPTLAs OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { Transport-UP-Layer-Addresses-Info-To-Add-ItemExtIEs } } OPTIONAL

}

Transport-UP-Layer-Addresses-Info-To-Add-ItemExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

Transport-UP-Layer-Addresses-Info-To-Remove-List ::= SEQUENCE (SIZE(1.. maxnoofTLAs)) OF Transport-UP-Layer-Addresses-Info-To-Remove-Item

Transport-UP-Layer-Addresses-Info-To-Remove-Item ::= SEQUENCE {

 iP-SecTransportLayerAddress TransportLayerAddress,

 gTPTransportLayerAddressesToRemove GTPTLAs OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { Transport-UP-Layer-Addresses-Info-To-Remove-ItemExtIEs } } OPTIONAL

}

Transport-UP-Layer-Addresses-Info-To-Remove-ItemExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TransmissionActionIndicator ::= ENUMERATED {stop, ..., restart }

TypeOfError ::= ENUMERATED {

 not-understood,

 missing,

 ...

}

Transport-Layer-Addresses-Info ::= SEQUENCE {

 transport-UP-Layer-Addresses-Info-To-Add-List Transport-UP-Layer-Addresses-Info-To-Add-List OPTIONAL,

 transport-UP-Layer-Addresses-Info-To-Remove-List Transport-UP-Layer-Addresses-Info-To-Remove-List OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { Transport-Layer-Addresses-Info-ExtIEs } } OPTIONAL

}

Transport-Layer-Addresses-Info-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TRP-Information-List ::= SEQUENCE (SIZE (1.. maxNoTRPs)) OF SEQUENCE {

 tRP-ID TRP-ID

 tRP-Information TRP-Information,

 iE-Extensions ProtocolExtensionContainer { {TRP-Information-ExtIEs} } OPTIONAL,

 ...

}

TRP-Information-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TRP-Information ::= SEQUENCE (SIZE (1..maxnoTRPInfoTypes)) OF TRP-Information-Item

TRP-Information-Item ::= CHOICE {

 pCI-NR INTEGER (0..1007,...),

 cGI-NGRAN NG-RAN-CGI,

 prs-ID INTEGER (0..255),

 aRFCN INTEGER (0..3279165),

 tRP-Type ENUMERATED (tx-only, rx-only, tx-and-rx. ...),

 pRS-Bandwidth-EUTRA PRS-Bandwidth-EUTRA,

-- other IEs to be added later

}

TRP-Information-Type ::= SEQUENCE (SIZE(1.. maxnoTRPInfoTypes)) OF ProtocolIE-Single-Container { { TRP-Information-TypeIEs} }

TRP-Information-TypeIEs F1AP-PROTOCOL-IES ::= {

 { ID id-TRP-Information-Type-Item CRITICALITY reject TYPE TRP-Information-Type-Item PRESENCE mandatory},

 ...

}

TRP-Information-Type-Item ::= SEQUENCE {

 tRP-Information-Type-Item TRP-Information-Item,

 iE-Extensions ProtocolExtensionContainer { { TRP-Information-Type-ItemExtIEs} } OPTIONAL,

 ...

}

TRP-Information-Item ::= ENUMERATED {

 pci,

 cellid,

 prsid,

 arfcn,

 trptype,

-- other items to be added here

 ...

}

TRP-Information-Type-ItemExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TRP-List ::= SEQUENCE (SIZE (0.. maxNoTRPs)) OF ProtocolIE-Single-Container { {TRP-List-ItemIEs} }

TRP-List-ItemIEs F1AP-PROTOCOL-IES ::= {

 { ID id-TRP-List-Item CRITICALITY reject TYPE TRP-List-Item PRESENCE mandatory}}

TRP-List-Item ::= SEQUENCE {

 tRP-List-Item TRP-ID,

 iE-Extensions ProtocolExtensionContainer { { TRP-List-Item-ExtIEs} } OPTIONAL,

 ...

}

TRP-List-Item-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

TRP-ID ::= INTEGER (1..256, ...)

**\*\* skip unchanged asn \*\***

END

-- ASN1STOP

**>>>> NEXT CHANGE <<<<**

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

F1AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) f1ap (3) version1 (1) f1ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM F1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Reset ProcedureCode ::= 0

id-F1Setup ProcedureCode ::= 1

id-ErrorIndication ProcedureCode ::= 2

id-gNBDUConfigurationUpdate ProcedureCode ::= 3

id-gNBCUConfigurationUpdate ProcedureCode ::= 4

id-UEContextSetup ProcedureCode ::= 5

id-UEContextRelease ProcedureCode ::= 6

id-UEContextModification ProcedureCode ::= 7

id-UEContextModificationRequired ProcedureCode ::= 8

id-UEMobilityCommand ProcedureCode ::= 9

id-UEContextReleaseRequest ProcedureCode ::= 10

id-InitialULRRCMessageTransfer ProcedureCode ::= 11

id-DLRRCMessageTransfer ProcedureCode ::= 12

id-ULRRCMessageTransfer ProcedureCode ::= 13

id-privateMessage ProcedureCode ::= 14

id-UEInactivityNotification ProcedureCode ::= 15

id-GNBDUResourceCoordination ProcedureCode ::= 16

id-SystemInformationDeliveryCommand ProcedureCode ::= 17

id-Paging ProcedureCode ::= 18

id-Notify ProcedureCode ::= 19

id-WriteReplaceWarning ProcedureCode ::= 20

id-PWSCancel ProcedureCode ::= 21

id-PWSRestartIndication ProcedureCode ::= 22

id-PWSFailureIndication ProcedureCode ::= 23

id-GNBDUStatusIndication ProcedureCode ::= 24

id-RRCDeliveryReport ProcedureCode ::= 25

id-F1Removal ProcedureCode ::= 26

id-NetworkAccessRateReduction ProcedureCode ::= 27

id-TraceStart ProcedureCode ::= 28

id-DeactivateTrace ProcedureCode ::= 29

id-DUCURadioInformationTransfer ProcedureCode ::= 30

id-CUDURadioInformationTransfer ProcedureCode ::= 31

id-tRPInformationExchange ProcedureCode ::= x

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxPrivateIEs INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxNRARFCN INTEGER ::= 3279165

maxnoofErrors INTEGER ::= 256

maxnoofIndividualF1ConnectionsToReset INTEGER ::= 65536

maxCellingNBDU INTEGER ::= 512

maxnoofSCells INTEGER ::= 32

maxnoofSRBs INTEGER ::= 8

maxnoofDRBs INTEGER ::= 64

maxnoofULUPTNLInformation INTEGER ::= 2

maxnoofDLUPTNLInformation INTEGER ::= 2

maxnoofBPLMNs INTEGER ::= 6

maxnoofCandidateSpCells INTEGER ::= 64

maxnoofPotentialSpCells INTEGER ::= 64

maxnoofNrCellBands INTEGER ::= 32

maxnoofSIBTypes INTEGER ::= 32

maxnoofSITypes INTEGER ::= 32

maxnoofPagingCells INTEGER ::= 512

maxnoofTNLAssociations INTEGER ::= 32

maxnoofQoSFlows INTEGER ::= 64

maxnoofSliceItems INTEGER ::= 1024

maxCellineNB INTEGER ::= 256

maxnoofExtendedBPLMNs INTEGER ::= 6

maxnoofUEIDs INTEGER ::= 65536

maxnoofBPLMNsNRminus1 INTEGER ::= 11

maxnoofUACPLMNs INTEGER ::= 12

maxnoofUACperPLMN INTEGER ::= 64

maxnoofAdditionalSIBs INTEGER ::= 63

maxnoofslots INTEGER ::= 320

maxnoofTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoTRPs INTEGER ::= 256

maxnoTRPInfoTypes INTEGER ::= 127

**\*\* skip unchanged asn \*\***

END

-- ASN1STOP