**3GPP TSG-RAN WG3 Meeting #109-eR3-205039**

**Online, August 17th – 28th 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.423** | **CR** | **0424** | **rev** |  | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Signalling Logged MDT configuration indication over XnAP |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | RAN3 |
|  |  |
| ***Work item code:*** | NR\_SON\_MDT |  | ***Date:*** | 2020-08-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In this contribution we make corrections to enable a simple enforcement of the RAN2 agreement: “Management based MDT should not overwrite signalling based MDT” in the case of inactive UEs. |
|  |  |
|  ***Summary of change:*** | It is important that the new serving RAN node receives an indication of whether the UE is configured with a Signalling Based Logged MDT configuration so to allow for a basic and simple mechanism for avoiding the possibility of overwriting signaling based configurations with management based configurations. This is achieved by adding a Logged MDT availability flag in the RETRIEVE UE CONTEXT RESPONSE message as specified in the CRImpact AnalysisThis CR has limited functional impact. The CR has limited ASN.1 impacts. |
|  |  |
| ***Consequences if not approved:*** | The RAN2 Agreement that specifies that “Management based MDT should not overwrite signalling based MDT” will not be supported |
|  |  |
| ***Clauses affected:*** | 8.2.4.2, 9.2.1.13, 9.3.4, 9.3.5, 9.3.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS38.413 CR0441 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<<<<<<<<<<<<<<<<<<<<Start of Changes >>>>>>>>>>>>>>>>>>>>

<<<<<<<<<<<<<<<<<<<< 1st set of Changes >>>>>>>>>>>>>>>>>>>>

#### 8.2.4.2 Successful Operation



Figure 8.2.4.2-1: Retrieve UE Context, successful operation

The new NG-RAN node initiates the procedure by sending the RETRIEVE UE CONTEXT REQUEST message to the old NG-RAN node.

If the old NG-RAN node is able to identify the UE context by means of the UE Context ID, and to successfully verify the UE by means of the integrity protection contained in the RETRIEVE UE CONTEXT REQUEST message, and decides to provide the UE context to the new NG-RAN node, it shall respond to the new NG-RAN node with the RETRIEVE UE CONTEXT RESPONSE message.

If the *Index to RAT/Frequency Selection Priority* IE is contained in the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall store this information and use it as defined in TS 23.501 [7].

If the *Location Reporting Information* IE is included in the RETRIEVE UE CONTEXT RESPONSE message, then the new NG-RAN node should initiate the requested location reporting functionality as defined in TS 38.413 [5].

If the *Trace Activation* IE is included in the RETRIEVE UE CONTEXT RESPONSE message which includes

- the *MDT Activation* IE set to "Immediate MDT and Trace", then the target NG-RAN node shall if supported, initiate the requested trace session and MDT session as described in TS 32.422 [23].

- the *MDT Activation* IE set to "Immediate MDT Only" or "Logged MDT only", the target NG-RAN node shall, if supported, initiate the requested MDT session as described in TS 32.422 [23] and the target NG-RAN node shall ignore the *Interfaces To Trace* IE, and the *Trace Depth* IE.

- the *MDT Location Information* IE, within the *MDT Configuration* IE, the target NG-RAN node shall, if supported, store this information and take it into account in the requested MDT session.

- the *MDT Activation* IE set to "Immediate MDT Only" or "Logged MDT only", and if the *Signalling based MDT PLMN List* IE is included in the *MDT Configuration* IE, the target NG-RAN node may use it to propagate the MDT Configuration as described in TS 37.320 [y].

- the *Bluetooth Measurement Configuration* IE, within the *MDT Configuration* IE, the target NG-RAN node shall, if supported, take it into account for MDT Configuration as described in TS 37.320 [y].

- the *WLAN Measurement Configuration* IE, within the *MDT Configuration* IE, the target NG-RAN node shall, if supported, take it into account for MDT Configuration as described in TS 37.320 [y].

- the *Sensor Measurement Configuration* IE, within the *MDT Configuration* IE, take it into account for MDT Configuration as described in TS 37.320 [x].

- the *MDT Configuration* IE and if the target NG-RAN Node is a gNB at least *the MDT Configuration-NR* IE shall be present, while if the target NG-RAN Node is an ng-eNB at least the *MDT Configuration-EUTRA* IE shall be present.

- the *MDT Activation* IE set to “Logged MDT only” and if the *Signalling Based MDT State* IE is present, the target NG-RAN node shall use the *Signalling Based MDT State* IE to determine whether to configure the UE according to the *MDT Activation* IE.

For each QoS flow in the RETRIEVE UE CONTEXT RESPONSE message, if the *QoS Monitoring Request* IE is included in the *QoS Flow Level QoS Parameters* IE in the *PDU Session Resources To Be Setup List* IE, the new NG-RAN node shall store this information, and, if supported, perform delay measurement and QoS monitoring, as specified in TS 23.501 [7].

If the *5GC Mobility Restriction List Container* IE is included in the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall, if supported, store this information in the UE context and use it as specified in TS 38.300 [9].

If the *NR V2X Services Authorized* IE is included in the RETRIEVE UE CONTEXT RESPONSE message and it contains one or more IEs set to "authorized", the new NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *LTE V2X Services Authorized* IE is included in the RETRIEVE UE CONTEXT RESPONSE message and it contains one or more IEs set to "authorized", the new NG-RAN node shall, if supported, consider that the UE is authorized for the relevant service(s).

If the *NR UE Sidelink Aggregate Maximum Bit Rate* IE is included in the *UE Context Information Retrieve UE Context Response* IE in the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for NR V2X services.

If the *LTE UE Sidelink Aggregate Maximum Bit Rate* IE is included in the *UE Context Information Retrieve UE Context Response* IE in the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall, if supported, use the received value for the concerned UE’s sidelink communication in network scheduled mode for LTE V2X services.

If the *PC5 QoS Parameters* IE is included in theRETRIEVE UE CONTEXT RESPONSE message, the target NG-RAN node shall, if supported, use it as defined in TS 23.287[38].

In case of RRC Re-establishment, the old NG-RAN may include the *UE History Information* IE or the *UE History Information from the UE* IE in the RETRIEVE UE CONTEXT RESPONSE message. Upon reception of the *UE History Information* IE or the *UE History Information from the UE* IE in the RETRIEVE UE CONTEXT RESPONSE message, the new NG-RAN node shall, if supported, store the collected information and use it for future handover preparations.

If the *UE Radio Capability ID* IE is contained in the RETRIEVE UE CONTEXT RESPONSE message, the new NG- RAN node shall, if supported store this information in the UE context and use it as defined in TS 23.501 [7] and TS 23.502 [13].

<<<<<<<<<<<<<<<<<<<< End of 1st set of Changes >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 2nd set of Changes >>>>>>>>>>>>>>>>>>>>

#### 9.2.1.13 UE Context Information – Retrieve UE Context Response

This IE contains the UE context information within the RETRIEVE UE CONTEXT RESPONSE message.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| NG-C UE associated Signalling reference | M |  | AMF UE NGAP ID9.2.3.26 | Allocated at the AMF on the old NG-C connection. | – |  |
| Signalling TNL Association Address at source NG-C side | M |  | CP Transport Layer Information9.2.3.31 | This IE indicates the AMF’s IP address of the SCTP association used at the source NG-C interface instance.Note: If no UE TNLA binding exists at the source NG-RAN node, the source NG-RAN node indicates the TNL association address it would have selected if it would have had to create a UE TNLA binding. | – |  |
| UE Security Capabilities | M |  | 9.2.3.49 |  | – |  |
| AS Security Information | M |  | 9.2.3.50 |  | – |  |
| UE Aggregate Maximum Bit Rate | M |  | 9.2.3.17 |  | – |  |
| PDU Session Resources To Be Setup List | M |  | 9.2.1.1 |  | – |  |
| RRC Context | M |  | OCTET STRING | Includes the *HandoverPreparationInformation* message as defined in subclause 11.2.2 of TS 38.331[10] if the old and new serving NG-RAN nodes are gNBs.Includes either the *HandoverPreparationInformation* message as defined in subclause 10.2.2 of TS 36.331 [14] or the *HandoverPreparationInformation-NB* message as defined in subclause 10.6.2 of TS 36.331 [14], if the old and new serving NG-RAN nodes are ng-eNBs. | – |  |
| Mobility Restriction List | O |  | 9.2.3.53 |  | – |  |
| Index to RAT/Frequency Selection Priority | O |  | 9.2.3.23 |  | – |  |
| 5GC Mobility Restriction List Container | O |  | 9.2.3.100 |  | YES | ignore |
| NR UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.2.3.107 | This IE applies only if the UE is authorized for NR V2X services. | YES | ignore |
| LTE UE Sidelink Aggregate Maximum Bit Rate | O |  | 9.2.3.108 | This IE applies only if the UE is authorized for LTE V2X services. | YES | Ignore |
| UE Radio Capability ID | O |  | 9.2.3.138 |  | YES | reject |
| Signalling Based MDT State | O |  | ENUMERATED (Configured, Pending, …) | This IE indicates whether the signalling based MDT configuration has been configured at the UE or it is pending configuration | YES | Ignore |

<<<<<<<<<<<<<<<<<<<< End of 2nd set of Changes >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< Start of 3rd Set of Changes >>>>>>>>>>>>>>>>>>>>

### 9.3.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for XnAP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 ActivationIDforCellActivation,

 AMF-Region-Information,

 AMF-UE-NGAP-ID,

 AS-SecurityInformation,

 AssistanceDataForRANPaging,

 BitRate,

 Cause,

 CellAndCapacityAssistanceInfo-EUTRA,

 CellAndCapacityAssistanceInfo-NR,

 CellAssistanceInfo-EUTRA,

 CellAssistanceInfo-NR,

 CHOinformation-Req,

 CHOinformation-Ack,

 CHO-MRDC-Indicator,

 CPTransportLayerInformation,

 TNLA-To-Add-List,

 TNLA-To-Update-List,

 TNLA-To-Remove-List,

 TNLA-Setup-List,

 TNLA-Failed-To-Setup-List,

 CriticalityDiagnostics,

 XnUAddressInfoperPDUSession-List,

 DAPSResponseInfo-List,

 DataTrafficResourceIndication,

 DeliveryStatus,

 DesiredActNotificationLevel,

 DRB-ID,

 DRB-List,

 DRB-Number,

 DRBsSubjectToDLDiscarding-List,

 DRBsSubjectToEarlyStatusTransfer-List,

 DRBsSubjectToStatusTransfer-List,

 DRBToQoSFlowMapping-List,

 E-UTRA-CGI,

 ExpectedUEBehaviour,

 FiveGCMobilityRestrictionListContainer,

 GlobalNG-RANNode-ID,

 GlobalNG-RANCell-ID,

 GUAMI,

 InterfaceInstanceIndication,

 I-RNTI,

 LocationInformationSNReporting,

 LocationReportingInformation,

 LowerLayerPresenceStatusChange,

 LTEUESidelinkAggregateMaximumBitRate,

 LTEV2XServicesAuthorized,

 MR-DC-ResourceCoordinationInfo,

 ServedCells-E-UTRA,

 ServedCells-NR,

 ServedCellsToUpdate-E-UTRA,

 ServedCellsToUpdate-NR,

 MAC-I,

 MaskedIMEISV,

 MDT-Configuration,

 MDTPLMNList,

 MobilityRestrictionList,

 NG-RAN-Cell-Identity,

 NG-RANnodeUEXnAPID,

 NR-CGI,

 NE-DC-TDM-Pattern,

 NRUESidelinkAggregateMaximumBitRate,

 NRV2XServicesAuthorized,

 PagingDRX,

 PagingPriority,

 PartialListIndicator,

 PLMN-Identity,

 PDCPChangeIndication,

 PDUSessionAggregateMaximumBitRate,

 PDUSession-ID,

 PDUSession-List,

 PDUSession-List-withCause,

 PDUSession-List-withDataForwardingFromTarget,

 PDUSession-List-withDataForwardingRequest,

 PDUSessionResourcesAdmitted-List,

 PDUSessionResourcesNotAdmitted-List,

 PDUSessionResourcesToBeSetup-List,

 PDUSessionResourceChangeRequiredInfo-SNterminated,

 PDUSessionResourceChangeRequiredInfo-MNterminated,

 PDUSessionResourceChangeConfirmInfo-SNterminated,

 PDUSessionResourceChangeConfirmInfo-MNterminated,

 PDUSessionResourceSecondaryRATUsageList,

 PDUSessionResourceSetupInfo-SNterminated,

 PDUSessionResourceSetupInfo-MNterminated,

 PDUSessionResourceSetupResponseInfo-SNterminated,

 PDUSessionResourceSetupResponseInfo-MNterminated,

 PDUSessionResourceModificationInfo-SNterminated,

 PDUSessionResourceModificationInfo-MNterminated,

 PDUSessionResourceModificationResponseInfo-SNterminated,

 PDUSessionResourceModificationResponseInfo-MNterminated,

 PDUSessionResourceModConfirmInfo-SNterminated,

 PDUSessionResourceModConfirmInfo-MNterminated,

 PDUSessionResourceModRqdInfo-SNterminated,

 PDUSessionResourceModRqdInfo-MNterminated,

 PDUSessionType,

 PC5QoSParameters,

 QoSFlowIdentifier,

 QoSFlowNotificationControlIndicationInfo,

 QoSFlows-List,

 RANPagingArea,

 ResetRequestTypeInfo,

 ResetResponseTypeInfo,

 RFSP-Index,

 RRCConfigIndication,

 RRCResumeCause,

 SCGConfigurationQuery,

 SecurityIndication,

 S-NG-RANnode-SecurityKey,

 SpectrumSharingGroupID,

 SplitSRBsTypes,

 S-NG-RANnode-Addition-Trigger-Ind,

 S-NSSAI,

 TargetCellList,

 TAISupport-List,

 Target-CGI,

 TimeToWait,

 TraceActivation,

 UEAggregateMaximumBitRate,

 UEContextID,

 UEContextInfoRetrUECtxtResp,

 UEContextKeptIndicator,

 UEHistoryInformation,

 UEIdentityIndexValue,

 UERadioCapabilityForPaging,

 UERadioCapabilityID,

 UERANPagingIdentity,

 UESecurityCapabilities,

 UPTransportLayerInformation,

 UserPlaneTrafficActivityReport,

 XnBenefitValue,

 RANPagingFailure,

 TNLConfigurationInfo,

 MaximumCellListSize,

 MessageOversizeNotification,

 NG-RANTraceID,

 MobilityInformation,

 InitiatingCondition-FailureIndication,

 HandoverReportType,

 TargetCellinEUTRAN,

 C-RNTI,

 UERLFReportContainer,

 Measurement-ID,

 RegistrationRequest,

 ReportCharacteristics,

 CellToReport,

 ReportingPeriodicity,

 CellMeasurementResult,

 UEHistoryInformationFromTheUE,

 MobilityParametersInformation,

 MobilityParametersModificationRange,

 RACHReportInformation,

 IABNodeIndication,

 SNTriggered,

 SignallingBasedMDTState

FROM XnAP-IEs

 PrivateIE-Container{},

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 ProtocolIE-ContainerList{},

 ProtocolIE-ContainerPair{},

 ProtocolIE-ContainerPairList{},

 ProtocolIE-Single-Container{},

 XNAP-PRIVATE-IES,

 XNAP-PROTOCOL-EXTENSION,

 XNAP-PROTOCOL-IES,

 XNAP-PROTOCOL-IES-PAIR

FROM XnAP-Containers

 id-ActivatedServedCells,

 id-ActivationIDforCellActivation,

 id-AdditionalDRBIDs,

 id-AMF-Region-Information,

 id-AMF-Region-Information-To-Add,

 id-AMF-Region-Information-To-Delete,

 id-AssistanceDataForRANPaging,

 id-AvailableDRBIDs,

 id-Cause,

 id-cellAssistanceInfo-EUTRA,

 id-cellAssistanceInfo-NR,

 id-CellAndCapacityAssistanceInfo-EUTRA,

 id-CellAndCapacityAssistanceInfo-NR,

 id-ConfigurationUpdateInitiatingNodeChoice,

 id-UEContextID,

 id-CriticalityDiagnostics,

 id-XnUAddressInfoperPDUSession-List,

 id-DesiredActNotificationLevel,

 id-DRBsSubjectToStatusTransfer-List,

 id-ExpectedUEBehaviour,

 id-FiveGCMobilityRestrictionListContainer,

 id-GlobalNG-RAN-node-ID,

 id-GUAMI,

 id-indexToRatFrequSelectionPriority,

 id-List-of-served-cells-E-UTRA,

 id-List-of-served-cells-NR,

 id-LocationInformationSN,

 id-LocationInformationSNReporting,

 id-LocationReportingInformation,

 id-LTEUESidelinkAggregateMaximumBitRate,

 id-LTEV2XServicesAuthorized,

 id-MAC-I,

 id-MaskedIMEISV,

 id-MDT-Configuration,

 id-MDTPLMNList,

 id-MN-to-SN-Container,

 id-MobilityRestrictionList,

 id-M-NG-RANnodeUEXnAPID,

 id-new-NG-RAN-Cell-Identity,

 id-newNG-RANnodeUEXnAPID,

 id-NRUESidelinkAggregateMaximumBitRate,

 id-NRV2XServicesAuthorized,

 id-oldNG-RANnodeUEXnAPID,

 id-OldtoNewNG-RANnodeResumeContainer,

 id-PagingDRX,

 id-PagingPriority,

 id-PartialListIndicator-EUTRA,

 id-PartialListIndicator-NR,

 id-PCellID,

 id-PDUSessionResourceSecondaryRATUsageList,

 id-PDUSessionResourcesActivityNotifyList,

 id-PDUSessionResourcesAdmitted-List,

 id-PDUSessionResourcesNotAdmitted-List,

 id-PDUSessionResourcesNotifyList,

 id-PDUSessionToBeAddedAddReq,

 id-PDUSessionToBeReleased-RelReqAck,

 id-procedureStage,

 id-RANPagingArea,

 id-requestedSplitSRB,

 id-RequiredNumberOfDRBIDs,

 id-ResetRequestTypeInfo,

 id-ResetResponseTypeInfo,

 id-RespondingNodeTypeConfigUpdateAck,

 id-RRCResumeCause,

 id-selectedPLMN,

 id-ServedCellsToActivate,

 id-servedCellsToUpdate-E-UTRA,

 id-ServedCellsToUpdateInitiatingNodeChoice,

 id-servedCellsToUpdate-NR,

 id-sourceNG-RANnodeUEXnAPID,

 id-SpareDRBIDs,

 id-S-NG-RANnodeMaxIPDataRate-UL,

 id-S-NG-RANnodeMaxIPDataRate-DL,

 id-S-NG-RANnodeUEXnAPID,

 id-TAISupport-list,

 id-Target2SourceNG-RANnodeTranspContainer,

 id-targetCellGlobalID,

 id-targetNG-RANnodeUEXnAPID,

 id-TimeToWait,

 id-TNLA-To-Add-List,

 id-TNLA-To-Update-List,

 id-TNLA-To-Remove-List,

 id-TNLA-Setup-List,

 id-TNLA-Failed-To-Setup-List,

 id-TraceActivation,

 id-UEContextInfoHORequest,

 id-UEContextInfoRetrUECtxtResp,

 id-UEContextKeptIndicator,

 id-UEContextRefAtSN-HORequest,

 id-UEHistoryInformation,

 id-UEIdentityIndexValue,

 id-UERANPagingIdentity,

 id-UESecurityCapabilities,

 id-UserPlaneTrafficActivityReport,

 id-XnRemovalThreshold,

 id-PDUSessionAdmittedAddedAddReqAck,

 id-PDUSessionNotAdmittedAddReqAck,

 id-SN-to-MN-Container,

 id-RRCConfigIndication,

 id-SplitSRB-RRCTransfer,

 id-UEReportRRCTransfer,

 id-PDUSessionReleasedList-RelConf,

 id-BearersSubjectToCounterCheck,

 id-PDUSessionToBeReleasedList-RelRqd,

 id-ResponseInfo-ReconfCompl,

 id-initiatingNodeType-ResourceCoordRequest,

 id-respondingNodeType-ResourceCoordResponse,

 id-PDUSessionToBeReleased-RelReq,

 id-PDUSession-SNChangeRequired-List,

 id-PDUSession-SNChangeConfirm-List,

 id-PDCPChangeIndication,

 id-PC5QoSParameters,

 id-SCGConfigurationQuery,

 id-UEContextInfo-SNModRequest,

 id-requestedSplitSRBrelease,

 id-PDUSessionAdmitted-SNModResponse,

 id-PDUSessionNotAdmitted-SNModResponse,

 id-admittedSplitSRB,

 id-admittedSplitSRBrelease,

 id-PDUSessionAdmittedModSNModConfirm,

 id-PDUSessionReleasedSNModConfirm,

 id-s-ng-RANnode-SecurityKey,

 id-PDUSessionToBeModifiedSNModRequired,

 id-S-NG-RANnodeUE-AMBR,

 id-PDUSessionToBeReleasedSNModRequired,

 id-target-S-NG-RANnodeID,

 id-S-NSSAI,

 id-MR-DC-ResourceCoordinationInfo,

 id-RANPagingFailure,

 id-UERadioCapabilityForPaging,

 id-PDUSessionDataForwarding-SNModResponse,

 id-Secondary-MN-Xn-U-TNLInfoatM,

 id-NE-DC-TDM-Pattern,

 id-InterfaceInstanceIndication,

 id-S-NG-RANnode-Addition-Trigger-Ind,

 id-SNTriggered,

 id-DRBs-transferred-to-MN,

 id-TNLConfigurationInfo,

 id-MessageOversizeNotification,

 id-NG-RANTraceID,

 id-FastMCGRecoveryRRCTransfer-SN-to-MN,

 id-FastMCGRecoveryRRCTransfer-MN-to-SN,

 id-RequestedFastMCGRecoveryViaSRB3,

 id-AvailableFastMCGRecoveryViaSRB3,

 id-RequestedFastMCGRecoveryViaSRB3Release,

 id-ReleaseFastMCGRecoveryViaSRB3,

 id-CHOinformation-Req,

 id-CHOinformation-Ack,

 id-targetCellsToCancel,

 id-requestedTargetCellGlobalID,

 id-DAPSResponseInfo-List,

 id-CHO-MRDC-Indicator,

 id-MobilityInformation,

 id-InitiatingCondition-FailureIndication,

 id-UEHistoryInformationFromTheUE,

 id-HandoverReportType,

 id-HandoverCause,

 id-SourceCellCGI,

 id-TargetCellCGI,

 id-ReEstablishmentCellCGI,

 id-TargetCellinEUTRAN,

 id-SourceCellCRNTI,

 id-UERLFReportContainer,

 id-NGRAN-Node1-Measurement-ID,

 id-NGRAN-Node2-Measurement-ID,

 id-RegistrationRequest,

 id-ReportCharacteristics,

 id-CellToReport,

 id-ReportingPeriodicity,

 id-CellMeasurementResult,

 id-NG-RANnode1CellID,

 id-NG-RANnode2CellID,

 id-NG-RANnode1MobilityParameters,

 id-NG-RANnode2ProposedMobilityParameters,

 id-MobilityParametersModificationRange,

 id-RACHReportInformation,

 id-IABNodeIndication,

 id-UERadioCapabilityID,

 id-SignallingBasedMDTState,

 maxnoofCellsinNG-RANnode,

 maxnoofDRBs,

 maxnoofPDUSessions,

 maxnoofQoSFlows

FROM XnAP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- HANDOVER REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

<<<<<<<<<<<<<<<<<<<< End of 3rd set of New Changes >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< Start of 4th Set of New Changes >>>>>>>>>>>>>>>>>>>>

### 9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-CNTypeRestrictionsForEquivalent,

 id-CNTypeRestrictionsForServing,

 id-Additional-UL-NG-U-TNLatUPF-List,

 id-AlternativeQoSParaSetList,

 id-CurrentQoSParaSetIndex,

 id-DefaultDRB-Allowed,

 id-DLCarrierList,

 id-EndpointIPAddressAndPort,

 id-ExtendedTAISliceSupportList,

 id-FiveGCMobilityRestrictionListContainer,

 id-SecondarydataForwardingInfoFromTarget-List,

 id-LastE-UTRANPLMNIdentity,

 id-IntendedTDD-DL-ULConfiguration-NR,

 id-MaxIPrate-DL,

 id-SecurityResult,

 id-OldQoSFlowMap-ULendmarkerexpected,

 id-PDUSessionCommonNetworkInstance,

 id-BPLMN-ID-Info-EUTRA,

 id-BPLMN-ID-Info-NR,

 id-DRBsNotAdmittedSetupModifyList,

 id-Secondary-MN-Xn-U-TNLInfoatM,

 id-ULForwardingProposal,

 id-DRB-IDs-takenintouse,

 id-SplitSessionIndicator,

 id-NonGBRResources-Offered,

 id-MDT-Configuration,

 id-TraceCollectionEntityURI,

 id-NPN-Broadcast-Information,

 id-NPNPagingAssistanceInformation,

 id-NPNMobilityInformation,

 id-NPN-Support,

 id-LTEUESidelinkAggregateMaximumBitRate,

 id-NRUESidelinkAggregateMaximumBitRate,

 id-ExtendedRATRestrictionInformation,

 id-QoSMonitoringRequest,

 id-DAPSRequestInfo,

 id-OffsetOfNbiotChannelNumberToDL-EARFCN,

 id-OffsetOfNbiotChannelNumberToUL-EARFCN,

 id-NBIoT-UL-DL-AlignmentOffset,

 id-TDDULDLConfigurationCommonNR,

 id-CarrierList,

 id-ULCarrierList,

 id-FrequencyShift7p5khz,

 id-SSB-PositionsInBurst,

 id-NRCellPRACHConfig,

 id-Redundant-UL-NG-U-TNLatUPF,

 id-Redundant-DL-NG-U-TNLatNG-RAN,

 id-CNPacketDelayBudgetDownlink,

 id-CNPacketDelayBudgetUplink,

 id-ExtendedPacketDelayBudget,

 id-Additional-Redundant-UL-NG-U-TNLatUPF-List,

 id-RedundantCommonNetworkInstance,

 id-TSCTrafficCharacteristics,

 id-RedundantQoSFlowIndicator,

 id-Additional-PDCP-Duplication-TNL-List,

 id-RedundantPDUSessionInformation,

 id-UsedRSNInformation,

 id-RLCDuplicationInformation,

 id-CSI-RSTransmissionIndication,

 id-UERadioCapabilityID,

 id-SignallingBasedMDTState,

 maxEARFCN,

 maxnoofAllowedAreas,

 maxnoofAMFRegions,

 maxnoofAoIs,

 maxnoofBPLMNs,

 maxnoofCAGs,

 maxnoofCAGsperPLMN,

 maxnoofCellsinAoI,

 maxnoofCellsinNG-RANnode,

 maxnoofCellsinRNA,

 maxnoofCellsinUEHistoryInfo,

 maxnoofCellsUEMovingTrajectory,

 maxnoofDRBs,

 maxnoofEPLMNs,

 maxnoofEPLMNsplus1,

 maxnoofEUTRABands,

 maxnoofEUTRABPLMNs,

 maxnoofForbiddenTACs,

 maxnoofMBSFNEUTRA,

 maxnoofMultiConnectivityMinusOne,

 maxnoofNeighbours,

 maxnoofNIDs,

 maxnoofNRCellBands,

 maxnoofPDUSessions,

 maxnoofPLMNs,

 maxnoofProtectedResourcePatterns,

 maxnoofQoSFlows,

 maxnoofQoSParaSets,

 maxnoofRANAreaCodes,

 maxnoofRANAreasinRNA,

 maxnoofSCellGroups,

 maxnoofSCellGroupsplus1,

 maxnoofSliceItems,

 maxnoofExtSliceItems,

 maxnoofSNPNIDs,

 maxnoofsupportedTACs,

 maxnoofsupportedPLMNs,

 maxnoofTAI,

 maxnoofTAIsinAoI,

 maxnoofTNLAssociations,

 maxnoofUEContexts,

 maxNRARFCN,

 maxNrOfErrors,

 maxnoofRANNodesinAoI,

 maxnooftimeperiods,

 maxnoofslots,

 maxnoofExtTLAs,

 maxnoofGTPTLAs,

 maxnoofCHOcells,

 maxnoofPC5QoSFlows,

 maxnoofSSBAreas,

 maxnoofNRSCSs,

 maxnoofPhysicalResourceBlocks,

 maxnoofRACHReports,

 maxnoofAdditionalPDCPDuplicationTNL,

 maxnoofRLCDuplicationstate,

 maxnoofBluetoothName,

 maxnoofCellIDforMDT,

 maxnoofMDTPLMNs,

 maxnoofTAforMDT,

 maxnoofWLANName,

 maxnoofSensorName,

 maxnoofNeighPCIforMDT,

 maxnoofFreqforMDT

FROM XnAP-Constants

 Criticality,

 ProcedureCode,

 ProtocolIE-ID,

 TriggeringMessage

FROM XnAP-CommonDataTypes

 ProtocolExtensionContainer{},

 ProtocolIE-Single-Container{},

 XNAP-PROTOCOL-EXTENSION,

 XNAP-PROTOCOL-IES

FROM XnAP-Containers;

**-- TEXT OMITTED –**

UEContextInfoRetrUECtxtResp ::= SEQUENCE {

 ng-c-UE-signalling-ref AMF-UE-NGAP-ID,

 signalling-TNL-at-source CPTransportLayerInformation,

 ueSecurityCapabilities UESecurityCapabilities,

 securityInformation AS-SecurityInformation,

 ue-AMBR UEAggregateMaximumBitRate,

 pduSessionResourcesToBeSetup-List PDUSessionResourcesToBeSetup-List,

 rrc-Context OCTET STRING,

 mobilityRestrictionList MobilityRestrictionList OPTIONAL,

 indexToRatFrequencySelectionPriority RFSP-Index OPTIONAL,

 iE-Extension ProtocolExtensionContainer { {UEContextInfoRetrUECtxtResp-ExtIEs} } OPTIONAL,

 ...

}

UEContextInfoRetrUECtxtResp-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {

 { ID id-FiveGCMobilityRestrictionListContainer CRITICALITY ignore EXTENSION FiveGCMobilityRestrictionListContainer PRESENCE optional }|

{ ID id-NRUESidelinkAggregateMaximumBitRate CRITICALITY ignore EXTENSION NRUESidelinkAggregateMaximumBitRate PRESENCE optional}|

{ ID id-LTEUESidelinkAggregateMaximumBitRate CRITICALITY ignore EXTENSION LTEUESidelinkAggregateMaximumBitRate PRESENCE optional}|

 { ID id-UERadioCapabilityID CRITICALITY reject EXTENSION UERadioCapabilityID PRESENCE optional }|

 { ID id-SignallingBasedMDTState CRITICALITY reject EXTENSION SignallingBasedMDTState PRESENCE optional},

 ...

}

<<<<<<<<<<<<<<<<<<<< End of 4th set of New Changes >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< Start of 5th Set of New Changes >>>>>>>>>>>>>>>>>>>>

### 9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) xnap (2) version1 (1) xnap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM XnAP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-handoverPreparation ProcedureCode ::= 0

id-sNStatusTransfer ProcedureCode ::= 1

id-handoverCancel ProcedureCode ::= 2

id-retrieveUEContext ProcedureCode ::= 3

id-rANPaging ProcedureCode ::= 4

id-xnUAddressIndication ProcedureCode ::= 5

id-uEContextRelease ProcedureCode ::= 6

id-sNGRANnodeAdditionPreparation ProcedureCode ::= 7

id-sNGRANnodeReconfigurationCompletion ProcedureCode ::= 8

id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation ProcedureCode ::= 9

id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation ProcedureCode ::= 10

id-mNGRANnodeinitiatedSNGRANnodeRelease ProcedureCode ::= 11

id-sNGRANnodeinitiatedSNGRANnodeRelease ProcedureCode ::= 12

id-sNGRANnodeCounterCheck ProcedureCode ::= 13

id-sNGRANnodeChange ProcedureCode ::= 14

id-rRCTransfer ProcedureCode ::= 15

id-xnRemoval ProcedureCode ::= 16

id-xnSetup ProcedureCode ::= 17

id-nGRANnodeConfigurationUpdate ProcedureCode ::= 18

id-cellActivation ProcedureCode ::= 19

id-reset ProcedureCode ::= 20

id-errorIndication ProcedureCode ::= 21

id-privateMessage ProcedureCode ::= 22

id-notificationControl ProcedureCode ::= 23

id-activityNotification ProcedureCode ::= 24

id-e-UTRA-NR-CellResourceCoordination ProcedureCode ::= 25

id-secondaryRATDataUsageReport ProcedureCode ::= 26

id-deactivateTrace ProcedureCode ::= 27

id-traceStart ProcedureCode ::= 28

id-handoverSuccess ProcedureCode ::= 29

id-conditionalHandoverCancel ProcedureCode ::= 30

id-earlyStatusTransfer ProcedureCode ::= 31

id-failureIndication ProcedureCode ::= 32

id-handoverReport ProcedureCode ::= 33

id-resourceStatusReportingInitiation ProcedureCode ::= 34

id-resourceStatusReporting ProcedureCode ::= 35

id-mobilitySettingsChange ProcedureCode ::= 36

id-accessAndMobilityIndication ProcedureCode ::= 37

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxEARFCN INTEGER ::= 262143

maxnoofAllowedAreas INTEGER ::= 16

maxnoofAMFRegions INTEGER ::= 16

maxnoofAoIs INTEGER ::= 64

maxnoofBluetoothName INTEGER ::= 4

maxnoofBPLMNs INTEGER ::= 12

maxnoofCAGs INTEGER ::= 12

maxnoofCAGsperPLMN INTEGER ::= 256

maxnoofCellIDforMDT INTEGER ::= 32

maxnoofCellsinAoI INTEGER ::= 256

maxnoofCellsinUEHistoryInfo INTEGER ::= 16

maxnoofCellsinNG-RANnode INTEGER ::= 16384

maxnoofCellsinRNA INTEGER ::= 32

maxnoofCellsUEMovingTrajectory INTEGER ::= 16

maxnoofDRBs INTEGER ::= 32

maxnoofEUTRABands INTEGER ::= 16

maxnoofEUTRABPLMNs INTEGER ::= 6

maxnoofEPLMNs INTEGER ::= 15

maxnoofExtSliceItems INTEGER ::= 65535

maxnoofEPLMNsplus1 INTEGER ::= 16

maxnoofForbiddenTACs INTEGER ::= 4096

maxnoofFreqforMDT INTEGER ::= 8

maxnoofMBSFNEUTRA INTEGER ::= 8

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofMultiConnectivityMinusOne INTEGER ::= 3

maxnoofNeighbours INTEGER ::= 1024

maxnoofNeighPCIforMDT INTEGER ::= 32

maxnoofNIDs INTEGER ::= 12

maxnoofNRCellBands INTEGER ::= 32

maxnoofPLMNs INTEGER ::= 16

maxnoofPDUSessions INTEGER ::= 256

maxnoofProtectedResourcePatterns INTEGER ::= 16

maxnoofQoSFlows INTEGER ::= 64

maxnoofQoSParaSets INTEGER ::= 8

maxnoofRANAreaCodes INTEGER ::= 32

maxnoofRANAreasinRNA INTEGER ::= 16

maxnoofRANNodesinAoI INTEGER ::= 64

maxnoofSCellGroups INTEGER ::= 3

maxnoofSCellGroupsplus1 INTEGER ::= 4

maxnoofSensorName INTEGER ::= 3

maxnoofSliceItems INTEGER ::= 1024

maxnoofSNPNIDs INTEGER ::= 12

maxnoofsupportedPLMNs INTEGER ::= 12

maxnoofsupportedTACs INTEGER ::= 256

maxnoofTAforMDT INTEGER ::= 8

maxnoofTAI INTEGER ::= 16

maxnoofTAIsinAoI INTEGER ::= 16

maxnooftimeperiods INTEGER ::= 2

maxnoofTNLAssociations INTEGER ::= 32

maxnoofUEContexts INTEGER ::= 8192

maxNRARFCN INTEGER ::= 3279165

maxNrOfErrors INTEGER ::= 256

maxnoofslots INTEGER ::= 5120

maxnoofExtTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoofCHOcells INTEGER ::= 8

maxnoofPC5QoSFlows INTEGER ::= 2064

maxnoofSSBAreas INTEGER ::= 64

maxnoofRACHReports INTEGER ::= 64

maxnoofNRSCSs INTEGER ::= 5

maxnoofPhysicalResourceBlocks INTEGER ::= 275

maxnoofAdditionalPDCPDuplicationTNL INTEGER ::= 2

maxnoofRLCDuplicationstate INTEGER ::= 3

maxnoofWLANName INTEGER ::= 4

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-ActivatedServedCells ProtocolIE-ID ::= 0

id-ActivationIDforCellActivation ProtocolIE-ID ::= 1

id-admittedSplitSRB ProtocolIE-ID ::= 2

id-admittedSplitSRBrelease ProtocolIE-ID ::= 3

id-AMF-Region-Information ProtocolIE-ID ::= 4

id-AssistanceDataForRANPaging ProtocolIE-ID ::= 5

id-BearersSubjectToCounterCheck ProtocolIE-ID ::= 6

id-Cause ProtocolIE-ID ::= 7

id-cellAssistanceInfo-NR ProtocolIE-ID ::= 8

id-ConfigurationUpdateInitiatingNodeChoice ProtocolIE-ID ::= 9

id-CriticalityDiagnostics ProtocolIE-ID ::= 10

id-XnUAddressInfoperPDUSession-List ProtocolIE-ID ::= 11

id-DRBsSubjectToStatusTransfer-List ProtocolIE-ID ::= 12

id-ExpectedUEBehaviour ProtocolIE-ID ::= 13

id-GlobalNG-RAN-node-ID ProtocolIE-ID ::= 14

id-GUAMI ProtocolIE-ID ::= 15

id-indexToRatFrequSelectionPriority ProtocolIE-ID ::= 16

id-initiatingNodeType-ResourceCoordRequest ProtocolIE-ID ::= 17

id-List-of-served-cells-E-UTRA ProtocolIE-ID ::= 18

id-List-of-served-cells-NR ProtocolIE-ID ::= 19

id-LocationReportingInformation ProtocolIE-ID ::= 20

id-MAC-I ProtocolIE-ID ::= 21

id-MaskedIMEISV ProtocolIE-ID ::= 22

id-M-NG-RANnodeUEXnAPID ProtocolIE-ID ::= 23

id-MN-to-SN-Container ProtocolIE-ID ::= 24

id-MobilityRestrictionList ProtocolIE-ID ::= 25

id-new-NG-RAN-Cell-Identity ProtocolIE-ID ::= 26

id-newNG-RANnodeUEXnAPID ProtocolIE-ID ::= 27

id-UEReportRRCTransfer ProtocolIE-ID ::= 28

id-oldNG-RANnodeUEXnAPID ProtocolIE-ID ::= 29

id-OldtoNewNG-RANnodeResumeContainer ProtocolIE-ID ::= 30

id-PagingDRX ProtocolIE-ID ::= 31

id-PCellID ProtocolIE-ID ::= 32

id-PDCPChangeIndication ProtocolIE-ID ::= 33

id-PDUSessionAdmittedAddedAddReqAck ProtocolIE-ID ::= 34

id-PDUSessionAdmittedModSNModConfirm ProtocolIE-ID ::= 35

id-PDUSessionAdmitted-SNModResponse ProtocolIE-ID ::= 36

id-PDUSessionNotAdmittedAddReqAck ProtocolIE-ID ::= 37

id-PDUSessionNotAdmitted-SNModResponse ProtocolIE-ID ::= 38

id-PDUSessionReleasedList-RelConf ProtocolIE-ID ::= 39

id-PDUSessionReleasedSNModConfirm ProtocolIE-ID ::= 40

id-PDUSessionResourcesActivityNotifyList ProtocolIE-ID ::= 41

id-PDUSessionResourcesAdmitted-List ProtocolIE-ID ::= 42

id-PDUSessionResourcesNotAdmitted-List ProtocolIE-ID ::= 43

id-PDUSessionResourcesNotifyList ProtocolIE-ID ::= 44

id-PDUSession-SNChangeConfirm-List ProtocolIE-ID ::= 45

id-PDUSession-SNChangeRequired-List ProtocolIE-ID ::= 46

id-PDUSessionToBeAddedAddReq ProtocolIE-ID ::= 47

id-PDUSessionToBeModifiedSNModRequired ProtocolIE-ID ::= 48

id-PDUSessionToBeReleasedList-RelRqd ProtocolIE-ID ::= 49

id-PDUSessionToBeReleased-RelReq ProtocolIE-ID ::= 50

id-PDUSessionToBeReleasedSNModRequired ProtocolIE-ID ::= 51

id-RANPagingArea ProtocolIE-ID ::= 52

id-PagingPriority ProtocolIE-ID ::= 53

id-requestedSplitSRB ProtocolIE-ID ::= 54

id-requestedSplitSRBrelease ProtocolIE-ID ::= 55

id-ResetRequestTypeInfo ProtocolIE-ID ::= 56

id-ResetResponseTypeInfo ProtocolIE-ID ::= 57

id-RespondingNodeTypeConfigUpdateAck ProtocolIE-ID ::= 58

id-respondingNodeType-ResourceCoordResponse ProtocolIE-ID ::= 59

id-ResponseInfo-ReconfCompl ProtocolIE-ID ::= 60

id-RRCConfigIndication ProtocolIE-ID ::= 61

id-RRCResumeCause ProtocolIE-ID ::= 62

id-SCGConfigurationQuery ProtocolIE-ID ::= 63

id-selectedPLMN ProtocolIE-ID ::= 64

id-ServedCellsToActivate ProtocolIE-ID ::= 65

id-servedCellsToUpdate-E-UTRA ProtocolIE-ID ::= 66

id-ServedCellsToUpdateInitiatingNodeChoice ProtocolIE-ID ::= 67

id-servedCellsToUpdate-NR ProtocolIE-ID ::= 68

id-s-ng-RANnode-SecurityKey ProtocolIE-ID ::= 69

id-S-NG-RANnodeUE-AMBR ProtocolIE-ID ::= 70

id-S-NG-RANnodeUEXnAPID ProtocolIE-ID ::= 71

id-SN-to-MN-Container ProtocolIE-ID ::= 72

id-sourceNG-RANnodeUEXnAPID ProtocolIE-ID ::= 73

id-SplitSRB-RRCTransfer ProtocolIE-ID ::= 74

id-TAISupport-list ProtocolIE-ID ::= 75

id-TimeToWait ProtocolIE-ID ::= 76

id-Target2SourceNG-RANnodeTranspContainer ProtocolIE-ID ::= 77

id-targetCellGlobalID ProtocolIE-ID ::= 78

id-targetNG-RANnodeUEXnAPID ProtocolIE-ID ::= 79

id-target-S-NG-RANnodeID ProtocolIE-ID ::= 80

id-TraceActivation ProtocolIE-ID ::= 81

id-UEContextID ProtocolIE-ID ::= 82

id-UEContextInfoHORequest ProtocolIE-ID ::= 83

id-UEContextInfoRetrUECtxtResp ProtocolIE-ID ::= 84

id-UEContextInfo-SNModRequest ProtocolIE-ID ::= 85

id-UEContextKeptIndicator ProtocolIE-ID ::= 86

id-UEContextRefAtSN-HORequest ProtocolIE-ID ::= 87

id-UEHistoryInformation ProtocolIE-ID ::= 88

id-UEIdentityIndexValue ProtocolIE-ID ::= 89

id-UERANPagingIdentity ProtocolIE-ID ::= 90

id-UESecurityCapabilities ProtocolIE-ID ::= 91

id-UserPlaneTrafficActivityReport ProtocolIE-ID ::= 92

id-XnRemovalThreshold ProtocolIE-ID ::= 93

id-DesiredActNotificationLevel ProtocolIE-ID ::= 94

id-AvailableDRBIDs ProtocolIE-ID ::= 95

id-AdditionalDRBIDs ProtocolIE-ID ::= 96

id-SpareDRBIDs ProtocolIE-ID ::= 97

id-RequiredNumberOfDRBIDs ProtocolIE-ID ::= 98

id-TNLA-To-Add-List ProtocolIE-ID ::= 99

id-TNLA-To-Update-List ProtocolIE-ID ::= 100

id-TNLA-To-Remove-List ProtocolIE-ID ::= 101

id-TNLA-Setup-List ProtocolIE-ID ::= 102

id-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 103

id-PDUSessionToBeReleased-RelReqAck ProtocolIE-ID ::= 104

id-S-NG-RANnodeMaxIPDataRate-UL ProtocolIE-ID ::= 105

id-PDUSessionResourceSecondaryRATUsageList ProtocolIE-ID ::= 107

id-Additional-UL-NG-U-TNLatUPF-List ProtocolIE-ID ::= 108

id-SecondarydataForwardingInfoFromTarget-List ProtocolIE-ID ::= 109

id-LocationInformationSNReporting ProtocolIE-ID ::= 110

id-LocationInformationSN ProtocolIE-ID ::= 111

id-LastE-UTRANPLMNIdentity ProtocolIE-ID ::= 112

id-S-NG-RANnodeMaxIPDataRate-DL ProtocolIE-ID ::= 113

id-MaxIPrate-DL ProtocolIE-ID ::= 114

id-SecurityResult ProtocolIE-ID ::= 115

id-S-NSSAI ProtocolIE-ID ::= 116

id-MR-DC-ResourceCoordinationInfo ProtocolIE-ID ::= 117

id-AMF-Region-Information-To-Add ProtocolIE-ID ::= 118

id-AMF-Region-Information-To-Delete ProtocolIE-ID ::= 119

id-OldQoSFlowMap-ULendmarkerexpected ProtocolIE-ID ::= 120

id-RANPagingFailure ProtocolIE-ID ::= 121

id-UERadioCapabilityForPaging ProtocolIE-ID ::= 122

id-PDUSessionDataForwarding-SNModResponse ProtocolIE-ID ::= 123

id-DRBsNotAdmittedSetupModifyList ProtocolIE-ID ::= 124

id-Secondary-MN-Xn-U-TNLInfoatM ProtocolIE-ID ::= 125

id-NE-DC-TDM-Pattern ProtocolIE-ID ::= 126

id-PDUSessionCommonNetworkInstance ProtocolIE-ID ::= 127

id-BPLMN-ID-Info-EUTRA ProtocolIE-ID ::= 128

id-BPLMN-ID-Info-NR ProtocolIE-ID ::= 129

id-InterfaceInstanceIndication ProtocolIE-ID ::= 130

id-S-NG-RANnode-Addition-Trigger-Ind ProtocolIE-ID ::= 131

id-DefaultDRB-Allowed ProtocolIE-ID ::= 132

id-DRB-IDs-takenintouse ProtocolIE-ID ::= 133

id-SplitSessionIndicator ProtocolIE-ID ::= 134

id-CNTypeRestrictionsForEquivalent ProtocolIE-ID ::= 135

id-CNTypeRestrictionsForServing ProtocolIE-ID ::= 136

id-DRBs-transferred-to-MN ProtocolIE-ID ::= 137

id-ULForwardingProposal ProtocolIE-ID ::= 138

id-EndpointIPAddressAndPort ProtocolIE-ID ::= 139

id-IntendedTDD-DL-ULConfiguration-NR ProtocolIE-ID ::= 140

id-TNLConfigurationInfo ProtocolIE-ID ::= 141

id-PartialListIndicator-NR ProtocolIE-ID ::= 142

id-MessageOversizeNotification ProtocolIE-ID ::= 143

id-CellAndCapacityAssistanceInfo-NR ProtocolIE-ID ::= 144

id-NG-RANTraceID ProtocolIE-ID ::= 145

id-NonGBRResources-Offered ProtocolIE-ID ::= 146

id-FastMCGRecoveryRRCTransfer-SN-to-MN ProtocolIE-ID ::= 147

id-RequestedFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 148

id-AvailableFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 149

id-RequestedFastMCGRecoveryViaSRB3Release ProtocolIE-ID ::= 150

id-ReleaseFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 151

id-FastMCGRecoveryRRCTransfer-MN-to-SN ProtocolIE-ID ::= 152

id-ExtendedRATRestrictionInformation ProtocolIE-ID ::= 153

id-QoSMonitoringRequest ProtocolIE-ID ::= 154

id-FiveGCMobilityRestrictionListContainer ProtocolIE-ID ::= 155

id-PartialListIndicator-EUTRA ProtocolIE-ID ::= 156

id-CellAndCapacityAssistanceInfo-EUTRA ProtocolIE-ID ::= 157

id-CHOinformation-Req ProtocolIE-ID ::= 158

id-CHOinformation-Ack ProtocolIE-ID ::= 159

id-targetCellsToCancel ProtocolIE-ID ::= 160

id-requestedTargetCellGlobalID ProtocolIE-ID ::= 161

id-procedureStage ProtocolIE-ID ::= 162

id-DAPSRequestInfo ProtocolIE-ID ::= 163

id-DAPSResponseInfo-List ProtocolIE-ID ::= 164

id-CHO-MRDC-Indicator ProtocolIE-ID ::= 165

id-OffsetOfNbiotChannelNumberToDL-EARFCN ProtocolIE-ID ::= 166

id-OffsetOfNbiotChannelNumberToUL-EARFCN ProtocolIE-ID ::= 167

id-NBIoT-UL-DL-AlignmentOffset ProtocolIE-ID ::= 168

id-LTEV2XServicesAuthorized ProtocolIE-ID ::= 169

id-NRV2XServicesAuthorized ProtocolIE-ID ::= 170

id-LTEUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 171

id-NRUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 172

id-PC5QoSParameters ProtocolIE-ID ::= 173

id-AlternativeQoSParaSetList ProtocolIE-ID ::= 174

id-CurrentQoSParaSetIndex ProtocolIE-ID ::= 175

id-MobilityInformation ProtocolIE-ID ::= 176

id-InitiatingCondition-FailureIndication ProtocolIE-ID ::= 177

id-UEHistoryInformationFromTheUE ProtocolIE-ID ::= 178

id-HandoverReportType ProtocolIE-ID ::= 179

id-HandoverCause ProtocolIE-ID ::= 180

id-SourceCellCGI ProtocolIE-ID ::= 181

id-TargetCellCGI ProtocolIE-ID ::= 182

id-ReEstablishmentCellCGI ProtocolIE-ID ::= 183

id-TargetCellinEUTRAN ProtocolIE-ID ::= 184

id-SourceCellCRNTI ProtocolIE-ID ::= 185

id-UERLFReportContainer ProtocolIE-ID ::= 186

id-NGRAN-Node1-Measurement-ID ProtocolIE-ID ::= 187

id-NGRAN-Node2-Measurement-ID ProtocolIE-ID ::= 188

id-RegistrationRequest ProtocolIE-ID ::= 189

id-ReportCharacteristics ProtocolIE-ID ::= 190

id-CellToReport ProtocolIE-ID ::= 191

id-ReportingPeriodicity ProtocolIE-ID ::= 192

id-CellMeasurementResult ProtocolIE-ID ::= 193

id-NG-RANnode1CellID ProtocolIE-ID ::= 194

id-NG-RANnode2CellID ProtocolIE-ID ::= 195

id-NG-RANnode1MobilityParameters ProtocolIE-ID ::= 196

id-NG-RANnode2ProposedMobilityParameters ProtocolIE-ID ::= 197

id-MobilityParametersModificationRange ProtocolIE-ID ::= 198

id-TDDULDLConfigurationCommonNR ProtocolIE-ID ::= 199

id-CarrierList ProtocolIE-ID ::= 200

id-ULCarrierList ProtocolIE-ID ::= 201

id-FrequencyShift7p5khz ProtocolIE-ID ::= 202

id-SSB-PositionsInBurst ProtocolIE-ID ::= 203

id-NRCellPRACHConfig ProtocolIE-ID ::= 204

id-RACHReportInformation ProtocolIE-ID ::= 205

id-IABNodeIndication ProtocolIE-ID ::= 206

id-Redundant-UL-NG-U-TNLatUPF ProtocolIE-ID ::= 207

id-CNPacketDelayBudgetDownlink ProtocolIE-ID ::= 208

id-CNPacketDelayBudgetUplink ProtocolIE-ID ::= 209

id-Additional-Redundant-UL-NG-U-TNLatUPF-List ProtocolIE-ID ::= 210

id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 211

id-TSCTrafficCharacteristics ProtocolIE-ID ::= 212

id-RedundantQoSFlowIndicator ProtocolIE-ID ::= 213

id-Redundant-DL-NG-U-TNLatNG-RAN ProtocolIE-ID ::= 214

id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 215

id-Additional-PDCP-Duplication-TNL-List ProtocolIE-ID ::= 216

id-RedundantPDUSessionInformation ProtocolIE-ID ::= 217

id-UsedRSNInformation ProtocolIE-ID ::= 218

id-RLCDuplicationInformation ProtocolIE-ID ::= 219

id-NPN-Broadcast-Information ProtocolIE-ID ::= 220

id-NPNPagingAssistanceInformation ProtocolIE-ID ::= 221

id-NPNMobilityInformation ProtocolIE-ID ::= 222

id-NPN-Support ProtocolIE-ID ::= 223

id-MDT-Configuration ProtocolIE-ID ::= 224

id-MDTPLMNList ProtocolIE-ID ::= 225

id-TraceCollectionEntityURI ProtocolIE-ID ::= 226

id-UERadioCapabilityID ProtocolIE-ID ::= 227

id-CSI-RSTransmissionIndication ProtocolIE-ID ::= 228

id-SNTriggered ProtocolIE-ID ::= 229

id-DLCarrierList ProtocolIE-ID ::= 230

id-ExtendedTAISliceSupportList ProtocolIE-ID ::= 231

id-cellAssistanceInfo-EUTRA ProtocolIE-ID ::= 232

id-SignallingBasedMDTState ProtocolIE-ID ::= xxx

END

-- ASN1STOP

<<<<<<<<<<<<<<<<<<<< End of New Changes >>>>>>>>>>>>>>>>>>>>