3GPP TSG-RAN WG3 Meeting #109-e R3-205752

**Online, 17th – 27th August 2020 was R3-205068**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **36.423** | **CR** | **1532** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introducing UE Radio Capability ID Mapping procedure | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, NEC, Huawei, CATT, Samsung | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | RACS\_RAN | | | | |  | ***Date:*** | | | 2020-08-06 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This CR introduces the missing UE Radio Capability ID Mapping procedure on X2AP. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Intorducing the UE Radio Capability ID Mapping procedure on X2AP. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The UE Radio Capability ID Mapping procedure would not exist on X2AP and an en-gNB would not be able to retrieve mapping information for RACS. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7, 8.1, 8.7.x1 (new), 9.1.4.x2 (new), 9.1.4.x3 (new), 9.1.4.x4 (new), 9.3.3, 9.3.4, 9.3.5, 9.3.7 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 36.420 CR0022 Rel-16 | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | rev 1: adding co-signers | | | | | | | | |

<<<<<<<<<<<<<<<<<<<< First Change >>>>>>>>>>>>>>>>>>>>

# 7 Functions of X2AP

The X2AP protocol provides the following functions:

- Mobility Management. This function allows the eNB to move the responsibility of a certain UE to another eNB. Forwarding of user plane data, Status Transfer and UE Context Release function are parts of the mobility management.

- Dual Connectivity. This function allows the eNB to request another eNB to provide radio resources for a certain UE while keeping responsibility for that UE.

- E-UTRA-NR Dual Connectivity. This function allows the eNB to request another en-gNB to provide radio resources for a certain UE while keeping responsibility for that UE.

- Load Management. This function is used by eNBs to indicate resource status, overload and traffic load to each other.

- Reporting of General Error Situations. This function allows reporting of general error situations, for which function specific error messages have not been defined.

- Resetting the X2. This function is used to reset the X2 interface.

- Setting up the X2. This function is used to exchange necessary data for the eNB or en-gNB for setup the X2 interface and implicitly perform an X2 Reset.

- eNB Configuration Update. This function allows updating of application level data needed for two eNBs to interoperate correctly over the X2 interface.

- Mobility Parameters Management. This function allows the eNB to coordinate adaptation of mobility parameter settings with a peer eNB.

- Mobility Robustness Optimisation. This function allows reporting of information related to mobility failure events.

- Energy Saving. This function allows decreasing energy consumption by enabling indication of cell activation/deactivation over the X2 interface.

- X2 Release. This function allows an eNB to be aware that the signalling connection to a peer eNB is unavailable.

- Message Transfer. This function allows indirect transport of X2AP messages to a peer eNB.

- Registration. This function allows registration of eNB in case indirect transport of X2AP messages is supported.

- Removing the X2. This function allows removing the signalling connection between two eNBs or between eNB and en-gNB in a controlled manner.

- Inter-eNB UE Context Retrieval. This function allows retrieval of a UE context in case of resumption or re-establishment of an RRC connection.

- Secondary RAT Data Usage Report. This function allows eNB to get the uplink and downlink data volumes for the Secondary RAT on a per E-RAB basis.

- E-UTRA - NR Spectrum Sharing. This function allows uplink and downlink spectrum sharing between a number of E - UTRA and a number of NR cells with overlapping coverage.

- EN-DC Configuration Transfer. This function supports en-gNB X2 TNL address discovery.

- EN-DC Load Management. This function is used by MeNB/en-gNB to indicate resource status, overload and traffic load to each other.

- UE Radio Capability ID Mapping.

The mapping between the above functions and X2 EPs is shown in the table below.

Table 7-1: Mapping between X2AP functions and X2AP EPs

| Function | Elementary Procedure(s) |
| --- | --- |
| Mobility Management | a) Handover Preparation b) SN Status Transfer c) UE Context Release  d) Handover Cancel  e) Handover Success  f) Conditional Handover Cancel |
| Dual Connectivity | a) SeNB Addition Preparation  b) SeNB Reconfiguration Completion  c) MeNB initiated SeNB Modification Preparation  d) SeNB initiated SeNB Modification  e) MeNB initiated SeNB Release  f) SeNB initiated SeNB Release  g) SeNB Counter Check |
| E-UTRA-NR Dual Connectivity | a) SgNB Addition Preparation  b) SgNB Reconfiguration Completion  c) MeNB initiated SgNB Modification Preparation  d) SgNB initiated SgNB Modification  e) SgNB change  f) MeNB initiated SgNB Release  g) SgNB initiated SgNB Release  h) SgNB Counter Check  i) RRC transfer  j) EN-DC X2 Setup  k) EN-DC Configuration Update  l) EN-DC Cell Activation  m) SgNB Activity Notification  n) EN-DC X2 Removal  o) gNB Status Indication  p) EN-DC Resource Status Reporting Initiation  q) EN-DC Resource Status Reporting  r) F1-C Traffic Transfer |
| Load Management | a) Load Indication  b) Resource Status Reporting Initiation  c) Resource Status Reporting |
| Reporting of General Error Situations | Error Indication |
| Resetting the X2 | Reset |
| Setting up the X2 | X2 Setup |
| eNB Configuration Update | a) eNB Configuration Update  b) Cell Activation |
| Mobility Parameters Management | Mobility Settings Change |
| Mobility Robustness Optimisation | a) Radio Link Failure Indication  b) Handover Report |
| Energy Saving | a) eNB Configuration Update  b) Cell Activation |
| X2 Release | X2 Release |
| Message Transfer Registration | X2AP Message Transfer |
| Removing the X2 | X2 Removal |
| Inter-eNB UE Context Retrieval | a) Retrieve UE Context  b) Data Forwarding Address Indication |
| Secondary RAT Data Usage Report | Secondary RAT Data Usage Report |
| E-UTRA – NR Spectrum Sharing | E-UTRA - NR Cell Resource Coordination |
| EN-DC Configuration Transfer | EN-DC Configuration Transfer |
| UE Radio Capability ID Mapping | UE Radio Capability ID Mapping |

# 8 X2AP procedures

## 8.1 Elementary procedures

In the following tables, all EPs are divided into Class 1 and Class 2 EPs.

Table 8.1-1: Class 1 Elementary Procedures

| Elementary Procedure | Initiating Message | Successful Outcome | Unsuccessful Outcome | |
| --- | --- | --- | --- | --- |
| Response message | Response message | |
| Handover Preparation | HANDOVER REQUEST | HANDOVER REQUEST ACKNOWLEDGE | HANDOVER PREPARATION FAILURE |
| Reset | RESET REQUEST | RESET RESPONSE |  |
| X2 Setup | X2 SETUP REQUEST | X2 SETUP RESPONSE | X2 SETUP FAILURE |
| eNB Configuration Update | ENB CONFIGURATION UPDATE | ENB CONFIGURATION UPDATE ACKNOWLEDGE | ENB CONFIGURATION UPDATE FAILURE |
| Resource Status Reporting Initiation | RESOURCE STATUS REQUEST | RESOURCE STATUS RESPONSE | RESOURCE STATUS FAILURE |
| Mobility Settings Change | MOBILITY CHANGE REQUEST | MOBILITY CHANGE ACKNOWLEDGE | MOBILITY CHANGE FAILURE |
| Cell Activation | CELL ACTIVATION REQUEST | CELL ACTIVATION RESPONSE | CELL ACTIVATION FAILURE |
| SeNB Addition Preparation | SENB ADDITION REQUEST | SENB ADDITION REQUEST ACKNOWLEDGE | SENB ADDITION REQUEST REJECT |
| MeNB initiated SeNB Modification Preparation | SENB MODIFICATION REQUEST | SENB MODIFICATION REQUEST ACKNOWLEDGE | SENB MODIFICATION REQUEST REJECT |
| SeNB initiated SeNB Modification | SENB MODIFICATION REQUIRED | SENB MODIFICATION CONFIRM | SENB MODIFICATION REFUSE |
| SeNB initiated SeNB Release | SENB RELEASE REQUIRED | SENB RELEASE CONFIRM |  |
| X2 Removal | X2 REMOVAL REQUEST | X2 REMOVAL RESPONSE | X2 REMOVAL FAILURE |
| Retrieve UE Context | RETRIEVE UE CONTEXT REQUEST | RETRIEVE UE CONTEXT RESPONSE | RETRIEVE UE CONTEXT FAILURE |
| SgNB Addition Preparation | SGNB ADDITION REQUEST | SGNB ADDITION REQUEST ACKNOWLEDGE | SGNB ADDITION REQUEST REJECT |
| MeNB initiated SgNB Modification Preparation | SGNB MODIFICATION REQUEST | SGNB MODIFICATION REQUEST ACKNOWLEDGE | SGNB MODIFICATION REQUEST REJECT |
| SgNB initiated SgNB Modification | SGNB MODIFICATION REQUIRED | SGNB MODIFICATION CONFIRM | SGNB MODIFICATION REFUSE |
| SgNB change | SGNB CHANGE REQUIRED | SGNB CHANGE CONFIRM | SGNB CHANGE REFUSE |
| MeNB initiated SgNB Release | SGNB RELEASE REQUEST | SGNB RELEASE REQUEST ACKNOWLEDGE | SGNB RELEASE REQUEST REJECT |
| SgNB initiated SgNB Release | SGNB RELEASE REQUIRED | SGNB RELEASE CONFIRM |  |
| EN-DC X2 Setup | EN-DC X2 SETUP REQUEST | EN-DC X2 SETUP RESPONSE | EN-DC X2 SETUP FAILURE |
| EN-DC Configuration Update | EN-DC CONFIGURATION UPDATE | EN-DC CONFIGURATION UPDATE ACKNOWLEDGE | EN-DC CONFIGURATION UPDATE FAILURE |
| EN-DC Cell Activation | EN-DC CELL ACTIVATION REQUEST | EN-DC CELL ACTIVATION RESPONSE | EN-DC CELL ACTIVATION FAILURE |
| E-UTRA - NR Cell Resource Coordination | E-UTRA - NR CELL RESOURCE COORDINATION REQUEST | E-UTRA - NR CELL RESOURCE COORDINATION RESPONSE |  |
| EN-DC X2 Removal | EN-DC X2 REMOVAL REQUEST | EN-DC X2 REMOVAL RESPONSE | EN-DC X2 REMOVAL FAILURE |
| EN-DC Resource Status Reporting Initiation | EN-DC RESOURCE STATUS REQUEST | EN-DC RESOURCE STATUS RESPONSE | EN-DC RESOURCE STATUS FAILURE |
| UE Radio Capability ID Mapping | UE RADIO CAPABILITY ID MAPPING REQUEST | UE RADIO CAPABILITY ID MAPPING RESPONSE |  |

Table 8.1-2: Class 2 Elementary Procedures

| Elementary Procedure | Initiating Message |
| --- | --- |
| Load Indication | LOAD INFORMATION |
| Handover Cancel | HANDOVER CANCEL |
| SN Status Transfer | SN STATUS TRANSFER |
| UE Context Release | UE CONTEXT RELEASE |
| Resource Status Reporting | RESOURCE STATUS UPDATE |
| Error Indication | ERROR INDICATION |
| Radio Link Failure Indication | RLF INDICATION |
| Handover Report | HANDOVER REPORT |
| X2 Release | X2 RELEASE |
| X2AP Message Transfer | X2AP MESSAGE TRANSFER |
| SeNB Reconfiguration Completion | SENB RECONFIGURATION COMPLETE |
| MeNB initiated SeNB Release | SENB RELEASE REQUEST |
| SeNB Counter Check | SENB COUNTER CHECK REQUEST |
| SgNB Reconfiguration Completion | SGNB RECONFIGURATION COMPLETE |
| SgNB Counter Check | SGNB COUNTER CHECK REQUEST |
| RRC Transfer | RRC TRANSFER |
| Secondary RAT Data Usage Report | SECONDARY RAT DATA USAGE REPORT |
| SgNB Activity Notification | SGNB ACTIVITY NOTIFICATION |
| Data Forwarding Address Indication | DATA FORWARDING ADDRESS INDICATION |
| gNB Status Indication | GNB STATUS INDICATION |
| EN-DC Configuration Transfer | EN-DC CONFIGURATION TRANSFER |
| Trace Start | TRACE START |
| Deactivate Trace | DEACTIVATE TRACE |
| Handover Success | HANDOVER SUCCESS |
| Conditional Handover Cancel | CONDITIONAL HANDOVER CANCEL |
| Early Status Transfer | EARLY STATUS TRANSFER |
| EN-DC Resource Status Reporting | EN-DC RESOURCE STATUS UPDATE |
| Cell Traffic Trace | CELL TRAFFIC TRACE |
| F1-C Traffic Transfer | F1-C TRAFFIC TRANSFER |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 8.7.x1 UE Radio Capability ID Mapping

#### 8.7.x1.1 General

The purpose of the UE Radio Capability ID Mapping procedure is to enable an en-gNB to request a connected eNB to provide the UE Radio Capability information that maps to a specific UE Radio Capability ID.

The procedure uses non-UE-associated signalling.

#### 8.7.x1.2 Successful Operation



Figure 8.7.x1.2-1: UE Radio Capability ID Mapping procedure. Successful operation

The en-gNB initiates the procedure by sending a UE RADIO CAPABILITY ID MAPPING REQUEST message to the eNB.

Upon receipt of the UE RADIO CAPABILITY ID MAPPING REQUEST message, the eNB shall include the UE Radio Capability information that maps to the UE Radio Capability ID indicated in the UE RADIO CAPABILITY ID MAPPING REQUEST message in the UE RADIO CAPABILITY ID MAPPING RESPONSE message.

#### 8.7.x1.3 Unsuccessful Operation

Not applicable.

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

#### 9.1.4.x2 UE Radio Capability ID Mapping Request

This message is sent by the en-gNB and is used to request the UE Radio Capability information that maps to a specific UE Radio Capability ID.

Direction: en-gNB → eNB

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.13 |  | YES | reject |
| UE Radio Capability ID | M |  | 9.2.171 |  | YES | reject |

#### 9.1.4.x3 UE Radio Capability ID Mapping Response

This message is sent by the eNB and is used to provide the UE Radio Capability information that maps to a specific UE Radio Capability ID indicated in the UE RADIO CAPABILITY ID MAPPING REQUEST message.

Direction: eNB → en-gNB.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.13 |  | YES | reject |
| UE Radio Capability ID | M |  | 9.2.171 |  | YES | reject |
| UE Radio Capability | M |  | 9.2.x4 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.2.7 |  | YES | ignore |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.2.x4 UE Radio Capability

This IE contains UE Radio Capability information.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| UE Radio Capability | M |  | OCTET STRING | Includes the *UERadioAccessCapabilityInformation* message as defined in 10.2.2 ofTS 36.331 [9]. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 

### 9.3.3 Elementary Procedure Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-PDU-Descriptions (0) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Criticality,

ProcedureCode

FROM X2AP-CommonDataTypes

CellActivationRequest,

CellActivationResponse,

CellActivationFailure,

ENBConfigurationUpdate,

ENBConfigurationUpdateAcknowledge,

ENBConfigurationUpdateFailure,

ErrorIndication,

HandoverCancel,

HandoverReport,

HandoverPreparationFailure,

HandoverRequest,

HandoverRequestAcknowledge,

LoadInformation,

PrivateMessage,

ResetRequest,

ResetResponse,

ResourceStatusFailure,

ResourceStatusRequest,

ResourceStatusResponse,

ResourceStatusUpdate,

RLFIndication,

SNStatusTransfer,

UEContextRelease,

X2SetupFailure,

X2SetupRequest,

X2SetupResponse,

MobilityChangeRequest,

MobilityChangeAcknowledge,

MobilityChangeFailure,

X2Release,

X2APMessageTransfer,

SeNBAdditionRequest,

SeNBAdditionRequestAcknowledge,

SeNBAdditionRequestReject,

SeNBReconfigurationComplete,

SeNBModificationRequest,

SeNBModificationRequestAcknowledge,

SeNBModificationRequestReject,

SeNBModificationRequired,

SeNBModificationConfirm,

SeNBModificationRefuse,

SeNBReleaseRequest,

SeNBReleaseRequired,

SeNBReleaseConfirm,

SeNBCounterCheckRequest,

X2RemovalFailure,

X2RemovalRequest,

X2RemovalResponse,

RetrieveUEContextRequest,

RetrieveUEContextResponse,

RetrieveUEContextFailure,

SgNBAdditionRequest,

SgNBAdditionRequestAcknowledge,

SgNBAdditionRequestReject,

SgNBReconfigurationComplete,

SgNBModificationRequest,

SgNBModificationRequestAcknowledge,

SgNBModificationRequestReject,

SgNBModificationRequired,

SgNBModificationConfirm,

SgNBModificationRefuse,

SgNBReleaseRequest,

SgNBReleaseRequestAcknowledge,

SgNBReleaseRequestReject,

SgNBReleaseRequired,

SgNBReleaseConfirm,

SgNBCounterCheckRequest,

SgNBChangeRequired,

SgNBChangeConfirm,

SgNBChangeRefuse,

RRCTransfer,

ENDCX2SetupRequest,

ENDCX2SetupResponse,

ENDCX2SetupFailure,

ENDCConfigurationUpdate,

ENDCConfigurationUpdateAcknowledge,

ENDCConfigurationUpdateFailure,

SecondaryRATDataUsageReport,

ENDCCellActivationRequest,

ENDCCellActivationResponse,

ENDCCellActivationFailure,

ENDCPartialResetRequired,

ENDCPartialResetConfirm,

EUTRANRCellResourceCoordinationRequest,

EUTRANRCellResourceCoordinationResponse,

SgNBActivityNotification,

ENDCX2RemovalRequest,

ENDCX2RemovalResponse,

ENDCX2RemovalFailure,

DataForwardingAddressIndication,

GNBStatusIndication,

ENDCConfigurationTransfer,

DeactivateTrace,

TraceStart,

HandoverSuccess,

EarlyStatusTransfer,

ConditionalHandoverCancel,

ENDCResourceStatusRequest,

ENDCResourceStatusResponse,

ENDCResourceStatusFailure,

ENDCResourceStatusUpdate,

CellTrafficTrace,

F1CTrafficTransfer,

UERadioCapabilityIDMappingRequest,

UERadioCapabilityIDMappingResponse

FROM X2AP-PDU-Contents

id-cellActivation,

id-eNBConfigurationUpdate,

id-errorIndication,

id-handoverCancel,

id-handoverReport,

id-handoverPreparation,

id-loadIndication,

id-privateMessage,

id-reset,

id-resourceStatusReporting,

id-resourceStatusReportingInitiation,

id-rLFIndication,

id-snStatusTransfer,

id-uEContextRelease,

id-x2Setup,

id-mobilitySettingsChange,

id-x2Release,

id-x2APMessageTransfer,

id-seNBAdditionPreparation,

id-seNBReconfigurationCompletion,

id-meNBinitiatedSeNBModificationPreparation,

id-seNBinitiatedSeNBModification,

id-meNBinitiatedSeNBRelease,

id-seNBinitiatedSeNBRelease,

id-seNBCounterCheck,

id-x2Removal,

id-retrieveUEContext,

id-sgNBAdditionPreparation,

id-sgNBReconfigurationCompletion,

id-meNBinitiatedSgNBModificationPreparation,

id-sgNBinitiatedSgNBModification,

id-meNBinitiatedSgNBRelease,

id-sgNBinitiatedSgNBRelease,

id-sgNBChange,

id-sgNBCounterCheck,

id-rRCTransfer,

id-endcX2Setup,

id-endcConfigurationUpdate,

id-secondaryRATDataUsageReport,

id-endcCellActivation,

id-endcPartialReset,

id-eUTRANRCellResourceCoordination,

id-SgNBActivityNotification,

id-endcX2Removal,

id-dataForwardingAddressIndication,

id-gNBStatusIndication,

id-endcConfigurationTransfer,

id-deactivateTrace,

id-traceStart,

id-handoverSuccess,

id-earlyStatusTransfer,

id-conditionalHandoverCancel,

id-endcresourceStatusReporting,

id-endcresourceStatusReportingInitiation,

id-cellTrafficTrace,

id-f1CTrafficTransfer,

id-UERadioCapabilityIDMapping

FROM X2AP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure Class

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-ELEMENTARY-PROCEDURE ::= CLASS {

&InitiatingMessage ,

&SuccessfulOutcome OPTIONAL,

&UnsuccessfulOutcome OPTIONAL,

&procedureCode ProcedureCode UNIQUE,

&criticality Criticality DEFAULT ignore

}

WITH SYNTAX {

INITIATING MESSAGE &InitiatingMessage

[SUCCESSFUL OUTCOME &SuccessfulOutcome]

[UNSUCCESSFUL OUTCOME &UnsuccessfulOutcome]

PROCEDURE CODE &procedureCode

[CRITICALITY &criticality]

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface PDU Definition

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-PDU ::= CHOICE {

initiatingMessage InitiatingMessage,

successfulOutcome SuccessfulOutcome,

unsuccessfulOutcome UnsuccessfulOutcome,

...

}

InitiatingMessage ::= SEQUENCE {

procedureCode X2AP-ELEMENTARY-PROCEDURE.&procedureCode ({X2AP-ELEMENTARY-PROCEDURES}),

criticality X2AP-ELEMENTARY-PROCEDURE.&criticality ({X2AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value X2AP-ELEMENTARY-PROCEDURE.&InitiatingMessage ({X2AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

SuccessfulOutcome ::= SEQUENCE {

procedureCode X2AP-ELEMENTARY-PROCEDURE.&procedureCode ({X2AP-ELEMENTARY-PROCEDURES}),

criticality X2AP-ELEMENTARY-PROCEDURE.&criticality ({X2AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value X2AP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome ({X2AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

UnsuccessfulOutcome ::= SEQUENCE {

procedureCode X2AP-ELEMENTARY-PROCEDURE.&procedureCode ({X2AP-ELEMENTARY-PROCEDURES}),

criticality X2AP-ELEMENTARY-PROCEDURE.&criticality ({X2AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value X2AP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome ({X2AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-ELEMENTARY-PROCEDURES X2AP-ELEMENTARY-PROCEDURE ::= {

X2AP-ELEMENTARY-PROCEDURES-CLASS-1 |

X2AP-ELEMENTARY-PROCEDURES-CLASS-2 ,

...

}

X2AP-ELEMENTARY-PROCEDURES-CLASS-1 X2AP-ELEMENTARY-PROCEDURE ::= {

handoverPreparation |

reset |

x2Setup |

resourceStatusReportingInitiation |

eNBConfigurationUpdate |

mobilitySettingsChange |

cellActivation |

seNBAdditionPreparation |

meNBinitiatedSeNBModificationPreparation |

seNBinitiatedSeNBModification |

seNBinitiatedSeNBRelease |

x2Removal |

retrieveUEContext |

sgNBAdditionPreparation |

meNBinitiatedSgNBModificationPreparation |

sgNBinitiatedSgNBModification |

meNBinitiatedSgNBRelease |

sgNBinitiatedSgNBRelease |

sgNBChange |

endcX2Setup |

endcConfigurationUpdate |

endcCellActivation |

endcPartialReset |

eUTRANRCellResourceCoordination |

endcX2Removal |

endcresourceStatusReportingInitiation |

uERadioCapabilityMapping ,

...

}

X2AP-ELEMENTARY-PROCEDURES-CLASS-2 X2AP-ELEMENTARY-PROCEDURE ::= {

snStatusTransfer |

uEContextRelease |

handoverCancel |

errorIndication |

resourceStatusReporting |

loadIndication |

privateMessage |

rLFIndication |

handoverReport |

x2Release |

x2APMessageTransfer |

seNBReconfigurationCompletion |

meNBinitiatedSeNBRelease |

seNBCounterCheck |

sgNBReconfigurationCompletion |

sgNBCounterCheck |

rRCTransfer |

secondaryRATDataUsageReport |

sgNBActivityNotification |

dataForwardingAddressIndication |

gNBStatusIndication |

endcConfigurationTransfer |

deactivateTrace |

traceStart |

handoverSuccess |

earlyStatusTransfer |

conditionalHandoverCancel |

endcresourceStatusReporting |

cellTrafficTrace |

f1CTrafficTransfer ,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

handoverPreparation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverRequest

SUCCESSFUL OUTCOME HandoverRequestAcknowledge

UNSUCCESSFUL OUTCOME HandoverPreparationFailure

PROCEDURE CODE id-handoverPreparation

CRITICALITY reject

}

snStatusTransfer X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SNStatusTransfer

PROCEDURE CODE id-snStatusTransfer

CRITICALITY ignore

}

uEContextRelease X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE UEContextRelease

PROCEDURE CODE id-uEContextRelease

CRITICALITY ignore

}

handoverCancel X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverCancel

PROCEDURE CODE id-handoverCancel

CRITICALITY ignore

}

handoverReport X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverReport

PROCEDURE CODE id-handoverReport

CRITICALITY ignore

}

errorIndication X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ErrorIndication

PROCEDURE CODE id-errorIndication

CRITICALITY ignore

}

reset X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ResetRequest

SUCCESSFUL OUTCOME ResetResponse

PROCEDURE CODE id-reset

CRITICALITY reject

}

x2Setup X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE X2SetupRequest

SUCCESSFUL OUTCOME X2SetupResponse

UNSUCCESSFUL OUTCOME X2SetupFailure

PROCEDURE CODE id-x2Setup

CRITICALITY reject

}

loadIndication X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE LoadInformation

PROCEDURE CODE id-loadIndication

CRITICALITY ignore

}

eNBConfigurationUpdate X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENBConfigurationUpdate

SUCCESSFUL OUTCOME ENBConfigurationUpdateAcknowledge

UNSUCCESSFUL OUTCOME ENBConfigurationUpdateFailure

PROCEDURE CODE id-eNBConfigurationUpdate

CRITICALITY reject

}

resourceStatusReportingInitiation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ResourceStatusRequest

SUCCESSFUL OUTCOME ResourceStatusResponse

UNSUCCESSFUL OUTCOME ResourceStatusFailure

PROCEDURE CODE id-resourceStatusReportingInitiation

CRITICALITY reject

}

resourceStatusReporting X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ResourceStatusUpdate

PROCEDURE CODE id-resourceStatusReporting

CRITICALITY ignore

}

rLFIndication X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE RLFIndication

PROCEDURE CODE id-rLFIndication

CRITICALITY ignore

}

privateMessage X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PrivateMessage

PROCEDURE CODE id-privateMessage

CRITICALITY ignore

}

mobilitySettingsChange X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MobilityChangeRequest

SUCCESSFUL OUTCOME MobilityChangeAcknowledge

UNSUCCESSFUL OUTCOME MobilityChangeFailure

PROCEDURE CODE id-mobilitySettingsChange

CRITICALITY reject

}

cellActivation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE CellActivationRequest

SUCCESSFUL OUTCOME CellActivationResponse

UNSUCCESSFUL OUTCOME CellActivationFailure

PROCEDURE CODE id-cellActivation

CRITICALITY reject

}

x2Release X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE X2Release

PROCEDURE CODE id-x2Release

CRITICALITY reject

}

x2APMessageTransfer X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE X2APMessageTransfer

PROCEDURE CODE id-x2APMessageTransfer

CRITICALITY reject

}

seNBAdditionPreparation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBAdditionRequest

SUCCESSFUL OUTCOME SeNBAdditionRequestAcknowledge

UNSUCCESSFUL OUTCOME SeNBAdditionRequestReject

PROCEDURE CODE id-seNBAdditionPreparation

CRITICALITY reject

}

seNBReconfigurationCompletion X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBReconfigurationComplete

PROCEDURE CODE id-seNBReconfigurationCompletion

CRITICALITY ignore

}

meNBinitiatedSeNBModificationPreparation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBModificationRequest

SUCCESSFUL OUTCOME SeNBModificationRequestAcknowledge

UNSUCCESSFUL OUTCOME SeNBModificationRequestReject

PROCEDURE CODE id-meNBinitiatedSeNBModificationPreparation

CRITICALITY reject

}

seNBinitiatedSeNBModification X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBModificationRequired

SUCCESSFUL OUTCOME SeNBModificationConfirm

UNSUCCESSFUL OUTCOME SeNBModificationRefuse

PROCEDURE CODE id-seNBinitiatedSeNBModification

CRITICALITY reject

}

meNBinitiatedSeNBRelease X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBReleaseRequest

PROCEDURE CODE id-meNBinitiatedSeNBRelease

CRITICALITY ignore

}

seNBinitiatedSeNBRelease X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBReleaseRequired

SUCCESSFUL OUTCOME SeNBReleaseConfirm

PROCEDURE CODE id-seNBinitiatedSeNBRelease

CRITICALITY reject

}

seNBCounterCheck X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SeNBCounterCheckRequest

PROCEDURE CODE id-seNBCounterCheck

CRITICALITY reject

}

x2Removal X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE X2RemovalRequest

SUCCESSFUL OUTCOME X2RemovalResponse

UNSUCCESSFUL OUTCOME X2RemovalFailure

PROCEDURE CODE id-x2Removal

CRITICALITY reject

}

retrieveUEContext X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE RetrieveUEContextRequest

SUCCESSFUL OUTCOME RetrieveUEContextResponse

UNSUCCESSFUL OUTCOME RetrieveUEContextFailure

PROCEDURE CODE id-retrieveUEContext

CRITICALITY reject

}

sgNBAdditionPreparation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBAdditionRequest

SUCCESSFUL OUTCOME SgNBAdditionRequestAcknowledge

UNSUCCESSFUL OUTCOME SgNBAdditionRequestReject

PROCEDURE CODE id-sgNBAdditionPreparation

CRITICALITY reject

}

sgNBReconfigurationCompletion X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBReconfigurationComplete

PROCEDURE CODE id-sgNBReconfigurationCompletion

CRITICALITY ignore

}

meNBinitiatedSgNBModificationPreparation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBModificationRequest

SUCCESSFUL OUTCOME SgNBModificationRequestAcknowledge

UNSUCCESSFUL OUTCOME SgNBModificationRequestReject

PROCEDURE CODE id-meNBinitiatedSgNBModificationPreparation

CRITICALITY reject

}

sgNBinitiatedSgNBModification X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBModificationRequired

SUCCESSFUL OUTCOME SgNBModificationConfirm

UNSUCCESSFUL OUTCOME SgNBModificationRefuse

PROCEDURE CODE id-sgNBinitiatedSgNBModification

CRITICALITY reject

}

meNBinitiatedSgNBRelease X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBReleaseRequest

SUCCESSFUL OUTCOME SgNBReleaseRequestAcknowledge

UNSUCCESSFUL OUTCOME SgNBReleaseRequestReject

PROCEDURE CODE id-meNBinitiatedSgNBRelease

CRITICALITY ignore

}

sgNBinitiatedSgNBRelease X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBReleaseRequired

SUCCESSFUL OUTCOME SgNBReleaseConfirm

PROCEDURE CODE id-sgNBinitiatedSgNBRelease

CRITICALITY reject

}

sgNBCounterCheck X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBCounterCheckRequest

PROCEDURE CODE id-sgNBCounterCheck

CRITICALITY reject

}

sgNBChange X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBChangeRequired

SUCCESSFUL OUTCOME SgNBChangeConfirm

UNSUCCESSFUL OUTCOME SgNBChangeRefuse

PROCEDURE CODE id-sgNBChange

CRITICALITY reject

}

rRCTransfer X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE RRCTransfer

PROCEDURE CODE id-rRCTransfer

CRITICALITY reject

}

endcX2Setup X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCX2SetupRequest

SUCCESSFUL OUTCOME ENDCX2SetupResponse

UNSUCCESSFUL OUTCOME ENDCX2SetupFailure

PROCEDURE CODE id-endcX2Setup

CRITICALITY reject

}

endcConfigurationUpdate X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCConfigurationUpdate

SUCCESSFUL OUTCOME ENDCConfigurationUpdateAcknowledge

UNSUCCESSFUL OUTCOME ENDCConfigurationUpdateFailure

PROCEDURE CODE id-endcConfigurationUpdate

CRITICALITY reject

}

secondaryRATDataUsageReport X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SecondaryRATDataUsageReport

PROCEDURE CODE id-secondaryRATDataUsageReport

CRITICALITY reject

}

endcCellActivation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCCellActivationRequest

SUCCESSFUL OUTCOME ENDCCellActivationResponse

UNSUCCESSFUL OUTCOME ENDCCellActivationFailure

PROCEDURE CODE id-endcCellActivation

CRITICALITY reject

}

endcPartialReset X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCPartialResetRequired

SUCCESSFUL OUTCOME ENDCPartialResetConfirm

PROCEDURE CODE id-endcPartialReset

CRITICALITY reject

}

eUTRANRCellResourceCoordination X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE EUTRANRCellResourceCoordinationRequest

SUCCESSFUL OUTCOME EUTRANRCellResourceCoordinationResponse

PROCEDURE CODE id-eUTRANRCellResourceCoordination

CRITICALITY reject

}

sgNBActivityNotification X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE SgNBActivityNotification

PROCEDURE CODE id-SgNBActivityNotification

CRITICALITY reject

}

endcX2Removal X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCX2RemovalRequest

SUCCESSFUL OUTCOME ENDCX2RemovalResponse

UNSUCCESSFUL OUTCOME ENDCX2RemovalFailure

PROCEDURE CODE id-endcX2Removal

CRITICALITY reject

}

dataForwardingAddressIndication X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE DataForwardingAddressIndication

PROCEDURE CODE id-dataForwardingAddressIndication

CRITICALITY ignore

}

gNBStatusIndication X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNBStatusIndication

PROCEDURE CODE id-gNBStatusIndication

CRITICALITY ignore

}

endcConfigurationTransfer X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCConfigurationTransfer

PROCEDURE CODE id-endcConfigurationTransfer

CRITICALITY ignore

}

deactivateTrace X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE DeactivateTrace

PROCEDURE CODE id-deactivateTrace

CRITICALITY ignore

}

traceStart X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE TraceStart

PROCEDURE CODE id-traceStart

CRITICALITY ignore

}

handoverSuccess X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE HandoverSuccess

PROCEDURE CODE id-handoverSuccess

CRITICALITY ignore

}

earlyStatusTransfer X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE EarlyStatusTransfer

PROCEDURE CODE id-earlyStatusTransfer

CRITICALITY ignore

}

conditionalHandoverCancel X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ConditionalHandoverCancel

PROCEDURE CODE id-conditionalHandoverCancel

CRITICALITY ignore

}

endcresourceStatusReportingInitiation X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCResourceStatusRequest

SUCCESSFUL OUTCOME ENDCResourceStatusResponse

UNSUCCESSFUL OUTCOME ENDCResourceStatusFailure

PROCEDURE CODE id-endcresourceStatusReportingInitiation

CRITICALITY reject

}

endcresourceStatusReporting X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ENDCResourceStatusUpdate

PROCEDURE CODE id-endcresourceStatusReporting

CRITICALITY ignore

}

cellTrafficTrace X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE CellTrafficTrace

PROCEDURE CODE id-cellTrafficTrace

CRITICALITY ignore

}

f1CTrafficTransfer X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE F1CTrafficTransfer

PROCEDURE CODE id-f1CTrafficTransfer

CRITICALITY ignore

}

uERadioCapabilityIDMapping X2AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE UERadioCapabilityIDMappingRequest

SUCCESSFUL OUTCOME UERadioCapabilityIDMappingResponse

PROCEDURE CODE id-UERadioCapabilityIDMapping

CRITICALITY reject

}

END

-- ASN1STOP

### 9.3.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for X2AP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

ABSInformation,

ABS-Status,

AS-SecurityInformation,

BearerType,

Cause,

CompositeAvailableCapacityGroup,

Correlation-ID,

COUNTvalue,

CellReportingIndicator,

AerialUEsubscriptionInformation,

CriticalityDiagnostics,

CRNTI,

CSGMembershipStatus,

CSG-Id,

DeactivationIndication,

DL-Forwarding,

DynamicDLTransmissionInformation,

E-RABsSubjectToDLDiscarding-List,

E-RABsSubjectToEarlyStatusTransfer-List,

ECGI,

E-RAB-ID,

E-RAB-Level-QoS-Parameters,

E-RAB-List,

EUTRANTraceID,

GlobalENB-ID,

GTPtunnelEndpoint,

GUGroupIDList,

GUMMEI,

HandoverReportType,

HandoverRestrictionList,

Masked-IMEISV,

InvokeIndication,

LocationReportingInformation,

LowerLayerPresenceStatusChange,

MDT-Configuration,

ManagementBasedMDTallowed,

MDTPLMNList,

Neighbour-Information,

PCI,

PDCP-SN,

PLMN-Identity,

ReceiveStatusofULPDCPSDUs,

Registration-Request,

RelativeNarrowbandTxPower,

RadioResourceStatus,

RLC-Status,

RRCConnReestabIndicator,

RRCConnSetupIndicator,

UE-RLF-Report-Container,

UEAppLayerMeasConfig,

RRC-Context,

ServedCell-Information,

ServedCells,

ShortMAC-I,

SRVCCOperationPossible,

SubscriberProfileIDforRFP,

TargetCellInUTRAN,

TargeteNBtoSource-eNBTransparentContainer,

TimeToWait,

TraceActivation,

TraceDepth,

TransportLayerAddress,

UEAggregateMaximumBitRate,

UE-HistoryInformation,

UE-HistoryInformationFromTheUE,

UE-S1AP-ID,

UESecurityCapabilities,

UEsToBeResetList,

UE-X2AP-ID,

UL-HighInterferenceIndicationInfo,

UL-InterferenceOverloadIndication,

HWLoadIndicator,

S1TNLLoadIndicator,

Measurement-ID,

ReportCharacteristics,

MobilityParametersInformation,

MobilityParametersModificationRange,

ReceiveStatusOfULPDCPSDUsExtended,

COUNTValueExtended,

SubframeAssignment,

ExtendedULInterferenceOverloadInfo,

ExpectedUEBehaviour,

SeNBSecurityKey,

MeNBtoSeNBContainer,

SeNBtoMeNBContainer,

SCGChangeIndication,

CoMPInformation,

ReportingPeriodicityRSRPMR,

RSRPMRList,

UE-RLF-Report-Container-for-extended-bands,

ProSeAuthorized,

CoverageModificationList,

ReportingPeriodicityCSIR,

CSIReportList,

ReceiveStatusOfULPDCPSDUsPDCP-SNlength18,

COUNTvaluePDCP-SNlength18,

LHN-ID,

UE-ContextKeptIndicator,

UE-X2AP-ID-Extension,

SIPTOBearerDeactivationIndication,

TunnelInformation,

V2XServicesAuthorized,

X2BenefitValue,

ResumeID,

EUTRANCellIdentifier,

MakeBeforeBreakIndicator,

WTID,

WT-UE-XwAP-ID,

UESidelinkAggregateMaximumBitRate,

SgNBSecurityKey,

MeNBtoSgNBContainer,

SgNBtoMeNBContainer,

SplitSRBs,

RRCContainer,

SRBType,

GlobalGNB-ID,

GNB-ID,

SCGConfigurationQuery,

SplitSRB,

NRUeReport,

EN-DC-ResourceConfiguration,

TAC,

NRFreqInfo,

NRCGI,

NRPCI,

NRUESecurityCapabilities,

PDCPChangeIndication,

ULConfiguration,

SgNB-UE-X2AP-ID,

SecondaryRATUsageReportList,

ActivationID,

MeNBResourceCoordinationInformation,

SgNBResourceCoordinationInformation,

NR-TxBW,

BroadcastPLMNs-Item,

AdditionalPLMNs-Item,

RLCMode,

GBR-QosInformation,

DRB-ID,

FiveGS-TAC,

SULInformation,

Packet-LossRate,

ResourceType,

DataTrafficResourceIndication,

SpectrumSharingGroupID,

RRC-Config-Ind,

SGNB-Addition-Trigger-Ind,

UserPlaneTrafficActivityReport,

ERABActivityNotifyItemList,

PDCPSnLength,

Subscription-Based-UE-DifferentiationInfo,

LCID,

DuplicationActivation,

GNBOverloadInformation,

NewDRBIDrequest,

DesiredActNotificationLevel,

LocationInformationSgNB,

LocationInformationSgNBReporting,

EndcSONConfigurationTransfer,

NRNeighbour-Information,

InterfaceInstanceIndication,

BPLMN-ID-Info-NR,

SNtriggered,

EPCHandoverRestrictionListContainer,

AdditionalRRMPriorityIndex,

RequestedFastMCGRecoveryViaSRB3,

AvailableFastMCGRecoveryViaSRB3,

RequestedFastMCGRecoveryViaSRB3Release,

ReleaseFastMCGRecoveryViaSRB3,

FastMCGRecovery,

PartialListIndicator,

MaximumCellListSize,

MessageOversizeNotification,

TNLConfigurationInfo,

TNLA-To-Add-List,

TNLA-To-Update-List,

TNLA-To-Remove-List,

TNLA-Setup-List,

TNLA-Failed-To-Setup-List,

RAN-UE-NGAP-ID,

CHOinformation-REQ,

CHOinformation-ACK,

DAPSRequestInfo,

DAPSResponseInfo,

LowerLayerPresenceStatusChange,

CandidateCellsToBeCancelledList,

CHO-DC-Indicator,

Ethernet-Type,

NRV2XServicesAuthorized,

NRUESidelinkAggregateMaximumBitRate,

PC5QoSParameters,

TargetCellInNGRAN,

Measurement-ID-ENDC,

Registration-Request-ENDC,

ReportCharacteristics-ENDC,

NRRadioResourceStatus,

TNLCapacityIndicator,

NRCompositeAvailableCapacityGroup,

SSBIndex,

TDDULDLConfigurationCommonNR,

NRCarrierList,

SSB-PositionsInBurst,

NRCellPRACHConfig,

NBIoT-RLF-Report-Container, PrivacyIndicator,

UERadioCapabilityID,

CSI-RSTransmissionIndication,

IABNodeIndication,

F1CTrafficContainer,

IABInformation,

UERadioCapability

FROM X2AP-IEs

PrivateIE-Container{},

ProtocolExtensionContainer{},

ProtocolIE-Container{},

ProtocolIE-ContainerList{},

ProtocolIE-ContainerPair{},

ProtocolIE-ContainerPairList{},

ProtocolIE-Single-Container{},

X2AP-PRIVATE-IES,

X2AP-PROTOCOL-EXTENSION,

X2AP-PROTOCOL-IES,

X2AP-PROTOCOL-IES-PAIR

FROM X2AP-Containers

id-ABSInformation,

id-ActivatedCellList,

id-BearerType,

id-Cause,

id-CellInformation,

id-CellInformation-Item,

id-CellMeasurementResult,

id-CellMeasurementResult-ENDC,

id-CellMeasurementResult-Item,

id-CellMeasurementResult-ENDC-Item,

id-CellToReport,

id-CellToReport-ENDC,

id-CellToReport-Item,

id-CellToReport-ENDC-Item,

id-CompositeAvailableCapacityGroup,

id-AerialUEsubscriptionInformation,

id-CriticalityDiagnostics,

id-DeactivationIndication,

id-DynamicDLTransmissionInformation,

id-E-RABs-Admitted-Item,

id-E-RABs-Admitted-List,

id-E-RABs-NotAdmitted-List,

id-E-RABs-SubjectToStatusTransfer-List,

id-E-RABs-SubjectToStatusTransfer-Item,

id-E-RABs-ToBeSetup-Item,

id-GlobalENB-ID,

id-GUGroupIDList,

id-GUGroupIDToAddList,

id-GUGroupIDToDeleteList,

id-GUMMEI-ID,

id-Masked-IMEISV,

id-InvokeIndication,

id-New-eNB-UE-X2AP-ID,

id-Old-eNB-UE-X2AP-ID,

id-Registration-Request,

id-ReportingPeriodicity,

id-RLC-Status,

id-ServedCells,

id-ServedCellsToActivate,

id-ServedCellsToAdd,

id-ServedCellsToModify,

id-ServedCellsToDelete,

id-SRVCCOperationPossible,

id-TargetCell-ID,

id-TargeteNBtoSource-eNBTransparentContainer,

id-TimeToWait,

id-TraceActivation,

id-UE-ContextInformation,

id-UE-HistoryInformation,

id-UE-X2AP-ID,

id-Measurement-ID,

id-ReportCharacteristics,

id-ENB1-Measurement-ID,

id-ENB2-Measurement-ID,

id-ENB1-Cell-ID,

id-ENB2-Cell-ID,

id-ENB2-Proposed-Mobility-Parameters,

id-ENB1-Mobility-Parameters,

id-ENB2-Mobility-Parameters-Modification-Range,

id-FailureCellPCI,

id-Re-establishmentCellECGI,

id-FailureCellCRNTI,

id-ShortMAC-I,

id-SourceCellECGI,

id-FailureCellECGI,

id-HandoverReportType,

id-UE-RLF-Report-Container,

id-PartialSuccessIndicator,

id-MeasurementInitiationResult-List,

id-MeasurementInitiationResult-Item,

id-MeasurementFailureCause-Item,

id-CompleteFailureCauseInformation-List,

id-CompleteFailureCauseInformation-Item,

id-CSGMembershipStatus,

id-CSG-Id,

id-MDTConfiguration,

id-ManagementBasedMDTallowed,

id-ABS-Status,

id-RRCConnSetupIndicator,

id-RRCConnReestabIndicator,

id-TargetCellInUTRAN,

id-MobilityInformation,

id-SourceCellCRNTI,

id-ManagementBasedMDTPLMNList,

id-ReceiveStatusOfULPDCPSDUsExtended,

id-ULCOUNTValueExtended,

id-DLCOUNTValueExtended,

id-IntendedULDLConfiguration,

id-ExtendedULInterferenceOverloadInfo,

id-RNL-Header,

id-x2APMessage,

id-UE-HistoryInformationFromTheUE,

id-ExpectedUEBehaviour,

id-MeNB-UE-X2AP-ID,

id-SeNB-UE-X2AP-ID,

id-UE-SecurityCapabilities,

id-SeNBSecurityKey,

id-SeNBUEAggregateMaximumBitRate,

id-ServingPLMN,

id-E-RABs-ToBeAdded-List,

id-E-RABs-ToBeAdded-Item,

id-MeNBtoSeNBContainer,

id-E-RABs-Admitted-ToBeAdded-List,

id-E-RABs-Admitted-ToBeAdded-Item,

id-SeNBtoMeNBContainer,

id-ResponseInformationSeNBReconfComp,

id-UE-ContextInformationSeNBModReq,

id-E-RABs-ToBeAdded-ModReqItem,

id-E-RABs-ToBeModified-ModReqItem,

id-E-RABs-ToBeReleased-ModReqItem,

id-E-RABs-Admitted-ToBeAdded-ModAckList,

id-E-RABs-Admitted-ToBeModified-ModAckList,

id-E-RABs-Admitted-ToBeReleased-ModAckList,

id-E-RABs-Admitted-ToBeAdded-ModAckItem,

id-E-RABs-Admitted-ToBeModified-ModAckItem,

id-E-RABs-Admitted-ToBeReleased-ModAckItem,

id-SCGChangeIndication,

id-E-RABs-ToBeReleased-ModReqd,

id-E-RABs-ToBeReleased-ModReqdItem,

id-E-RABs-ToBeReleased-List-RelReq,

id-E-RABs-ToBeReleased-RelReqItem,

id-E-RABs-ToBeReleased-List-RelConf,

id-E-RABs-ToBeReleased-RelConfItem,

id-E-RABs-SubjectToCounterCheck-List,

id-E-RABs-SubjectToCounterCheckItem,

id-CoMPInformation,

id-ReportingPeriodicityRSRPMR,

id-RSRPMRList,

id-UE-RLF-Report-Container-for-extended-bands,

id-ProSeAuthorized,

id-CoverageModificationList,

id-ReportingPeriodicityCSIR,

id-CSIReportList,

id-ReceiveStatusOfULPDCPSDUsPDCP-SNlength18,

id-ULCOUNTValuePDCP-SNlength18,

id-DLCOUNTValuePDCP-SNlength18,

id-LHN-ID,

id-Correlation-ID,

id-SIPTO-Correlation-ID,

id-UE-ContextReferenceAtSeNB,

id-UE-ContextReferenceAtWT,

id-UE-ContextKeptIndicator,

id-UEs-ToBeReset,

id-UEs-Admitted-ToBeReset,

id-WT-UE-ContextKeptIndicator,

id-New-eNB-UE-X2AP-ID-Extension,

id-Old-eNB-UE-X2AP-ID-Extension,

id-MeNB-UE-X2AP-ID-Extension,

id-SeNB-UE-X2AP-ID-Extension,

id-SIPTO-BearerDeactivationIndication,

id-Tunnel-Information-for-BBF,

id-SIPTO-L-GW-TransportLayerAddress,

id-GW-TransportLayerAddress,

id-X2RemovalThreshold,

id-CellReportingIndicator,

id-V2XServicesAuthorized,

id-resumeID,

id-UE-ContextInformationRetrieve,

id-E-RABs-ToBeSetupRetrieve-Item,

id-NewEUTRANCellIdentifier,

id-MakeBeforeBreakIndicator,

id-UESidelinkAggregateMaximumBitRate,

id-uL-GTPtunnelEndpoint,

id-SgNBSecurityKey,

id-SgNBUEAggregateMaximumBitRate,

id-E-RABs-ToBeAdded-SgNBAddReqList,

id-MeNBtoSgNBContainer,

id-SgNB-UE-X2AP-ID,

id-RequestedSplitSRBs,

id-E-RABs-ToBeAdded-SgNBAddReq-Item,

id-E-RABs-Admitted-ToBeAdded-SgNBAddReqAckList,

id-SgNBtoMeNBContainer,

id-AdmittedSplitSRBs,

id-E-RABs-Admitted-ToBeAdded-SgNBAddReqAck-Item,

id-ResponseInformationSgNBReconfComp,

id-UE-ContextInformation-SgNBModReq,

id-E-RABs-ToBeAdded-SgNBModReq-Item,

id-E-RABs-ToBeModified-SgNBModReq-Item,

id-E-RABs-ToBeReleased-SgNBModReq-Item,

id-E-RABs-Admitted-ToBeAdded-SgNBModAckList,

id-E-RABs-Admitted-ToBeModified-SgNBModAckList,

id-E-RABs-Admitted-ToBeReleased-SgNBModAckList,

id-E-RABs-Admitted-ToBeAdded-SgNBModAck-Item,

id-E-RABs-Admitted-ToBeModified-SgNBModAck-Item,

id-E-RABs-Admitted-ToBeReleased-SgNBModAck-Item,

id-E-RABs-Admitted-ToBeReleased-SgNBRelReqAckList,

id-E-RABs-Admitted-ToBeReleased-SgNBRelReqAck-Item,

id-E-RABs-ToBeReleased-SgNBModReqdList,

id-E-RABs-ToBeModified-SgNBModReqdList,

id-E-RABs-ToBeReleased-SgNBModReqd-Item,

id-E-RABs-ToBeModified-SgNBModReqd-Item,

id-E-RABs-ToBeReleased-SgNBChaConfList,

id-E-RABs-ToBeReleased-SgNBChaConf-Item,

id-E-RABs-ToBeReleased-SgNBRelReqList,

id-E-RABs-ToBeReleased-SgNBRelReq-Item,

id-E-RABs-ToBeReleased-SgNBRelConfList,

id-E-RABs-ToBeReleased-SgNBRelConf-Item,

id-E-RABs-ToBeReleased-SgNBRelReqdList,

id-E-RABs-ToBeReleased-SgNBRelReqd-Item,

id-E-RABs-SubjectToSgNBCounterCheck-List,

id-E-RABs-SubjectToSgNBCounterCheck-Item,

id-Target-SgNB-ID,

id-RRCContainer,

id-SRBType,

id-HandoverRestrictionList,

id-SCGConfigurationQuery,

id-SplitSRB,

id-NRUeReport,

id-InitiatingNodeType-EndcX2Setup,

id-InitiatingNodeType-EndcConfigUpdate,

id-RespondingNodeType-EndcX2Setup,

id-RespondingNodeType-EndcConfigUpdate,

id-NRUESecurityCapabilities,

id-PDCPChangeIndication,

id-ServedEUTRAcellsENDCX2ManagementList,

id-ServedEUTRAcellsToModifyListENDCConfUpd,

id-ServedEUTRAcellsToDeleteListENDCConfUpd,

id-ServedNRcellsToModifyListENDCConfUpd,

id-ServedNRcellsToDeleteListENDCConfUpd,

id-CellAssistanceInformation,

id-Globalen-gNB-ID,

id-ServedNRcellsENDCX2ManagementList,

id-Old-SgNB-UE-X2AP-ID,

id-UE-ContextReferenceAtSgNB,

id-SecondaryRATUsageReportList,

id-ActivationID,

id-ServedNRCellsToActivate,

id-ActivatedNRCellList,

id-MeNBResourceCoordinationInformation,

id-SgNBResourceCoordinationInformation,

id-UEAppLayerMeasConfig,

id-SelectedPLMN,

id-SubscriberProfileIDforRFP,

id-InitiatingNodeType-EutranrCellResourceCoordination,

id-RespondingNodeType-EutranrCellResourceCoordination,

id-DataTrafficResourceIndication,

id-SpectrumSharingGroupID,

id-ListofEUTRACellsinEUTRACoordinationReq,

id-ListofEUTRACellsinEUTRACoordinationResp,

id-ListofEUTRACellsinNRCoordinationReq,

id-ListofNRCellsinNRCoordinationReq,

id-ListofNRCellsinNRCoordinationResp,

id-RRCConfigIndication,

id-SGNB-Addition-Trigger-Ind,

id-RequestedSplitSRBsrelease,

id-AdmittedSplitSRBsrelease,

id-E-RABs-AdmittedToBeModified-SgNBModConfList,

id-E-RABs-AdmittedToBeModified-SgNBModConf-Item,

id-UEContextLevelUserPlaneActivity,

id-ERABActivityNotifyItemList,

id-MeNBCell-ID,

id-InitiatingNodeType-EndcX2Removal,

id-RespondingNodeType-EndcX2Removal,

id-uLpDCPSnLength,

id-dL-Forwarding,

id-E-RABs-DataForwardingAddress-List,

id-E-RABs-DataForwardingAddress-Item,

id-Subscription-Based-UE-DifferentiationInfo,

id-RLCMode-transferred,

id-dLPDCPSnLength,

id-secondarysgNBDLGTPTEIDatPDCP,

id-secondarymeNBULGTPTEIDatPDCP,

id-lCID,

id-duplicationActivation,

id-GNBOverloadInformation,

id-new-drb-ID-req,

id-NRNeighbourInfoToModify,

id-DesiredActNotificationLevel,

id-LocationInformationSgNB,

id-LocationInformationSgNBReporting,

id-endcSONConfigurationTransfer,

id-EUTRANTraceID,

id-additionalPLMNs-Item,

id-InterfaceInstanceIndication,

id-BPLMN-ID-Info-NR,

id-SNtriggered,

id-EPCHandoverRestrictionListContainer,

id-ERABs-transferred-to-MeNB,

id-AdditionalRRMPriorityIndex,

id-LowerLayerPresenceStatusChange,

id-FastMCGRecovery-SN-to-MN,

id-FastMCGRecovery-MN-to-SN,

id-RequestedFastMCGRecoveryViaSRB3,

id-AvailableFastMCGRecoveryViaSRB3,

id-RequestedFastMCGRecoveryViaSRB3Release,

id-ReleaseFastMCGRecoveryViaSRB3,

id-PartialListIndicator,

id-MaximumCellListSize,

id-MessageOversizeNotification,

id-CellandCapacityAssistInfo,

id-TNLConfigurationInfo,

id-TNLA-To-Add-List,

id-TNLA-To-Update-List,

id-TNLA-To-Remove-List,

id-TNLA-Setup-List,

id-TNLA-Failed-To-Setup-List,

id-UEContextReferenceatSourceNGRAN,

id-CHOinformation-REQ,

id-CHOinformation-ACK,

id-DAPSRequestInfo,

id-RequestedTargetCellID,

id-CandidateCellsToBeCancelledList,

id-DAPSResponseInfo,

id-ProcedureStage,

id-CHO-DC-Indicator,

id-Ethernet-Type,

id-NRV2XServicesAuthorized,

id-NRUESidelinkAggregateMaximumBitRate,

id-PC5QoSParameters,

id-TargetCellInNGRAN,

id-eNB-Measurement-ID-ENDC,

id-engNB-Measurement-ID-ENDC,

id-TDDULDLConfigurationCommonNR,

id-CarrierList,

id-ULCarrierList,

id-SSB-PositionsInBurst,

id-NRCellPRACHConfig,

id-NBIoT-RLF-Report-Container,

id-MDTConfigurationNR,

id-PrivacyIndicator,

id-TraceCollectionEntityIPAddress,

id-UERadioCapabilityID,

id-CSI-RSTransmissionIndication,

id-DLCarrierList,

id-IABNodeIndication,

id-F1CTrafficContainer,

id-IABInformation,

id-UERadioCapability,

maxCellineNB,

maxnoofBearers,

maxnoofPDCP-SN,

maxFailedMeasObjects,

maxnoofCellIDforMDT,

maxnoofTAforMDT,

maxCellinengNB,

maxnoofCellIDforQMC,

maxnoofTAforQMC,

maxnoofPLMNforQMC,

maxnoofProtectedResourcePatterns,

maxnoNRcellsSpectrumSharingWithE-UTRA,

maxnoofNrCellBands,

maxnoofSSBAreas

FROM X2AP-Constants;

<<<<<<<<<<<<<<<<<<<< Unmodified Text omitted >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- UE RADIO CAPABILITY ID MAPPING REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UERadioCapabilityIDMappingRequest::= SEQUENCE {

protocolIEs ProtocolIE-Container { { UERadioCapabilityIDMappingRequestIEs} },

...

}

UERadioCapabilityIDMappingRequestIEs X2AP-PROTOCOL-IES ::= {

{ ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- UE RADIO CAPABILITY ID MAPPING RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UERadioCapabilityIDMappingResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { UERadioCapabilityIDMappingResponseIEs} },

...

}

UERadioCapabilityIDMappingResponseIEs X2AP-PROTOCOL-IES ::= {

{ ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE mandatory }|

{ ID id-UERadioCapability CRITICALITY ignore TYPE UERadioCapability PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

<<<<<<<<<<<<<<<<<<<< Unmodified Text omitted >>>>>>>>>>>>>>>>>>>>

-- U

UEAggregateMaximumBitRate ::= SEQUENCE {

uEaggregateMaximumBitRateDownlink BitRate,

uEaggregateMaximumBitRateUplink BitRate,

iE-Extensions ProtocolExtensionContainer { {UEAggregate-MaximumBitrate-ExtIEs} } OPTIONAL,

...

}

UEAggregate-MaximumBitrate-ExtIEs X2AP-PROTOCOL-EXTENSION ::= {

{ ID id-extended-uEaggregateMaximumBitRateDownlink CRITICALITY ignore EXTENSION ExtendedBitRate PRESENCE optional}|

{ ID id-extended-uEaggregateMaximumBitRateUplink CRITICALITY ignore EXTENSION ExtendedBitRate PRESENCE optional},

...

}

UEAppLayerMeasConfig ::= SEQUENCE {

containerForAppLayerMeasConfig OCTET STRING (SIZE(1..1000)),

areaScopeOfQMC AreaScopeOfQMC,

iE-Extensions ProtocolExtensionContainer { {UEAppLayerMeasConfig-ExtIEs} } OPTIONAL,

...

}

UEAppLayerMeasConfig-ExtIEs X2AP-PROTOCOL-EXTENSION ::= {

{ID id-serviceType CRITICALITY ignore EXTENSION ServiceType PRESENCE optional},

...

}

UE-ContextKeptIndicator ::= ENUMERATED {

true,

...

}

UEID ::= BIT STRING (SIZE (16))

UE-HistoryInformation ::= SEQUENCE (SIZE(1..maxnoofCells)) OF LastVisitedCell-Item

UE-HistoryInformationFromTheUE ::= OCTET STRING

-- This IE is a transparent container and shall be encoded as the VisitedCellInfoList field contained in the UEInformationResponse message as defined in TS 36.331 [9]

UE-S1AP-ID ::= INTEGER (0.. 4294967295)

UE-X2AP-ID ::= INTEGER (0..4095)

UE-X2AP-ID-Extension ::= INTEGER (0..4095, ...)

UERadioCapability ::= OCTET STRING

UERadioCapabilityID ::= OCTET STRING

<<<<<<<<<<<<<<<<<<<< Last Change >>>>>>>>>>>>>>>>>>>>

### 9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

ProcedureCode,

ProtocolIE-ID

FROM X2AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-handoverPreparation ProcedureCode ::= 0

id-handoverCancel ProcedureCode ::= 1

id-loadIndication ProcedureCode ::= 2

id-errorIndication ProcedureCode ::= 3

id-snStatusTransfer ProcedureCode ::= 4

id-uEContextRelease ProcedureCode ::= 5

id-x2Setup ProcedureCode ::= 6

id-reset ProcedureCode ::= 7

id-eNBConfigurationUpdate ProcedureCode ::= 8

id-resourceStatusReportingInitiation ProcedureCode ::= 9

id-resourceStatusReporting ProcedureCode ::= 10

id-privateMessage ProcedureCode ::= 11

id-mobilitySettingsChange ProcedureCode ::= 12

id-rLFIndication ProcedureCode ::= 13

id-handoverReport ProcedureCode ::= 14

id-cellActivation ProcedureCode ::= 15

id-x2Release ProcedureCode ::= 16

id-x2APMessageTransfer ProcedureCode ::= 17

id-x2Removal ProcedureCode ::= 18

id-seNBAdditionPreparation ProcedureCode ::= 19

id-seNBReconfigurationCompletion ProcedureCode ::= 20

id-meNBinitiatedSeNBModificationPreparation ProcedureCode ::= 21

id-seNBinitiatedSeNBModification ProcedureCode ::= 22

id-meNBinitiatedSeNBRelease ProcedureCode ::= 23

id-seNBinitiatedSeNBRelease ProcedureCode ::= 24

id-seNBCounterCheck ProcedureCode ::= 25

id-retrieveUEContext ProcedureCode ::= 26

id-sgNBAdditionPreparation ProcedureCode ::= 27

id-sgNBReconfigurationCompletion ProcedureCode ::= 28

id-meNBinitiatedSgNBModificationPreparation ProcedureCode ::= 29

id-sgNBinitiatedSgNBModification ProcedureCode ::= 30

id-meNBinitiatedSgNBRelease ProcedureCode ::= 31

id-sgNBinitiatedSgNBRelease ProcedureCode ::= 32

id-sgNBCounterCheck ProcedureCode ::= 33

id-sgNBChange ProcedureCode ::= 34

id-rRCTransfer ProcedureCode ::= 35

id-endcX2Setup ProcedureCode ::= 36

id-endcConfigurationUpdate ProcedureCode ::= 37

id-secondaryRATDataUsageReport ProcedureCode ::= 38

id-endcCellActivation ProcedureCode ::= 39

id-endcPartialReset ProcedureCode ::= 40

id-eUTRANRCellResourceCoordination ProcedureCode ::= 41

id-SgNBActivityNotification ProcedureCode ::= 42

id-endcX2Removal ProcedureCode ::= 43

id-dataForwardingAddressIndication ProcedureCode ::= 44

id-gNBStatusIndication ProcedureCode ::= 45

id-deactivateTrace ProcedureCode ::= 46

id-traceStart ProcedureCode ::= 47

id-endcConfigurationTransfer ProcedureCode ::= 48

id-handoverSuccess ProcedureCode ::= 49

id-conditionalHandoverCancel ProcedureCode ::= 50

id-earlyStatusTransfer ProcedureCode ::= 51

id-cellTrafficTrace ProcedureCode ::= 52

id-endcresourceStatusReporting ProcedureCode ::= 53

id-endcresourceStatusReportingInitiation ProcedureCode ::= 54

id-f1CTrafficTransfer ProcedureCode ::= 55

id-UERadioCapabilityIDMapping ProcedureCode ::= 99 -- to be assigned

<<<<<<<<<<<<<<<<<<<< Unmodified Text omitted >>>>>>>>>>>>>>>>>>>>

id-SSB-PositionsInBurst ProtocolIE-ID ::= 389

id-NRCellPRACHConfig ProtocolIE-ID ::= 390

id-CellToReport-ENDC ProtocolIE-ID ::= 391

id-CellToReport-ENDC-Item ProtocolIE-ID ::= 392

id-CellMeasurementResult-ENDC ProtocolIE-ID ::= 393

id-CellMeasurementResult-ENDC-Item ProtocolIE-ID ::= 394

id-IABNodeIndication ProtocolIE-ID ::= 395

id-QoS-Mapping-Information ProtocolIE-ID ::= 396

id-F1CTrafficContainer ProtocolIE-ID ::= 397

id-IABInformation ProtocolIE-ID ::= 398

id-UERadioCapability ProtocolIE-ID ::= 999 -- to be assigned

END

-- ASN1STOP

<<<<<<<<<<<<<<<<<<<< End of Changes >>>>>>>>>>>>>>>>>>>>