**3GPP TSG-RAN3 Meeting #110-e R3-20xxxx**

**2 – 12 November 2020 E-Meeting**

**Title:** (TP on MDT in MR-DC for 38.423) Addition of immediate MDT in NGEN-DC and NE-DC

**Source:** CATT

**Agenda item:** 10.3.2.2

**Document Type:** other

1. Introduction

This contributionis the TP for TS38.423 v16.3.0 with addition of immediate MDT in NGEN-DC and NE-DC.

2. Discussion

At the RAN3 meeting #109-e, the following agreement has been achieved:

|  |
| --- |
| For management based immediate MDT in NR-DC, OAM provides the MDT configuration to MN and SN independently.For MDT in NGEN-DC and NE-DC, the SN receiving the management based immediate MDT and the signalling based immediate MDT in EN-DC is taken as baseline. |

This contribution is the TP for TS38.423 to support immediate MDT in NGEN-DC and NE-DC.

3. Annex – TP

*Start of the first change*

# 8 XnAP procedures

Table 8.1-2: Class 2 Elementary Procedures

| Elementary Procedure | Initiating Message |
| --- | --- |
| Handover Cancel | HANDOVER CANCEL |
| SN Status Transfer | SN STATUS TRANSFER |
| RAN Paging | RAN PAGING |
| Xn-U Address Indication | XN-U ADDRESS INDICATION |
| S-NG-RAN node Reconfiguration Completion | S-NODE RECONFIGURATION COMPLETE |
| S-NG-RAN node Counter Check | S-NODE COUNTER CHECK REQUEST |
| UE Context Release | UE CONTEXT RELEASE |
| RRC Transfer | RRC TRANSFER |
| Error Indication | ERROR INDICATION |
| Notification Control Indication | NOTIFICATION CONTROL INDICATION |
| Activity Notification | ACTIVITY NOTIFICATION |
| Secondary RAT Data Usage Report | SECONDARY RAT DATA USAGE REPORT |
| Trace Start | TRACE START |
| Deactivate Trace | DEACTIVATE TRACE |
| Handover Success | HANDOVER SUCCESS |
| Conditional Handover Cancel | CONDITIONAL HANDOVER CANCEL |
| Early Status Transfer | EARLY STATUS TRANSFER |
| Failure Indication | FAILURE INDICATION |
| Handover Report | HANDOVER REPORT |
| Resource Status Reporting | RESOURCE STATUS UPDATE |
| Access And Mobility Indication | ACCESS AND MOBILITY INDICATION |
| Cell Traffic Trace | CELL TRAFFIC TRACE |

### 8.3.1 S-NG-RAN node Addition Preparation

#### 8.3.1.1 General

The purpose of the S-NG-RAN node Addition Preparation procedure is to request the S-NG-RAN node to allocate resources for dual connectivity operation for a specific UE.

The procedure uses UE-associated signalling.

#### 8.3.1.2 Successful Operation



Figure 8.3.1.2-1: S-NG-RAN node Addition Preparation, successful operation

The M-NG-RAN node initiates the procedure by sending the S-NODE ADDITION REQUEST message to the S-NG-RAN node.

When the M-NG-RAN node sends the S-NODE ADDITION REQUEST message, it shall start the timer TXnDCprep.

The allocation of resources according to the values of the *Allocation and Retention Priority* IE included in the *QoS Flow Level QoS Parameters* IE for each QoS flow shall follow the principles specified for the PDU Session Resource Setup procedure in TS 38.413 [5].

The S-NG-RAN node shall choose the ciphering algorithm based on the information in the *UE Security Capabilities* IE and locally configured priority list of AS encryption algorithms and apply the key indicated in the *S-NG-RAN node Security Key* IE as specified in TS 33.501 [28].

If the *TSC Traffic Characteristics* IE is included for a QoS flow in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall behave the same as the NG-RAN node in the PDU Session Resource Setup procedure, specified in TS 38.413 [5].

If the *Additional QoS* *Flow Information* IE is included for a QoS flow in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall behave the same as the NG-RAN node in the PDU Session Resource Setup procedure, specified in TS 38.413 [5].

For each PDU session, if the *Network Instance* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE contained in the *PDU Session Resources To Be Added List* IE and the *Common Network Instance* IE is not present, the S-NG-RAN node shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [7].

For each GBR QoS flow, if the *Offered GBR QoS Flow Information* IE is included in the *QoS Flows To Be Setup List* IE contained in the *PDU Session Resource Setup Info – SN terminated* IE, the S-NG-RAN node may request the M-NG-RAN node to configure the DRB to which that QoS flow is mapped with MCG resources.

For each PDU session, if the *Non-GBR Resources Offered* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE contained in the *PDU Session Resources To Be Added List* IE and set to "true", the S-NG-RAN node may request the M-NG-RAN node to configure DRBs to which non-GBR QoS flows of the PDU session are mapped with MCG resources.

For each PDU session, if the *Common* *Network Instance* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE contained in the *PDU Session Resources To Be Added List* IE, the S-NG-RAN node shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [7].

Redundant transmission:

- For each PDU session, if the *Redundant UL NG-U UP TNL Information at UPF* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE, the S-NG-RAN node shall, if supported, use it as the uplink termination point for the user plane data for this PDU session for the redundant transmission and it shall include the *Redundant DL NG-U UP TNL Information at NG-RAN* IE in the *PDU Session Resource Setup Response Info – SN terminated* IE as described in TS 23.501 [9].

- For each PDU session, if the *Redundant Common Network Instance* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE the S-NG-RAN node shall, if supported, use it when selecting transport network resource for the redundant transmission as specified in TS 23.501 [7].

- For each PDU session for which the *Redundant QoS Flow Indicator* IE is include in *QoS Flows To Be Setup List* IE contained in the *S-NODE ADDITION REQUEST* message, the S-NG-RAN node shall, if supported, store and use it as specified in TS 23.501 [7].

- For each PDU session, if the *Redundant PDU Session Information* IE is included in the *PDU Session Resource Setup Info - SN terminated* IE in the S-NODE ADDITION REQUEST message, the S-NODE-RAN node shall, if supported, store the received information in the UE context and setup the redundant user plane resources for the concerned PDU session, as specified in TS 23.501 [7].

- For each PDU session resource successfully setup for which the *Redundant PDU Session Information* IE is included in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, include the *Used RSN Information* IE in the *PDU Session Resource Setup Response Info – SN terminated* IE in the S-NODE ADDITION REQUEST ACKNOWLEDGE message.

If the S-NODE ADDITION REQUEST message contains the *Selected PLMN* IE, the S-NG-RAN node may use it for RRM purposes.

If the S-NODE ADDITION REQUEST message contains the *Expected UE Behaviour* IE, the S-NG-RAN node shall, if supported, store this information and may use it to optimize resource allocation.

If the S-NODE ADDITION REQUEST message contains the *Mobility Restriction List* IE, the S-NG-RAN node, if supported, shall store this information and use it to select an appropriate SCG.

If the S-NODE ADDITION REQUEST message contains the *Index to RAT/Frequency Selection Priority* IE, the S-NG-RAN node may use it for RRM purposes.

If the S-NG-RAN node is a gNB and the S-NODE ADDITION REQUEST message contains the *PCell ID* IE, the S-NG-RAN node shall search for the target NR cell among the NR neighbour cells of the PCell indicated, as specified in the TS 37.340 [8].

If the S-NODE ADDITION REQUEST message contains the *S-NG-RAN node PDU Session Aggregate Maximum Bit Rate* IE, the S-NG-RAN node may use it for RRM purposes.

If the S-NODE ADDITION REQUEST message contains the *MR-DC Resource Coordination Information* IE, the S-NG-RAN node should forward it to lower layers and it may use it for the purpose of resource coordination with the M-NG-RAN node. The S-NG-RAN node shall consider the value of the received *UL Coordination Information* IE valid until reception of a new update of the IE for the same UE. The S-NG-RAN node shall consider the value of the received *DL Coordination Information* IE valid until reception of a new update of the IE for the same UE. If the *E-UTRA Coordination Assistance Information* IE or the *NR Coordination Assistance Information* IE is contained in the *MR-DC Resource Coordination Information* IE, the S-NG-RAN node shall, if supported, use the information to determine further coordination of resource utilisation between the S-NG-RAN node and the M-NG-RAN node.

If the S-NODE ADDITION REQUEST message contains the *NE-DC TDM Pattern* IE, the S-NG-RAN node should forward it to lower layers and use it for the purpose of single uplink transmission. The S-NG-RAN node shall consider the value of the received *NE-DC TDM Pattern* IE valid until reception of a new update of the IE for the same UE.

If the S-NODE ADDITION REQUEST message contains the *QoS Flow Mapping Indication* IE, the S-NG-RAN node may take it into account that only the uplink or downlink QoS flow is mapped to the DRB.

For each bearer for which allocation of the PDCP entity is requested at the S-NG-RAN node:

- the M-NG-RAN node may propose to apply forwarding of downlink data by including the *DL Forwarding* IE within *PDU Session Resource Setup Info – SN terminated* IE of the S-NODE ADDITION REQUEST message. For each bearer that it has decided to admit, the S-NG-RAN node may include the *DL Forwarding GTP Tunnel Endpoint* IE within the *PDU Session Resource Setup Response Info – SN terminated* IE of the S-NODE ADDITION REQUEST ACKNOWLEDGE message to indicate that it accepts the proposed forwarding of downlink data for this bearer.

- the S-NG-RAN node may include for each bearer in the *PDU Session Resource Setup Response Info – SN terminated* IE the *UL Forwarding GTP Tunnel Endpoint* IE to indicates it request data forwarding of uplink packets to be performed for that bearer.

- the M-NG-RAN node shall include *RLC Mode* IE for each bearer offloaded from M-NG-RAN node to S-NG-RAN node in the *DRBs to QoS Flow Mapping List* IE within the *PDU Session Resource Setup Info – SN terminated* IE of the S-NODE ADDTION REQUEST message, and the *RLC Mode* IE indicates the mode that the M-NG-RAN used for the DRB when it was hosted at the M-NG-RAN node.

For each bearer for which the PDCP entity is at the M-NG-RAN node:

- the M-NG-RAN node shall include the *RLC mode* IE for each bearer in the *DRBs To Be Setup List* IE within the *PDU Session Resource Setup Info – MN terminated* IE of the S-NODE ADDTION REQUEST message to indicate the RLC mode has been configured at the M-NG-RAN node, so that the S-NG-RAN node shall configure the same RLC mode for this MN terminated split bearer.

The M-NG-RAN node may also propose to apply forwarding of UL data when offloading QoS flows for which in-order delivery is requested by including the *UL Forwarding* *Proposal* IE in the *Data Forwarding and Offloading Info from source NG-RAN node* IE within the *PDU Session Resource Setup Info – SN terminated* IE of the S-NODE ADDITION REQUEST message. The S-NG-RAN node may include the *PDU Session Level UL Data Forwarding UP TNL Information* IE in the *Data Forwarding Info from target NG-RAN node* IE within the *PDU Session Resource Setup Response Info – SN terminated* IE of the S-NODE ADDITION REQUEST ACKNOWLEDGE message to indicate that it accepts the proposed forwarding.

If the *Masked IMEISV* IE is contained in the S-NODE ADDITION REQUEST message the S-NG-RAN node shall, if supported, use it to determine the characteristics of the UE for subsequent handling.

If the *UE Radio Capability ID* IE is contained in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, store this information in the UE context and use it as defined in TS 23.501 [7] and TS 23.502 [13].

The S-NG-RAN node shall report to the M-NG-RAN node, in the S-NODE ADDITION REQUEST ACKNOWLEDGE message, the result for all the requested PDU session resources in the following way:

- A list of PDU session resources which are successfully established shall be included in the *PDU Session Resources Admitted To Be Added List* IE.

- A list of PDU session resources which failed to be established shall be included in the *PDU Session Resources Not Admitted List* IE.

Upon reception of the S-NODE ADDITION REQUEST ACKNOWLEDGE message the M-NG-RAN node shall stop the timer TXnDCprep.

If the S-NODE ADDITION REQUEST ACKNOWLEDGE message contains the *MR-DC Resource Coordination Information* IE, the M-NG-RAN node may use it for the purpose of resource coordination with the S-NG-RAN node. The M-NG-RAN node shall consider the value of the received *UL Coordination Information* IE valid until reception of a new update of the IE for the same UE. The M-NG-RAN node shall consider the value of the received *DL Coordination Information* IE valid until reception of a new update of the IE for the same UE. If the *E-UTRA Coordination Assistance Information* IE or the *NR Coordination Assistance Information* IE is contained in the *MR-DC Resource Coordination Information* IE, the M-NG-RAN node shall, if supported, use the information to determine further coordination of resource utilisation between the M-NG-RAN node and the S-NG-RAN node.

The S-NG-RAN node may include for each bearer in the *DRBs To Be Setup List* IE in the S-NODE ADDITION REQUEST ACKNOWLEDGE message the *PDCP SN Length* IE to indicate the PDCP SN length for that DRB.

If the *S-NG-RAN node UE XnAP ID* IE is contained in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, store this information and use it as defined in TS 37.340 [8].

If the S-NODE ADDITION REQUEST message contains the *PDCP SN Length* IE, the S-NG-RAN node shall, if supported, store this information and use it for lower layer configuration of the concerned MN terminated bearer.

If the S-NODE ADDITION REQUEST message contains the *SN Addition Trigger Indication* IE, the S-NG-RAN node shall include the *RRC config indication* IE in the S-NODE ADDITION REQUEST ACKNOWLEDGE message to inform the M-NG-RAN node if the S-NG-RAN node applied full or delta configuration, as specified in TS 37.340 [8].

If the S-NODE ADDITION REQUEST message contains the *S-NG-RAN node Maximum Integrity Protected Data Rate* *Uplink* IE or the *S-NG-RAN node Maximum Integrity Protected Data Rate Downlink* IE, the S-NG-RAN node shall use the received information when enforcing the maximum integrity protected data rate for the UE.

If the *Security Indication* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE of the S-NODE ADDITION REQUEST message, the behaviour of the S-NG-RAN node shall be the same as specified for the same IE in the *PDU Session Resources To Be Setup List* IE in the Handover Preparation procedure, for the concerned PDU session, and the S-NG-RAN node shall include the *Security Result* IE in the *PDU Session Resource Setup Response Info – SN terminated* IE.

If the *Security Result* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE of the S-NODE ADDITION REQUEST message, the S-NG-RAN node may take the information into account when deciding whether to perform user plane integrity protection or ciphering for the DRBs that it establishes for the concerned PDU session, except if the *Split Session Indicator* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE and set to "split", in which case it shall perform user plane integrity protection or ciphering according to the information in the *Security Result* IE*.* If the S-NG-RAN node is an ng-eNB, it shall reject all PDU sessions for which the *Integrity Protection Indication* IE is set to "required" as specified in TS 33.501 [28]. If either the S-NG-RAN node or the M-NG-RAN node is an ng-eNB, the S-NG-RAN node shall behave according to clause 6.10.4 of TS 33.501 [28] for PDU sessions for which the *Integrity Protection Indication* IE is set to "preferred".

The S-NG-RAN node may include the *Location Information at S-NODE* IE in the S-NODE ADDITION REQUEST ACKNOWLEDGE message, if respective information is available at the S-NG-RAN node.

If the *Location Information at S-NODE Reporting* IE set to "pscell" is included in the S-NODE ADDITION REQUEST, the S-NG-RAN node shall, start providing information about the current location of the UE. If the *Location Information at S-NODE* IE is included in the S-NODE ADDITION REQUEST ACKNOWLEDGE, the M-NG-RAN node shall store the included information so that it may be transferred towards the AMF.

If the *Default DRB Allowed* IE is included in the *PDU Session Resource Setup Info – SN terminated* IE of the S-NODE ADDITION REQUEST message and set to "true", the S-NG-RAN node may configure the default DRB for the PDU session.

If the S-NODE ADDITION REQUEST ACKNOWLEDGE message includes the *DRB IDs taken into use* IE, the M-NG-RAN node, if applicable, shall act as specified in TS 37.340 [8].

If *Trace Activation* IE has previously been received for this UE, it shall be included in the S-NODE ADDITION REQUEST message. If the *Trace Activation* IE is included in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, initiate the requested trace function as described in TS 32.422 [23].

If the *Requested Fast MCG recovery via SRB3* IE set to "true" is included in the S-NODE ADDITION REQUEST message and the S-NG-RAN node decides to configure fast MCG link recovery via SRB3 as specified in TS 37.340 [8], the S-NG-RAN shall, if supported, include the *Available fast MCG recovery via SRB3* IE set to "true" in the S-NODE ADDITION REQUEST ACKNOWLEDGE message.

If the *QoS Monitoring Request* IE is included in the *QoS Flow Level QoS Parameters* IE for a QoS flow contained in the *DRBs To Be Setup List* IE of the *PDU Session Resource Setup Info – MN terminated* IE, the S-NG-RAN node shall, if supported, use it to configure lower layers for the purpose of delay measurement and QoS monitoring as specified in TS 23.501 [7].

For each QoS flow which has been successfully established in the S-NG-RAN node, if the *QoS Monitoring Request* IE was included in the *QoS Flow Level QoS Parameters* IE contained in the *PDU Session Resource Setup Info – SN terminated* IE, the S-NG-RAN node shall store this information, and, if supported, perform delay measurement and QoS monitoring as specified in TS 23.501 [7]. In case such a QoS flow is included in the *DRBs To Be Setup List* IE of the *PDU Session Resource Setup Response Info – SN terminated* IE, the M-NG-RAN node shall, if supported, use it to configure lower layers for the purpose of delay measurement and QoS monitoring.

If the *Management Based MDT PLMN List* IE is contained in the S-NODE ADDITION REQUEST message, the S-NG-RAN node shall, if supported, store the received information in the UE context, and use this information to allow subsequent selection of the UE for management based MDT defined in TS 32.422 [23].

### 8.3.X Cell Traffic Trace

#### 8.3.X.1 General

The purpose of the Cell Traffic Trace procedure is to send the allocated Trace Recording Session Reference and the Trace Reference to the M-NG-RAN node. The procedure uses UE-associated signalling.

#### 8.3.X.2 Successful Operation



Figure 8.3.X-1: Cell Traffic Trace procedure. Successful operation.

The procedure is initiated with a CELL TRAFFIC TRACE message sent from the S-NG-RAN node to the M-NG-RAN node.

If the *Privacy Indicator* IE is included in the message, the M-NG-RAN node shall take the information into account for anonymisation of MDT data as specified in TS 32.422 [23].

#### 9.1.2.1 S-NODE ADDITION REQUEST

This message is sent by the M-NG-RAN node to the S-NG-RAN node to request the preparation of resources for dual connectivity operation for a specific UE.

Direction: M-NG-RAN node → S-NG-RAN node.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | reject |
| M-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID9.2.3.16 | Allocated at the M-NG-RAN node | YES | reject |
| UE Security Capabilities | M |  | 9.2.3.49 |  | YES | reject |
| S-NG-RAN node Security Key | M |  | 9.2.3.51 |  | YES | reject |
| S-NG-RAN node UE Aggregate Maximum Bit Rate | M |  | UE Aggregate Maximum Bit Rate9.2.3.17 | The UE Aggregate Maximum Bit Rate is split into M-NG-RAN node UE Aggregate Maximum Bit Rate and S-NG-RAN node UE Aggregate Maximum Bit Rate which are enforced by M-NG-RAN node and S-NG-RAN node respectively. | YES | reject |
| Selected PLMN | O |  | PLMN Identity9.2.2.4 | The selected PLMN of the SCG in the S-NG-RAN node. | YES | ignore |
| Mobility Restriction List | O |  | 9.2.3.53 |  | YES | ignore |
| Index to RAT/Frequency Selection Priority | O |  | 9.2.3.23 |  | YES | reject |
| **PDU Session Resources To Be Added List** |  | *1* |  |  | YES | reject |
| **>PDU Session Resources To Be Added Item** |  | *1 .. <maxnoofPDUSessions>* |  | NOTE: If neither the *PDU Session Resource Setup Info – SN terminated* IE nor the*PDU Session Resource Setup Info – MN terminated* IEis present in a *PDU Session Resources To Be Added Item* IE, abnormal conditions as specified in clause 8.3.1.4 apply. | – |  |
| >>PDU Session ID | M |  | 9.2.3.18 |  | – |  |
| >>S-NSSAI | M |  | 9.2.3.21 |  | – |  |
| >>S-NG-RAN node PDU Session Aggregate Maximum Bit Rate | O |  | PDU Session Aggregate Maximum Bit Rate9.2.3.69 |  | – |  |
| >>PDU Session Resource Setup Info – SN terminated | O |  | 9.2.1.5 |  | – |  |
| >>PDU Session Resource Setup Info – MN terminated | O |  | 9.2.1.7 |  | – |  |
| M-NG-RAN node to S-NG-RAN node Container | M |  | OCTET STRING | Includes the *CG-ConfigInfo* message as defined in subclause 11.2.2 of TS 38.331 [10] | YES | reject |
| S-NG-RAN node UE XnAP ID | O |  | NG-RAN node UE XnAP ID9.2.3.16 | Allocated at the S-NG-RAN node | YES | reject |
| Expected UE Behaviour | O |  | 9.2.3.81 |  | YES | ignore |
| Requested Split SRBs | O |  | ENUMERATED (srb1, srb2, srb1&2, ...) | Indicates that resources for Split SRBs are requested. | YES | reject |
| PCell ID | O |  | Global NG-RAN Cell Identity9.2.2.27 |  | YES | reject |
| Desired Activity Notification Level | O |  | 9.2.3.77 |  | YES | ignore |
| Available DRB IDs | C-ifSNterminated |  | DRB List9.2.1.29 | Indicates the list of DRB IDs that the S-NG-RAN node may use for SN-terminated bearers. | YES | reject |
| S-NG-RAN node Maximum Integrity Protected Data Rate Uplink | O |  | Bit Rate9.2.3.4 | The S-NG-RAN node Maximum Integrity Protected Data Rate Uplink is a portion of the UE’s Maximum Integrity Protected Data Rate in the Uplink, which is enforced by the S-NG-RAN node for the UE’s SN terminated PDU sessions. If the *S-NG-RAN node Maximum Integrity Protected Data Rate Downlink* IE is not present, this IE applies to both UL and DL. | YES | reject |
| S-NG-RAN node Maximum Integrity Protected Data Rate Downlink | O |  | Bit Rate9.2.3.4 | The S-NG-RAN node Maximum Integrity Protected Data Rate Downlink is a portion of the UE’s Maximum Integrity Protected Data Rate in the Downlink, which is enforced by the S-NG-RAN node for the UE’s SN terminated PDU sessions. | YES | reject |
| Location Information at S-NODE reporting | O |  | ENUMERATED (pscell, ...) | Indicates that the user’s Location Information at S-NODE is to be provided. | YES | ignore |
| MR-DC Resource Coordination Information | O |  | 9.2.2.33 | Information used to coordinate resource utilisation between M-NG-RAN node and S-NG-RAN node.  | YES | ignore |
| Masked IMEISV | O |  | 9.2.3.32 |  | YES | ignore |
| NE-DC TDM Pattern | O |  | 9.2.2.38 |  | YES | ignore |
| SN Addition Trigger Indication | O |  | ENUMERATED (SN change, inter-MN HO, intra-MN HO, ...) | This IE indicates the trigger for S-NG-RAN node Addition Preparation procedure | YES | reject |
| Trace Activation | O |  | 9.2.3.55 |  | YES | ignore |
| Requested Fast MCG recovery via SRB3 | O |  | ENUMERATED (true, ...) | Indicates that the resources for fast MCG recovery via SRB3 are requested. | YES | ignore |
| UE Radio Capability ID | O |  | 9.2.3.138 |  | YES | reject |
| Management Based MDT PLMN List | O |  | MDT PLMN List9.2.3.133 |  |  |  |

### 9.1.2.x CELL TRAFFIC TRACE

This message is sent by S-NG-RAN node to transfer the trace information to the M-NG-RAN node.

Direction: S-NG-RAN node → M-NG-RAN node

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | ignore |
| M-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID9.2.3.16 | Allocated at the M-NG-RAN node | YES | reject |
| S-NG-RAN node UE XnAP ID | M |  | NG-RAN node UE XnAP ID9.2.3.16 | Allocated at the S-NG-RAN node | YES | reject |
| NG-RAN Trace ID | M |  | OCTET STRING (SIZE(8)) | As per NG-RAN Trace ID in *Trace Activation* IE | YES | ignore |
| Trace Collection Entity IP Address | M |  | Transport Layer Address9.2.3.29 | For File based Reporting.Defined in TS 32.422 [23] Should be ignored if the *Trace Collection Entity* URI IE is present. | – |  |
| Privacy Indicator | O |  | ENUMERATED (Immediate MDT, ...) |  | YES | ignore |
| Trace Collection Entity URI | O |  | URI9.2.3.124 | For Streaming based Reporting.Defined in TS 32.422 [23]Replaces Trace Collection Entity IP Address if present | YES | ignore |

### 9.3.3 Elementary Procedure Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-PDU-Descriptions (0) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 Criticality,

 ProcedureCode

FROM XnAP-CommonDataTypes

 HandoverRequest,

 HandoverRequestAcknowledge,

 HandoverPreparationFailure,

 SNStatusTransfer,

 UEContextRelease,

 HandoverCancel,

 NotificationControlIndication,

 RANPaging,

 RetrieveUEContextRequest,

 RetrieveUEContextResponse,

 RetrieveUEContextFailure,

 XnUAddressIndication,

 SecondaryRATDataUsageReport,

 SNodeAdditionRequest,

 SNodeAdditionRequestAcknowledge,

 SNodeAdditionRequestReject,

 SNodeReconfigurationComplete,

 SNodeModificationRequest,

 SNodeModificationRequestAcknowledge,

 SNodeModificationRequestReject,

 SNodeModificationRequired,

 SNodeModificationConfirm,

 SNodeModificationRefuse,

 SNodeReleaseRequest,

 SNodeReleaseRequestAcknowledge,

 SNodeReleaseReject,

 SNodeReleaseRequired,

 SNodeReleaseConfirm,

 SNodeCounterCheckRequest,

 SNodeChangeRequired,

 SNodeChangeConfirm,

 SNodeChangeRefuse,

 RRCTransfer,

 XnRemovalRequest,

 XnRemovalResponse,

 XnRemovalFailure,

 XnSetupRequest,

 XnSetupResponse,

 XnSetupFailure,

 NGRANNodeConfigurationUpdate,

 NGRANNodeConfigurationUpdateAcknowledge,

 NGRANNodeConfigurationUpdateFailure,

 E-UTRA-NR-CellResourceCoordinationRequest,

 E-UTRA-NR-CellResourceCoordinationResponse,

 ActivityNotification,

 CellActivationRequest,

 CellActivationResponse,

 CellActivationFailure,

 ResetRequest,

 ResetResponse,

 ErrorIndication,

 PrivateMessage,

 DeactivateTrace,

 TraceStart,

 HandoverSuccess,

 ConditionalHandoverCancel,

 EarlyStatusTransfer,

 FailureIndication,

 HandoverReport,

 ResourceStatusRequest,

 ResourceStatusResponse,

 ResourceStatusFailure,

 ResourceStatusUpdate,

 MobilityChangeRequest,

 MobilityChangeAcknowledge,

 MobilityChangeFailure,

 AccessAndMobilityIndication,

CellTrafficTrace

FROM XnAP-PDU-Contents

 id-handoverPreparation,

 id-sNStatusTransfer,

 id-handoverCancel,

 id-notificationControl,

 id-retrieveUEContext,

 id-rANPaging,

 id-xnUAddressIndication,

 id-uEContextRelease,

 id-secondaryRATDataUsageReport,

 id-sNGRANnodeAdditionPreparation,

 id-sNGRANnodeReconfigurationCompletion,

 id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation,

 id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation,

 id-mNGRANnodeinitiatedSNGRANnodeRelease,

 id-sNGRANnodeinitiatedSNGRANnodeRelease,

 id-sNGRANnodeCounterCheck,

 id-sNGRANnodeChange,

 id-activityNotification,

 id-rRCTransfer,

 id-xnRemoval,

 id-xnSetup,

 id-nGRANnodeConfigurationUpdate,

 id-e-UTRA-NR-CellResourceCoordination,

 id-cellActivation,

 id-reset,

 id-errorIndication,

 id-privateMessage,

 id-deactivateTrace,

 id-traceStart,

 id-handoverSuccess,

 id-conditionalHandoverCancel,

 id-earlyStatusTransfer,

 id-failureIndication,

 id-handoverReport,

 id-resourceStatusReportingInitiation,

 id-resourceStatusReporting,

 id-mobilitySettingsChange,

 id-accessAndMobilityIndication,

id-cellTrafficTrace

FROM XnAP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure Class

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-ELEMENTARY-PROCEDURE ::= CLASS {

 &InitiatingMessage ,

 &SuccessfulOutcome OPTIONAL,

 &UnsuccessfulOutcome OPTIONAL,

 &procedureCode ProcedureCode UNIQUE,

 &criticality Criticality DEFAULT ignore

}

WITH SYNTAX {

 INITIATING MESSAGE &InitiatingMessage

 [SUCCESSFUL OUTCOME &SuccessfulOutcome]

 [UNSUCCESSFUL OUTCOME &UnsuccessfulOutcome]

 PROCEDURE CODE &procedureCode

 [CRITICALITY &criticality]

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface PDU Definition

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU ::= CHOICE {

 initiatingMessage InitiatingMessage,

 successfulOutcome SuccessfulOutcome,

 unsuccessfulOutcome UnsuccessfulOutcome,

 ...

}

InitiatingMessage ::= SEQUENCE {

 procedureCode XNAP-ELEMENTARY-PROCEDURE.&procedureCode ({XNAP-ELEMENTARY-PROCEDURES}),

 criticality XNAP-ELEMENTARY-PROCEDURE.&criticality ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode}),

 value XNAP-ELEMENTARY-PROCEDURE.&InitiatingMessage ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

SuccessfulOutcome ::= SEQUENCE {

 procedureCode XNAP-ELEMENTARY-PROCEDURE.&procedureCode ({XNAP-ELEMENTARY-PROCEDURES}),

 criticality XNAP-ELEMENTARY-PROCEDURE.&criticality ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode}),

 value XNAP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

UnsuccessfulOutcome ::= SEQUENCE {

 procedureCode XNAP-ELEMENTARY-PROCEDURE.&procedureCode ({XNAP-ELEMENTARY-PROCEDURES}),

 criticality XNAP-ELEMENTARY-PROCEDURE.&criticality ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode}),

 value XNAP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome ({XNAP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XNAP-ELEMENTARY-PROCEDURES XNAP-ELEMENTARY-PROCEDURE ::= {

 XNAP-ELEMENTARY-PROCEDURES-CLASS-1 |

 XNAP-ELEMENTARY-PROCEDURES-CLASS-2 ,

 ...

}

XNAP-ELEMENTARY-PROCEDURES-CLASS-1 XNAP-ELEMENTARY-PROCEDURE ::= {

 handoverPreparation |

 retrieveUEContext |

 sNGRANnodeAdditionPreparation |

 mNGRANnodeinitiatedSNGRANnodeModificationPreparation |

 sNGRANnodeinitiatedSNGRANnodeModificationPreparation |

 mNGRANnodeinitiatedSNGRANnodeRelease |

 sNGRANnodeinitiatedSNGRANnodeRelease |

 sNGRANnodeChange |

 xnRemoval |

 xnSetup |

 nGRANnodeConfigurationUpdate |

 e-UTRA-NR-CellResourceCoordination |

 cellActivation |

 reset |

 resourceStatusReportingInitiation |

 mobilitySettingsChange ,

 ...

}

XNAP-ELEMENTARY-PROCEDURES-CLASS-2 XNAP-ELEMENTARY-PROCEDURE ::= {

 sNStatusTransfer |

 handoverCancel |

 rANPaging |

 xnUAddressIndication |

 uEContextRelease |

 sNGRANnodeReconfigurationCompletion |

 sNGRANnodeCounterCheck |

 rRCTransfer |

 errorIndication |

 privateMessage |

 notificationControl |

 activityNotification |

 secondaryRATDataUsageReport |

 deactivateTrace |

 traceStart |

 handoverSuccess |

 conditionalHandoverCancel |

 earlyStatusTransfer |

 failureIndication |

 handoverReport |

 resourceStatusReporting |

cellTrafficTrace |

 accessAndMobilityIndication ,

 ...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

handoverPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE HandoverRequest

 SUCCESSFUL OUTCOME HandoverRequestAcknowledge

 UNSUCCESSFUL OUTCOME HandoverPreparationFailure

 PROCEDURE CODE id-handoverPreparation

 CRITICALITY reject

}

sNStatusTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNStatusTransfer

 PROCEDURE CODE id-sNStatusTransfer

 CRITICALITY ignore

}

handoverCancel XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE HandoverCancel

 PROCEDURE CODE id-handoverCancel

 CRITICALITY ignore

}

retrieveUEContext XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE RetrieveUEContextRequest

 SUCCESSFUL OUTCOME RetrieveUEContextResponse

 UNSUCCESSFUL OUTCOME RetrieveUEContextFailure

 PROCEDURE CODE id-retrieveUEContext

 CRITICALITY reject

}

rANPaging XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE RANPaging

 PROCEDURE CODE id-rANPaging

 CRITICALITY reject

}

xnUAddressIndication XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE XnUAddressIndication

 PROCEDURE CODE id-xnUAddressIndication

 CRITICALITY reject

}

uEContextRelease XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE UEContextRelease

 PROCEDURE CODE id-uEContextRelease

 CRITICALITY reject

}

sNGRANnodeAdditionPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeAdditionRequest

 SUCCESSFUL OUTCOME SNodeAdditionRequestAcknowledge

 UNSUCCESSFUL OUTCOME SNodeAdditionRequestReject

 PROCEDURE CODE id-sNGRANnodeAdditionPreparation

 CRITICALITY reject

}

sNGRANnodeReconfigurationCompletion XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeReconfigurationComplete

 PROCEDURE CODE id-sNGRANnodeReconfigurationCompletion

 CRITICALITY reject

}

mNGRANnodeinitiatedSNGRANnodeModificationPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeModificationRequest

 SUCCESSFUL OUTCOME SNodeModificationRequestAcknowledge

 UNSUCCESSFUL OUTCOME SNodeModificationRequestReject

 PROCEDURE CODE id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation

 CRITICALITY reject

}

sNGRANnodeinitiatedSNGRANnodeModificationPreparation XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeModificationRequired

 SUCCESSFUL OUTCOME SNodeModificationConfirm

 UNSUCCESSFUL OUTCOME SNodeModificationRefuse

 PROCEDURE CODE id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation

 CRITICALITY reject

}

mNGRANnodeinitiatedSNGRANnodeRelease XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeReleaseRequest

 SUCCESSFUL OUTCOME SNodeReleaseRequestAcknowledge

 UNSUCCESSFUL OUTCOME SNodeReleaseReject

 PROCEDURE CODE id-mNGRANnodeinitiatedSNGRANnodeRelease

 CRITICALITY reject

}

sNGRANnodeinitiatedSNGRANnodeRelease XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeReleaseRequired

 SUCCESSFUL OUTCOME SNodeReleaseConfirm

 PROCEDURE CODE id-sNGRANnodeinitiatedSNGRANnodeRelease

 CRITICALITY reject

}

sNGRANnodeCounterCheck XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeCounterCheckRequest

 PROCEDURE CODE id-sNGRANnodeCounterCheck

 CRITICALITY reject

}

sNGRANnodeChange XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SNodeChangeRequired

 SUCCESSFUL OUTCOME SNodeChangeConfirm

 UNSUCCESSFUL OUTCOME SNodeChangeRefuse

 PROCEDURE CODE id-sNGRANnodeChange

 CRITICALITY reject

}

rRCTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE RRCTransfer

 PROCEDURE CODE id-rRCTransfer

 CRITICALITY reject

}

xnRemoval XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE XnRemovalRequest

 SUCCESSFUL OUTCOME XnRemovalResponse

 UNSUCCESSFUL OUTCOME XnRemovalFailure

 PROCEDURE CODE id-xnRemoval

 CRITICALITY reject

}

xnSetup XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE XnSetupRequest

 SUCCESSFUL OUTCOME XnSetupResponse

 UNSUCCESSFUL OUTCOME XnSetupFailure

 PROCEDURE CODE id-xnSetup

 CRITICALITY reject

}

nGRANnodeConfigurationUpdate XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE NGRANNodeConfigurationUpdate

 SUCCESSFUL OUTCOME NGRANNodeConfigurationUpdateAcknowledge

 UNSUCCESSFUL OUTCOME NGRANNodeConfigurationUpdateFailure

 PROCEDURE CODE id-nGRANnodeConfigurationUpdate

 CRITICALITY reject

}

e-UTRA-NR-CellResourceCoordination XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE E-UTRA-NR-CellResourceCoordinationRequest

 SUCCESSFUL OUTCOME E-UTRA-NR-CellResourceCoordinationResponse

 PROCEDURE CODE id-e-UTRA-NR-CellResourceCoordination

 CRITICALITY reject

}

cellActivation XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE CellActivationRequest

 SUCCESSFUL OUTCOME CellActivationResponse

 UNSUCCESSFUL OUTCOME CellActivationFailure

 PROCEDURE CODE id-cellActivation

 CRITICALITY reject

}

reset XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE ResetRequest

 SUCCESSFUL OUTCOME ResetResponse

 PROCEDURE CODE id-reset

 CRITICALITY reject

}

errorIndication XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE ErrorIndication

 PROCEDURE CODE id-errorIndication

 CRITICALITY ignore

}

notificationControl XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE NotificationControlIndication

 PROCEDURE CODE id-notificationControl

 CRITICALITY ignore

}

activityNotification XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE ActivityNotification

 PROCEDURE CODE id-activityNotification

 CRITICALITY ignore

}

privateMessage XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE PrivateMessage

 PROCEDURE CODE id-privateMessage

 CRITICALITY ignore

}

secondaryRATDataUsageReport XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE SecondaryRATDataUsageReport

 PROCEDURE CODE id-secondaryRATDataUsageReport

 CRITICALITY reject

}

deactivateTrace XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE DeactivateTrace

 PROCEDURE CODE id-deactivateTrace

 CRITICALITY ignore

}

traceStart XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE TraceStart

 PROCEDURE CODE id-traceStart

 CRITICALITY ignore

}

handoverSuccess XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE HandoverSuccess

 PROCEDURE CODE id-handoverSuccess

 CRITICALITY ignore

}

conditionalHandoverCancel XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE ConditionalHandoverCancel

 PROCEDURE CODE id-conditionalHandoverCancel

 CRITICALITY ignore

}

earlyStatusTransfer XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE EarlyStatusTransfer

 PROCEDURE CODE id-earlyStatusTransfer

 CRITICALITY ignore

}

failureIndication XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE FailureIndication

 PROCEDURE CODE id-failureIndication

 CRITICALITY ignore

}

handoverReport XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE HandoverReport

 PROCEDURE CODE id-handoverReport

 CRITICALITY ignore

}

resourceStatusReportingInitiation XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE ResourceStatusRequest

 SUCCESSFUL OUTCOME ResourceStatusResponse

 UNSUCCESSFUL OUTCOME ResourceStatusFailure

 PROCEDURE CODE id-resourceStatusReportingInitiation

 CRITICALITY reject

}

resourceStatusReporting XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE ResourceStatusUpdate

 PROCEDURE CODE id-resourceStatusReporting

 CRITICALITY ignore

}

mobilitySettingsChange XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE MobilityChangeRequest

 SUCCESSFUL OUTCOME MobilityChangeAcknowledge

 UNSUCCESSFUL OUTCOME MobilityChangeFailure

PROCEDURE CODE id-mobilitySettingsChange

 CRITICALITY reject

}

accessAndMobilityIndication XNAP-ELEMENTARY-PROCEDURE ::={

 INITIATING MESSAGE AccessAndMobilityIndication

 PROCEDURE CODE id-accessAndMobilityIndication

 CRITICALITY ignore

}

cellTrafficTrace XNAP-ELEMENTARY-PROCEDURE ::= {

 INITIATING MESSAGE CellTrafficTrace

 PROCEDURE CODE id-cellTrafficTrace

 CRITICALITY ignore

}

END

-- ASN1STOP

### 9.3.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for XnAP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) xnap (2) version1 (1) xnap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 ActivationIDforCellActivation,

 AMF-Region-Information,

 AMF-UE-NGAP-ID,

 AS-SecurityInformation,

 AssistanceDataForRANPaging,

 BitRate,

 Cause,

 CellAndCapacityAssistanceInfo-EUTRA,

 CellAndCapacityAssistanceInfo-NR,

 CellAssistanceInfo-EUTRA,

 CellAssistanceInfo-NR,

 CHOinformation-Req,

 CHOinformation-Ack,

 CHO-MRDC-Indicator,

 CPTransportLayerInformation,

 TNLA-To-Add-List,

 TNLA-To-Update-List,

 TNLA-To-Remove-List,

 TNLA-Setup-List,

 TNLA-Failed-To-Setup-List,

 CriticalityDiagnostics,

 XnUAddressInfoperPDUSession-List,

 DAPSResponseInfo-List,

 DataTrafficResourceIndication,

 DeliveryStatus,

 DesiredActNotificationLevel,

 DRB-ID,

 DRB-List,

 DRB-Number,

 DRBsSubjectToDLDiscarding-List,

 DRBsSubjectToEarlyStatusTransfer-List,

 DRBsSubjectToStatusTransfer-List,

 DRBToQoSFlowMapping-List,

 E-UTRA-CGI,

 ExpectedUEBehaviour,

 FiveGCMobilityRestrictionListContainer,

 GlobalCell-ID,

 GlobalNG-RANNode-ID,

 GlobalNG-RANCell-ID,

 GUAMI,

 InterfaceInstanceIndication,

 I-RNTI,

 LocationInformationSNReporting,

 LocationReportingInformation,

 LowerLayerPresenceStatusChange,

 LTEUESidelinkAggregateMaximumBitRate,

 LTEV2XServicesAuthorized,

 MR-DC-ResourceCoordinationInfo,

 ServedCells-E-UTRA,

 ServedCells-NR,

 ServedCellsToUpdate-E-UTRA,

 ServedCellsToUpdate-NR,

 MAC-I,

 MaskedIMEISV,

 MDT-Configuration,

 MDTPLMNList,

 MobilityRestrictionList,

 NG-RAN-Cell-Identity,

 NG-RANnodeUEXnAPID,

 NR-CGI,

 NE-DC-TDM-Pattern,

 NRUESidelinkAggregateMaximumBitRate,

 NRV2XServicesAuthorized,

 PagingDRX,

 PagingPriority,

 PartialListIndicator,

 PLMN-Identity,

 PDCPChangeIndication,

 PDUSessionAggregateMaximumBitRate,

 PDUSession-ID,

 PDUSession-List,

 PDUSession-List-withCause,

 PDUSession-List-withDataForwardingFromTarget,

 PDUSession-List-withDataForwardingRequest,

 PDUSessionResourcesAdmitted-List,

 PDUSessionResourcesNotAdmitted-List,

 PDUSessionResourcesToBeSetup-List,

 PDUSessionResourceChangeRequiredInfo-SNterminated,

 PDUSessionResourceChangeRequiredInfo-MNterminated,

 PDUSessionResourceChangeConfirmInfo-SNterminated,

 PDUSessionResourceChangeConfirmInfo-MNterminated,

 PDUSessionResourceSecondaryRATUsageList,

 PDUSessionResourceSetupInfo-SNterminated,

 PDUSessionResourceSetupInfo-MNterminated,

 PDUSessionResourceSetupResponseInfo-SNterminated,

 PDUSessionResourceSetupResponseInfo-MNterminated,

 PDUSessionResourceModificationInfo-SNterminated,

 PDUSessionResourceModificationInfo-MNterminated,

 PDUSessionResourceModificationResponseInfo-SNterminated,

 PDUSessionResourceModificationResponseInfo-MNterminated,

 PDUSessionResourceModConfirmInfo-SNterminated,

 PDUSessionResourceModConfirmInfo-MNterminated,

 PDUSessionResourceModRqdInfo-SNterminated,

 PDUSessionResourceModRqdInfo-MNterminated,

 PDUSessionType,

 PC5QoSParameters,

 QoSFlowIdentifier,

 QoSFlowNotificationControlIndicationInfo,

 QoSFlows-List,

 RANPagingArea,

 ResetRequestTypeInfo,

 ResetResponseTypeInfo,

 RFSP-Index,

 RRCConfigIndication,

 RRCResumeCause,

 SCGConfigurationQuery,

 SecurityIndication,

 S-NG-RANnode-SecurityKey,

 SpectrumSharingGroupID,

 SplitSRBsTypes,

 S-NG-RANnode-Addition-Trigger-Ind,

 S-NSSAI,

 TargetCellList,

 TAISupport-List,

 Target-CGI,

 TimeToWait,

 TraceActivation,

 UEAggregateMaximumBitRate,

 UEContextID,

 UEContextInfoRetrUECtxtResp,

 UEContextKeptIndicator,

 UEHistoryInformation,

 UEIdentityIndexValue,

 UERadioCapabilityForPaging,

 UERadioCapabilityID,

 UERANPagingIdentity,

 UESecurityCapabilities,

 UPTransportLayerInformation,

 UserPlaneTrafficActivityReport,

 XnBenefitValue,

 RANPagingFailure,

 TNLConfigurationInfo,

 MaximumCellListSize,

 MessageOversizeNotification,

 NG-RANTraceID,

 MobilityInformation,

 InitiatingCondition-FailureIndication,

 HandoverReportType,

 TargetCellinEUTRAN,

 C-RNTI,

 UERLFReportContainer,

 Measurement-ID,

 RegistrationRequest,

 ReportCharacteristics,

 CellToReport,

 ReportingPeriodicity,

 CellMeasurementResult,

 UEHistoryInformationFromTheUE,

 MobilityParametersInformation,

 MobilityParametersModificationRange,

 RACHReportInformation,

 IABNodeIndication,

 SNTriggered

FROM XnAP-IEs

 PrivateIE-Container{},

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 ProtocolIE-ContainerList{},

 ProtocolIE-ContainerPair{},

 ProtocolIE-ContainerPairList{},

 ProtocolIE-Single-Container{},

 XNAP-PRIVATE-IES,

 XNAP-PROTOCOL-EXTENSION,

 XNAP-PROTOCOL-IES,

 XNAP-PROTOCOL-IES-PAIR

FROM XnAP-Containers

 id-ActivatedServedCells,

 id-ActivationIDforCellActivation,

 id-AdditionalDRBIDs,

 id-AMF-Region-Information,

 id-AMF-Region-Information-To-Add,

 id-AMF-Region-Information-To-Delete,

 id-AssistanceDataForRANPaging,

 id-AvailableDRBIDs,

 id-Cause,

 id-cellAssistanceInfo-EUTRA,

 id-cellAssistanceInfo-NR,

 id-CellAndCapacityAssistanceInfo-EUTRA,

 id-CellAndCapacityAssistanceInfo-NR,

 id-ConfigurationUpdateInitiatingNodeChoice,

 id-UEContextID,

 id-CriticalityDiagnostics,

 id-XnUAddressInfoperPDUSession-List,

 id-DesiredActNotificationLevel,

 id-DRBsSubjectToStatusTransfer-List,

 id-ExpectedUEBehaviour,

 id-FiveGCMobilityRestrictionListContainer,

 id-GlobalNG-RAN-node-ID,

 id-GUAMI,

 id-indexToRatFrequSelectionPriority,

 id-List-of-served-cells-E-UTRA,

 id-List-of-served-cells-NR,

 id-LocationInformationSN,

 id-LocationInformationSNReporting,

 id-LocationReportingInformation,

 id-LTEUESidelinkAggregateMaximumBitRate,

 id-LTEV2XServicesAuthorized,

 id-MAC-I,

 id-MaskedIMEISV,

 id-MDT-Configuration,

 id-MDTPLMNList,

 id-MN-to-SN-Container,

 id-MobilityRestrictionList,

 id-M-NG-RANnodeUEXnAPID,

 id-new-NG-RAN-Cell-Identity,

 id-newNG-RANnodeUEXnAPID,

 id-NRUESidelinkAggregateMaximumBitRate,

 id-NRV2XServicesAuthorized,

 id-oldNG-RANnodeUEXnAPID,

 id-OldtoNewNG-RANnodeResumeContainer,

 id-PagingDRX,

 id-PagingPriority,

 id-PartialListIndicator-EUTRA,

 id-PartialListIndicator-NR,

 id-PCellID,

 id-PDUSessionResourceSecondaryRATUsageList,

 id-PDUSessionResourcesActivityNotifyList,

 id-PDUSessionResourcesAdmitted-List,

 id-PDUSessionResourcesNotAdmitted-List,

 id-PDUSessionResourcesNotifyList,

 id-PDUSessionToBeAddedAddReq,

 id-PDUSessionToBeReleased-RelReqAck,

 id-procedureStage,

 id-RANPagingArea,

 id-requestedSplitSRB,

 id-RequiredNumberOfDRBIDs,

 id-ResetRequestTypeInfo,

 id-ResetResponseTypeInfo,

 id-RespondingNodeTypeConfigUpdateAck,

 id-RRCResumeCause,

 id-selectedPLMN,

 id-ServedCellsToActivate,

 id-servedCellsToUpdate-E-UTRA,

 id-ServedCellsToUpdateInitiatingNodeChoice,

 id-servedCellsToUpdate-NR,

 id-sourceNG-RANnodeUEXnAPID,

 id-SpareDRBIDs,

 id-S-NG-RANnodeMaxIPDataRate-UL,

 id-S-NG-RANnodeMaxIPDataRate-DL,

 id-S-NG-RANnodeUEXnAPID,

 id-TAISupport-list,

 id-Target2SourceNG-RANnodeTranspContainer,

 id-targetCellGlobalID,

 id-targetNG-RANnodeUEXnAPID,

 id-TimeToWait,

 id-TNLA-To-Add-List,

 id-TNLA-To-Update-List,

 id-TNLA-To-Remove-List,

 id-TNLA-Setup-List,

 id-TNLA-Failed-To-Setup-List,

 id-TraceActivation,

 id-UEContextInfoHORequest,

 id-UEContextInfoRetrUECtxtResp,

 id-UEContextKeptIndicator,

 id-UEContextRefAtSN-HORequest,

 id-UEHistoryInformation,

 id-UEIdentityIndexValue,

 id-UERANPagingIdentity,

 id-UESecurityCapabilities,

 id-UserPlaneTrafficActivityReport,

 id-XnRemovalThreshold,

 id-PDUSessionAdmittedAddedAddReqAck,

 id-PDUSessionNotAdmittedAddReqAck,

 id-SN-to-MN-Container,

 id-RRCConfigIndication,

 id-SplitSRB-RRCTransfer,

 id-UEReportRRCTransfer,

 id-PDUSessionReleasedList-RelConf,

 id-BearersSubjectToCounterCheck,

 id-PDUSessionToBeReleasedList-RelRqd,

 id-ResponseInfo-ReconfCompl,

 id-initiatingNodeType-ResourceCoordRequest,

 id-respondingNodeType-ResourceCoordResponse,

 id-PDUSessionToBeReleased-RelReq,

 id-PDUSession-SNChangeRequired-List,

 id-PDUSession-SNChangeConfirm-List,

 id-PDCPChangeIndication,

 id-PC5QoSParameters,

 id-SCGConfigurationQuery,

 id-UEContextInfo-SNModRequest,

 id-requestedSplitSRBrelease,

 id-PDUSessionAdmitted-SNModResponse,

 id-PDUSessionNotAdmitted-SNModResponse,

 id-admittedSplitSRB,

 id-admittedSplitSRBrelease,

 id-PDUSessionAdmittedModSNModConfirm,

 id-PDUSessionReleasedSNModConfirm,

 id-s-ng-RANnode-SecurityKey,

 id-PDUSessionToBeModifiedSNModRequired,

 id-S-NG-RANnodeUE-AMBR,

 id-PDUSessionToBeReleasedSNModRequired,

 id-target-S-NG-RANnodeID,

 id-S-NSSAI,

 id-MR-DC-ResourceCoordinationInfo,

 id-RANPagingFailure,

 id-UERadioCapabilityForPaging,

 id-PDUSessionDataForwarding-SNModResponse,

 id-Secondary-MN-Xn-U-TNLInfoatM,

 id-NE-DC-TDM-Pattern,

 id-InterfaceInstanceIndication,

 id-S-NG-RANnode-Addition-Trigger-Ind,

 id-SNTriggered,

 id-DRBs-transferred-to-MN,

 id-TNLConfigurationInfo,

 id-MessageOversizeNotification,

 id-NG-RANTraceID,

 id-FastMCGRecoveryRRCTransfer-SN-to-MN,

 id-FastMCGRecoveryRRCTransfer-MN-to-SN,

 id-RequestedFastMCGRecoveryViaSRB3,

 id-AvailableFastMCGRecoveryViaSRB3,

 id-RequestedFastMCGRecoveryViaSRB3Release,

 id-ReleaseFastMCGRecoveryViaSRB3,

 id-CHOinformation-Req,

 id-CHOinformation-Ack,

 id-targetCellsToCancel,

 id-requestedTargetCellGlobalID,

 id-DAPSResponseInfo-List,

 id-CHO-MRDC-Indicator,

 id-MobilityInformation,

 id-InitiatingCondition-FailureIndication,

 id-UEHistoryInformationFromTheUE,

 id-HandoverReportType,

 id-HandoverCause,

 id-SourceCellCGI,

 id-TargetCellCGI,

 id-ReEstablishmentCellCGI,

 id-TargetCellinEUTRAN,

 id-SourceCellCRNTI,

 id-UERLFReportContainer,

 id-NGRAN-Node1-Measurement-ID,

 id-NGRAN-Node2-Measurement-ID,

 id-RegistrationRequest,

 id-ReportCharacteristics,

 id-CellToReport,

 id-ReportingPeriodicity,

 id-CellMeasurementResult,

 id-NG-RANnode1CellID,

 id-NG-RANnode2CellID,

 id-NG-RANnode1MobilityParameters,

 id-NG-RANnode2ProposedMobilityParameters,

 id-MobilityParametersModificationRange,

 id-RACHReportInformation,

 id-IABNodeIndication,

 id-UERadioCapabilityID,

id-ManagementBasedMDTPLMNList,

id-PrivacyIndicator,

id-TraceCollectionEntityIPAddress,

 maxnoofCellsinNG-RANnode,

 maxnoofDRBs,

 maxnoofPDUSessions,

 maxnoofQoSFlows

FROM XnAP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- S-NODE ADDITION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SNodeAdditionRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container {{ SNodeAdditionRequest-IEs}},

 ...

}

SNodeAdditionRequest-IEs XNAP-PROTOCOL-IES ::= {

 { ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

 { ID id-UESecurityCapabilities CRITICALITY reject TYPE UESecurityCapabilities PRESENCE mandatory}|

 { ID id-s-ng-RANnode-SecurityKey CRITICALITY reject TYPE S-NG-RANnode-SecurityKey PRESENCE mandatory}|

 { ID id-S-NG-RANnodeUE-AMBR CRITICALITY reject TYPE UEAggregateMaximumBitRate PRESENCE mandatory}|

 { ID id-selectedPLMN CRITICALITY ignore TYPE PLMN-Identity PRESENCE optional }|

 { ID id-MobilityRestrictionList CRITICALITY ignore TYPE MobilityRestrictionList PRESENCE optional }|

 { ID id-indexToRatFrequSelectionPriority CRITICALITY reject TYPE RFSP-Index PRESENCE optional }|

 { ID id-PDUSessionToBeAddedAddReq CRITICALITY reject TYPE PDUSessionToBeAddedAddReq PRESENCE mandatory}|

 { ID id-MN-to-SN-Container CRITICALITY reject TYPE OCTET STRING PRESENCE mandatory}|

 { ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE optional }|

 { ID id-ExpectedUEBehaviour CRITICALITY ignore TYPE ExpectedUEBehaviour PRESENCE optional }|

 { ID id-requestedSplitSRB CRITICALITY reject TYPE SplitSRBsTypes PRESENCE optional }|

 { ID id-PCellID CRITICALITY reject TYPE GlobalNG-RANCell-ID PRESENCE optional }|

 { ID id-DesiredActNotificationLevel CRITICALITY ignore TYPE DesiredActNotificationLevel PRESENCE optional }|

 { ID id-AvailableDRBIDs CRITICALITY reject TYPE DRB-List PRESENCE conditional}

 -- The IE shall be present if there is at least one PDUSessionResourceSetupInfo-SNterminated included --|

 { ID id-S-NG-RANnodeMaxIPDataRate-UL CRITICALITY reject TYPE BitRate PRESENCE optional }|

 { ID id-S-NG-RANnodeMaxIPDataRate-DL CRITICALITY reject TYPE BitRate PRESENCE optional }|

 { ID id-LocationInformationSNReporting CRITICALITY ignore TYPE LocationInformationSNReporting PRESENCE optional}|

 { ID id-MR-DC-ResourceCoordinationInfo CRITICALITY ignore TYPE MR-DC-ResourceCoordinationInfo PRESENCE optional }|

 { ID id-MaskedIMEISV CRITICALITY ignore TYPE MaskedIMEISV PRESENCE optional}|

 { ID id-NE-DC-TDM-Pattern CRITICALITY ignore TYPE NE-DC-TDM-Pattern PRESENCE optional}|

 { ID id-S-NG-RANnode-Addition-Trigger-Ind CRITICALITY reject TYPE S-NG-RANnode-Addition-Trigger-Ind PRESENCE optional}|

 { ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional}|

 { ID id-RequestedFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE RequestedFastMCGRecoveryViaSRB3 PRESENCE optional}|

 { ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional}|

{ ID id-ManagementBasedMDTPLMNList CRITICALITY ignore TYPE MDTPLMNList PRESENCE optional },

 ...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- CELL TRAFFIC TRACE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

CellTrafficTrace ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { {CellTrafficTraceIEs} },

 ...

}

CellTrafficTraceIEs XNAP-PROTOCOL-IES ::= {

 { ID id-M-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

 { ID id-S-NG-RANnodeUEXnAPID CRITICALITY reject TYPE NG-RANnodeUEXnAPID PRESENCE mandatory}|

 { ID id-NG-RANTraceID CRITICALITY ignore TYPE NG-RANTraceID PRESENCE mandatory }|

 { ID id-TraceCollectionEntityIPAddress CRITICALITY ignore TYPE TransportLayerAddress PRESENCE mandatory }|

 { ID id-PrivacyIndicator CRITICALITY ignore TYPE PrivacyIndicator PRESENCE optional }|

{ ID id-TraceCollectionEntityURI CRITICALITY ignore TYPE URIaddress PRESENCE optional},

 ...

}

### 9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-E-RAB-Item,

 id-Number-of-Antennaports,

 id-MBSFN-Subframe-Info,

 id-PRACH-Configuration,

 id-CSG-Id,

 id-MDTConfiguration,

 id-SignallingBasedMDTPLMNList,

 id-MultibandInfoList,

 id-FreqBandIndicatorPriority,

 id-NeighbourTAC,

 id-Time-UE-StayedInCell-EnhancedGranularity,

 id-MBMS-Service-Area-List,

 id-HO-cause,

 id-eARFCNExtension,

 id-DL-EARFCNExtension,

 id-UL-EARFCNExtension,

 id-M3Configuration,

 id-M4Configuration,

 id-M5Configuration,

 id-MDT-Location-Info,

 id-NRrestrictioninEPSasSecondaryRAT,

 id-NRrestrictionin5GS,

 id-AdditionalSpecialSubframe-Info,

 id-UEID,

 id-enhancedRNTP,

 id-ProSeUEtoNetworkRelaying,

 id-M6Configuration,

 id-M7Configuration,

 id-OffsetOfNbiotChannelNumberToDL-EARFCN,

 id-OffsetOfNbiotChannelNumberToUL-EARFCN,

 id-AdditionalSpecialSubframeExtension-Info,

 id-BandwidthReducedSI,

 id-extended-e-RAB-MaximumBitrateDL,

 id-extended-e-RAB-MaximumBitrateUL,

 id-extended-e-RAB-GuaranteedBitrateDL,

 id-extended-e-RAB-GuaranteedBitrateUL,

 id-extended-uEaggregateMaximumBitRateDownlink,

 id-extended-uEaggregateMaximumBitRateUplink,

 id-E-RABUsageReport-Item,

 id-SecondaryRATUsageReport-Item,

 id-UEAppLayerMeasConfig,

 id-DL-scheduling-PDCCH-CCE-usage,

 id-UL-scheduling-PDCCH-CCE-usage,

 id-DownlinkPacketLossRate,

 id-UplinkPacketLossRate,

 id-serviceType,

 id-ProtectedEUTRAResourceIndication,

 id-NRS-NSSS-PowerOffset,

 id-NSSS-NumOccasionDifferentPrecoder,

 id-CNTypeRestrictions,

 id-BluetoothMeasurementConfiguration,

 id-WLANMeasurementConfiguration,

 id-ECGI,

 id-NRCGI,

 id-MeNBCoordinationAssistanceInformation,

 id-SgNBCoordinationAssistanceInformation,

 id-NRNeighbourInfoToAdd,

 id-LastNG-RANPLMNIdentity,

 id-BPLMN-ID-Info-EUTRA,

 id-NBIoT-UL-DL-AlignmentOffset,

 id-UnlicensedSpectrumRestriction,

 id-CarrierList,

 id-FrequencyShift7p5khz,

 id-NPRACHConfiguration,

 id-MDTConfigurationNR,

 id-CSI-RSTransmissionIndication,

 id-QoS-Mapping-Information,

 id-IntendedTDD-DL-ULConfiguration-NR,

 maxnoofBearers,

 maxCellineNB,

 maxEARFCN,

 maxEARFCNPlusOne,

 newmaxEARFCN,

 maxInterfaces,

 maxnoofBands,

 maxnoofBPLMNs,

 maxnoofAdditionalPLMNs,

 maxnoofCells,

 maxnoofEPLMNs,

 maxnoofEPLMNsPlusOne,

 maxnoofForbLACs,

 maxnoofForbTACs,

 maxnoofNeighbours,

 maxnoofPRBs,

 maxNrOfErrors,

 maxPools,

 maxnoofMBSFN,

 maxnoofTAforMDT,

 maxnoofCellIDforMDT,

 maxnoofMBMSServiceAreaIdentities,

 maxnoofMDTPLMNs,

 maxnoofCoMPHypothesisSet,

 maxnoofCoMPCells,

 maxUEReport,

 maxCellReport,

 maxnoofPA,

 maxCSIProcess,

 maxCSIReport,

 maxSubband,

 maxnooftimeperiods,

 maxnoofCellIDforQMC,

 maxnoofTAforQMC,

 maxnoofPLMNforQMC,

 maxUEsinengNBDU,

 maxnoofProtectedResourcePatterns,

 maxnoNRcellsSpectrumSharingWithE-UTRA,

 maxnoofNrCellBands,

 maxnoofBluetoothName,

 maxnoofWLANName,

 maxofNRNeighbours,

 maxnoofextBPLMNs,

 maxnoofTLAs,

 maxnoofGTPTLAs,

 maxnoofTNLAssociations,

 maxnoofCellsinCHO, maxnoofPC5QoSFlows,

 maxnoofSSBAreas,

 maxnoofNRSCSs,

 maxnoofNRPhysicalResourceBlocks,

 maxnoofNonAnchorCarrierFreqConfig

FROM X2AP-Constants

 Criticality,

 ProcedureCode,

 ProtocolIE-ID,

 TriggeringMessage

FROM X2AP-CommonDataTypes

 ProtocolExtensionContainer{},

 ProtocolIE-Single-Container{},

 X2AP-PROTOCOL-EXTENSION,

 X2AP-PROTOCOL-IES

FROM X2AP-Containers;

-- P

PrivacyIndicator ::= ENUMERATED {

 immediate-MDT,

 logged-MDT,

 ...

}

### 9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

XnAP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) xnap (2) version1 (1) xnap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM XnAP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-handoverPreparation ProcedureCode ::= 0

id-sNStatusTransfer ProcedureCode ::= 1

id-handoverCancel ProcedureCode ::= 2

id-retrieveUEContext ProcedureCode ::= 3

id-rANPaging ProcedureCode ::= 4

id-xnUAddressIndication ProcedureCode ::= 5

id-uEContextRelease ProcedureCode ::= 6

id-sNGRANnodeAdditionPreparation ProcedureCode ::= 7

id-sNGRANnodeReconfigurationCompletion ProcedureCode ::= 8

id-mNGRANnodeinitiatedSNGRANnodeModificationPreparation ProcedureCode ::= 9

id-sNGRANnodeinitiatedSNGRANnodeModificationPreparation ProcedureCode ::= 10

id-mNGRANnodeinitiatedSNGRANnodeRelease ProcedureCode ::= 11

id-sNGRANnodeinitiatedSNGRANnodeRelease ProcedureCode ::= 12

id-sNGRANnodeCounterCheck ProcedureCode ::= 13

id-sNGRANnodeChange ProcedureCode ::= 14

id-rRCTransfer ProcedureCode ::= 15

id-xnRemoval ProcedureCode ::= 16

id-xnSetup ProcedureCode ::= 17

id-nGRANnodeConfigurationUpdate ProcedureCode ::= 18

id-cellActivation ProcedureCode ::= 19

id-reset ProcedureCode ::= 20

id-errorIndication ProcedureCode ::= 21

id-privateMessage ProcedureCode ::= 22

id-notificationControl ProcedureCode ::= 23

id-activityNotification ProcedureCode ::= 24

id-e-UTRA-NR-CellResourceCoordination ProcedureCode ::= 25

id-secondaryRATDataUsageReport ProcedureCode ::= 26

id-deactivateTrace ProcedureCode ::= 27

id-traceStart ProcedureCode ::= 28

id-handoverSuccess ProcedureCode ::= 29

id-conditionalHandoverCancel ProcedureCode ::= 30

id-earlyStatusTransfer ProcedureCode ::= 31

id-failureIndication ProcedureCode ::= 32

id-handoverReport ProcedureCode ::= 33

id-resourceStatusReportingInitiation ProcedureCode ::= 34

id-resourceStatusReporting ProcedureCode ::= 35

id-mobilitySettingsChange ProcedureCode ::= 36

id-accessAndMobilityIndication ProcedureCode ::= 37

id-cellTrafficTrace ProcedureCode ::= XX

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxEARFCN INTEGER ::= 262143

maxnoofAllowedAreas INTEGER ::= 16

maxnoofAMFRegions INTEGER ::= 16

maxnoofAoIs INTEGER ::= 64

maxnoofBluetoothName INTEGER ::= 4

maxnoofBPLMNs INTEGER ::= 12

maxnoofCAGs INTEGER ::= 12

maxnoofCAGsperPLMN INTEGER ::= 256

maxnoofCellIDforMDT INTEGER ::= 32

maxnoofCellsinAoI INTEGER ::= 256

maxnoofCellsinUEHistoryInfo INTEGER ::= 16

maxnoofCellsinNG-RANnode INTEGER ::= 16384

maxnoofCellsinRNA INTEGER ::= 32

maxnoofCellsUEMovingTrajectory INTEGER ::= 16

maxnoofDRBs INTEGER ::= 32

maxnoofEUTRABands INTEGER ::= 16

maxnoofEUTRABPLMNs INTEGER ::= 6

maxnoofEPLMNs INTEGER ::= 15

maxnoofExtSliceItems INTEGER ::= 65535

maxnoofEPLMNsplus1 INTEGER ::= 16

maxnoofForbiddenTACs INTEGER ::= 4096

maxnoofFreqforMDT INTEGER ::= 8

maxnoofMBSFNEUTRA INTEGER ::= 8

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofMultiConnectivityMinusOne INTEGER ::= 3

maxnoofNeighbours INTEGER ::= 1024

maxnoofNeighPCIforMDT INTEGER ::= 32

maxnoofNIDs INTEGER ::= 12

maxnoofNRCellBands INTEGER ::= 32

maxnoofPLMNs INTEGER ::= 16

maxnoofPDUSessions INTEGER ::= 256

maxnoofProtectedResourcePatterns INTEGER ::= 16

maxnoofQoSFlows INTEGER ::= 64

maxnoofQoSParaSets INTEGER ::= 8

maxnoofRANAreaCodes INTEGER ::= 32

maxnoofRANAreasinRNA INTEGER ::= 16

maxnoofRANNodesinAoI INTEGER ::= 64

maxnoofSCellGroups INTEGER ::= 3

maxnoofSCellGroupsplus1 INTEGER ::= 4

maxnoofSensorName INTEGER ::= 3

maxnoofSliceItems INTEGER ::= 1024

maxnoofSNPNIDs INTEGER ::= 12

maxnoofsupportedPLMNs INTEGER ::= 12

maxnoofsupportedTACs INTEGER ::= 256

maxnoofTAforMDT INTEGER ::= 8

maxnoofTAI INTEGER ::= 16

maxnoofTAIsinAoI INTEGER ::= 16

maxnooftimeperiods INTEGER ::= 2

maxnoofTNLAssociations INTEGER ::= 32

maxnoofUEContexts INTEGER ::= 8192

maxNRARFCN INTEGER ::= 3279165

maxNrOfErrors INTEGER ::= 256

maxnoofslots INTEGER ::= 5120

maxnoofExtTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoofCHOcells INTEGER ::= 8

maxnoofPC5QoSFlows INTEGER ::= 2064

maxnoofSSBAreas INTEGER ::= 64

maxnoofRACHReports INTEGER ::= 64

maxnoofNRSCSs INTEGER ::= 5

maxnoofPhysicalResourceBlocks INTEGER ::= 275

maxnoofAdditionalPDCPDuplicationTNL INTEGER ::= 2

maxnoofRLCDuplicationstate INTEGER ::= 3

maxnoofWLANName INTEGER ::= 4

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-ActivatedServedCells ProtocolIE-ID ::= 0

id-ActivationIDforCellActivation ProtocolIE-ID ::= 1

id-admittedSplitSRB ProtocolIE-ID ::= 2

id-admittedSplitSRBrelease ProtocolIE-ID ::= 3

id-AMF-Region-Information ProtocolIE-ID ::= 4

id-AssistanceDataForRANPaging ProtocolIE-ID ::= 5

id-BearersSubjectToCounterCheck ProtocolIE-ID ::= 6

id-Cause ProtocolIE-ID ::= 7

id-cellAssistanceInfo-NR ProtocolIE-ID ::= 8

id-ConfigurationUpdateInitiatingNodeChoice ProtocolIE-ID ::= 9

id-CriticalityDiagnostics ProtocolIE-ID ::= 10

id-XnUAddressInfoperPDUSession-List ProtocolIE-ID ::= 11

id-DRBsSubjectToStatusTransfer-List ProtocolIE-ID ::= 12

id-ExpectedUEBehaviour ProtocolIE-ID ::= 13

id-GlobalNG-RAN-node-ID ProtocolIE-ID ::= 14

id-GUAMI ProtocolIE-ID ::= 15

id-indexToRatFrequSelectionPriority ProtocolIE-ID ::= 16

id-initiatingNodeType-ResourceCoordRequest ProtocolIE-ID ::= 17

id-List-of-served-cells-E-UTRA ProtocolIE-ID ::= 18

id-List-of-served-cells-NR ProtocolIE-ID ::= 19

id-LocationReportingInformation ProtocolIE-ID ::= 20

id-MAC-I ProtocolIE-ID ::= 21

id-MaskedIMEISV ProtocolIE-ID ::= 22

id-M-NG-RANnodeUEXnAPID ProtocolIE-ID ::= 23

id-MN-to-SN-Container ProtocolIE-ID ::= 24

id-MobilityRestrictionList ProtocolIE-ID ::= 25

id-new-NG-RAN-Cell-Identity ProtocolIE-ID ::= 26

id-newNG-RANnodeUEXnAPID ProtocolIE-ID ::= 27

id-UEReportRRCTransfer ProtocolIE-ID ::= 28

id-oldNG-RANnodeUEXnAPID ProtocolIE-ID ::= 29

id-OldtoNewNG-RANnodeResumeContainer ProtocolIE-ID ::= 30

id-PagingDRX ProtocolIE-ID ::= 31

id-PCellID ProtocolIE-ID ::= 32

id-PDCPChangeIndication ProtocolIE-ID ::= 33

id-PDUSessionAdmittedAddedAddReqAck ProtocolIE-ID ::= 34

id-PDUSessionAdmittedModSNModConfirm ProtocolIE-ID ::= 35

id-PDUSessionAdmitted-SNModResponse ProtocolIE-ID ::= 36

id-PDUSessionNotAdmittedAddReqAck ProtocolIE-ID ::= 37

id-PDUSessionNotAdmitted-SNModResponse ProtocolIE-ID ::= 38

id-PDUSessionReleasedList-RelConf ProtocolIE-ID ::= 39

id-PDUSessionReleasedSNModConfirm ProtocolIE-ID ::= 40

id-PDUSessionResourcesActivityNotifyList ProtocolIE-ID ::= 41

id-PDUSessionResourcesAdmitted-List ProtocolIE-ID ::= 42

id-PDUSessionResourcesNotAdmitted-List ProtocolIE-ID ::= 43

id-PDUSessionResourcesNotifyList ProtocolIE-ID ::= 44

id-PDUSession-SNChangeConfirm-List ProtocolIE-ID ::= 45

id-PDUSession-SNChangeRequired-List ProtocolIE-ID ::= 46

id-PDUSessionToBeAddedAddReq ProtocolIE-ID ::= 47

id-PDUSessionToBeModifiedSNModRequired ProtocolIE-ID ::= 48

id-PDUSessionToBeReleasedList-RelRqd ProtocolIE-ID ::= 49

id-PDUSessionToBeReleased-RelReq ProtocolIE-ID ::= 50

id-PDUSessionToBeReleasedSNModRequired ProtocolIE-ID ::= 51

id-RANPagingArea ProtocolIE-ID ::= 52

id-PagingPriority ProtocolIE-ID ::= 53

id-requestedSplitSRB ProtocolIE-ID ::= 54

id-requestedSplitSRBrelease ProtocolIE-ID ::= 55

id-ResetRequestTypeInfo ProtocolIE-ID ::= 56

id-ResetResponseTypeInfo ProtocolIE-ID ::= 57

id-RespondingNodeTypeConfigUpdateAck ProtocolIE-ID ::= 58

id-respondingNodeType-ResourceCoordResponse ProtocolIE-ID ::= 59

id-ResponseInfo-ReconfCompl ProtocolIE-ID ::= 60

id-RRCConfigIndication ProtocolIE-ID ::= 61

id-RRCResumeCause ProtocolIE-ID ::= 62

id-SCGConfigurationQuery ProtocolIE-ID ::= 63

id-selectedPLMN ProtocolIE-ID ::= 64

id-ServedCellsToActivate ProtocolIE-ID ::= 65

id-servedCellsToUpdate-E-UTRA ProtocolIE-ID ::= 66

id-ServedCellsToUpdateInitiatingNodeChoice ProtocolIE-ID ::= 67

id-servedCellsToUpdate-NR ProtocolIE-ID ::= 68

id-s-ng-RANnode-SecurityKey ProtocolIE-ID ::= 69

id-S-NG-RANnodeUE-AMBR ProtocolIE-ID ::= 70

id-S-NG-RANnodeUEXnAPID ProtocolIE-ID ::= 71

id-SN-to-MN-Container ProtocolIE-ID ::= 72

id-sourceNG-RANnodeUEXnAPID ProtocolIE-ID ::= 73

id-SplitSRB-RRCTransfer ProtocolIE-ID ::= 74

id-TAISupport-list ProtocolIE-ID ::= 75

id-TimeToWait ProtocolIE-ID ::= 76

id-Target2SourceNG-RANnodeTranspContainer ProtocolIE-ID ::= 77

id-targetCellGlobalID ProtocolIE-ID ::= 78

id-targetNG-RANnodeUEXnAPID ProtocolIE-ID ::= 79

id-target-S-NG-RANnodeID ProtocolIE-ID ::= 80

id-TraceActivation ProtocolIE-ID ::= 81

id-UEContextID ProtocolIE-ID ::= 82

id-UEContextInfoHORequest ProtocolIE-ID ::= 83

id-UEContextInfoRetrUECtxtResp ProtocolIE-ID ::= 84

id-UEContextInfo-SNModRequest ProtocolIE-ID ::= 85

id-UEContextKeptIndicator ProtocolIE-ID ::= 86

id-UEContextRefAtSN-HORequest ProtocolIE-ID ::= 87

id-UEHistoryInformation ProtocolIE-ID ::= 88

id-UEIdentityIndexValue ProtocolIE-ID ::= 89

id-UERANPagingIdentity ProtocolIE-ID ::= 90

id-UESecurityCapabilities ProtocolIE-ID ::= 91

id-UserPlaneTrafficActivityReport ProtocolIE-ID ::= 92

id-XnRemovalThreshold ProtocolIE-ID ::= 93

id-DesiredActNotificationLevel ProtocolIE-ID ::= 94

id-AvailableDRBIDs ProtocolIE-ID ::= 95

id-AdditionalDRBIDs ProtocolIE-ID ::= 96

id-SpareDRBIDs ProtocolIE-ID ::= 97

id-RequiredNumberOfDRBIDs ProtocolIE-ID ::= 98

id-TNLA-To-Add-List ProtocolIE-ID ::= 99

id-TNLA-To-Update-List ProtocolIE-ID ::= 100

id-TNLA-To-Remove-List ProtocolIE-ID ::= 101

id-TNLA-Setup-List ProtocolIE-ID ::= 102

id-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 103

id-PDUSessionToBeReleased-RelReqAck ProtocolIE-ID ::= 104

id-S-NG-RANnodeMaxIPDataRate-UL ProtocolIE-ID ::= 105

id-PDUSessionResourceSecondaryRATUsageList ProtocolIE-ID ::= 107

id-Additional-UL-NG-U-TNLatUPF-List ProtocolIE-ID ::= 108

id-SecondarydataForwardingInfoFromTarget-List ProtocolIE-ID ::= 109

id-LocationInformationSNReporting ProtocolIE-ID ::= 110

id-LocationInformationSN ProtocolIE-ID ::= 111

id-LastE-UTRANPLMNIdentity ProtocolIE-ID ::= 112

id-S-NG-RANnodeMaxIPDataRate-DL ProtocolIE-ID ::= 113

id-MaxIPrate-DL ProtocolIE-ID ::= 114

id-SecurityResult ProtocolIE-ID ::= 115

id-S-NSSAI ProtocolIE-ID ::= 116

id-MR-DC-ResourceCoordinationInfo ProtocolIE-ID ::= 117

id-AMF-Region-Information-To-Add ProtocolIE-ID ::= 118

id-AMF-Region-Information-To-Delete ProtocolIE-ID ::= 119

id-OldQoSFlowMap-ULendmarkerexpected ProtocolIE-ID ::= 120

id-RANPagingFailure ProtocolIE-ID ::= 121

id-UERadioCapabilityForPaging ProtocolIE-ID ::= 122

id-PDUSessionDataForwarding-SNModResponse ProtocolIE-ID ::= 123

id-DRBsNotAdmittedSetupModifyList ProtocolIE-ID ::= 124

id-Secondary-MN-Xn-U-TNLInfoatM ProtocolIE-ID ::= 125

id-NE-DC-TDM-Pattern ProtocolIE-ID ::= 126

id-PDUSessionCommonNetworkInstance ProtocolIE-ID ::= 127

id-BPLMN-ID-Info-EUTRA ProtocolIE-ID ::= 128

id-BPLMN-ID-Info-NR ProtocolIE-ID ::= 129

id-InterfaceInstanceIndication ProtocolIE-ID ::= 130

id-S-NG-RANnode-Addition-Trigger-Ind ProtocolIE-ID ::= 131

id-DefaultDRB-Allowed ProtocolIE-ID ::= 132

id-DRB-IDs-takenintouse ProtocolIE-ID ::= 133

id-SplitSessionIndicator ProtocolIE-ID ::= 134

id-CNTypeRestrictionsForEquivalent ProtocolIE-ID ::= 135

id-CNTypeRestrictionsForServing ProtocolIE-ID ::= 136

id-DRBs-transferred-to-MN ProtocolIE-ID ::= 137

id-ULForwardingProposal ProtocolIE-ID ::= 138

id-EndpointIPAddressAndPort ProtocolIE-ID ::= 139

id-IntendedTDD-DL-ULConfiguration-NR ProtocolIE-ID ::= 140

id-TNLConfigurationInfo ProtocolIE-ID ::= 141

id-PartialListIndicator-NR ProtocolIE-ID ::= 142

id-MessageOversizeNotification ProtocolIE-ID ::= 143

id-CellAndCapacityAssistanceInfo-NR ProtocolIE-ID ::= 144

id-NG-RANTraceID ProtocolIE-ID ::= 145

id-NonGBRResources-Offered ProtocolIE-ID ::= 146

id-FastMCGRecoveryRRCTransfer-SN-to-MN ProtocolIE-ID ::= 147

id-RequestedFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 148

id-AvailableFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 149

id-RequestedFastMCGRecoveryViaSRB3Release ProtocolIE-ID ::= 150

id-ReleaseFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 151

id-FastMCGRecoveryRRCTransfer-MN-to-SN ProtocolIE-ID ::= 152

id-ExtendedRATRestrictionInformation ProtocolIE-ID ::= 153

id-QoSMonitoringRequest ProtocolIE-ID ::= 154

id-FiveGCMobilityRestrictionListContainer ProtocolIE-ID ::= 155

id-PartialListIndicator-EUTRA ProtocolIE-ID ::= 156

id-CellAndCapacityAssistanceInfo-EUTRA ProtocolIE-ID ::= 157

id-CHOinformation-Req ProtocolIE-ID ::= 158

id-CHOinformation-Ack ProtocolIE-ID ::= 159

id-targetCellsToCancel ProtocolIE-ID ::= 160

id-requestedTargetCellGlobalID ProtocolIE-ID ::= 161

id-procedureStage ProtocolIE-ID ::= 162

id-DAPSRequestInfo ProtocolIE-ID ::= 163

id-DAPSResponseInfo-List ProtocolIE-ID ::= 164

id-CHO-MRDC-Indicator ProtocolIE-ID ::= 165

id-OffsetOfNbiotChannelNumberToDL-EARFCN ProtocolIE-ID ::= 166

id-OffsetOfNbiotChannelNumberToUL-EARFCN ProtocolIE-ID ::= 167

id-NBIoT-UL-DL-AlignmentOffset ProtocolIE-ID ::= 168

id-LTEV2XServicesAuthorized ProtocolIE-ID ::= 169

id-NRV2XServicesAuthorized ProtocolIE-ID ::= 170

id-LTEUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 171

id-NRUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 172

id-PC5QoSParameters ProtocolIE-ID ::= 173

id-AlternativeQoSParaSetList ProtocolIE-ID ::= 174

id-CurrentQoSParaSetIndex ProtocolIE-ID ::= 175

id-MobilityInformation ProtocolIE-ID ::= 176

id-InitiatingCondition-FailureIndication ProtocolIE-ID ::= 177

id-UEHistoryInformationFromTheUE ProtocolIE-ID ::= 178

id-HandoverReportType ProtocolIE-ID ::= 179

id-HandoverCause ProtocolIE-ID ::= 180

id-SourceCellCGI ProtocolIE-ID ::= 181

id-TargetCellCGI ProtocolIE-ID ::= 182

id-ReEstablishmentCellCGI ProtocolIE-ID ::= 183

id-TargetCellinEUTRAN ProtocolIE-ID ::= 184

id-SourceCellCRNTI ProtocolIE-ID ::= 185

id-UERLFReportContainer ProtocolIE-ID ::= 186

id-NGRAN-Node1-Measurement-ID ProtocolIE-ID ::= 187

id-NGRAN-Node2-Measurement-ID ProtocolIE-ID ::= 188

id-RegistrationRequest ProtocolIE-ID ::= 189

id-ReportCharacteristics ProtocolIE-ID ::= 190

id-CellToReport ProtocolIE-ID ::= 191

id-ReportingPeriodicity ProtocolIE-ID ::= 192

id-CellMeasurementResult ProtocolIE-ID ::= 193

id-NG-RANnode1CellID ProtocolIE-ID ::= 194

id-NG-RANnode2CellID ProtocolIE-ID ::= 195

id-NG-RANnode1MobilityParameters ProtocolIE-ID ::= 196

id-NG-RANnode2ProposedMobilityParameters ProtocolIE-ID ::= 197

id-MobilityParametersModificationRange ProtocolIE-ID ::= 198

id-TDDULDLConfigurationCommonNR ProtocolIE-ID ::= 199

id-CarrierList ProtocolIE-ID ::= 200

id-ULCarrierList ProtocolIE-ID ::= 201

id-FrequencyShift7p5khz ProtocolIE-ID ::= 202

id-SSB-PositionsInBurst ProtocolIE-ID ::= 203

id-NRCellPRACHConfig ProtocolIE-ID ::= 204

id-RACHReportInformation ProtocolIE-ID ::= 205

id-IABNodeIndication ProtocolIE-ID ::= 206

id-Redundant-UL-NG-U-TNLatUPF ProtocolIE-ID ::= 207

id-CNPacketDelayBudgetDownlink ProtocolIE-ID ::= 208

id-CNPacketDelayBudgetUplink ProtocolIE-ID ::= 209

id-Additional-Redundant-UL-NG-U-TNLatUPF-List ProtocolIE-ID ::= 210

id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 211

id-TSCTrafficCharacteristics ProtocolIE-ID ::= 212

id-RedundantQoSFlowIndicator ProtocolIE-ID ::= 213

id-Redundant-DL-NG-U-TNLatNG-RAN ProtocolIE-ID ::= 214

id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 215

id-Additional-PDCP-Duplication-TNL-List ProtocolIE-ID ::= 216

id-RedundantPDUSessionInformation ProtocolIE-ID ::= 217

id-UsedRSNInformation ProtocolIE-ID ::= 218

id-RLCDuplicationInformation ProtocolIE-ID ::= 219

id-NPN-Broadcast-Information ProtocolIE-ID ::= 220

id-NPNPagingAssistanceInformation ProtocolIE-ID ::= 221

id-NPNMobilityInformation ProtocolIE-ID ::= 222

id-NPN-Support ProtocolIE-ID ::= 223

id-MDT-Configuration ProtocolIE-ID ::= 224

id-MDTPLMNList ProtocolIE-ID ::= 225

id-TraceCollectionEntityURI ProtocolIE-ID ::= 226

id-UERadioCapabilityID ProtocolIE-ID ::= 227

id-CSI-RSTransmissionIndication ProtocolIE-ID ::= 228

id-SNTriggered ProtocolIE-ID ::= 229

id-DLCarrierList ProtocolIE-ID ::= 230

id-ExtendedTAISliceSupportList ProtocolIE-ID ::= 231

id-cellAssistanceInfo-EUTRA ProtocolIE-ID ::= 232

id-ConfiguredTACIndication ProtocolIE-ID ::= 233

id-secondary-SN-UL-PDCP-UP-TNLInfo ProtocolIE-ID ::= 234

id-pdcpDuplicationConfiguration ProtocolIE-ID ::= 235

id-duplicationActivation ProtocolIE-ID ::= 236

id-ManagementBasedMDTPLMNList

 ProtocolIE-ID ::= XXX

id-PrivacyIndicator

 ProtocolIE-ID ::= XXX

id-TraceCollectionEntityIPAddress

ProtocolIE-ID ::= XXX

END

-- ASN1STOP

*End of the last change*