**3GPP TSG- Meeting #**

 **- November 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Support of release on CAG subscription change |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NG\_RAN\_PRN |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | At RAN3#108-3, RAN3 sent an LS to SA2 (S2-2004808/R3-204324) raising concern that the HO procedure triggered by the mobility restriction list change is a new behaviour (and that the MRL is only used to control subsequent mobility in CM-CONNECTED).SA2 has now changed their specifications as per LS sent (S2-2005904). As a result, at least in some cases as described in the CRs, the AMF requests the release of the AN connection after a CAG subscription change.However currently the existing cause values for NPN are tightly linked to access rejection only. Typical use case for release is instead when the mobility restriction is updated while the UE is in connected mode (i.e. not linked to access). |
|  |  |
| ***Summary of change:*** | The scope of an existing NPN cause value is extended to cover also the release use case. Note that this would already be the case anyway at access from a procedural point of view (i.e. the RAN receives a release command), but the release would happen immediately after the UE’s access.Impact analysis: This CR has isolated impact towards the previous version of the specification (same release). The impact can be considered isolated because the change only affects the PNI-NPN functionality, and because it only extends the use of an existing cause value. |
|  |  |
| ***Consequences if not approved:*** | No support for the flows in stage 2 specification. |
|  |  |
| ***Clauses affected:*** | 9.3.1.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### 9.3.1.2 Cause

The purpose of the *Cause* IE is to indicate the reason for a particular event for the NGAP protocol.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Cause Group* | M |  |  |  |
| >*Radio Network Layer* |  |  |  |  |
| >>Radio Network Layer Cause  | M |  | ENUMERATED(Unspecified,TXnRELOCOverall expiry,Successful handover,Release due to NG-RAN generated reason,Release due to 5GC generated reason,Handover cancelled,Partial handover,Handover failure in target 5GC/NG-RAN node or target system,Handover target not allowed,TNGRELOCoverall expiry,TNGRELOCprep expiry,Cell not available,Unknown target ID,No radio resources available in target cell,Unknown local UE NGAP ID,Inconsistent remote UE NGAP ID,Handover desirable for radio reasons,Time critical handover,Resource optimisation handover,Reduce load in serving cell,User inactivity,Radio connection with UE lost,Radio resources not available,Invalid QoS combination,Failure in the radio interface procedure,Interaction with other procedure,Unknown PDU Session ID,Unknown QoS Flow ID,Multiple PDU Session ID Instances,Multiple QoS Flow ID Instances,Encryption and/or integrity protection algorithms not supported,NG intra-system handover triggered,NG inter-system handover triggered,Xn handover triggered,Not supported 5QI value,UE context transfer,IMS voice EPS fallback or RAT fallback triggered,UP integrity protection not possible,UP confidentiality protection not possible,Slice(s) not supported,UE in RRC\_INACTIVE state not reachable,Redirection,Resources not available for the slice(s),UE maximum integrity protected data rate reason,Release due to CN-detected mobility,…, N26 interface not available, Release due to pre-emption,Multiple Location Reporting Reference ID Instances, RSN not available for the UP,NPN access denied,CAG only access denied) |  |
| *>Transport Layer* |  |  |  |  |
| >>Transport Layer Cause | M |  | ENUMERATED(Transport resource unavailable,Unspecified,…) |  |
| *>NAS* |  |  |  |  |
| >>NAS Cause | M |  | ENUMERATED(Normal release,Authentication failure,Deregister,Unspecified, …) |  |
| *>Protocol* |  |  |  |  |
| >>Protocol Cause | M |  | ENUMERATED(Transfer syntax error,Abstract syntax error (reject),Abstract syntax error (ignore and notify),Message not compatible with receiver state,Semantic error,Abstract syntax error (falsely constructed message),Unspecified,…) |  |
| *>Miscellaneous* |  |  |  |  |
| >>Miscellaneous Cause | M |  | ENUMERATED(Control processing overload, Not enough user plane processing resources,Hardware failure,O&M intervention,Unknown PLMN,Unspecified, …) |  |

The meaning of the different cause values is described in the following tables. In general, "not supported" cause values indicate that the related capability is missing. On the other hand, "not available" cause values indicate that the related capability is present, but insufficient resources were available to perform the requested action.

|  |  |
| --- | --- |
| Radio Network Layer cause | Meaning |
| Unspecified | Sent for radio network layer cause when none of the specified cause values applies. |
| TXnRELOCOverall expiry | The timer guarding the handover that takes place over Xn has abnormally expired. |
| Successful handover | Successful handover. |
| Release due to NG-RAN generated reason | Release is initiated due to NG-RAN generated reason. |
| Release due to 5GC generated reason | Release is initiated due to 5GC generated reason. |
| Handover cancelled | The reason for the action is cancellation of Handover. |
| Partial handover | Provides a reason for the handover cancellation. The HANDOVER COMMAND message from AMF contained *PDU Session Resource to Release List* IEor *QoS flow to Release List* and the source NG-RAN node estimated service continuity for the UE would be better by not proceeding with handover towards this particular target NG-RAN node. |
| Handover failure in target 5GC/ NG-RAN node or target system | The handover failed due to a failure in target 5GC/NG-RAN node or target system. |
| Handover target not allowed | Handover to the indicated target cell is not allowed for the UE in question. |
| TNGRELOCoverall expiry | The reason for the action is expiry of timer TNGRELOCoverall. |
| TNGRELOCprep expiry | Handover Preparation procedure is cancelled when timer TNGRELOCprep expires. |
| Cell not available | The concerned cell is not available. |
| Unknown target ID | Handover rejected because the target ID is not known to the AMF. |
| No radio resources available in target cell | Load on target cell is too high. |
| Unknown local UE NGAP ID | The action failed because the receiving node does not recognise the local UE NGAP ID. |
| Inconsistent remote UE NGAP ID | The action failed because the receiving node considers that the received remote UE NGAP ID is inconsistent. |
| Handover desirable for radio reasons | The reason for requesting handover is radio related. |
| Time critical handover | Handover is requested for time critical reason i.e., this cause value is reserved to represent all critical cases where the connection is likely to be dropped if handover is not performed. |
| Resource optimisation handover | The reason for requesting handover is to improve the load distribution with the neighbour cells. |
| Reduce load in serving cell | Load on serving cell needs to be reduced. When applied to handover preparation, it indicates the handover is triggered due to load balancing. |
| User inactivity | The action is requested due to user inactivity on all PDU sessions, e.g., NG is requested to be released in order to optimise the radio resources. |
| Radio connection with UE lost | The action is requested due to losing the radio connection to the UE. |
| Radio resources not available | No requested radio resources are available. |
| Invalid QoS combination | The action was failed because of invalid QoS combination. |
| Failure in the radio interface procedure | Radio interface procedure has failed. |
| Interaction with other procedure | The action is due to an ongoing interaction with another procedure. |
| Unknown PDU Session ID | The action failed because the PDU Session ID is unknown in the NG-RAN node. |
| Unknown QoS Flow ID | The action failed because the QoS Flow ID is unknown in the NG-RAN node. |
| Multiple PDU Session ID instances | The action failed because multiple instance of the same PDU Session had been provided to/from the NG-RAN node. |
| Multiple QoS Flow ID instances | The action failed because multiple instances of the same QoS flow had been provided to the NG-RAN node. |
| Encryption and/or integrity protection algorithms not supported | The NG-RAN node is unable to support any of the encryption and/or integrity protection algorithms supported by the UE. |
| NG intra-system handover triggered | The action is due to a NG intra-system handover that has been triggered. |
| NG inter-system handover triggered | The action is due to a NG inter-system handover that has been triggered. |
| Xn handover triggered | The action is due to an Xn handover that has been triggered. |
| Not supported 5QI value | The QoS flow setup failed because the requested 5QI is not supported. |
| UE context transfer | The action is due to a UE resumes from the NG-RAN node different from the one which sent the UE into RRC\_INACTIVE state. |
| IMS voice EPS fallback or RAT fallback triggered | The setup of QoS flow is failed due to EPS fallback or RAT fallback for IMS voice using handover or redirection. |
| UP integrity protection not possible | The PDU session cannot be accepted according to the required user plane integrity protection policy. |
| UP confidentiality protection not possible | The PDU session cannot be accepted according to the required user plane confidentiality protection policy. |
| Slice(s) not supported | Slice(s) not supported. |
| UE in RRC\_INACTIVE state not reachable | The action is requested due to RAN paging failure. |
| Redirection | The release is requested due to inter-system redirection or intra-system redirection. |
| Resources not available for the slice(s) | The requested resources are not available for the slice(s). |
| UE maximum integrity protected data rate reason | The request is not accepted in order to comply with the maximum data rate for integrity protection supported by the UE. |
| Release due to CN-detected mobility | The context release is requested by the AMF because the UE is already served by another CN node (same or different system), or another NG interface of the same CN node. |
| N26 interface not available | The action failed due to a temporary failure of the N26 interface. |
| Release due to pre-emption | Release is initiated due to pre-emption. |
| Multiple Location Reporting Reference ID Instances | The action failed because multiple areas of interest are set with the same Location Reporting Reference ID. |
| RSN not available for the UP | The redundant user plane resources indicated by RSN are not available. |
| NPN access denied | Access was denied, or release is requested, for NPN reasons. |
| CAG only access denied | Access was denied because the cell is a non-CAG cell and UE is only allowed to access CAG cells. |