3GPP TSG-RAN WG3 Meeting #110-e R3-206967

E-meeting, 2 – 12 November, 2020

**Agenda item: 9.3.7.1**

**Source: Ericsson (moderator)**

**Title: CB: # 95\_InsuffUEcapCauseValue**

**Document for: Approval**

# 1 Introduction

This paper provides summary of discussions at RAN#110-e on:

**CB: # 95\_InsuffUEcapCauseValue**

**- clarify usage**

(E/// - moderator)

# 2 For the Chairman’s Notes

[To be completed]

# 3 Discussion

R3-206763 presents the need to add two new cause values, listed as follows:

|  |  |
| --- | --- |
| Radio Network Layer cause | Meaning |
| Insufficient UE Capabilities | The procedure can’t proceed due to insufficient UE capabilities. |
| Normal Release | The release is due to normal reasons. |

The first cause value “Insufficient UE Capabilities” is needed for those cases where a UE cannot be served by a node due to the fact that the node capabilities and the UE capabilities are not compatible.

A typical example is the one of EN-DC. We describe this case with an example.

A UE supports Frequency Band 1 for LTE and Frequency Band 2 and 3 for NR.

An MeNB supports Frequency Band 1 and serves the UE on such band. A potential SgNB PSCell supports Frequency Band 4 and 5.

The MeNB attempts to add the SgNB PSCell, but the SgNB will reject the addition because the UE capabilities (support for Band 2 and 3) do not match the PSCell capabilities (support for Band 4 and 5).

Note that the MeNB is not mandated to decode the NR capabilities of the UE and it cannot prevent the failure by avoiding to add the PSCell.

A similar scenario can be built for MR-DC in NG-RAN.

During online discussions it was questioned whether other cause values can be used to correctly express this failure. This option does not seem to exist. In fact, the failure in question would mean that the MeNB should never try to add the same PScell again for the same UE. On the contrary, if for example cause value “No Radio Resources Available” is used for the failure, the MeNB will understand that it is possible to re-try the PSCell addition at a later stage, when radio resource availability will improve.

**Conclusion: the purpose of introducing the “Insufficient UE Capabilities” cause value is that of triggering a behaviour in the receiving node for which it will not be attempted to connect the UE to the cell/node for which the failure occurred.**

**In light of the above companies are invited to provide their view on the introduction of the new cause value “Insufficient UE Capabilities” and if this is not believed needed, how can it be ensured that the node receiving the failure message derives a correct behaviour**

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | In order to ensure a correct node behaviour and avoid re-attempts of the UE connection with the cell for which the failure occurred, we support the introduction of the new cause value. |
|  |  |
|  |  |

The Normal Release cause value is already present over the F1AP, as reported below:

|  |  |
| --- | --- |
| Normal Release | The action is due to a normal release of the UE (e.g. because of mobility) and does not indicate an error. |

However, this cause value is not present over the Xn and X2 interfaces. In order to be able to communicate over the Xn and X2 that a release is not due to any issue, but due to a normal release condition, it is suggested to introduce the Normal Release cause also in the Xn and X2 protocols.

**In light of the above companies are invited to provide their view on the introduction of the new cause value “Normal Release” over the Xn and X2 interfaces**

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | We support the introduction of this cause value |
|  |  |
|  |  |

# 4 Conclusion, Recommendations [if needed]

If needed