**3GPP TSG-RAN WG3 Meeting #112-e *R3-212845***

**E-meeting, 17-28 May 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.463** | **CR** | **0598** | **rev** | **1** | **Current version:** | 16.5.0 |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction for UL Data Notification over E1 |
|  |  |
| ***Source to WG:*** | Huawei, Intel Corporation, CATT, China Telecom |
| ***Source to TSG:*** | RAN3 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2021-05-01 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The UL DATA NOTIFICATION procedure is described as follows. * This procedure is initiated by the gNB-CU-UP to notify the gNB-CU-CP that an UL packet including a QFI value in the SDAP header not configured by the *Flow Mapping Information* IE is received for the first time at the default DRB. The procedure uses UE-associated signalling.

But here only the *Flow Mapping Information* IE, which is included in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, is mentioned. This means, the UL DATA NOTIFICATION can only be applied to the DRB modify case, but not DRB setup case for the default DRB. In addtion, the *QoS Flows Information To Be Setup* IE is mandatorily included for DRB setup in the Bearer Context Setup/Modification procedure. However, as described in TS 38.300 Annex A.6, there are cases where the NG-RAN may decide not to configure the mapping rule for certain QoS flows immediately when establishing PDU sessions, but decide the mapping rule only when it receives the UL data flows from the UE over the default DRB. That is, over E1, there may be the case where CU-CP does not configure mapping rule for the default DRB during PDU session establishment.  |
|  |  |
| ***Summary of change:*** | 1. Update the text description for the UL Data Notification procedure to include the case of the QoS Flows Information To Be Setup IE.
2. Introduce a new IE to ignore the mapping rule of the *QoS Flows Information To Be Setup* IE for the default DRB

 Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has isolated impact with the previous version of the specification (same release) because it impacts on the UL DATA NOTIFICATION procedure for the default DRB. The impact can be considered isolated. |
|  |  |
| ***Consequences if not approved:*** | The UL Data Notification can not be used by the CU-UP to notify the arrival for those QoS flows at DRB setup phase. The procedure specified in TS 38.300 Annex A.6 can not be fully supported by E1AP.  |
|  |  |
| ***Clauses affected:*** | 8.3.1, 8.3.2, 8.3.10, 9.3.3.2, 9.3.3.10, 9.3.3.11, 9.4.5, 9.4.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev0: R3-211995Rev1: R3-212845 Update the cover page.Update the criticality of Ignore Mapping Rule Indication as reject.  |

### 8.3.1 Bearer Context Setup

#### 8.3.1.1 General

The purpose of the Bearer Context Setup procedure is to allow the gNB-CU-CP to establish a bearer context in the gNB-CU-UP. The procedure uses UE-associated signalling.

#### 8.3.1.2 Successful Operation



Figure 8.3.1.2-1: Bearer Context Setup procedure: Successful Operation.

**<Unchanged Text Omitted>**

If the *DRB QoS* IE is contained within the *DRB To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall, if supported, take it into account as specified in TS 28.552 [22].

If the *gNB-DU-ID* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall store the information received.

If the *RAN UE ID* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall store the information received.

For each successfully established DRB, the gNB-CU-UP shall provide, in the respective *UL UP Parameters* IE of the BEARER CONTEXT SETUP RESPONSE, one UL UP Transport Layer Information Item per cell group entry contained in the respective *Cell Group Information* IE of the BEARER CONTEXT SETUP REQUEST message.

If the *Ignore Mapping Rule Indication* IE is contained within the *DRB To Setup List* IE for a DRB in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall, if supported, ignore the QoS flow mapping information indicated by the *QoS Flows Information To Be Setup* IE for the concerned DRB.

**<Unchanged Text Omitted>**

### 8.3.2 Bearer Context Modification (gNB-CU-CP initiated)

#### 8.3.2.1 General

The purpose of the Bearer Context Modification procedure is to allow the gNB-CU-CP to modify a bearer context in the gNB-CU-UP. The procedure uses UE-associated signalling.

#### 8.3.2.2 Successful Operation



Figure 8.3.2.2-1: Bearer Context Modification procedure: Successful Operation.

**<Unchanged Text Omitted>**

If the *DRB QoS* IE is contained within the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, replace any previously received value and take it into account for each DRB, as specifed in TS 28.552 [22].

If the *gNB-DU-ID* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store and replace any previous information received.

If the *RAN UE ID* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store and replace any previous information received.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message including *Activity Notification Level* IE and its value does not match the current bearer context, the gNB-CU-UP shall ignore the *Activity Notification Level* IE and also the requested modification of inactivity timer.

For each successfully established DRB, the gNB-CU-UP shall provide, in the respective *UL UP Parameters* IE of the BEARER CONTEXT MODIFICATION RESPONSE, one UL UP Transport Layer Information Item per cell group entry contained in the respective *Cell Group Information* IE of the BEARER CONTEXT MODIFICATION REQUEST message.

If the *Old QoS Flow List - UL End Marker expected* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message for a DRB to be modified, the gNB-CU-UP shall consider that the source NG-RAN node has initiated QoS flow re-mapping and has not yet received SDAP end markers, as described in TS 38.300 [8]. The gNB-CU-UP shall consider that the *Old QoS Flow List - UL End Marker expected* IE only contains UL QoS flow information for QoS flows for which no SDAP end marker has been yet received on the source side.

If the *Ignore Mapping Rule Indication* IE is contained within the *DRB To Setup List* IE for a DRB in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, ignore the QoS flow mapping information indicated by the *QoS Flows Information To Be Setup* IE for the concerned DRB.

**<Unchanged Text Omitted>**

### 8.3.10 UL Data Notification

#### 8.3.10.1 General

This procedure is initiated by the gNB-CU-UP to notify the gNB-CU-CP that an UL packet including a QFI value in the SDAP header not configured by the *QoS Flows Information To Be Setup* IE or the *Flow Mapping Information* IE is received for the first time at the default DRB. The procedure uses UE-associated signalling.

#### 8.3.10.2 Successful Operation



Figure 8.3.10.2-1: UL Data Notification procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the UL DATA NOTIFICATION message to the gNB-CU-CP.

#### 8.3.10.3 Abnormal Conditions

Not applicable.

**<Unchanged Text Omitted>**

#### 9.3.3.2 PDU Session Resource To Setup List

This IE contains PDU session resource related information used at Bearer Context Setup Request

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **PDU Session Resource To Setup Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID  | M |  | 9.3.1.21 |  | - | - |
| >PDU Session Type  | M |  | 9.3.1.22 |  | - | - |
| >S-NSSAI  | M |  | 9.3.1.9 |  | - | - |
| >Security Indication  | M |  | 9.3.1.23 |  | - | - |
| >PDU Session Resource DL Aggregate Maximum Bit Rate | O |  | Bit Rate9.3.1.20 | This IE shall be present when at least one Non-GBR QoS Flows is being setup. | - | - |
| >NG UL UP Transport Layer Information | M |  | UP Transport Layer Information9.3.2.1 |  | - | - |
| >PDU Session Data Forwarding Information Request | O |  | Data Forwarding Information Request 9.3.2.5 |  | - | - |
| >PDU Session Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to PDU Session. | - | - |
| >Existing Allocated NG DL UP Transport Layer Information | O |  | UP Transport Layer Information9.3.2.1 |  | - | - |
| >Network Instance | O |  | 9.3.1.62 | This IE is ignored if the *Common Network Instance* IE is included. | YES | ignore |
| >Common Network Instance | O |  | 9.3.1.66 |  | YES | ignore |
| **>DRB To Setup List** |  | *1* |  |  | - | - |
| **>>DRB To Setup Item**  |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | M  |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | M |  | 9.3.1.38 |  | - | - |
| >>>Cell Group Information | M |  | 9.3.1.11 |  | - | - |
| >>>QoS Flows Information To Be Setup | M |  | QoS Flow QoS Parameters List9.3.1.25 |  | - | - |
| >>>DRB Data forwarding information Request | O |  | Data Forwarding Information Request 9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Contains the PDCP SN Status at setup after Resume. | - | - |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB. | YES | ignore |
| >>>DAPS Request Information | O |  | 9.3.1.91 |  | YES | ignore |
| >>>Ignore Mapping Rule Indication | O |  | ENUMERATED (True, …) | Included if the QoS flow mapping rule for the DRB has not been decided by gNB-CU-CP. | YES | reject |
| >Redundant NG UL UP Transport Layer Information | O |  | UP Transport Layer Information9.3.2.1 |  | YES | Ignore |
| >Redundant Common Network Instance | O |  | Common Network Instance9.3.1.66 |  | YES | ignore |
| >Redundant PDU Session Information | O |  | 9.3.1.80 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource  | Maximum no. of PDU Sessions for a UE. Value is 256. |

**<Unchanged Text Omitted>**

#### 9.3.3.10 PDU Session Resource To Setup Modification List

This IE contains PDU session resource to setup related information used at Bearer Context Modification Request

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **PDU Session Resource To Setup Modification Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID  | M |  | 9.3.1.21 |  | - | - |
| >PDU Session Type  | M |  | 9.3.1.22 |  | - | - |
| >S-NSSAI  | M |  | 9.3.1.9 |  | - | - |
| >Security Indication  | M |  | 9.3.1.23 |  | - | - |
| >PDU Session Resource DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 | This IE shall be present when Non-GBR QoS Flows are setting up. | - | - |
| >NG UL UP Transport Layer Information | M |  | UP Transport Layer Information9.3.2.1 |  | - | - |
| >PDU Session Data Forwarding Information Request | O |  | Data Forwarding Information Request 9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. | - | - |
| >PDU Session Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to PDU Session. | - | - |
| >Network Instance | O |  | 9.3.1.62 |  | - | - |
| >Common Network Instance | O |  | 9.3.1.66 |  | YES | ignore |
| **>DRB To Setup List** |  | *1* |  |  | - | - |
| **>>DRB To Setup Item**  |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | M  |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | M |  | 9.3.1.38 |  | - | - |
| >>>Cell Group Information | M |  | 9.3.1.11 |  | - | - |
| >>>QoS Flows Information To Be Setup | M |  | QoS Flow QoS Parameters List9.3.1.25 |  | - | - |
| >>>DRB Data forwarding information Request | O |  | Data Forwarding Information Request 9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status at setup after Resume to the target gNB-CU-UP. | - | - |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB | YES | ignore |
| >>>Ignore Mapping Rule Indication | O |  | ENUMERATED (True, …) | Included if the QoS flow mapping rule for the DRB has not been decided by gNB-CU-CP. | YES | reject |
| >Redundant NG UL UP Transport Layer Information | O |  | UP Transport Layer Information9.3.2.1 |  | YES | ignore |
| >Redundant Common Network Instance | O |  | Common Network Instance9.3.1.66 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource  | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.11 PDU Session Resource To Modify List

This IE contains PDU session resource to modify related information used at Bearer Context Modification Request

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **PDU Session Resource To Modify Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID  | M |  | 9.3.1.21 |  | - | - |
| >Security Indication  | O |  | 9.3.1.23 | This IE is not used in this release. | - | - |
| >PDU Session Resource DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 |  | - | - |
| >NG UL UP Transport Layer Information | O |  | UP Transport Layer Information9.3.2.1 |  | - | - |
| >PDU Session Data Forwarding Information Request | O |  | Data Forwarding Information Request 9.3.2.5 | Requesting forwarding information from the target gNB-CU-UP. | - | - |
| >PDU Session Data Forwarding Information | O |  | Data Forwarding Information 9.3.2.6 | Providing forwarding information to the source gNB-CU-UP. | - | - |
| >PDU Session Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to PDU Session. | - | - |
| >Network Instance | O |  | 9.3.1.62 | This IE is ignored if the *Common Network Instance* IE is included. | YES | ignore |
| >Common Network Instance | O |  | 9.3.1.66 |  | YES | ignore |
| **>DRB To Setup List** |  | *0..1* |  |  | - | - |
| **>>DRB To Setup Item**  |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | M |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | M |  | 9.3.1.38 |  | - | - |
| >>>Cell Group Information | M |  | 9.3.1.11 |  | - | - |
| >>>QoS Flow Information To Be Setup  | M |  | QoS Flow QoS Parameters List9.3.1.25 |  | - | - |
| >>>DRB Data Forwarding Information Request | O |  | Data Forwarding Information Request 9.3.2.5 | Requesting forwarding information from the target gNB-CU-UP. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status at setup after Resume to the target gNB-CU-UP. | - | - |
| >>>DRB QoS  | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB  | YES | ignore |
| >>>Ignore Mapping Rule Indication | O |  | ENUMERATED (True, …) | Included if the QoS flow mapping rule for the DRB has not been decided by gNB-CU-CP. | YES | reject |
| **>DRB To Modify List** |  | *0.. 1* |  |  | - | - |
| **>>DRB To Modify Item**  |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID  | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | O |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration  | O |  | 9.3.1.38 |  | - | - |
| >>>DRB Data forwarding information | O |  | Data Forwarding Information 9.3.2.6 | Providing forwarding information to the source gNB-CU-UP. | - | - |
| >>>PDCP SN Status Request | O |  | ENUMERATED (requested, …) | The gNB-CU-CP requests the gNB-CU-UP to provide the PDCP SN Status in the response message. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status to the target gNB-CU-UP. | - | - |
| >>>DL UP Parameters | O |  | UP Parameters 9.3.1.13 |  | - | - |
| >>>Cell Group To Add | O |  | Cell Group Information 9.3.1.11 |  | - | - |
| >>>Cell Group To Modify  | O |  | Cell Group Information 9.3.1.11 |  | - | - |
| >>>Cell Group To Remove  | O |  | Cell Group Information 9.3.1.11 |  | - | - |
| >>>Flow Mapping Information  | O |  | QoS Flow QoS Parameters List9.3.1.25 | Overrides previous mapping information.  | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>Old QoS Flow List - UL End Marker expected | O |  | QoS Flow List9.3.1.12 | Indicates that the source NG-RAN node has initiated QoS flow re-mapping and has not yet received SDAP end markers, as described in TS 38.300 [8]. | YES | reject |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB | YES | ignore |
| >>>Early Forwarding COUNT Request | O |  | ENUMERATED (First DL count, DL discarding, …) | Requests early data forwarding information from the source gNB-CU-UP | YES | reject |
| >>>Early Forwarding COUNT Information | O |  | 9.3.1.92 | Provides early data forwarding information to the target gNB-CU-UP. | YES | reject |
| **>DRB To Remove List** |  | *0.. 1* |  |  | - | - |
| **>>DRB To Remove Item**  |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID  | M |  | 9.3.1.16 |  | - | - |
| >S-NSSAI | O |  | 9.3.1.9 |  | YES | reject |
| >Redundant NG UL UP Transport Layer Information | O |  | UP Transport Layer Information9.3.2.1 |  | YES | ignore |
| >Redundant Common Network Instance | O |  | Common Network Instance9.3.1.66 |  | YES | ignore |
| **>Data Forwarding to E-UTRAN Information List** |  | *0.. 1* |  | Contains a list of DL Data Forwarding tunnels and the associated QoS Flows to be forwarded on each tunnel | YES | ignore |
| **>>Data Forwarding to E-UTRAN Information List Item** |  | *1..<maxnoofDataForwardingTunneltoE-UTRAN>* |  |  | - | - |
| >>>Data forwarding tunnel information | M |  | UP Transport Layer Information 9.3.2.1 |  | - | - |
| >>>QoS Flows to be forwarded List |  | *1* |  |   | - | - |
| >>>>QoS Flows to be forwarded Item |  | *1..<maxnoofQoSflows>* |  |  | - | - |
| >>>>>QoS Flow Identifier | M |  | QoS Flow Identifier9.3.1.24 |  | - | - |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource  | Maximum no. of PDU Sessions for a UE. Value is 256. |
| maxnoofDataForwardingTunneltoE-UTRAN | Maximum no. of Data Forwarding Tunnels to E-UTRAN for a UE. Value is 256. |
| maxnoofQoSflows | Maximum no. of QoS flows in a PDU Session. Value is 64. |

**<Unchanged Text Omitted>**

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

**<Unchanged Text Omitted>**

 id-EarlyForwardingCOUNTReq,

 id-EarlyForwardingCOUNTInfo,

 id-AlternativeQoSParaSetList,

 id-MCG-OfferedGBRQoSFlowInfo,

 id-Number-of-tunnels,

 id-DataForwardingtoE-UTRANInformationList,

 id-ignoreMappingRuleIndication,

**<Unchanged Text Omitted>**

DRB-To-Setup-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Setup-Item-NG-RAN

DRB-To-Setup-Item-NG-RAN ::= SEQUENCE {

 dRB-ID DRB-ID,

 sDAP-Configuration SDAP-Configuration,

 pDCP-Configuration PDCP-Configuration,

 cell-Group-Information Cell-Group-Information,

 qos-flow-Information-To-Be-Setup QoS-Flow-QoS-Parameter-List,

 dRB-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

 dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

 pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { DRB-To-Setup-Item-NG-RAN-ExtIEs } } OPTIONAL,

 ...

}

DRB-To-Setup-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 {ID id-DRB-QoS CRITICALITY ignore EXTENSION QoSFlowLevelQoSParameters PRESENCE optional}|

 {ID id-DAPSRequestInfo CRITICALITY ignore EXTENSION DAPSRequestInfo PRESENCE optional}|

 {ID id-ignoreMappingRuleIndication CRITICALITY reject EXTENSION IgnoreMappingRuleIndication PRESENCE optional},

 ...

}

DRB-To-Setup-Mod-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Setup-Mod-Item-NG-RAN

DRB-To-Setup-Mod-Item-NG-RAN ::= SEQUENCE {

 dRB-ID DRB-ID,

 sDAP-Configuration SDAP-Configuration,

 pDCP-Configuration PDCP-Configuration,

 cell-Group-Information Cell-Group-Information,

 flow-Mapping-Information QoS-Flow-QoS-Parameter-List,

 dRB-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

 dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

 pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { { DRB-To-Setup-Mod-Item-NG-RAN-ExtIEs } } OPTIONAL,

 ...

}

DRB-To-Setup-Mod-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 {ID id-DRB-QoS CRITICALITY ignore EXTENSION QoSFlowLevelQoSParameters PRESENCE optional}|

 {ID id-ignoreMappingRuleIndication CRITICALITY reject EXTENSION IgnoreMappingRuleIndication PRESENCE optional},

 ...

}

**<Unchanged Text Omitted>**

IgnoreMappingRuleIndication ::= ENUMERATED {

 true,

 ...

}

**<Unchanged Text Omitted>**

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**<Unchanged Text Omitted>**

id-QosMonitoringReportingFrequency ProtocolIE-ID ::= 132

id-QoSMonitoringDisabled ProtocolIE-ID ::= 133

id-ignoreMappingRuleIndication ProtocolIE-ID ::= aaa

END

-- ASN1STOP

**<Unchanged Text Omitted>**