3GPP TSG-RAN WG3 #114-e R3-21xxxx

**E-meeting, 1st – 11th November 2021**

Source: CATT

Title: (TP for BL CR for TS 38.300) On country policy handling

Agenda Item: 20.2.5

Document for: Approval

# Introduction

The TP is to capture the agreement of CB: # 2005\_NTN\_Country\_Routing.

# TP for BL CR for TS 38.300

/////////////////////////////////////////////////////////////////////// Begin of change /////////////////////////////////////////////////////////////////

16.x.x RAN (Re)Selection of CN Entity

The NG-RAN node implements the NAS Node Selection Function specified in TS 38.410 [16].

For a RRC\_CONNECTED UE, when the NG-RAN node is configured to ensure that the UE is using an AMF that serves the country in which the UE is located.

If the NG-RAN node detects that the UE is in a different country to that served by the serving AMF, it should

* perform an NG handover to change to an appropriate AMF, or
* initiate an *UE Context Release Request* procedure towards the serving AMF with a suitable cause value (e.g. if mobility towards an appropriate target AMF cannot be initiated).

NOTE: The AMF may decide to trigger UE context release if it determines that the serving PLMN is not allowed to serve the UE in its current location.

/////////////////////////////////////////////////////////////////////// End of Change ///////////////////////////////////////////////////////////////////////