3GPP TSG-RAN WG3 #114-e R3-21xxxx

**E-meeting, 1st – 11th November 2021**

Source: CATT

Title: (TP for BL CR for TS 38.300) On country policy handling

Agenda Item: 20.2.5

Document for: Approval

# Introduction

The TP is to capture the agreement of CB: # 2005\_NTN\_Country\_Routing.

# TP for BL CR for TS 38.300 (on top of R3-214663)

/////////////////////////////////////////////////////////////////////// Begin of change /////////////////////////////////////////////////////////////////

16.x.6 AMF (Re-)Selection by gNB

The gNB implements the NAS Node Selection Function specified in TS 38.410 [16].

For a RRC\_CONNECTED UE, when the gNB is configured to ensure that the UE is using an AMF that serves the country in which the UE is located.

If the gNB detects that the UE is in a different country to that served by the serving AMF, it should

* perform an NG handover to change to an appropriate AMF, or
* initiate an *UE Context Release Request* procedure towards the serving AMF with a suitable cause value (e.g. if mobility towards an appropriate target AMF cannot be initiated).

NOTE: The AMF may decide to trigger UE context release if it determines that the serving PLMN is not allowed to serve the UE in its current location.

/////////////////////////////////////////////////////////////////////// End of Change ///////////////////////////////////////////////////////////////////////