|  |  |
| --- | --- |
|  |  |

**3GPP T****SG-RAN WG3 Meeting #114-e R3-216074**

**1 – 11 November 2021**

**Online**

**Agenda Item: 30.4**

**Source: Huawei, Telecom Italia**

**Title: (TP for BL CR TS 38.401) Use of node ID in eNB**

**Document for: Other**

1 Introduction

This TP captures the agreement of CB: # 61\_eNBarchEvo

Annex: TP for TS 38.401

### 6.2.4 gNB-CU-UP ID

The gNB-CU-UP ID is configured at the gNB-CU-CP and used to uniquely identify the gNB-CU-UP at least within a gNB-CU-CP. The gNB-CU-UP provides its gNB-CU-UP ID to the gNB-CU-CP during the E1 Setup procedure. The gNB-CP-UP ID is used only within E1AP procedures.

NOTE 1: This identity is also used to uniquely identify the ng-eNB-CU-UP at least within an ng-eNB-CU-CP in case CP/UP separation is implemented in ng-eNB,.

NOTE 2: This identity is also used to uniquely identify the eNB at least within an eNB-CP in case CP/UP separation is implemented in eNB.