**3GPP TSG-RAN WG3 Meeting #116-e *R3-223977***

**E-meeting, 09 May – 19 May 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.473** | **CR** | **0902** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Lenovo | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_ENDC\_SON\_MDT\_enh-Core | | | | |  | ***Date:*** | | | 2022-05-09 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Semantics description for *Successful HO Report Container* IE in ACCESS AND MOBILITY INDICATION message is missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add semantics description for *Successful HO Report Container* IE in ACCESS AND MOBILITY INDICATION message.  Impact Analysis:  Impact assessment towards the previous version of the specification (same release):  This CR has isolated impact with the previous version of the specification (same release) because it only impact SHR feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | How to understand *Successful HO Report Container* IE in ACCESS AND MOBILITY INDICATION message is not clear. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.2.10.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Rev 1: Removal of issues solved in other CRs and update the cover page | | | | | | | | |

9.2.10.1 ACCESS AND MOBILITY INDICATION

This message is sent by gNB-CU to gNB-DU to provide access and mobility information to the gNB-DU.

Direction: gNB-CU → gNB-DU.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| Transaction ID | M |  | 9.3.1.23 |  | YES | reject |
| **RACH Report Information List** |  | *0..1* |  |  | YES | ignore |
| **>RACH Report Information Item** |  | *1 .. <maxnoofRACHReports>* |  |  | - |  |
| >>RACH Report Container | M |  | OCTET STRING | *RA-ReportList-r16* IE as defined in subclause 6.2.2 in TS 38.331 [8]. | - |  |
| >>UE Assistant Identifier | O |  | gNB-DU UE F1AP ID  9.3.1.5 |  | - |  |
| **RLF Report Information List** |  | *0..1* |  |  | YES | ignore |
| **>RLF Report Information Item** |  | *1 .. <maxnoofRLFReports>* |  |  | - |  |
| >>NR UE RLF Report Container | M |  | OCTET STRING | *nr-RLF-Report-r16* IE contained in the *UEInformationResponse* message defined in TS 38.331 [8]. | - |  |
| >>UE Assistant Identifier | O |  | gNB-DU UE F1AP ID  9.3.1.5 |  | - |  |
| **Successful HO Report Information List** |  | *0..1* |  |  | YES | ignore |
| **>Successful HO Report Information Item** |  | *1 .. <maxnoofSuccessfulHOReports>* |  |  | - |  |
| >>Successful HO Report Container | M |  | OCTET STRING | *SuccessHO-Report-r17* IE as defined in subclause 6.2.2 in TS 38.331 [8]. | - |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofRACHReports | Maximum no. of RACH Reports, the maximum value is 64. |
| maxnoofRLFReports | Maximum no. of RLF Reports, the maximum value is 64. |
| maxnoofSuccessfulHOReports | Maximum no. of Successful HO Reports, the maximum value is 64. |