**3GPP TSG RAN3 meeting #117-e R3-225992**

**E-meeting, 10th – 18th Oct. 2022**

**Title:** **[draft]** LS for the signaling based logged MDT override protection

**Release:** Rel-18

**Work Item:** NR\_ENDC\_SON\_MDT\_enh2-Core

**Source:** CATT [to be RAN3]

**To:** RAN2

**Cc:**

**Contact Person:**

**Name: Jiaying Sun**

**E-mail Address:** **sunjiaying (at) catt (dot) cn**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** -

1. **Overall Description:**

The WI in REL-18 for signalling based logged MDT override protection is as follows:

- Support of signalling based logged MDT override protection to address the scenario where the signalling based MDT is configured in E-UTRAN when [RAN2, RAN3]:

- UE reselects to NR while logged measurements are collected

- UE reselects to NR after logged measurements are collected and before uploading the logged MDT report.

Based on the “E-UTRAN” in the WI, RAN3 understands that signaling based logged MDT override protection for only inter-system inter-RAT scenario is defined in the scope of WID. We want to check whether RAN2 will only define solution for the inter-system inter–RAT scenario. What more, if RAN2 defines a generic solution that also applies for intra-system inter- RAT, then the scope can be clarified in stage-2 specifications

**2. Actions:**

**To RAN2**

**ACTION:** RAN3 kindly asks RAN2 take the above information into consideration and feedback if needed.

**3. Date of Next TSG-RAN WG3 Meetings:**

TSG-RAN3 Meeting #118 14th Nov - 18th Nov 2022