**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The gNB-CU-UP UE ID is mandatory in the RESOURCE STATUS UPDATE message, but optional in the ASN.1. The correct is the tabular definition – for an UE-associated signalling both IDs shall always be included.  On the other hand, the HW Capacity information is optional in tabular definition of the message, while mandatory in ASN.1 – again, the tabular definition is correct definition considering intented functionality (the HW Capacity can be explicitly requested, so possibly may not be needed to be signalled). | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | A non-bakward compatible correction of the ASN.1 is too invasive for a Rel-16 CR. Therefore, it is proposed to correct the tabular definition. To provide the designed functionality, following additional changes are needed:   * The inclusion of the UE ID is to be mandated with a procedural text. * An additional flag is added to enable the CU-UP to declare the HW Capacity is to be ignored.   Impact assessment towards the previous version of the specification (same release):  The impact can be considered isolated because the change only aligns the tabular to the ASN.1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Discrepancy between the tabular and the ASN.1 definitions remains. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.2.10.4, 9.2.1.22, ASN.1 (9.4.4, 9.4.5, 9.4.7) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 38.463 CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This Cat. A CR to TS 37.483 is a mirror CR of previous release of TS 38.463.  No Rel-17 CR to TS 38.463 is needed as TS 38.463 Rel-17 is an empty pointer specification to TS 37.483. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First change, ommited text not changed** |

### 8.2.10 Resource Status Reporting

#### 8.2.10.1 General

This procedure is initiated by gNB-CU-UP to report the result of measurements admitted by gNB-CU-UP following a successful Resource Status Reporting Initiation procedure.

The procedure uses non UE-associated signalling.

#### 8.2.10.2 Successful Operation



Figure 8.2.10.2-1: Resource Status Reporting, successful operation

The gNB-CU-UP shall report the results of the admitted measurements in RESOURCE STATUS UPDATE message. The admitted measurements are the measurements that were successfully initiated during the preceding Resource Status Reporting Initiation procedure.

The gNB-CU-UP shall include the *gNB-CU-UP Measurement ID* IE in the RESOURCE STATUS UPDATE message.

If the *HW-CapacityIndicator-relevance* IE is included in the RESOURCE STATUS UPDATE message, the gNB-CU-CP shall ignore the information provided in the *HW Capacity Indicator* IE.

#### 8.2.10.3 Unsuccessful Operation

Not applicable.

#### 8.2.10.4 Abnormal Conditions

Void.

|  |
| --- |
| **Next change, ommited text not changed** |

#### 9.2.1.22 RESOURCE STATUS UPDATE

This message is sent by gNB-CU-UP to gNB-CU-CP to report the results of the requested measurements.

Direction: gNB-CU-UP → gNB-CU-CP.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality | |
| Message Type | M |  | 9.3.1.1 |  | YES | Ignore | |
| Transaction ID | M |  | 9.3.1.53 |  | YES | Reject | |
| gNB-CU-CP Measurement ID | M |  | INTEGER (1..4095,...) | Allocated by gNB-CU-CP | YES | Reject |
| gNB-CU-UP Measurement ID | O |  | INTEGER (1..4095,...) | Allocated by gNB-CU-UP | YES | Reject |
| TNL Available Capacity Indicator | O |  | 9.3.1.72 |  | YES | Ignore |
| HW Capacity Indicator | M |  | 9.3.1.73 |  | YES | Ignore |
| HW Capacity Indicator Relevance | O |  | ENUMERATED (ignore-hw-capacity, ...) |  | YES | Ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofSPLMNs | Maximum no. of Supported PLMN Ids. Value is 12. |
| maxnoofSliceItems | Maximum no. of signalled slice support items. Value is 1024. |

|  |
| --- |
| **Next change, ommited text not changed** |

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for E1AP

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Cause,

CriticalityDiagnostics,

GNB-CU-CP-MBS-E1AP-ID,

GNB-CU-UP-MBS-E1AP-ID,

GNB-CU-CP-UE-E1AP-ID,

GNB-CU-UP-UE-E1AP-ID,

UE-associatedLogicalE1-ConnectionItem,

GNB-CU-UP-ID,

GNB-CU-UP-Name,

Extended-GNB-CU-UP-Name,

GNB-CU-CP-Name,

Extended-GNB-CU-CP-Name,

CNSupport,

PLMN-Identity,

Slice-Support-List,

NR-CGI-Support-List,

QoS-Parameters-Support-List,

SecurityInformation,

BitRate,

BearerContextStatusChange,

DRB-To-Setup-List-EUTRAN,

DRB-Setup-List-EUTRAN,

DRB-Failed-List-EUTRAN,

DRB-To-Modify-List-EUTRAN,

DRB-Measurement-Results-Information-List,

DRB-Modified-List-EUTRAN,

DRB-Failed-To-Modify-List-EUTRAN,

DRB-To-Remove-List-EUTRAN,

DRB-Required-To-Remove-List-EUTRAN,

DRB-Required-To-Modify-List-EUTRAN,

DRB-Confirm-Modified-List-EUTRAN,

DRB-To-Setup-Mod-List-EUTRAN,

DRB-Setup-Mod-List-EUTRAN,

DRB-Failed-Mod-List-EUTRAN,

ExtendedSliceSupportList,

PDU-Session-Resource-To-Setup-List,

PDU-Session-Resource-Setup-List,

PDU-Session-Resource-Failed-List,

PDU-Session-Resource-To-Modify-List,

PDU-Session-Resource-Modified-List,

PDU-Session-Resource-Failed-To-Modify-List,

PDU-Session-Resource-To-Remove-List,

PDU-Session-Resource-Required-To-Modify-List,

PDU-Session-Resource-Confirm-Modified-List,

PDU-Session-Resource-To-Setup-Mod-List,

PDU-Session-Resource-Setup-Mod-List,

PDU-Session-Resource-Failed-Mod-List,

PDU-Session-To-Notify-List,

DRB-Status-Item,

DRB-Activity-Item,

Data-Usage-Report-List,

TimeToWait,

ActivityNotificationLevel,

ActivityInformation,

New-UL-TNL-Information-Required,

GNB-CU-CP-TNLA-Setup-Item,

GNB-CU-CP-TNLA-Failed-To-Setup-Item,

GNB-CU-CP-TNLA-To-Add-Item,

GNB-CU-CP-TNLA-To-Remove-Item,

GNB-CU-CP-TNLA-To-Update-Item,

GNB-CU-UP-TNLA-To-Remove-Item,

TransactionID,

Inactivity-Timer,

DRBs-Subject-To-Counter-Check-List-EUTRAN,

DRBs-Subject-To-Counter-Check-List-NG-RAN,

PPI,

GNB-CU-UP-Capacity,

GNB-CU-UP-OverloadInformation,

DataDiscardRequired,

PDU-Session-Resource-Data-Usage-List,

RANUEID,

GNB-DU-ID,

TraceID,

TraceActivation,

SubscriberProfileIDforRFP,

AdditionalRRMPriorityIndex,

RetainabilityMeasurementsInfo,

Transport-Layer-Address-Info,

HW-CapacityIndicator,

RegistrationRequest,

ReportCharacteristics,

ReportingPeriodicity,

TNL-AvailableCapacityIndicator,

DLUPTNLAddressToUpdateItem,

ULUPTNLAddressToUpdateItem,

NPNContextInfo,

NPNSupportInfo,

MDTPLMNList,

PrivacyIndicator,

URIaddress,

DRBs-Subject-To-Early-Forwarding-List,

CHOInitiation,

ExtendedSliceSupportList,

TransportLayerAddress,

AdditionalHandoverInfo,

Extended-NR-CGI-Support-List,

DirectForwardingPathAvailability,

IAB-Donor-CU-UPPSKInfo-Item,

ECGI-Support-List,

MDTPollutedMeasurementIndicator,

UESliceMaximumBitRateList,

SCGActivationStatus,

GlobalMBSSessionID,

BCBearerContextToSetup,

BCBearerContextToSetupResponse,

BCBearerContextToModify,

BCBearerContextToModifyResponse,

BCBearerContextToModifyRequired,

BCBearerContextToModifyConfirm,

MCBearerContextToSetup,

MCBearerContextToSetupResponse,

MCBearerContextToModify,

MCBearerContextToModifyResponse,

MCBearerContextToModifyRequired,

MCBearerContextToModifyConfirm,

MBSMulticastF1UContextDescriptor,

GNB-CU-UP-MBS-Support-Info,

SDTContinueROHC,

MDTPLMNModificationList

FROM E1AP-IEs

PrivateIE-Container{},

ProtocolExtensionContainer{},

ProtocolIE-Container{},

ProtocolIE-ContainerList{},

ProtocolIE-SingleContainer{},

E1AP-PRIVATE-IES,

E1AP-PROTOCOL-EXTENSION,

E1AP-PROTOCOL-IES

FROM E1AP-Containers

id-Cause,

id-CriticalityDiagnostics,

id-gNB-CU-CP-UE-E1AP-ID,

id-gNB-CU-UP-UE-E1AP-ID,

id-ResetType,

id-UE-associatedLogicalE1-ConnectionItem,

id-UE-associatedLogicalE1-ConnectionListResAck,

id-gNB-CU-UP-ID,

id-gNB-CU-UP-Name,

id-Extended-GNB-CU-UP-Name,

id-gNB-CU-CP-Name,

id-Extended-GNB-CU-CP-Name,

id-CNSupport,

id-SupportedPLMNs,

id-NPNSupportInfo,

id-NPNContextInfo,

id-SecurityInformation,

id-UEDLAggregateMaximumBitRate,

id-BearerContextStatusChange,

id-System-BearerContextSetupRequest,

id-System-BearerContextSetupResponse,

id-System-BearerContextModificationRequest,

id-System-BearerContextModificationResponse,

id-System-BearerContextModificationConfirm,

id-System-BearerContextModificationRequired,

id-DRB-Status-List,

id-Data-Usage-Report-List,

id-TimeToWait,

id-ActivityNotificationLevel,

id-ActivityInformation,

id-New-UL-TNL-Information-Required,

id-GNB-CU-CP-TNLA-Setup-List,

id-GNB-CU-CP-TNLA-Failed-To-Setup-List,

id-GNB-CU-CP-TNLA-To-Add-List,

id-GNB-CU-CP-TNLA-To-Remove-List,

id-GNB-CU-CP-TNLA-To-Update-List,

id-GNB-CU-UP-TNLA-To-Remove-List,

id-DRB-To-Setup-List-EUTRAN,

id-DRB-To-Modify-List-EUTRAN,

id-DRB-To-Remove-List-EUTRAN,

id-DRB-Required-To-Modify-List-EUTRAN,

id-DRB-Required-To-Remove-List-EUTRAN,

id-DRB-Setup-List-EUTRAN,

id-DRB-Failed-List-EUTRAN,

id-DRB-Measurement-Results-Information-List,

id-DRB-Modified-List-EUTRAN,

id-DRB-Failed-To-Modify-List-EUTRAN,

id-DRB-Confirm-Modified-List-EUTRAN,

id-DRB-To-Setup-Mod-List-EUTRAN,

id-DRB-Setup-Mod-List-EUTRAN,

id-DRB-Failed-Mod-List-EUTRAN,

id-PDU-Session-Resource-To-Setup-List,

id-PDU-Session-Resource-To-Modify-List,

id-PDU-Session-Resource-To-Remove-List,

id-PDU-Session-Resource-Required-To-Modify-List,

id-PDU-Session-Resource-Setup-List,

id-PDU-Session-Resource-Failed-List,

id-PDU-Session-Resource-Modified-List,

id-PDU-Session-Resource-Failed-To-Modify-List,

id-PDU-Session-Resource-Confirm-Modified-List,

id-PDU-Session-Resource-Setup-Mod-List,

id-PDU-Session-Resource-Failed-Mod-List,

id-PDU-Session-Resource-To-Setup-Mod-List,

id-PDU-Session-To-Notify-List,

id-TransactionID,

id-Serving-PLMN,

id-UE-Inactivity-Timer,

id-System-GNB-CU-UP-CounterCheckRequest,

id-DRBs-Subject-To-Counter-Check-List-EUTRAN,

id-DRBs-Subject-To-Counter-Check-List-NG-RAN,

id-PPI,

id-gNB-CU-UP-Capacity,

id-GNB-CU-UP-OverloadInformation,

id-UEDLMaximumIntegrityProtectedDataRate,

id-DataDiscardRequired,

id-PDU-Session-Resource-Data-Usage-List,

id-RANUEID,

id-GNB-DU-ID,

id-TraceID,

id-TraceActivation,

id-SubscriberProfileIDforRFP,

id-AdditionalRRMPriorityIndex,

id-RetainabilityMeasurementsInfo,

id-Transport-Layer-Address-Info,

id-gNB-CU-CP-Measurement-ID,

id-gNB-CU-UP-Measurement-ID,

id-RegistrationRequest,

id-ReportCharacteristics,

id-ReportingPeriodicity,

id-TNL-AvailableCapacityIndicator,

id-HW-CapacityIndicator,

id-DLUPTNLAddressToUpdateList,

id-ULUPTNLAddressToUpdateList,

id-ManagementBasedMDTPLMNList,

id-TraceCollectionEntityIPAddress,

id-PrivacyIndicator,

id-URIaddress,

id-DRBs-Subject-To-Early-Forwarding-List,

id-CHOInitiation,

id-ExtendedSliceSupportList,

id-AdditionalHandoverInfo,

id-Extended-NR-CGI-Support-List,

id-DirectForwardingPathAvailability, id-IAB-Donor-CU-UPPSKInfo,

id-ECGI-Support-List,

id-MDTPollutedMeasurementIndicator,

id-UESliceMaximumBitRateList,

id-SCGActivationStatus,

id-GNB-CU-CP-MBS-E1AP-ID,

id-GNB-CU-UP-MBS-E1AP-ID,

id-GlobalMBSSessionID,

id-BCBearerContextToSetup,

id-BCBearerContextToSetupResponse,

id-BCBearerContextToModify,

id-BCBearerContextToModifyResponse,

id-BCBearerContextToModifyRequired,

id-BCBearerContextToModifyConfirm,

id-MCBearerContextToSetup,

id-MCBearerContextToSetupResponse,

id-MCBearerContextToModify,

id-MCBearerContextToModifyResponse,

id-MCBearerContextToModifyRequired,

id-MCBearerContextToModifyConfirm,

id-MBSMulticastF1UContextDescriptor,

id-gNB-CU-UP-MBS-Support-Info,

id-SDTContinueROHC,

id-ManagementBasedMDTPLMNModificationList,

id-HW-CapacityIndicator-relevance

maxnoofErrors,

maxnoofSPLMNs,

maxnoofDRBs,

maxnoofTNLAssociations,

maxnoofIndividualE1ConnectionsToReset,

maxnoofTNLAddresses,

maxnoofPSKs

FROM E1AP-Constants;

|  |
| --- |
| **Next change, ommited text not changed** |

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESOURCE STATUS UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResourceStatusUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { ResourceStatusUpdateIEs } },

...

}

ResourceStatusUpdateIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory}|

{ ID id-gNB-CU-CP-Measurement-ID CRITICALITY reject TYPE INTEGER (1..4095, ...) PRESENCE mandatory}|

{ ID id-gNB-CU-UP-Measurement-ID CRITICALITY ignore TYPE INTEGER (1..4095, ...) PRESENCE optional}|

{ ID id-TNL-AvailableCapacityIndicator CRITICALITY ignore TYPE TNL-AvailableCapacityIndicator PRESENCE optional}|

{ ID id-HW-CapacityIndicator CRITICALITY ignore TYPE HW-CapacityIndicator PRESENCE mandatory}|

{ ID id-HW-CapacityIndicator-relevance CRITICALITY ignore TYPE HW-CapacityIndicator-relevance PRESENCE optional},

...

}

|  |
| --- |
| **Ommited text not changed** |

### 9.4.5 Information Element Definitions

|  |
| --- |
| **Next change, ommited text not changed** |

HW-CapacityIndicator ::= SEQUENCE {

offeredThroughput INTEGER (1..16777216, ...),

availableThroughput INTEGER (0..100, ...),

iE-Extensions ProtocolExtensionContainer { { HW-CapacityIndicator-ExtIEs } },

...

}

HW-CapacityIndicator-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

HW-CapacityIndicator-relevance ::= ENUMERATED {ignore-hw-capacity, ...}

|  |
| --- |
| **Ommited text not changed** |

### 9.4.7 Constant Definitions

|  |
| --- |
| **Next change, ommited text not changed** |

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Cause ProtocolIE-ID ::= 0

id-CriticalityDiagnostics ProtocolIE-ID ::= 1

id-gNB-CU-CP-UE-E1AP-ID ProtocolIE-ID ::= 2

id-gNB-CU-UP-UE-E1AP-ID ProtocolIE-ID ::= 3

id-ResetType ProtocolIE-ID ::= 4

id-UE-associatedLogicalE1-ConnectionItem ProtocolIE-ID ::= 5

id-UE-associatedLogicalE1-ConnectionListResAck ProtocolIE-ID ::= 6

id-gNB-CU-UP-ID ProtocolIE-ID ::= 7

id-gNB-CU-UP-Name ProtocolIE-ID ::= 8

id-gNB-CU-CP-Name ProtocolIE-ID ::= 9

id-CNSupport ProtocolIE-ID ::= 10

id-SupportedPLMNs ProtocolIE-ID ::= 11

id-TimeToWait ProtocolIE-ID ::= 12

id-SecurityInformation ProtocolIE-ID ::= 13

id-UEDLAggregateMaximumBitRate ProtocolIE-ID ::= 14

id-System-BearerContextSetupRequest ProtocolIE-ID ::= 15

id-System-BearerContextSetupResponse ProtocolIE-ID ::= 16

id-BearerContextStatusChange ProtocolIE-ID ::= 17

id-System-BearerContextModificationRequest ProtocolIE-ID ::= 18

id-System-BearerContextModificationResponse ProtocolIE-ID ::= 19

id-System-BearerContextModificationConfirm ProtocolIE-ID ::= 20

id-System-BearerContextModificationRequired ProtocolIE-ID ::= 21

id-DRB-Status-List ProtocolIE-ID ::= 22

id-ActivityNotificationLevel ProtocolIE-ID ::= 23

id-ActivityInformation ProtocolIE-ID ::= 24

id-Data-Usage-Report-List ProtocolIE-ID ::= 25

id-New-UL-TNL-Information-Required ProtocolIE-ID ::= 26

id-GNB-CU-CP-TNLA-To-Add-List ProtocolIE-ID ::= 27

id-GNB-CU-CP-TNLA-To-Remove-List ProtocolIE-ID ::= 28

id-GNB-CU-CP-TNLA-To-Update-List ProtocolIE-ID ::= 29

id-GNB-CU-CP-TNLA-Setup-List ProtocolIE-ID ::= 30

id-GNB-CU-CP-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 31

id-DRB-To-Setup-List-EUTRAN ProtocolIE-ID ::= 32

id-DRB-To-Modify-List-EUTRAN ProtocolIE-ID ::= 33

id-DRB-To-Remove-List-EUTRAN ProtocolIE-ID ::= 34

id-DRB-Required-To-Modify-List-EUTRAN ProtocolIE-ID ::= 35

id-DRB-Required-To-Remove-List-EUTRAN ProtocolIE-ID ::= 36

id-DRB-Setup-List-EUTRAN ProtocolIE-ID ::= 37

id-DRB-Failed-List-EUTRAN ProtocolIE-ID ::= 38

id-DRB-Modified-List-EUTRAN ProtocolIE-ID ::= 39

id-DRB-Failed-To-Modify-List-EUTRAN ProtocolIE-ID ::= 40

id-DRB-Confirm-Modified-List-EUTRAN ProtocolIE-ID ::= 41

id-PDU-Session-Resource-To-Setup-List ProtocolIE-ID ::= 42

id-PDU-Session-Resource-To-Modify-List ProtocolIE-ID ::= 43

id-PDU-Session-Resource-To-Remove-List ProtocolIE-ID ::= 44

id-PDU-Session-Resource-Required-To-Modify-List ProtocolIE-ID ::= 45

id-PDU-Session-Resource-Setup-List ProtocolIE-ID ::= 46

id-PDU-Session-Resource-Failed-List ProtocolIE-ID ::= 47

id-PDU-Session-Resource-Modified-List ProtocolIE-ID ::= 48

id-PDU-Session-Resource-Failed-To-Modify-List ProtocolIE-ID ::= 49

id-PDU-Session-Resource-Confirm-Modified-List ProtocolIE-ID ::= 50

id-DRB-To-Setup-Mod-List-EUTRAN ProtocolIE-ID ::= 51

id-DRB-Setup-Mod-List-EUTRAN ProtocolIE-ID ::= 52

id-DRB-Failed-Mod-List-EUTRAN ProtocolIE-ID ::= 53

id-PDU-Session-Resource-Setup-Mod-List ProtocolIE-ID ::= 54

id-PDU-Session-Resource-Failed-Mod-List ProtocolIE-ID ::= 55

id-PDU-Session-Resource-To-Setup-Mod-List ProtocolIE-ID ::= 56

id-TransactionID ProtocolIE-ID ::= 57

id-Serving-PLMN ProtocolIE-ID ::= 58

id-UE-Inactivity-Timer ProtocolIE-ID ::= 59

id-System-GNB-CU-UP-CounterCheckRequest ProtocolIE-ID ::= 60

id-DRBs-Subject-To-Counter-Check-List-EUTRAN ProtocolIE-ID ::= 61

id-DRBs-Subject-To-Counter-Check-List-NG-RAN ProtocolIE-ID ::= 62

id-PPI ProtocolIE-ID ::= 63

id-gNB-CU-UP-Capacity ProtocolIE-ID ::= 64

id-GNB-CU-UP-OverloadInformation ProtocolIE-ID ::= 65

id-UEDLMaximumIntegrityProtectedDataRate ProtocolIE-ID ::= 66

id-PDU-Session-To-Notify-List ProtocolIE-ID ::= 67

id-PDU-Session-Resource-Data-Usage-List ProtocolIE-ID ::= 68

id-SNSSAI ProtocolIE-ID ::= 69

id-DataDiscardRequired ProtocolIE-ID ::= 70

id-OldQoSFlowMap-ULendmarkerexpected ProtocolIE-ID ::= 71

id-DRB-QoS ProtocolIE-ID ::= 72

id-GNB-CU-UP-TNLA-To-Remove-List ProtocolIE-ID ::= 73

id-endpoint-IP-Address-and-Port ProtocolIE-ID ::= 74

id-TNLAssociationTransportLayerAddressgNBCUUP ProtocolIE-ID ::= 75

id-RANUEID ProtocolIE-ID ::= 76

id-GNB-DU-ID ProtocolIE-ID ::= 77

id-CommonNetworkInstance ProtocolIE-ID ::= 78

id-NetworkInstance ProtocolIE-ID ::= 79

id-QoSFlowMappingIndication ProtocolIE-ID ::= 80

id-TraceActivation ProtocolIE-ID ::= 81

id-TraceID ProtocolIE-ID ::= 82

id-SubscriberProfileIDforRFP ProtocolIE-ID ::= 83

id-AdditionalRRMPriorityIndex ProtocolIE-ID ::= 84

id-RetainabilityMeasurementsInfo ProtocolIE-ID ::= 85

id-Transport-Layer-Address-Info ProtocolIE-ID ::= 86

id-QoSMonitoringRequest ProtocolIE-ID ::= 87

id-PDCP-StatusReportIndication ProtocolIE-ID ::= 88

id-gNB-CU-CP-Measurement-ID ProtocolIE-ID ::= 89

id-gNB-CU-UP-Measurement-ID ProtocolIE-ID ::= 90

id-RegistrationRequest ProtocolIE-ID ::= 91

id-ReportCharacteristics ProtocolIE-ID ::= 92

id-ReportingPeriodicity ProtocolIE-ID ::= 93

id-TNL-AvailableCapacityIndicator ProtocolIE-ID ::= 94

id-HW-CapacityIndicator ProtocolIE-ID ::= 95

id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 96

id-redundant-nG-UL-UP-TNL-Information ProtocolIE-ID ::= 97

id-redundant-nG-DL-UP-TNL-Information ProtocolIE-ID ::= 98

id-RedundantQosFlowIndicator ProtocolIE-ID ::= 99

id-TSCTrafficCharacteristics ProtocolIE-ID ::= 100

id-CNPacketDelayBudgetDownlink ProtocolIE-ID ::= 101

id-CNPacketDelayBudgetUplink ProtocolIE-ID ::= 102

id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 103

id-AdditionalPDCPduplicationInformation ProtocolIE-ID ::= 104

id-RedundantPDUSessionInformation ProtocolIE-ID ::= 105

id-RedundantPDUSessionInformation-used ProtocolIE-ID ::= 106

id-QoS-Mapping-Information ProtocolIE-ID ::= 107

id-DLUPTNLAddressToUpdateList ProtocolIE-ID ::= 108

id-ULUPTNLAddressToUpdateList ProtocolIE-ID ::= 109

id-NPNSupportInfo ProtocolIE-ID ::= 110

id-NPNContextInfo ProtocolIE-ID ::= 111

id-MDTConfiguration ProtocolIE-ID ::= 112

id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 113

id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 114

id-PrivacyIndicator ProtocolIE-ID ::= 115

id-TraceCollectionEntityURI ProtocolIE-ID ::= 116

id-URIaddress ProtocolIE-ID ::= 117

id-EHC-Parameters ProtocolIE-ID ::= 118

id-DRBs-Subject-To-Early-Forwarding-List ProtocolIE-ID ::= 119

id-DAPSRequestInfo ProtocolIE-ID ::= 120

id-CHOInitiation ProtocolIE-ID ::= 121

id-EarlyForwardingCOUNTReq ProtocolIE-ID ::= 122

id-EarlyForwardingCOUNTInfo ProtocolIE-ID ::= 123

id-AlternativeQoSParaSetList ProtocolIE-ID ::= 124

id-ExtendedSliceSupportList ProtocolIE-ID ::= 125

id-MCG-OfferedGBRQoSFlowInfo ProtocolIE-ID ::= 126

id-Number-of-tunnels ProtocolIE-ID ::= 127

id-DRB-Measurement-Results-Information-List ProtocolIE-ID ::= 128

id-Extended-GNB-CU-CP-Name ProtocolIE-ID ::= 129

id-Extended-GNB-CU-UP-Name ProtocolIE-ID ::= 130

id-DataForwardingtoE-UTRANInformationList ProtocolIE-ID ::= 131

id-QosMonitoringReportingFrequency ProtocolIE-ID ::= 132

id-QoSMonitoringDisabled ProtocolIE-ID ::= 133

id-AdditionalHandoverInfo ProtocolIE-ID ::= 134

id-Extended-NR-CGI-Support-List ProtocolIE-ID ::= 135

id-DataForwardingtoNG-RANQoSFlowInformationList ProtocolIE-ID ::= 136

id-MaxCIDEHCDL ProtocolIE-ID ::= 137

id-ignoreMappingRuleIndication ProtocolIE-ID ::= 138

id-DirectForwardingPathAvailability ProtocolIE-ID ::= 139

id-EarlyDataForwardingIndicator ProtocolIE-ID ::= 140

id-QoSFlowsDRBRemapping ProtocolIE-ID ::= 141

id-DataForwardingSourceIPAddress ProtocolIE-ID ::= 142

id-SecurityIndicationModify ProtocolIE-ID ::= 143

id-IAB-Donor-CU-UPPSKInfo ProtocolIE-ID ::= 144

id-ECGI-Support-List ProtocolIE-ID ::= 145

id-MDTPollutedMeasurementIndicator ProtocolIE-ID ::= 146

id-M4ReportAmount ProtocolIE-ID ::= 147

id-M6ReportAmount ProtocolIE-ID ::= 148

id-M7ReportAmount ProtocolIE-ID ::= 149

id-UESliceMaximumBitRateList ProtocolIE-ID ::= 150

id-PDUSession-PairID ProtocolIE-ID ::= 151

id-SurvivalTime ProtocolIE-ID ::= 152

id-UDC-Parameters ProtocolIE-ID ::= 153

id-SCGActivationStatus ProtocolIE-ID ::= 154

id-GNB-CU-CP-MBS-E1AP-ID ProtocolIE-ID ::= 155

id-GNB-CU-UP-MBS-E1AP-ID ProtocolIE-ID ::= 156

id-GlobalMBSSessionID ProtocolIE-ID ::= 157

id-BCBearerContextToSetup ProtocolIE-ID ::= 158

id-BCBearerContextToSetupResponse ProtocolIE-ID ::= 159

id-BCBearerContextToModify ProtocolIE-ID ::= 160

id-BCBearerContextToModifyResponse ProtocolIE-ID ::= 161

id-BCBearerContextToModifyRequired ProtocolIE-ID ::= 162

id-BCBearerContextToModifyConfirm ProtocolIE-ID ::= 163

id-MCBearerContextToSetup ProtocolIE-ID ::= 164

id-MCBearerContextToSetupResponse ProtocolIE-ID ::= 165

id-MCBearerContextToModify ProtocolIE-ID ::= 166

id-MCBearerContextToModifyResponse ProtocolIE-ID ::= 167

id-MCBearerContextToModifyRequired ProtocolIE-ID ::= 168

id-MCBearerContextToModifyConfirm ProtocolIE-ID ::= 169

id-MBSMulticastF1UContextDescriptor ProtocolIE-ID ::= 170

id-gNB-CU-UP-MBS-Support-Info ProtocolIE-ID ::= 171

id-SecurityIndication ProtocolIE-ID ::= 172

id-SecurityResult ProtocolIE-ID ::= 173

id-SDTContinueROHC ProtocolIE-ID ::= 174

id-SDTindicatorSetup ProtocolIE-ID ::= 175

id-SDTindicatorMod ProtocolIE-ID ::= 176

id-DiscardTimerExtended ProtocolIE-ID ::= 177

id-ManagementBasedMDTPLMNModificationList ProtocolIE-ID ::= 178

id-MCForwardingResourceRequest ProtocolIE-ID ::= 179

id-MCForwardingResourceIndication ProtocolIE-ID ::= 180

id-MCForwardingResourceResponse ProtocolIE-ID ::= 181

id-MCForwardingResourceRelease ProtocolIE-ID ::= 182

id-MCForwardingResourceReleaseIndication ProtocolIE-ID ::= 183

id-PDCP-COUNT-Reset ProtocolIE-ID ::= 184

id-MBSSessionAssociatedInfoNonSupportToSupport ProtocolIE-ID ::= 185

id-HW-CapacityIndicator-relevance ProtocolIE-ID ::= XXX

|  |
| --- |
| **Remaining text not changed** |