**3GPP TSG-RAN WG3 #119bis-e R3-231915**

**Online, 17th – 26th April 2023**

**Title: [DRAFT]** LS for clarification on the maximum length of Routing ID

**Response to:** -

**Release:** Rel-16

**Work Items:** NR\_pos-Core

**Source:** NTTDOCOMO, INC. [to be RAN3]

**To:** SA2, CT4

**CC:**

**Contact Person:** Tianyang Min

#### Name:

E-mail Address: tianyang.min.ex@nttdocomo.com

**Attachment:** R3-231913, R3-231914

**1. Overall Description:**

Regarding LMF Routing ID in NRPPa transport message, RAN3 clarified the maximum length of Routing ID is 16 octets, referring to the value of NfInstanceId defined in TS 29.571 (and IETF RFC 4122).

**2. Actions:**

**To SA2 and CT4**

**ACTION:** RAN3 respectfully asks SA2 and CT4 to take the above information into account.

**3. Date of Next RAN WG Meetings:**

TSG-RAN3 Meeting #120 May 22 to May 26, 2023 Incheon

TSG-RAN3 Meeting #121 August 21 to August 25, 2023 Toulouse