**3GPP TSG-RAN3 Meeting #122R3-237836**

**Chicago, US, 13-17 Nov, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.420** | **CR** | **0037** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (BL CR to 38.420) Support of mobile IAB |
|  |  |
| ***Source to WG:*** | Lenovo |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_mobile\_IAB-Core |  | ***Date:*** | 2023-11-17 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Add change to support mobile IAB. |
|  |  |
| ***Summary of change:*** | The following changes are made:1. Support IAB Transport Migration function between F1-terminating IAB-donor-CU and RRC-terminating IAB-donor-CU of a mobile IAB-node.
2. Support IAB Resource Coordination function between F1-terminating IAB-donor-CU and RRC-terminating IAB-donor-CU of a mobile IAB-node.
 |
|  |  |
| ***Consequences if not approved:*** | The mobile IAB cannot be supported. |
|  |  |
| ***Clauses affected:*** | 3.1, 5.2.10.2, 5.2.10.3, 6.2.10 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS 38.423  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

-------------------------------------------Start of Change------------------------------------------

3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Boundary IAB-node:** as defined in TS 38.401 [2].

**corresponding node:** as defined in TS 38.425 [7].

**F1-terminating IAB-donor-CU**: as defined in TS 38.401 [2].

**IAB-DU:** as defined in TS 38.300 [8].

**IAB-MT:** as defined in TS 38.300 [8].

Mobile IAB-node: as defined in TS 38.300 [8].

**Non-F1-terminating IAB-donor-CU**: as defined in TS 38.401 [2].

**NG-RAN node:** as defined in TS 38.300 [8].

RRC-terminating IAB-donor-CU: as defined in TS 38.401 [2].

**secondary node:** as defined in TS 37.340 [9].

-------------------------------------------Next Change------------------------------------------

5.2.10.2 IAB Transport Migration function

This function allows the exchange of information between the F1-terminating IAB-donor-CU and the non-F1-terminating IAB-donor-CU of a boundary IAB-node, for the purpose of managing the migration of the boundary and descendant IAB-node traffic between the topologies managed by the two IAB-donor-CUs. This function also allows the exchange of information between the F1-terminating IAB-donor-CU and the RRC-terminating IAB-donor-CU of a mobile IAB-node, for the purpose of managing the migration of the mobile IAB-node traffic between the topologies managed by the two IAB-donor-CUs.

5.2.10.3 IAB Resource Coordination function

This function is used to exchange information between the F1-terminating IAB-donor-CU and the non-F1-terminating IAB-donor-CU of a boundary IAB-node in order to support resource multiplexing between the IAB-MT and the IAB-DU of the boundary IAB-node. This function is also used to exchange information between the F1-terminating IAB-donor-CU and the RRC-terminating IAB-donor-CU of a mobile IAB-node in order to support resource multiplexing between the IAB-MT and the IAB-DU of the mobile IAB-node.

-------------------------------------------Next Change------------------------------------------

6.2.10 IAB procedures

The IAB procedures are used to enable the transfer of F1/non-F1 traffic for IAB, to exchange information between the F1-terminating IAB-donor-CU and the non-F1-terminating IAB-donor-CU of a boundary IAB-node, to enable the delivery of F1-C traffic between the M-NG-RAN node and the S-NG-RAN node serving a dual-connected non-boundary IAB-node, to exchange resource multiplexing related information between the F1-terminating IAB-donor-CU and the non-F1-terminating IAB-donor-CU of a boundary IAB-node, to exchange information between the F1-terminating IAB-donor-CU and the RRC-terminating IAB-donor-CU of a mobile IAB-node, and to exchange resource multiplexing related information between the F1-terminating IAB-donor-CU and the RRC-terminating IAB-donor-CU of a mobile IAB-node:

- F1-C Traffic Transfer

- IAB Transport Migration Management

- IAB Transport Migration Modification

- IAB Resource Coordination

-------------------------------------------End of Change-------------------------------------------