**3GPP TSG-RAN3 Meeting #125bisR3-24xxxx**

**Hefei, China, October 14 – 18, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.300** | **CR** | **-** | **rev** | **-** | **Current version:** | **19.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Introduction to Wireless Access and Backhaul | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_WAB\_5GFemto | | | | |  | ***Date:*** | | | 2024-10-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Introduction of Wireless Access and Backhaul (WAB) to the specification | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clause 3.1: Add WAB abbreviation  Clause 3.2: Add WAB related terms  Clause 4.X: Add WAB functionality | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No RAN support for Wireless Access and Backhaul. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.1, 3.2, 4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | - | | | | | | | | |

|  |  |
| --- | --- |
| ***This CR's revision history:*** | Rev 0: Added WAB based on agreements of R3#125bis: |

|  |
| --- |
| *--- Begin of Changes ---* |

# 3 Abbreviations and Definitions

## 3.1 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1], in TS 36.300 [2] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1] and TS 36.300 [2].

>>>>> SKIP

WAB Wireless Access and Backhaul

>>>>> SKIP

## 3.2 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1], in TS 36.300 [2] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1] and TS 36.300 [2].

>>>>> SKIP

**WAB-gNB**: gNB supported by the WAB-node to terminate the NR access interface to UEs and to terminate the NG protocol to the 5GC, as defined in TS 23.501 [3]. The WAB-gNB function used in 38-series of 3GPP Specifications corresponds to the MWAB-gNB function defined in TS 23.501 [3].

**WAB-MT**: WAB-node function that terminates the Uu interface to the BH RAN using the procedures and behaviours specified for UEs unless stated otherwise. The WAB-MT function used in 38-series of 3GPP Specifications corresponds to MWAB-UE function defined in TS 23.501 [3].

**WAB-node**: RAN node that supports NR Uu access links to UEs and NR Uu to a stationary RAN.

>>>>> SKIP

## 4.X Wireless Access and Backhaul

### 4.X.1 General

*Wireless Access and Backhaul (WAB)* introduces the *WAB-node*, which provides NR access links to UEs via a gNB functionality, referred to as WAB-gNB, and supports physical mobility across the RAN area. The WAB-node further supports a UE functionality, referred to as WAB-MT, which terminates an NR access link to a stationary RAN that is used for the backhauling of the WAB-gNB’s traffic.

The WAB architecture, the integration of the WAB-node into the stationary RAN used for backhauling, and the support of the WAB-node’s mobility is defined in TS 23.501 [3] and TS 38.401 [4].

|  |
| --- |
| *--- End of Changes ---* |