3GPP TSG-RAN WG4 Meeting #101bis-e R4-220xxxx

Electronic Meeting, 17-25 Jan., 2022

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** |  | **Current version:** | **17.4.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR R17 TS38.101-1 1 to correct intra-band CA REFSENS MSD test points. | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Skyworks Solutions Inc., Qualcomm Inc. | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CA\_R17\_Intra-Core | | | | |  | | ***Date:*** | | 2022-01-19 |
|  |  | | | |  | | |  | |  |
| ***Category:*** | **F** |  | | | | | | ***Release:*** | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | * There are contradictory statements for PCC UL/DL carrier location relative to the SCC UL/DL location; * The specified MSD test points are not consistent with legacy conventions of PCC/SCC placement for E-UTRA; * The UL RB configurations for CA\_n7B 2UL/2DL is not set proportional to the PCC/SCC CBW ratio; * Parameter ΔRIBNC is not appropriate since it is intended for Non-Contiguous intra-band carrier operation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. UL/DL PCC placement relative to SCC is corrected in NOTE 2 Table 7.3A.2.1-1; 2. MSD specifications for CA\_n5B and CA\_n7B are corrected to reflect PCC/SCC placement swap; 3. With corrected PCC/SCC placement, 1 uplink MSD test points are removed from Table 7.3A.2.1-1 and from core requirement text; 4. ΔRIBNC is replaced with ΔRIBC and ΔRIBC is introduced in core requirements sub-clause 7.3A.2.1; 5. ΔRIBNC and ΔRIBC are introduced in sub-clause 3.2 Symbols Definitions. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | CA\_n5A-n28A MSD is under-estimated. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.2, 7.3A.2.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | |  | | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | TS/TR ... CR ... | | | |
| ***affected:*** | | **X** |  | Test specifications | | | TS38.521-1 | | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | TS/TR ... CR ... | | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Refer to R4-2202039 and R4-2202028 for more details. | | | | | | | | |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |  |

## << Start of change >>

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

ΔFGlobal Granularity of the global frequency raster

ΔFRaster Band dependent channel raster granularity

ΔfOOB Δ Frequency of Out Of Band emission

ΔFTX-RX Maximum deviation to the Tx-Rx carrier center frequency separation for asymmetric uplink/downlink channel bandwidth operation

∆MPRc Allowed Maximum Power Reduction relaxation for serving cell *c*

ΔPPowerClass Adjustment to maximum output power for a given power class

RB The starting frequency offset between the allocated RB and the measured non-allocated RB

ΔRIB,c Allowed reference sensitivity relaxation due to support for inter-band CA operation, for serving cell *c*

ΔRIBC Allowed reference sensitivity relaxation due to support for intra-band contiguous CA operation

ΔRIBNC Allowed reference sensitivity relaxation due to support for intra-band non-contiguous CA operation

ΔRIB,4R Reference sensitivity adjustment due to support for 4 antenna ports

ΔShift Channel raster offset

TC Allowed operating band edge transmission power relaxation

TC,*c*Allowed operating band edge transmission power relaxation for serving cell *c*

ΔTIB,c Allowed maximum configured output power relaxation due to support for inter-band CA operation, inter-band NR-DC operation and due to support for SUL operations, for serving cell *c*

BWChannel Channel bandwidth

BWChannel,block Sub-block bandwidth, expressed in MHz. BWChannel,block= Fedge,block,high- Fedge,block,low

BWChannel\_CA Aggregated channel bandwidth, expressed in MHz

BWChannel,max Maximum channel bandwidth supported among all bands in a release

BWGB max( BWGB,Channel(*k*) )

BWGB,Channel(k) Minimum guard band defined in clause 5.3A.1 of carrier *k*

BWDL Channel bandwidth for DL

BWUL Channel bandwidth for UL

BWinterferer Bandwidth of the interferer

Ceil(x) Rounding upwards; ceil(x) is the smallest integer such that ceil(x) ≥ x

Floor(x) Rounding downwards; floor(x) is the greatest integer such that floor(x) ≤ x

FC *RF reference frequency* on the channel raster, given in table 5.4.2.2-1

FC,block, high Fc of the highest transmitted/received carrier in a *sub-block*

FC,block, low Fc of the lowest transmitted/received carrier in a *sub-block*

FC,low The Fc of the lowest carrier, expressed in MHz

FC,high The Fc of the highest carrier, expressed in MHz

FDL\_low The lowest frequency of the downlink *operating band*

FDL\_high The highest frequency of the downlink *operating band*

FUL\_low The lowest frequency of the uplink *operating band*

FUL\_high The highest frequency of the uplink *operating band*

Fedge,block,low The lower *sub-block* edge, where Fedge,block,low = FC,block,low - Foffset, low.

Fedge,block,high The upper *sub-block* edge, where Fedge,block,high = FC,block,high + Foffset, high.

Fedge , low The *lower edge* of *aggregated channel bandwidth*, expressed in MHz. Fedge,low = FC,low - Foffset,low.

Fedge, high The *higher edge* of *aggregated channel bandwidth*, expressed in MHz. Fedge,high = FC,high + Foffset,high.

FInterferer (offset) Frequency offset of the interferer (between the center frequency of the interferer and the carrier frequency of the carrier measured)

FInterferer Frequency of the interferer

FIoffset Frequency offset of the interferer (between the center frequency of the interferer and the closest edge of the carrier measured)

Foffset Frequency offset from FC\_high to the *higher edge* or FC\_low to the *lower edge.*

Foffset,high Frequency offset from FC,high to the upper *UE RF Bandwidth edge*, or from FC,block, high to the upper sub-block edge

Foffset,low Frequency offset from FC,low to the lower *UE RF Bandwidth edge*, or from FC,block, low to the lower sub-block edge

FOOB The boundary between the NR out of band emission and spurious emission domains

FREF RF reference frequency

FREF-Offs Offset used for calculating FREF

FREF, shift RF reference frequency for Supplementary Uplink (SUL) bands, the uplink of all FDD bands, and TDD bands

Fuw (offset) The frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer

GBChannel Minimum guard band defined in clause 5.3.3

LCRB Transmission bandwidth which represents the length of a contiguous resource block allocation expressed in units of resources blocks

Max() The largest of given numbers

Min() The smallest of given numbers

 Physical resource block number

NRACLR NR ACLR

NRB Transmission bandwidth configuration, expressed in units of resource blocks

NRB\_agg The number of the aggregated RBs within the fully allocated aggregated channel bandwidth

for carrier 1 to j, where *μ* is defined in TS 38.211 [6]

NRB,c The transmission bandwidth configuration of component carrier c, expressed in units of resource blocks

for carrier j, where *μ* is defined in TS 38.211 [6]

NRB,largest BW The largest transmission bandwidth configuration of the component carriers in the bandwidth combination, expressed in units of resource blocks

NRB,low The transmission bandwidth configurations according to Table 5.3.2-1 for the lowest assigned component carrier in clause 5.3A.1

NRB,high The transmission bandwidth configurations according to Table 5.3.2-1 for the highest assigned component carrier in clause 5.3A.1

NREF NR Absolute Radio Frequency Channel Number (NR-ARFCN)

NREF-Offs Offset used for calculating NREF

PCMAX The configured maximum UE output power

PCMAX, *c* The configured maximum UE output power for serving cell *c*

PCMAX, *f*, *c* The configured maximum UE output power for carrier *f* of serving cell *c* in each slot

PEMAX Maximum allowed UE output power signalled by higher layers

PEMAX, *c* Maximum allowed UE output power signalled by higher layers for serving cell *c*

PInterferer Modulated mean power of the interferer

Plargest BW Power of the largest transmission bandwidth configuration of the component carriers in the bandwidth combination

PPowerClass The nominal UE power (i.e., no tolerance)

P-MPR*c* Power Management Maximum Power Reduction for serving cell *c*

PRB The transmitted power per allocated RB, measured in dBm

PUMAX The measured configured maximum UE output power

Puw Power of an unwanted DL signal

Pw Power of a wanted DL signal

RBstart The lowest RB index of transmitted resource blocks

RBstart\_CA The lowest RB index of transmitted resource blocks for intra-band contiguous CA

SCSc SCS for the component carrier c

SCSlargest BW SCS for the largest transmission bandwidth configuration of the component carriers in the bandwidth combination

SCSlow SCS for the lowest assigned component carrier in clause 5.3A.1

SCShigh SCS for the highest assigned component carrier in clause 5.3A.1

*tp* Transient Period value signalled by the UE

*tpstart* Start position of transient period relative to the symbol boundary

T(PCMAX, *f*, *c*) Tolerance for applicable values of PCMAX, *f*, *c* for configured maximum UE output power for carrier *f* of serving cell *c*

TL,c Absolute value of the lower tolerance for the applicable *operating band* as specified in clause 6.2.1

SSREF SS block reference frequency position

UTRAACLR UTRA ACLR

## << Next change >>

## 7.3A Reference sensitivity for CA

### 7.3A.1 General

The reference sensitivity power level REFSENS is the minimum mean power applied to each one of the UE antenna ports for all UE categories, at which the throughput shall meet or exceed the requirements for the specified reference measurement channel.

### 7.3A.2 Reference sensitivity power level for CA

#### 7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA

For intra-band contiguous carrier aggregation, the throughput of each component carrier shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in Annexes A.2.2.2, A.3.2, and A.3.3 (with one sided dynamic OCNG Pattern OP.1 FDD/TDD for the DL-signal as described in Annex A.5.1.1/A.5.2.1) with parameters specified in Table 7.3.2-1, Table 7.3.2-2, and Table 7.3.2-3.

For UE(s) supporting one uplink carrier, the uplink configuration of the PCC shall be in accordance with Table 7.3.2-3 and the downlink PCC carrier center frequency shall be configured closer to uplink operating band than any of the downlink SCC center frequency.

For aggregation of two or more downlink FDD carriers with two uplink carriers, the reference sensitivity is defined only for the specific uplink and downlink test points which are specified in Table 7.3A.2.1-1 and the reference sensitivity power level increased by ΔRIBC. The requirements apply with all downlink carriers active. Unless given by Table 7.3.2-4, the reference sensitivity requirements shall be verified with the network signaling value NS\_01 (Table 6.2.3.1-1) configured.

Table 7.3A.2.1-1: Intra-band contiguous CA uplink configuration for reference sensitivity

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS  (PCC/SCC)  (kHz) | Aggregated channel bandwidth (PCC+SCC) | UL PCC allocation  (LCRB) | UL SCC allocation  (LCRB) | PCC ΔRIBC (dB) | SCC ΔRIBC (dB) | Duplex mode |
| CA\_n5B | 15/15 | 10MHz + 10MHz | 10 (RBstart = 0) | 10 (RBstart = 42) | 30.8 | 26.1 | FDD |
| CA\_n7B | 15/15 | 10MHz + 40MHz | 9 (RBstart = 26) | 36 (RBstart = 180) | 34 | 25 | FDD |
| NOTE 1: All combinations of channel bandwidths defined in Table 5.5A.1-1.  NOTE 2: The carrier centre frequency of SCC in the UL operating band is configured closer to the DL operating band.  NOTE 3: The transmitted power over both PCC and SCC shall be set to PUMAX as defined in subclause 6.2A.4.  NOTE 4: The PCC allocation is same as Transmission bandwidth configuration NRB as defined in Table 5.3.2-1. | | | | | | | |

## << End change >>