**3GPP TSG-RAN4 Meeting #102-eR4-220xxxx**

**Electronic Meeting, January 17-25, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **Draft** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on 38.133 for L1 measurement impact of NCSG |
|  |  |
| ***Source to WG:*** | MediaTek inc. |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_MG\_enh-Core |  | ***Date:*** | 2022-01-10 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | As agreed in R4-2120414, calrifications on how to determine the factor P in RLM, BFD, CBD, L1-RSRP are needed, when NCSG is configured.  |
|  |  |
| ***Summary of change:*** | Add calrifications on how to determine the factor P in RLM, BFD, CBD, L1-RSRP when NCSG us configured |
|  |  |
| ***Consequences if not approved:*** | NCSG may have problem when joinly considered with L1 measurements |
|  |  |
| ***Clauses affected:*** | 8.1.2.2, 8.1.3.2, 8.1A.2.2, 8.5.2.2, 8.5.3.2, 8.5A.2.2, 8.5A.5.2, 9.5.4, 9.5A.4, 9.8.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.533  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | This is the revision of R4-2200492. |

<Start of 1st change>

#### 8.1.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_SSB [ms] period becomes worse than the threshold Qout\_SSB within TEvaluate\_out\_SSB [ms] evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_SSB [ms] period becomes better than the threshold Qin\_SSB within TEvaluate\_in\_SSB [ms] evaluation period.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in Table 8.1.2.2-1 for FR1.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in Table 8.1.2.2-2 for FR2 with scaling factor N=8.

For FR1,

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, and these gaps are overlapping with some but not all occasions of the SSB; and

- P = 1 when in the monitored cell there are no gaps overlapping with any occasion of the SSB.

For FR2,

- , when RLM-RS resource is not overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when the RLM-RS resource is not overlapped with gap and RLM-RS resource is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- , when the RLM-RS is partially overlapped with gap and the RLM-RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TSSB = 0.5 × TSMTCperiod

-- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the RLM-RS resource outside gap is

* not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,
* not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

where,

 If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

 When measurement gap is configured,

* an RLM-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
* xRP = MGRP

When NCSG is configured,

* an RLM-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
* xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

Longer evaluation period would be expected if the combination of RLM-RS resource, SMTC occasion and gap configurations does not meet previous conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 8.1.2.2-1: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR1

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms)  | TEvaluate\_in\_SSB (ms)  |
| no DRX | Max(200, Ceil(10 × P) × TSSB) | Max(100, Ceil(5 × P) × TSSB) |
| DRX cycle≤320ms | Max(200, Ceil(15 × P) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P) × Max(TDRX,TSSB)) |
| DRX cycle>320ms | Ceil(10 × P) × TDRX | Ceil(5 × P) × TDRX |
| NOTE: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length. |

Table 8.1.2.2-2: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR2

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms)  | TEvaluate\_in\_SSB (ms)  |
| no DRX | Max(200, Ceil(10 × P × N) × TSSB) | Max(100, Ceil(5 × P × N) × TSSB) |
| DRX cycle≤320ms | Max(200, Ceil(15 × P × N) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P × N) × Max(TDRX,TSSB)) |
| DRX cycle>320ms | Ceil(10 × P × N) × TDRX | Ceil(5 × P × N) × TDRX |
| NOTE: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length. |

<End of 1st change>

<Start of 2nd change>

#### 8.1.3.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_CSI-RS ms period becomes worse than the threshold Qout\_CSI-RS within TEvaluate\_out\_CSI-RS ms evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_CSI-RS ms period becomes better than the threshold Qin\_CSI-RS within TEvaluate\_in\_CSI-RS ms evaluation period.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in Table 8.1.3.2-1 for FR1.

- TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS are defined in Table 8.1.3.2-2 for FR2 with scaling factor N=1.

The requirements of TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS apply provided that the CSI-RS for RLM is not in a resource set configured with repetition ON. The requirements do not apply when the CSI-RS resource in the active TCI state of CORESET is the same CSI-RS resource for RLM and the TCI state information of the CSI-RS resource is not given, wherein the TCI state information means QCL Type-D to SSB for L1-RSRP or CSI-RS with repetition ON.

For FR1,

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, and these gaps are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the CSI-RS.

For FR2,

- P=1, when the RLM-RS resource is not overlapped with gap and also not overlapped with SMTC occasion.

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is not overlapped with SMTC occasion (TCSI-RS < xRP)

- , when the RLM-RS resource is not overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P = Psharing factor, when the RLM-RS resource is not overlapped with gap and RLM-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TCSI-RS = 0.5 × TSMTCperiod

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap

- , when the RLM-RS resource is partially overlapped with gap and the RLM-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the RLM-RS resource outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

where,

If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

When measurement gap is configured,

* an RLM-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
* xRP = MGRP

When NCSG is configured,

* an RLM-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
* xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

Note: The overlap between CSI-RS for RLM and SMTC means that CSI-RS based RLM is within the SMTC window duration.

Longer evaluation period would be expected if the combination of RLM-RS resource, SMTC occasion and gap configurations does not meet previous conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of Mout and Min used in Table 8.1.3.2-1 and Table 8.1.3.2-2 are defined as:

- Mout = 20 and Min = 10, if the CSI-RS resource configured for RLM is transmitted with higher layer CSI-RS parameter *density* [6, clause 7.4.1] set to 3 and over the bandwidth ≥ 24 PRBs.

Table 8.1.3.2-1: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR1

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms)  | TEvaluate\_in\_CSI-RS (ms)  |
| no DRX | Max(200, Ceil(Mout×P)×TCSI-RS) | Max(100, Ceil(Min×P) × TCSI-RS) |
| DRX ≤ 320ms | Max(200, Ceil(1.5×Mout×P)× Max(TDRX, TCSI-RS)) | Max(100, Ceil(1.5×Min×P)× Max(TDRX, TCSI-RS)) |
| DRX > 320ms | Ceil(Mout×P) × TDRX | Ceil(Min×P) × TDRX |
| NOTE: TCSI-RS is the periodicity of the CSI-RS resource configured for RLM. The requirements in this table apply for TCSI-RS equal to 5 ms, 10ms, 20 ms or 40 ms. TDRX is the DRX cycle length. |

Table 8.1.3.2-2: Evaluation period TEvaluate\_out\_CSI-RS and TEvaluate\_in\_CSI-RS for FR2

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_CSI-RS (ms)  | TEvaluate\_in\_CSI-RS (ms)  |
| no DRX | Max(200, Ceil(Mout×P×N)×TCSI-RS) | Max(100, Ceil(Min×P×N) × TCSI-RS) |
| DRX ≤ 320ms | Max(200, Ceil(1.5×Mout×P×N)× Max(TDRX, TCSI-RS)) | Max(100, Ceil(1.5×Min×P×N)× Max(TDRX, TCSI-RS)) |
| DRX > 320ms | Ceil(Mout×P×N) × TDRX | Ceil(Min×P×N) × TDRX |
| NOTE: TCSI-RS is the periodicity of the CSI-RS resource configured for RLM. The requirements in this table apply for TCSI-RS equal to 5 ms, 10 ms, 20 ms or 40 ms. TDRX is the DRX cycle length. |

<End of 2nd change>

<Start of 3rd change>

#### 8.1A.2.2 Minimum Requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_SSB,CCA [ms] period becomes worse than the threshold Qout\_SSB,CCA within TEvaluate\_out\_SSB,CCA [ms] evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_SSB,CCA [ms] period becomes better than the threshold Qin\_SSB,CCA within TEvaluate\_in\_SSB,CCA [ms] evaluation period. During the in-sync evaluation procedure, layer 1 of the UE shall not send any in-sync indication for the cell to the higher layers when Lin exceeds Lin,max, where Lin and Lin,max are defined in Table 8.1A.2.2-1.

TEvaluate\_out\_SSB,CCA and TEvaluate\_in\_SSB,CCA are defined in Table 8.1A.2.2-1, where

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, and these gaps are overlapping with some but not all occasions of the SSB RLM-RS resources; and

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the SSB RLM-RS resources.

- When measurement gap is configured,

* an RLM-RS resource is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
* xRP = MGRP

- When NCSG is configured,

* an RLM-RS resource is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
* xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

Longer evaluation period would be expected if the combination of RLM-RS, SMTC occasion, and gap configurations does not meet previous conditions.

Table 8.1A.2.2-1: Evaluation period TEvaluate\_out\_SSB,CCA and TEvaluate\_in\_SSB,CCA

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB,CCA (ms) | TEvaluate\_in\_SSB,CCA (ms) |
|  | RLM-RS SSB Es/IotNote4 ≥-7 dB | RLM-RS SSB Es/Iot Note4 <-7 dB |  |
| no DRX | Max(200, Ceil(17\*P)\*TSSB) | Max(200, Ceil(24\*P)\*TSSB) | Max(100, Ceil((5+Lin)\*P)\*TSSB) |
| DRX cycle≤320 | Max(200, Ceil(1.5\*15\*P)\*Max(TDRX,TSSB)) | Max(200, Ceil(1.5\*20\*P)\*Max(TDRX,TSSB)) | Max(100, Ceil(1.5\*(5+Lin)\*P)\*Max(TDRX,TSSB)) |
| DRX cycle>320 | Ceil(13\*P)\*TDRX | Ceil(16\*P)\*TDRX | Ceil((5+Lin)\*P)\*TDRX |
| NOTE 1: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length.NOTE 2: When DRX is not configured, Lin is the number of RLM-RS SSB occasions which are not available at the UE during TEvaluate\_in\_SSB,CCA, where Lin ≤ Lin,max. When DRX is configured, Lin is the number of DRX cycles in which at least one RLM-RS SSB occasion is not available at the UE during TEvaluate\_in\_SSB,CCA, where Lin ≤ Lin,max. The UE is not required to determine the availability of SSB occasions more frequent than once per DRX cycle length, when configured with DRX.NOTE 3: Lin,max=7 for Max(TDRX,TSSB) ≤ 40 assuming TDRX=0 for non-DRX case,  Lin,max=5 for 40<Max(TDRX,TSSB)≤320, Lin,max=3 for TDRX>320.NOTE 4: RLM-RS SSB Es/Iot is the averaged Es/Iot over the most recent previous out-of-sync evaluation period. |

<End of 3rd change>

<Start of 4th change>

#### 8.5.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured SSB resource in set  estimated over the last TEvaluate\_BFD\_SSB ms period becomes worse than the threshold Qout\_LR\_SSB within TEvaluate\_BFD\_SSB ms period.

The value of TEvaluate\_BFD\_SSB is defined in Table 8.5.2.2-1 for FR1.

The value of TEvaluate\_BFD\_SSB is defined in Table 8.5.2.2-2 for FR2 with scaling factor N=8

For FR1,

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB.

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the SSB.

For FR2,

- , when BFD-RS resource is not overlapped with gap and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P = Psharing factor, when the BFD-RS resource is not overlapped with gap and the BFD-RS resource is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TSSB = 0.5\*TSMTCperiod

- , when the BFD-RS resource is partially overlapped with gap (TSSB <xRP) and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap.

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the BFD-RS resource outside gap is

- not overlapped with the SSB symbols indicated by SSB-ToMeasure and 1 data symbol before each consecutive SSB symbols indicated by SSB-ToMeasure and 1 data symbol after each consecutive SSB symbols indicated by SSB-ToMeasure, given that SSB-ToMeasure is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and;

- not overlapped with the RSSI symbols indicated by ss-RSSI-Measurement and 1 data symbol before each RSSI symbol indicated by ss-RSSI-Measurement and 1 data symbol after each RSSI symbol indicated by ss-RSSI-Measurement, given that ss-RSSI-Measurement is configured.

- Psharing factor = 3, otherwise.

where,

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, given the SMTC offset of all CCs in FR2 provided the same offset.

When measurement gap is configured,

* + a BFD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + a BFD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

Longer evaluation period would be expected if the combination of BFD-RS resource, SMTC occasion and gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer BFD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 8.5.2.2-1: Evaluation period TEvaluate\_BFD\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms)  |
| no DRX | Max(50, Ceil(5 × P) × TSSB) |
| DRX cycle ≤ 320ms | Max(50, Ceil(7.5 × P) × Max(TDRX,TSSB)) |
| DRX cycle > 320ms | Ceil(5 × P) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

Table 8.5.2.2-2: Evaluation period TEvaluate\_BFD\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms)  |
| no DRX | Max(50, Ceil(5 × P × N) × TSSB) |
| DRX cycle ≤ 320ms | Max(50, Ceil(7.5 × P × N) × Max(TDRX,TSSB)) |
| DRX cycle > 320ms | Ceil(5 × P × N) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

<End of 4th change>

<Start of 5th change>

#### 8.5.3.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the CSI-RS resource in set  estimated over the last TEvaluate\_BFD\_CSI-RS ms period becomes worse than the threshold Qout\_LR\_CSI-RS within TEvaluate\_BFD\_CSI-RS ms period.

The value of TEvaluate\_BFD\_CSI-RS is defined in Table 8.5.3.2-1 for FR1.

The value of TEvaluate\_BFD\_CSI-RS is defined in Table 8.5.3.2-2 for FR2 with N=1. The requirements of TEvaluate\_BFD\_CSI-RS apply provided that the CSI-RS for BFD is not in a resource set configured with repetition ON. The requirements shall not apply when the CSI-RS resource in the active TCI state of CORESET is the same CSI-RS resource for BFD and the TCI state information of the CSI-RS resource is not given, wherein the TCI state information means QCL Type-D to SSB for L1-RSRP or CSI-RS with repetition ON.

For FR1,

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS.

- P = 1 when in the monitored cell there are no gaps overlapping with any occasion of the CSI-RS.

For FR2,

- P = 1, when the BFD-RS resource is not overlapped with gap and also not overlapped with SMTC occasion.

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is not overlapped with SMTC occasion (TCSI-RS < xRP)

- , when the BFD-RS resource is not overlapped with gap and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P = Psharing factor, when the BFD-RS resource is not overlapped with gap and the BFD-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xGRP and TCSI-RS < 0.5 × TSMTCperiod

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TCSI-RS = 0.5 × TSMTCperiod

- , when the BFD-RS resource is partially overlapped with gap (TCSI-RS < xRP) and the BFD-RS resource is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap.

- , when the BFD-RS resource is partially overlapped with gap and the BFD-RS resource is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the BFD-RS resource outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and;

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured,

- Psharing factor = 3, otherwise.

where,

 If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

When measurement gap is configured,

* + a BFD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + a BFD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

Note: The overlap between CSI-RS for BFD and SMTC means that CSI-RS for BFD is within the SMTC window duration.

Longer evaluation period would be expected if the combination of the BFD-RS resource, SMTC occasion and gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer BFD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of MBFD used in Table 8.5.3.2-1 and Table 8.5.3.2-2 are defined as

- MBFD = 10, if the CSI-RS resource(s) in set  used for BFD is transmitted with Density = 3 and over the bandwidth ≥ 24 PRBs.

The values of PBFD used in Table 8.5.3.2-1 and Table 8.5.3.2-2 are defined as

 For each CSI-RS resource in the set  configured for PCell or PSCell in EN-DC or NE-DC or SA; or PCell in NR-DC

- PBFD = 1.

For each CSI-RS resource in the set  configured for PSCell in NR-DC

PBFD = 2 if UE is configured for beam failure detection on SCell, 1 otherwise.

 For each CSI-RS resource in the set  configured for a SCell

- PBFD = Z in EN-DC or NE-DC or SA.

- PBFD = 2\* Z in NR-DC.

Where Z is the number of band(s) on which UE is performing beam failure detection only for SCell.

**Table 8.5.3.2-1: Evaluation period TEvaluate\_BFD\_CSI-RS for FR1**

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_CSI-RS (ms)  |
| no DRX | Max(50, Ceil(MBFD × P × PBFD) × TCSI-RS) |
| DRX cycle ≤ 320ms | Max(50, Ceil(1.5 × MBFD × P × PBFD) × Max(TDRX, TCSI-RS)) |
| DRX cycle > 320ms | Ceil(MBFD × P × PBFD) × TDRX |
| Note: TCSI-RS is the periodicity of CSI-RS resource in the set . TDRX is the DRX cycle length. |

**Table 8.5.3.2-2: Evaluation period TEvaluate\_BFD\_CSI-RS for FR2**

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_CSI-RS (ms)  |
| no DRX | Max(50, Ceil(MBFD × P × N × PBFD) × TCSI-RS) |
| DRX cycle ≤ 320ms | Max(50, Ceil(1.5 × MBFD × P × N × PBFD) × Max(TDRX, TCSI-RS)) |
| DRX cycle > 320ms | Ceil(MBFD × P × N × PBFD) × TDRX |
| Note: TCSI-RS is the periodicity of CSI-RS resource in the set . TDRX is the DRX cycle length. |

<End of 5th change>

<Start of 6th change>

#### 8.5.5.2 Minimum requirement

Upon request the UE shall be able to evaluate whether the L1-RSRP measured on the configured SSB resource in set  estimated over the last TEvaluate\_CBD\_SSB ms period becomes better than the threshold Qin\_LR provided SSB\_RP and SSB Ês/Iot are according to Annex Table B.2.4.1 for a corresponding band.

The UE shall monitor the configured SSB resources using the evaluation period in table 8.5.5.2-1 and 8.5.5.2-2 corresponding to the non-DRX mode, if the configured DRX cycle ≤ 320ms.

The value of TEvaluate\_CBD\_SSB is defined in Table 8.5.5.2-1 for FR1.

The value of TEvaluate\_CBD\_SSB is defined in Table 8.5.5.2-2 for FR2 with scaling factor N=8.

where,

For FR1,

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB,

- P = 1 when in the monitored cell there are no gaps overlapping with any occasion of the SSB.

For FR2,

- , when candidate beam detection RS is not overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when candidate beam detection RS is not overlapped with gap and candidate beam detection RS is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- , when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5 × TSMTCperiod

- , when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TSSB = 0.5 × TSMTCperiod

- , when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap

- , when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the candidate beam detection RS outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and;

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured

- Psharing factor = 3, otherwise.

where,

 If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

When measurement gap is configured,

* + a CBD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + a CBD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

Longer evaluation period would be expected if the combination of the CBD-RS resource, SMTC occasion and gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer CBD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of PCBD used in Table 8.5.5.2-1 and Table 8.5.5.2-2 are defined as

 For each SSB resource in the set  configured for PCell or PSCell in EN-DC or NE-DC or SA; or PCell in NR-DC

- PCBD = 1.

For each SSB resource in the set  configured for PSCell in NR-DC

- PCBD = 2 if UE is configured for candidate beam detection on SCell, 1 otherwise.

 For each SSB resource in the set  configured for a SCell

- PCBD = Z in EN-DC or NE-DC or SA.

- PCBD = 2\* Z in NR-DC.

 Where Z is the number of band(s) on which UE is performing beam failure detection only for SCell

- PCBD is the number of band(s) on which UE is performing candidate beam detection only for SCell.

**Table 8.5.5.2-1: Evaluation period TEvaluate\_CBD\_SSB for FR1**

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_CBD\_SSB (ms)**  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil(3 × P × PCBD) × TSSB) |
| DRX cycle > 320ms | Ceil(3 × P × PCBD) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

**Table 8.5.5.2-2: Evaluation period TEvaluate\_CBD\_SSB for FR2**

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_CBD\_SSB (ms)**  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil(3 × P × N × PCBD) × TSSB) |
| DRX cycle > 320ms | Ceil(3 × P × N × PCBD) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

<End of 6th change>

<Start of 7th change>

#### 8.5.6.2 Minimum requirement

Upon request the UE shall be able to evaluate whether the L1-RSRP measured on the configured CSI-RS resource in set  estimated over the last TEvaluate\_CBD\_CSI-RS [ms] period becomes better than the threshold Qin\_LR within TEvaluate\_CBD\_CSI-RS [ms] period provided CSI-RS Ês/Iot is according to Annex Table B.2.4.2 for a corresponding band.

The UE shall monitor the configured CSI-RS resources using the evaluation period in table 8.5.6.2-1 and 8.5.6.2-2 corresponding to the non-DRX mode, if the configured DRX cycle ≤ 320ms.

The value of TEvaluate\_CBD\_CSI-RS is defined in Table 8.5.6.2-1 for FR1.

The value of TEvaluate\_CBD\_CSI-RS is defined in Table 8.5.6.2-2 for FR2 with scaling factor N=8.

For FR1,

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P = 1 when in the monitored cell there are no gaps overlapping with any occasion of the CSI-RS.

For FR2,

- P = 1, when candidate beam detection RS is not overlapped with gap and also not overlapped with SMTC occasion.

- when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- , when candidate beam detection RS is not overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P =Psharing factor, when candidate beam detection RS is not overlapped with gap and candidate beam detection RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- ,, when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5 × TSMTCperiod

- , when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TCSI-RS = 0.5 × TSMTCperiod

- , when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap

- ,, when candidate beam detection RS is partially overlapped with gap and candidate beam detection RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the candidate beam detection RS outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and;

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

where,

 If the high layer in TS 38.331 [2] signaling of *smtc2* is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

When measurement gap is configured,

* + a CBD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + a CBD-RS resource or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

Note: The overlap between CSI-RS for CBD and SMTC means that CSI-RS for CBD is within the SMTC window duration.

Longer evaluation period would be expected if the combination of the CBD-RS resource, SMTC occasion and gap configurations does not meet pervious conditions.

Longer evaluation period would be expected if the CSI-RS is on the same OFDM symbols with RLM, BFD, BM-RS, or other CBD-RS, according to the measurement restrictions defined in clause 8.5.6.3.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer CBD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of MCBD used in Table 8.5.6.2-1 and Table 8.5.6.2-2 are defined as

- MCBD = 3, if the CSI-RS resource configured in the set  is transmitted with Density = 3 and over the bandwidth ≥ 24 PRBs.

The values of PCBD used in Table 8.5.6.2-1 and Table 8.5.6.2-2 are defined as

 For each CSI-RS resource in the set  configured for PCell or PSCell in EN-DC or NE-DC or SA; or PCell in NR-DC

- PCBD = 1.

For each CSI-RS resource in the set  configured for PSCell in NR-DC

- PCBD = 2 if UE configured for candidate beam detection on SCell, 1 otherwise.

 For each CSI-RS resource in the set  configured for a SCell

- PCBD = Z in EN-DC or NE-DC or SA.

- PCBD = 2\* Z in NR-DC.

 Where Z is the number of band(s) on which UE is performing beam failure detection only for SCell

- PCBD is the number of band(s) on which UE is performing candidate beam detection only for SCell.

**Table 8.5.6.2-1: Evaluation period TEvaluate\_CBD\_CSI-RS for FR1**

|  |  |
| --- | --- |
| **Configuration** | **TEvaluateC\_CBD\_CSI-RS (ms)**  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil(MCBD × P × PCBD) × TCSI-RS) |
| DRX cycle > 320ms | Ceil(MCBD × P × PCBD) × TDRX |
| Note: TCSI-RS is the periodicity of CSI-RS resource in the set . TDRX is the DRX cycle length. |

**Table 8.5.6.2-2: Evaluation period TEvaluate\_CBD\_CSI-RS for FR2**

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_CBD\_CSI-RS (ms)**  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil(MCBD × P × N × PCBD) × TCSI-RS) |
| DRX cycle > 320ms | Ceil(MCBD × P × N × PCBD) × TDRX |
| Note: TCSI-RS is the periodicity of CSI-RS resource in the set . TDRX is the DRX cycle length. |

<End of 7th change>

<Start of 8th change>

#### 8.5A.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured BFD-RS SSB resource in set estimated over the last TEvaluate\_BFD\_SSB\_CCA ms period becomes worse than the threshold Qout\_LR\_SSB,CCA within TEvaluate\_BFD\_SSB\_CCA ms period.

The value of TEvaluate\_BFD\_SSB\_CCA is defined in Table 8.5A.2.2-1, where

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the BFD-RS SSB.

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the BFD-RS SSB.

- When measurement gap is configured,

* a BFD-RS resource is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
* xRP = MGRP

- When NCSG is configured,

* a BFD-RS resource is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
* xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*.

Longer evaluation period would be expected if the combination of BFD-RS SSB resource, SMTC occasion and gap configurations does not meet pervious conditions.

Table 8.5A.2.2-1: Evaluation period TEvaluate\_BFD\_SSB\_CCA

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB\_CCA (ms)  |
|  | BFD-RS SSB Es/Iot Note2 ≥ -7 dB | BFD-RS SSB Es/Iot Note2 < -7 dB |
| no DRX | Max(50, Ceil((10 × P) × TSSB)) | Max(50, Ceil((12 × P) × TSSB)) |
| DRX cycle ≤ 320ms | Max(50, Ceil(1.5 × 8 × P) × Max(TDRX,TSSB)) | Max(50, Ceil(1.5 × 10 × P) × Max(TDRX,TSSB)) |
| DRX cycle > 320ms | Ceil(7 × P) × TDRX | Ceil(8 × P) × TDRX |
| Note 1: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length.Note 2: BFD-RS SSB Es/Iot is the averaged BFD-RS SSB Es/Iot over the most recent previous evaluation period. |

<End of 8th change>

<Start of 9th change>

#### 8.5A.5.2 Minimum requirement

Upon request the UE shall be able to evaluate whether the L1-RSRP measured on the configured CBD-RS SSB resource in set  estimated over the last TEvaluate\_CBD\_SSB\_CCA ms period becomes better than the threshold Qin\_LR,CCA provided SSB\_RP and SSB Ês/Iot are according to Annex Table B.2.4.1 for a corresponding band.

The UE shall monitor the configured SSB resources using the evaluation period in table 8.5A.5.2-1 corresponding to the non-DRX mode, if the configured DRX cycle ≤ 320ms.

The value of TEvaluate\_CBD\_SSB\_CCA is defined in Table 8.5A.5.2-1, where

- , when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CBD-RS SSB,

- P = 1 when in the monitored cell there are no gaps overlapping with any occasion of the CBD-RS SSB.

- When measurement gap is configured,

* a CBD-RS resource is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
* xRP = MGRP

- When NCSG is configured,

* a CBD-RS resource is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
* xRP = VIRP

Table 8.5A.5.2-1: Evaluation period TEvaluate\_CBD\_SSB\_CCA

|  |  |
| --- | --- |
| Configuration | TEvaluate\_CBD\_SSB\_CCA (ms)  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil((3 + LCBD) × P) × TSSB) |
| DRX cycle > 320ms | Ceil((3 + LCBD) × P) × TDRX |
| Note 1: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length.Note 2: When DRX is not configured, LCBD is the number of CBD-RS SSB occasions not available at the UE during TEvaluate\_CBD\_SSB\_CCA where LCBD ≤ LCBD,max. When DRX is configured, LCBD is the number of DRX cycles in which at least one of the CBD-RS SSB occasions not available at the UE during TEvaluate\_CBD\_SSB\_CCA where LCBD ≤ LCBD,max. The UE is not required to determine the availability of SSB occasions more frequent than once per DRX cycle length, when configured with DRX.Note 3: LCBD,max=7 for Max(TDRX, TSSB) ≤ 40 assuming TDRX=0 for non-DRX, LCBD,max=5 for 40 < Max(TDRX, TSSB) ≤ 320, LCBD,max=3 for TDRX > 320.Note 4 If LCBD>LCBD,max, the UE shall assume no new candidate beams are found for this evaluation period. |

<End of 9th change>

<Start of 10th change>

### 9.5.4 L1-RSRP measurement requirements

#### 9.5.4.1 SSB based L1-RSRP Reporting

The UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB.

The value of TL1-RSRP\_Measurement\_Period\_SSB is defined in Table 9.5.4.1-1 for FR1 and Table 9.5.4.1-2 for FR2, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- N= 8.

For FR1,

- P=, when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB; and

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the SSB.

For FR2,

- P=, when SSB is not overlapped with gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when SSB is not overlapped with gap and SSB is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- P=, when SSB is partially overlapped with gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- P is , when SSB is partially overlapped with gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TSSB = 0.5\*TSMTCperiod

- P=, when S SSB is partially overlapped with gap (TSSB <xRP) and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap.

- P is , when SSB is partially overlapped with gap and SSB is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the SSB configured for L1-RSRP measurement outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured,

- Psharing factor = 3, otherwise.

Where:

- TSSB = ssb-periodicityServingCell

- TSMTCperiod = the configured SMTC period

- When measurement gap is configured,

* + an SSB or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

- When NCSG is configured,

* + an SSB or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer L1 RSRP measurement period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 9.5.4.1-1: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: K = 1 when TSSB ≤ 40 ms and *highSpeedMeasFlag-r16* are configured; otherwise K = 1.5.Note 3: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *[intraRAT-MeasurementEnhancement-r16].* |

Table 9.5.4.1-2: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. |

#### 9.5.4.2 CSI-RS based L1-RSRP Reporting

The UE shall be capable of performing L1-RSRP measurements based on the configured CSI-RS resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_CSI-RS.

The value of TL1-RSRP\_Measurement\_Period\_CSI-RS is defined in Table 9.5.4.2-1 for FR1 and in Table 9.5.4.2-2 for FR2, where

- For periodic and semi-persistent CSI-RS resources, M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- For aperiodic CSI-RS resources M=1

- For periodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured with QCL-TypeD for all resources in the resource set.

- For semi-persistent CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided with QCL-TypeD for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided *qcl-info* is configured for all resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clause 10.1.19.2 and 10.1.20.2 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requirements apply provided *qcl-info* is configured with QCL-TypeD for all resources in the resource set.

For FR1,

- P=, when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the CSI-RS.

For FR2,

- P=1, when CSI-RS is not overlapped with gap and also not overlapped with SMTC occasion.

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- P=, when CSI-RS is not overlapped with gap and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P=Psharing factor, when CSI-RS is not overlapped with gap and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- P=1, when aperiodic CSI-RS resource is not overlapped with gap

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TCSI-RS = 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with gap (TCSI-RS < xRP) and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap.

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

- Psharing factor = 1, if the CSI-RS configured for L1-RSRP measurement outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured

- Psharing factor = 3, otherwise.

Where:

 TSMTCperiod = the configured SMTC period.

 TCSI-RS = the periodicity of CSI-RS configured for L1-RSRP measurement

 When measurement gap is configured,

* + a CSI-RS or an SMTC occasion is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + a CSI-RS or an SMTC occasion is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

Note: The overlap between CSI-RS for L1-RSRP measurement and SMTC means that CSI-RS for L1-RSRP measurement is within the SMTC window duration.

Longer evaluation period would be expected if the combination of CSI-RS, SMTC occasion and gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer L1 RSRP measurement period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 9.5.4.2-1: Measurement period TL1-RSRP\_Measurement\_Period\_CSI-RS for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_CSI-RS (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-RSRP measurement is transmitted with Density = 3.Note 3: K = 1 when TCSI-RS ≤ 40 ms and *highSpeedMeasFlag-r16* are configured; otherwise K = 1.5.Note 4: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *[intraRAT-MeasurementEnhancement-r16].* |

Table 9.5.4.2-2: Measurement period TL1-RSRP\_Measurement\_Period\_CSI-RS for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_CSI-RS (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P\*N)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-RSRP measurement is transmitted with Density = 3. |

<End of 10th change>

<Start of 11th change>

### 9.5A.4 L1-RSRP measurement requirements

#### 9.5A.4.1 SSB based L1-RSRP Reporting

The UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB\_CCA.

The value of TL1-RSRP\_Measurement\_Period\_SSB\_CCA is defined in Table 9.5A.4.1-1 for FR1, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

For FR1,

- P=, when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB; and

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the SSB.

Where:

 TSSB = ssb-periodicityServingCell

 TSMTCperiod = the configured SMTC1 period or SMTC2 period if configured

 When measurement gap is configured,

* + an SSB is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + an SSB is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and gap configurations does not meet pervious conditions.

UE shall report RSRP\_0 (Not valid) if L1>L1max, where L1 and L1max are defined in Table 9.5A.4.1-1.

Table 9.5A.4.1-1: Measurement period TL1-RSRP\_Measurement\_Period\_SSB\_CCA for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_CCA (ms)  |
| non-DRX | max(TReport, ceil((M+L1)\*P)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*(M+L1)\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil((M+L1)\*P)\*TDRX |
| Note 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: L1=0 if higher layer parameter timeRestrictionForChannelMeasurement is configured. Otherwise, when DRX is not configured L1 is the number of SSBs not available at the UE during TL1-RSRP\_Measurement\_Period\_SSB\_CCA, and when DRX is configured L1 is the number of DRX cycles in which at least one SSB is not available at the UE during TL1-RSRP\_Measurement\_Period\_SSB\_CCA, where L1 ≤ L1max.Note 3: L1max =7 for Max(TDRX,TSSB) ≤ 40ms assuming TDRX=0 for non-DRX,L1max =5 for 40ms < Max(TDRX, TSSB) ≤ 320ms, L1max =3 for TDRX > 320ms. |

<End of 11th change>

<Start of 12th change>

#### 9.8.4.1 L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured

edicated resource configured as IMR for L1-SINR computation, and the UE physical layer shall be capable of reporting L1-SINR measured over the measurement period of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only.

The value of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only is defined in Table 9.8.4.1-1 for FR1 and in Table 9.8.4.1-2 for FR2, where

For the value of M,

- For periodic and semi-persistent CSI-RS resources as CMR, M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise;

- For aperiodic CSI-RS resources as CMR, M=1.

For the value of N in FR2

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured for all resources in the resource set.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requriements apply provided *qcl-info* is configured for all resources in the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clause 10.1.28.1 and 10.1.28.3 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requriements apply provided *qcl-info* is configured for all resources in the resource set.

For the value of P in FR1,

- P=, when in the monitored cell there are gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no gaps overlapping with any occasion of the CSI-RS.

For the value of P in FR2,

- P=1, when CSI-RS is not overlapped with gap and also not overlapped with SMTC occasion.

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- P=, when CSI-RS is not overlapped with gap and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P=3, when CSI-RS is not overlapped with gap and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with gap and TSMTCperiod = xRP and TCSI-RS = 0.5\*TSMTCperiod

- P=, when CSI-RS is partially overlapped with gap (TCSI-RS < xRP) and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with gap.

- P=, when CSI-RS is partially overlapped with gap and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with gap (TSMTCperiod < xRP)

Where:

 TSMTCperiod = the configured SMTC1 period or SMTC2 period if configured.

 TCSI-RS = the periodicity of CSI-RS configured for L1-SINR measurement

 When measurement gap is configured,

* + a CSI-RS is condiered as overlapped with gap if it overlaps the measurement gap occasion, and
	+ xRP = MGRP

When NCSG is configured,

* + a CSI-RS is condiered as overlapped with gap if it overlaps the VIL1 or VIL2 of NCSG, and
	+ xRP = VIRP

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*.

Note: The overlap between CSI-RS for L1-SINR measurement and SMTC means that CSI-RS for L1-SINR measurement is within the SMTC window duration.

Longer evaluation period would be expected if the combination of CSI-RS, SMTC occasion and gap configurations does not meet pervious conditions.

Table 9.8.4.1-1: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only for FR1

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3. |

Table 9.8.4.1-2: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only for FR2

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P\*N)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3. |

<End of 12th change>