**3GPP TSG-RAN WG4 Meeting #101-bis-e R4-**

**Online Meeting, 17 January – 25 January 2022**

**Source: ZTE Corporation**

**Title: WF on IAB enhancement RRM**

**Agenda item: 6.17.3**

**Document for: Approval**

1 Way Forward

**On Case 1 Timing**

No new RRM requirements are needed for Case #1 timing procedures.

Clarify in the TS 38.174 that current transmit timing requirements apply to case#1 timing mode.

**On Case 6 Timing**

There is no RRM impact of case#6 timing.

**On Case 7 Timing**

The existing timing advance step size accuracy requirements in clause 12.2.3, TS 38.174, are applicable for Case # 7 timings.

No new RRM requirements are needed for Case # 7 timing procedures.

**CLI**

Option 1: For CLI measurements by IAB-MT, no new RRM requirements need to be specified in R17.

Option 2: all Rel 16 UE CLI measurement performance requirement shall be adopted for Rel 17 eIAB RRM.

References