**3GPP TSG-RAN WG4 Meeting #102-e  Rev. 1 of R4-2205570**

**Electronic Meeting, 21 Feb - 03 Mar, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** | **draft** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | draftCR to add CA\_n1A-n3A-n7A-n28A-n78(2A) to 38.101-1 |
|  |  |
| ***Source to WG:*** | Nokia, BT |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_CADC\_R17\_5BDL\_xBUL |  | ***Date:*** | 2022-02-21 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Addition of CA\_n1A-n3A-n7A-n28A-n78(2A) |
|  |  |
| ***Summary of change:*** | Added CA\_n1A-n3A-n7A-n28A-n78(2A) |
|  |  |
| ***Consequences if not approved:*** | Operator cannot use this bandcombination |
|  |  |
| ***Clauses affected:*** | 5.5A.3.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### 5.5A.3.4 Configurations for inter-band CA (five bands)

Table 5.5A.3.4-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (five bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration | NR Band | Channel bandwidth (MHz) (NOTE 1) | Bandwidth combination set |
|  |  |  | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
|  | CA\_n1A-n3ACA\_n1A-n5A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  | CA\_n1A-n7ACA\_n1A-n78A | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n1A-n3A-n5A-n7A-n78A | CA\_n3A-n5ACA\_n3A-n7A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  | CA\_n3A-n78ACA\_n5A-n7A | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
|  | CA\_n5A-n78ACA\_n7A-n78A | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
|  | CA\_n1A-n3ACA\_n1A-n5A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  | CA\_n1A-n7ACA\_n1A-n78A | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n1A-n3A-n5A-n7B-n78A | CA\_n3A-n5ACA\_n3A-n7A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  | CA\_n3A-n78ACA\_n5A-n7A | n7 | See CA\_n7B bandwidth combination set 0 in Table 5.5A.1-1 |  |
|  | CA\_n5A-n78ACA\_n7A-n78ACA\_n7B | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78A | - | n1 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 0 |
|  |  | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
|  |  | n28 | 5 | 10 | 15 | 202 |  | 302 |  |  |  |  |  |  |  |  |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
|  | CA\_n1A-n3ACA\_n1A-n7ACA\_n1A-n28ACA\_n1A-n78A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  | CA\_n3A-n7ACA\_n3A-n28ACA\_n3A-n78A | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
|  | CA\_n7A-n28ACA\_n7A-n78A | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
|  | CA\_n28A-n78A | n28 | 5 | 10 | 15 | 202 |  |  |  |  |  |  |  |  |  |  |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n1A-n3A-n7B-n28A-n78A | CA\_n1A-n3ACA\_n1A-n7ACA\_n1A-n28ACA\_n1A-n78ACA\_n3A-n7ACA\_n3A-n28ACA\_n3A-n78ACA\_n7A-n28ACA\_n7A-n78ACA\_n28A-n78ACA\_n7B | n1 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 0 |
|  |  | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
|  |  | n7 | See CA\_n7B Bandwidth Combination Set 0 in Table 5.5A.1-1 |  |
|  |  | n28 | 5 | 10 | 15 | 20 |  | 30 |  |  |  |  |  |  |  |  |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78(2A) | CA\_n1A-n3ACA\_n1A-n7ACA\_n1A-n28ACA\_n1A-n78ACA\_n3A-n7ACA\_n3A-n28ACA\_n3A-n78ACA\_n7A-n28ACA\_n7A-n78ACA\_n28A-n78A | n1 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 0 |
|  |  | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
|  |  | n28 | 5 | 10 | 15 | 20 |  | 30 |  |  |  |  |  |  |  |  |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 |  |
| NOTE 1: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*