**3GPP TSG-RAN WG4 Meeting #102-eR4-2203631**

**Electronic Meeting, February 21 – March 3, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR to 38.101-1 Correct the descriptions on power class requirements applications for UE maximum output power for CA | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | China Telecom | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_PC2\_CA\_R17\_2BDL\_2BUL-Core | | | | |  | ***Date:*** | | | 2022-02-10 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Correct the descriptions on power class requirements applications in clause 6.2A.1.1, 6.2A.1.2 and 6.2A.1.3 to make them aligned across inter-band CA, intra-band CA, with one uplink carrier. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | For intra-band contiguous CA:  1) Change the type of description for power class except class 3 for intra-band CA with one uplink carrier to be divided in two paragraph, one is for power class 3, the other is for other power class. Because we think this way will explicitly indicate that the high power class is cofigured in CA channel bandwidth configuration table according to questions from RAN5 experts working on the testing project in parallel, and also is aligned with for inter-band CA.  2) Correct the typo of description for intra-band contiguous power class 3 CA, the outpout power is specified in table 6.2.1-1 rather than 6.2.2-1.  3) Remove the origional description for intra-band CA with one uplink carrier as shown in the paragraph just below the Table 6.2A.1.3-2, which is in wrong place.  For intra-band non contiguous CA:  Correct the typo of description for intra-band non-contiguous power class 3 CA, the requirements in clause 6.2.1 apply, rather than in clause 6.2.2.  For inter-band CA:  Change the type of description for power class except class 3 for inter-band CA with one uplink carrier… to be aligned with that for power class 3… | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The descriptions for power class requirements applications are not clear and not friendly to read. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2A.1.1, 6.2A.1.2, 6.2A.1.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## <Start of Change>

## 6.2A Transmitter power for CA

### 6.2A.1 UE maximum output power for CA

#### 6.2A.1.1 UE maximum output power for Intra-band contiguous CA

For uplink intra-band contiguous carrier aggregation, the maximum output power is specified in Table 6.2A.1.1-1.

For downlink intra-band contiguous carrier aggregation with a single uplink component carrier configured in the NR band, the maximum output power is specified in Table 6.2.1-1 for power class 3 and other power classes if indicated in clause 5.5A.1.

Table 6.2A.1.1-1: UE Power Class for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Class 1 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance (dB) | Class 3 (dBm) | Tolerance (dB) | Class 4 (dBm) | Tolerance (dB) |
| CA\_n7B |  |  |  |  | 23 | +2/-21 |  |  |
| CA\_n41C |  |  | 26 | +2/-31 | 23 | +2/-21 |  |  |
| CA\_n48B |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n77C |  |  | 26 | +2/-31 | 23 | +2/-3 |  |  |
| CA\_n78C |  |  | 26 | +2/-31 | 23 | +2/-3 |  |  |
| CA\_n79C |  |  |  |  | 23 | +2/-3 |  |  |
| NOTE 1: If all transmitted resource blocks over all component carriers are confined within FUL\_low and FUL\_low + 4 MHz or/and FUL\_high – 4 MHz and FUL\_high, the maximum output power requirement is relaxed by reducing the lower tolerance limit by 1.5 dB  NOTE 2: PPowerClass is the maximum UE power specified without taking into account the tolerance  NOTE 3: For intra-band contiguous carrier aggregation the maximum power requirement shall apply to the total transmitted power over all component carriers (per UE). | | | | | | | | |

#### 6.2A.1.2 UE maximum output power for Intra-band non-contiguous CA

For intra-band non-contiguous carrier aggregation with one uplink carrier on the PCC, the requirements in clause 6.2.1 apply for power class 3 and other power classes if indicated in clause 5.5A.2.

For intra-band non-contiguous carrier aggregation with two uplink carriers the maximum output power is specified in Table 6.2A.1.2-1.

Table 6.2A.1.2-1: UE Power Class for intraband non-contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Class 1 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance (dB) | Class 3 (dBm) | Tolerance (dB) | Class 4 (dBm) | Tolerance (dB) |
| CA\_n41(2A) |  |  |  |  | 23 | +2/-31 |  |  |
| CA\_n77(2A) |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n78(2A) |  |  |  |  | 23 | +2/-3 |  |  |
| NOTE 1: For transmission bandwidths confined within FUL\_low and FUL\_low + 4 MHz or FUL\_high – 4 MHz and FUL\_high, the maximum output power requirement is relaxed by reducing the lower tolerance limit by 1.5 dB  NOTE 2: PPowerClass is the maximum UE power specified without taking into account the tolerance  NOTE 3: For intra-band non-contiguous carrier aggregation the maximum power requirement shall apply to the total transmitted power over all component carriers (per UE). | | | | | | | | |

#### 6.2A.1.3 UE maximum output power for Inter-band CA

For inter-band downlink carrier aggregation with one uplink carrier assigned to one NR band, the transmitter power requirements in Table 6.2.1-1 apply for power class 3 and other power classes if indicated in clause 5.5A.3.

.

For inter-band carrier aggregation with two uplink contiguous carrier assigned to one NR band, the transmitter power requirements specified in subclause 6.2A.1.1 apply.

For inter-band carrier aggregation with two uplink non-contiguous carrier assigned to one NR band, the transmitter power requirements specified in subclause 6.2A.1.2 apply.

For inter-band uplink carrier aggregation with uplink assigned to two NR bands, UE maximum output power shall be measured over all component carriers from different bands. If each band has separate antenna connectors, maximum output power is defined as the sum of maximum output power from each UE antenna connector. The period of measurement shall be at least one sub frame (1 ms). The maximum output power is specified in Table 6.2A.1.3-1.

Table 6.2A.1.3-1 UE Power Class for uplink inter-band CA (two bands)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Uplink CA Configuration | Class 1 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance  (dB) | Class 3 (dBm) | Tolerance (dB) | Class 4 (dBm) | Tolerance (dB) |
| CA\_n1A-n3A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n5A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n7A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n8A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n18A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n28A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n40A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n41A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n74A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n1A-n78A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n1A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n5A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n7A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n12A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n14A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n30A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n48A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n2A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n2A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n5A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n7A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n8A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n18A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n28A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n34A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3-n38A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n40A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n41A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n3A-n74A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n3A-n78A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n3A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n7A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n12A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n14A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n25A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n30A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n48A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n5A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n5A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n7A-n25A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n7A-n28A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n7A-n46A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n7A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n7A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n7A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n34A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n39A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n40A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n41A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n8A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n12A-n30A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n12A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n12A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n13A-n25A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n13A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n13A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n14A-n30A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n14A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n14A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n18A-n28A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n18A-n41A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n18A-n74A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n18A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n18A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n20A-n28A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n20A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n24A-n41A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n24A-n48A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n24A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n25A-n38A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n25A-n41A |  |  | 266 | +2/-32 | 23 | +2/-3 |  |  |
| CA\_25A-n48A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n25A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n25A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n25A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n26A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n26A-n70A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n40A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n41A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n28A-n46A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n50A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n74A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n28A-n79A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n34A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n30A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n30A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n34A-n40A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n38A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n38A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n39A-n40A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n39A-n41A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n39A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n40A-n41A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n40A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n40A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n41A-n48A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n41A-n50A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n41A-n66A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n41A-n71A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n41A-n74A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n41A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n41A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n41A-n79A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n46A-n48A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n46A-n48B |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n46A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n48A-n66A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n48A-n70A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n48A-n71A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n48A-n96A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n48B-n96A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n50A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n66A-n71A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n66A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n66A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n70A-n71A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n71A-n77A |  |  | 266 | +2/-3 | 23 | +2/-3 |  |  |
| CA\_n71A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n74A-n77A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n74A-n78A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n77A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n78A-n79A |  |  |  |  | 23 | +2/-3 |  |  |
| CA\_n78A-n92A |  |  |  |  | 23 | +2/-3 |  |  |
| NOTE 1: Void  NOTE 2: An uplink CA configuration in which at least one of the bands has NOTE 3 in Table 6.2.1-1 is allowed to reduce the lower tolerance limit by 1.5 dB when the transmission bandwidths of at least one of the bands is confined within FUL\_low and FUL\_low + 4 MHz or FUL\_high - 4 MHz and FUL\_high.  NOTE 3: PPowerClass is the maximum UE power specified without taking into account the tolerance  NOTE 4: For inter-band carrier aggregation the maximum power requirement should apply to the total transmitted power over all component carriers (per UE).  NOTE 5: Power class 3 is the default power class unless otherwise stated.  NOTE 6: The UE supports PC3 within NR FDD band, and supports either PC3 or PC2 within NR TDD band. | | | | | | | | |

If a UE supports a different power class than the default UE power class for the band combination listed in Table 6.2A.1.3-1 and the supported power class enables the higher maximum output power than that of the default power class:

– if the field of UE capability maxUplinkDutyCycle-interBandCA-PC2 is not absent and the average percentage of uplink symbols transmitted in a certain evaluation period is larger than maxUplinkDutyCycle-interBandCA-PC2 as defined in TS 38.331 (The exact evaluation period is no less than one radio frame); or

– if the IE P-Max as defined in TS 38.331 [7] is provided and set to the maximum output power of the default power class or lower;

– shall apply all requirements for the default power class to the supported power class and set the configured transmitted power as specified in clause 6.2A.4;

– else;

– shall apply all requirements for the supported power class and set the configured transmitted power as specified in clause 6.2A.4 (regardless of the average percentage of uplink symbols if the field of UE capability *maxUplinkDutyCycle-interBandCA-PC2* is absent).

The average percentage of uplink symbols is defined as 50% × ( DutyNR, x /maxDutyNR,x + DutyNR, y /maxDutyNR,y, ). DutyNR, x, DutyNR, y represent the actual percentage of uplink symbols transmitted in the same evaluation period (The exact evaluation period is no less than one radio frame) for NR Band x, NR Band y respectively; maxDutyNR,x,maxDutyNR,y represent the field of UE capability *maxUplinkDutyCycle-PC2-FR1* per band as defined in TS 38.331. For NR Band x or NR Band y,

– if power class of one or both of the bands within the band combination is power class 2 and the corresponding UE capability maxUplinkDutyCycle-PC2-FR1 is absent;

– the corresponding maxDutyNR,x or maxDutyNR,y is equal to 50%;

– else if the band is configured with power class 3;

– the corresponding maxDutyNR,x or maxDutyNR,y is equal to 100%.

Table 6.2A.1.3-2 Void

#### 6.2A.1.4 Void

## <End of Changes>