**3GPP TSG-RAN4 Meeting #102-e *R4-22xxxxx***

**Electronic Meeting, Feb 21st - March 3rd 2022 revision of R4-2205927**

|  |
| --- |
| *CR-Form-v12.1* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** |  | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR for 38.101-1: Corrections related to PC2 and PC1.5 with DL CA |
|  |  |
| ***Source to WG:*** | T-Mobile USA, Interdigital, Skyworks Solutions, Inc. |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_PC2\_CA\_R17\_2BDL\_2BUL-Core |  | ***Date:*** | 2022-02-13 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Concerns were raised at RAN4#101-e that it was not clear if Ppowerclass or Ppowerclass,CA applied when UL CA was configured. Also, it was pointed out that UL CA for PC1.5 is mentioned but it does not exist yet. There were also some errors in the MSD tables identified. |
|  |  |
| ***Summary of change:*** | Corrects the Pcmax equations to change Ppowerclass to Ppowerclass,CA in a few places. Clarifies that the uplink CA clauses are identified as for uplink CA. Corrects errors in the MSD tables.  |
|  |  |
| ***Consequences if not approved:*** | Errors and inconsistencies remain in the spec |
|  |  |
| ***Clauses affected:*** | 6.2A.4, 6.2A.4.1, 6.2A.4.1.1, 6.2A.4.1.2, 6.2A.4.1.3, 7.3A.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev1 removed the changes to the clause titles. Also removed some unnecessary references to PC3 and PC2.  |

<First changed section>

### 6.2A.4 Configured output power for CA

#### 6.2A.4.1 Configured transmitted power level

##### 6.2A.4.1.1 Configured transmitted power for Intra-band contiguous CA

For uplink carrier aggregation the UE is allowed to set its configured maximum output power PCMAX,*c* for serving cell *c* and its total configured maximum output power PCMAX.

The configured maximum output power PCMAX,*c* on serving cell *c* shall be set as specified in clause 6.2.4, but with MPR*c* = MPR and A-MPR*c* = A-MPR with MPR and A-MPR as determined by subclause 6.2A.2 and 6.2A.3, respectively. For PH reporting the following exception applies: if the UE is configured with multiple uplink serving cells, the power PCMAX,*c* used for the purpose of PH reporting on first serving cell *c* = *c*1 does not consider for computation of the PH report transmissions on a second serving cell *c*2 as exempted in subclause 7.7.1 in [8]. There is one power management term for the UE, denoted P-MPR, and P-MPR*c* = P-MPR.

The total configured maximum output power PCMAX shall be set within the following bounds:

 PCMAX\_L ≤ PCMAX ≤ PCMAX\_H

For uplink intra-band contiguous carrier aggregation when same slot pattern is used in all aggregated serving cells,

 PCMAX\_L  = MIN{10 log10 ∑ pEMAX,c  - TC , PEMAX,CA,(PPowerClass,CA– ΔPPowerClass,CA) – MAX(MAX(MPR, A-MPR) + ΔTIB,c + TC + TRxSRS, P-MPRc ) }

 PCMAX\_H  = MIN{10 log10 ∑ pEMAX,c , PEMAX,CA ,PPowerClass,CA– ΔPPowerClass,CA }

where

- pEMAX,c is the linear value of PEMAX,*c* which is given by IE *P-Max* for serving cell *c* in [7];

- PPowerClass,CA is the maximum UE power specified in Table 6.2A.1.1-1 without taking into account the tolerance;

- MPR and A-MPR are specified in clause 6.2A.2 and 6.2A.3, respectively;

- ΔPPowerClass,CA = 3 dB for a power class 2 capable UE when 10 log10 ∑ pEMAX,c of 23 dBm or lower is indicated; or when PEMAX,CA of 23dBm or lower is indicated; or when the field of UE capability *maxUplinkDutyCycle-PC2-FR1* is absent and the percentage of total uplink symbols transmitted on all UL CCs in a certain evaluation period is larger than 50%; or when the field of UE capability *maxUplinkDutyCycle-PC2-FR1* is not absent and the percentage of total uplink symbols transmitted in a certain evaluation period is larger than *maxUplinkDutyCycle-PC2-FR1* as defined in TS 38.331 (The exact evaluation period is no less than one radio frame); otherwise ΔPPowerClass,CA = 0 dB;

- TIB,c is the additional tolerance for serving cell *c* as specified in clause 6.2A.4.2 for NR CA, clause 6.2C.2 for SUL, or TS 38.101-3 clause 6.2B.4.2 for EN-DC; In case the UE supports more than one of band combinations for CA, SUL or DC, and an operating band belongs to more than one band combinations then

a) When the operating band frequency range is ≤ 1 GHz, the applicable additional ∆TIB,c shall be the average value for all band combinations defined in clause 6.2A.4.2, 6.2C.2 in this specification and 6.2B.4.2 in TS 38.101-3 [3], truncated to one decimal place that apply for that operating band among the supported band combinations. In case there is a harmonic relation between low band UL and high band DL, then the maximum ∆TIB,c among the different supported band combinations involving such band shall be applied

b) When the operating band frequency range is > 1 GHz, the applicable additional ∆TIB,c shall be the maximum value for all band combinations defined in clause 6.2A.4.2, 6.2C.2 in this specification and 6.2B.4.2 in TS 38.101-3 [3] for the applicable operating bands.

- P-MPR is the power management term for the UE;

- TC is the highest value TC,c among all serving cells *c*;

- ∆TRxSRS is the highest value among all serving cells *c;*

- PEMAX,CA is the value indicated by *p-NR-FR1* or by *p-UE-FR1* whichever is the smallest if both are present*.*

For uplink intra-band contiguous carrier aggregation, when at least one different numerology/slot pattern is used in aggregated cells, the UE is allowed to set its configured maximum output power PCMAX,c(i),i for serving cell c(i) of slot numerology type *i*, and its total configured maximum output power PCMAX.

The configured maximum output power PCMAX,c(i),i (p) in slot p of serving cell c(i) on slot numerology type *i* shall be set within the following bounds:

PCMAX\_L,f,c(i),i (p) ≤ PCMAX,f,c(i), i (p) ≤ PCMAX\_H,f,c(i),i (p)

where PCMAX\_L,f,c (i),i (p) and PCMAX\_H,f,c(i),i (p) are the limits for a serving cell c(i) of slot numerology type i as specified in clause 6.2.4.

The total UE configured maximum output power PCMAX (p,q) in a slot p of slot numerology or symbol pattern *i*, and a slot q of slot numerology or symbol pattern *j* that overlap in time shall be set within the following bounds unless stated otherwise:

PCMAX\_L(p,q) ≤ PCMAX (p,q) ≤ PCMAX\_H (p,q)

When slots p and q have different transmissions lengths and belong to different cells on different or same bands:

PCMAX\_L (p,q) = MIN {10 log10 [pCMAX\_L,f,c(i),i (p) + pCMAX\_L,f,c(i),j (q)], PPowerClass,CA, PEMAX,CA}

PCMAX\_H (p,q) = MIN {10 log10 [pCMAX\_ H,f,c(i),i (p) + pCMAX\_ H,f,c(i),j (q)], PPowerClass,CA, PEMAX,CA}

where pCMAX\_L,f,c (i),i and pCMAX\_ H,f,c(i),i are the respective limits PCMAX\_L,f,c (i),i and PCMAX\_H,f,c(i),i expressed in linear scale.

TREF and Teval are specified in Table 6.2A.4.1.1-0 when same and different slot patterns are used in aggregated carriers. For each TREF, the PCMAX\_L is evaluated per Teval and given by the minimum value taken over the transmission(s) within the Teval; the minimum PCMAX\_L over the one or more Teval is then applied for the entire TREF. The lesser of PPowerClass,CA and PEMAX,CA shall not be exceeded by the UE during any period of time.

Table 6.2A.4.1.1-0: PCMAX evaluation window for different slot and channel durations

|  |  |  |
| --- | --- | --- |
| TREF | Teval | Teval with frequency hopping |
| TREF of largest slot duration over both UL CCs | Physical channel length | Min(Tno\_hopping, Physical Channel Length) |

If the UE is configured with multiple TAGs and transmissions of the UE on slot *i* for any serving cell in one TAG overlap some portion of the first symbol of the transmission on slot *i* +1 for a different serving cell in another TAG, the UE minimum of PCMAX\_L for slots *i* and *i* + 1 applies for any overlapping portion of slots *i* and *i* + 1. The lesser of PPowerClass,CA and PEMAX,CA shall not be exceeded by the UE during any period of time.

The measured maximum output power PUMAX over all serving cells with same slot pattern shall be within the following range:

 PCMAX\_L – MAX{TL, TLOW(PCMAX\_L) } ≤ PUMAX  ≤ PCMAX\_H + THIGH(PCMAX\_H)

 PUMAX = 10 log10 ∑ pUMAX,c

where pUMAX,c denotes the measured maximum output power for serving cell *c* expressed in linear scale. The tolerances TLOW(PCMAX) and THIGH(PCMAX) for applicable values of PCMAX are specified in Table 6.2A.4.1.1-1. The tolerance TL is the absolute value of the lower tolerance for applicable NR CA configuration as specified in Table 6.2A.1.1-1 for intra-band carrier aggregation.

The measured maximum output power PUMAX over all serving cells, when at least one slot has a different transmission numerology or slot pattern, shall be within the following range:

 P'CMAX\_L– MAX{TL, TLOW (P'CMAX\_L)} ≤ P'UMAX  ≤ P'CMAX\_H + THIGH (P'CMAX\_H)

 P'UMAX = 10 log10 ∑ p'UMAX,c

where p'UMAX,c denotes the average measured maximum output power for serving cell *c* expressed in linear scale over TREF. The tolerances TLOW(P'CMAX) and THIGH(P'CMAX) for applicable values of P'CMAX are specified in Table 6.2A.4.1.1-1 for intra-band carrier aggregation. The tolerance TL is the absolute value of the lower tolerance for applicable NR CA configuration as specified in Table 6.2A.1.1-1 for inter-band carrier aggregation.

where:

 P'CMAX\_L  = MIN{ MIN {10log10∑( pCMAX\_L,f,c(i),i), PPowerClass,CA} over all overlapping slots in TREF}

 P'CMAX\_H = MAX{ MIN{10 log10 ∑ pEMAX,c , PPowerClass,CA} over all overlapping slots in TREF}

Table 6.2A.4.1.1-1: PCMAX tolerance for uplink intra-band contiguous CA

|  |  |  |
| --- | --- | --- |
| PCMAX(dBm) | ToleranceTLOW(PCMAX)(dB) | ToleranceTHIGH(PCMAX)(dB) |
| 23 < PCMAX ≤ 26 | 3 | 2 |
| 21 ≤ PCMAX ≤ 23 | 2.0 |
| 20 ≤ PCMAX < 21 | 2.5 |
| 19 ≤ PCMAX < 20 | 3.5 |
| 18 ≤ PCMAX < 19 | 4.0 |
| 13 ≤ PCMAX < 18 | 5.0 |
| 8 ≤ PCMAX < 13 | 6.0 |
| -40 ≤ PCMAX < 8 | 7.0 |

##### 6.2A.4.1.2 Configured transmitted power for Intra-band non-contiguous CA

For uplink carrier aggregation the UE is allowed to set its configured maximum output power PCMAX,*c* for serving cell *c* and its total configured maximum output power PCMAX.

The configured maximum output power PCMAX,*c* on serving cell *c* shall be set as specified in subclause 6.2.4.

The configured maximum output power PCMAX,c on serving cell c shall be set as specified in subclause 6.2.4, but with MPRc = MPR and A-MPRc = A-MPR with MPR and A-MPR as determined by subclause 6.2A.2 and 6.2A.3, respectively. For PH reporting the following exception applies: if the UE is configured with multiple uplink serving cells, the power PCMAX,c used for the purpose of PH reporting on first serving cell c = c1 does not consider for computation of the PH report transmissions on a second serving cell c2 as exempted in subclause 7.7.1 in [8]. There is one power management term for the UE, denoted P-MPR, and P-MPR c = P-MPR.

The total configured maximum output power PCMAX shall be set within the following bounds:

 PCMAX\_L ≤ PCMAX ≤ PCMAX\_H

For uplink intra-band non-contiguous carrier aggregation when same slot pattern is used in all aggregated serving cells,

 PCMAX\_L  = MIN{10 log10 ∑ pEMAX,c  - TC , PEMAX,CA,PPowerClass,CA – MAX(MAX(MPRc, A-MPRc) + ΔTIB,c + TC + DTRxSRS, P-MPR) }

 PCMAX\_H  = MIN{10 log10 ∑ pEMAX,c , PEMAX,CA ,PPowerClass,CA}

where

- pEMAX,c is the linear value of PEMAX,*c* which is given by IE *P-Max* for serving cell *c* in [7];

- PPowerClass,CA is the maximum UE power specified in Table 6.2A.1.2-1 without taking into account the tolerance;

- MPR and A-MPR are specified in subclause 6.2A.2 and subclause 6.2A.3 respectively;

- TIB,c is the additional tolerance for serving cell *c* as specified in clause 6.2A.4.2 for NR CA, clause 6.2C.2 for SUL, or TS 38.101-3 clause 6.2B.4.2 for EN-DC; In case the UE supports more than one of band combinations for CA, SUL or DC, and an operating band belongs to more than one band combinations then

a) When the operating band frequency range is ≤ 1 GHz, the applicable additional ∆TIB,c shall be the average value for all band combinations defined in clause 6.2A.4.2, 6.2C.2 in this specification and 6.2B.4.2 in TS 38.101-3 [3], truncated to one decimal place that apply for that operating band among the supported band combinations. In case there is a harmonic relation between low band UL and high band DL, then the maximum ∆TIB,c among the different supported band combinations involving such band shall be applied

b) When the operating band frequency range is > 1 GHz, the applicable additional ∆TIB,c shall be the maximum value for all band combinations defined in clause 6.2A.4.2, 6.2C.2 in this specification and 6.2B.4.2 in TS 38.101-3 [3] for the applicable operating bands.

- P-MPR is the power management term for the UE;

- TC is the highest value TC,c among all serving cells *c*;

- ∆TRxSRS is the highest value among all serving cells *c;*

- PEMAX,CA is the value indicated by *p-NR-FR1* or by *p-UE-FR1* whichever is the smallest if both are present*.*

[For uplink intra-band non-contiguous carrier aggregation, when at least one different numerology/slot pattern is used in aggregated cells, the UE is allowed to set its configured maximum output power PCMAX,c(i),i for serving cell c(i) of slot numerology type *i*, and its total configured maximum output power PCMAX.

The configured maximum output power PCMAX,c(i),i (p) in slot p of serving cell c(i) on slot numerology type *i* shall be set within the following bounds:

 PCMAX\_L,f,c(i),i (p) ≤ PCMAX,f,c(i), i (p) ≤ PCMAX\_H,f,c(i),i (p)

where PCMAX\_L,f,c (i),i (p) and PCMAX\_H,f,c(i),i (p) are the limits for a serving cell c(i) of slot numerology type i as specified in subclause 6.2.4.

The total UE configured maximum output power PCMAX (p,q) in a slot p of slot numerology or symbol pattern *i*, and a slot q of slot numerology or symbol pattern *j* that overlap in time shall be set within the following bounds unless stated otherwise:

 PCMAX\_L(p,q) ≤ PCMAX (p,q) ≤ PCMAX\_H (p,q)

When slots p and q have different transmissions lengths and belong to different cells on different or same bands:

 PCMAX\_L (p,q) = MIN {10 log10 [pCMAX\_L,f,c(i),i (p) + pCMAX\_L,f,c(i),j (q)], PPowerClass,CA, PEMAX,CA}

 PCMAX\_H (p,q) = MIN {10 log10 [pCMAX\_ H,f,c(i),i (p) + pCMAX\_ H,f,c(i),j (q)], PPowerClass,CA, PEMAX,CA}

where pCMAX\_L,f,c (i),i and pCMAX\_ H,f,c(i),i are the respective limits PCMAX\_L,f,c (i),i and PCMAX\_H,f,c(i),i expressed in linear scale.]

TREF and Teval are specified in Table 6.2A.4.1.2-1 when same and different slot patterns are used in aggregated carriers. For each TREF, the PCMAX\_L is evaluated per Teval and given by the minimum value taken over the transmission(s) within the Teval; the minimum PCMAX\_L over the one or more Teval is then applied for the entire TREF. The lesser of PPowerClass,CA and PEMAX,CA shall not be exceeded by the UE during any period of time.

Table 6.2A.4.1.2-1: PCMAX evaluation window for different slot and channel durations

|  |  |  |
| --- | --- | --- |
| TREF | Teval | Teval with frequency hopping |
| TREF of largest slot duration over both UL CCs | Physical channel length | Min(Tno\_hopping, Physical Channel Length) |

If the UE is configured with multiple TAGs and transmissions of the UE on slot *i* for any serving cell in one TAG overlap some portion of the first symbol of the transmission on slot *i* +1 for a different serving cell in another TAG, the UE minimum of PCMAX\_L for slots *i* and *i* + 1 applies for any overlapping portion of slots *i* and *i* + 1. The lesser of PPowerClass,CA and PEMAX,CA shall not be exceeded by the UE during any period of time.

The measured maximum output power PUMAX over all serving cells with same slot pattern shall be within the following range:

 PCMAX\_L – MAX{TL, TLOW(PCMAX\_L) } ≤ PUMAX  ≤ PCMAX\_H + THIGH(PCMAX\_H)

 PUMAX = 10 log10 ∑ pUMAX,c

where pUMAX,c denotes the measured maximum output power for serving cell *c* expressed in linear scale. The tolerances TLOW(PCMAX) and THIGH(PCMAX) for applicable values of PCMAX are specified in Table 6.2A.4.1.2-2. The tolerance TL is the absolute value of the lower tolerance for applicable NR CA configuration as specified in Table 6.2A.1.2-1 for intra-band carrier aggregation.

The measured maximum output power PUMAX over all serving cells, when at least one slot has a different transmission numerology or slot pattern, shall be within the following range:

 P'CMAX\_L– MAX{TL, TLOW (P'CMAX\_L)} ≤ P'UMAX  ≤ P'CMAX\_H + THIGH (P'CMAX\_H)

 P'UMAX = 10 log10 ∑ p'UMAX,c

where p'UMAX,c denotes the average measured maximum output power for serving cell *c* expressed in linear scale over TREF. The tolerances TLOW(P'CMAX) and THIGH(P'CMAX) for applicable values of P'CMAX are specified in Table 6.2A.4.1.2-2 for intra-band carrier aggregation. The tolerance TL is the absolute value of the lower tolerance for applicable NR CA configuration as specified in Table 6.2A.1.2-2 for intra-band carrier aggregation.

where:

 P'CMAX\_L  = MIN{ MIN {10log10∑( pCMAX\_L,f,c(i),i), PPowerClass,CA} over all overlapping slots in TREF}

 P'CMAX\_H = MAX{ MIN{10 log10 ∑ pEMAX,c , PPowerClass,CA} over all overlapping slots in TREF}

Table 6.2A.4.1.2-2: PCMAX tolerance for uplink intra-band non-contiguous CA

|  |  |  |
| --- | --- | --- |
| PCMAX(dBm) | ToleranceTLOW(PCMAX)(dB) | ToleranceTHIGH(PCMAX)(dB) |
| 21 ≤ PCMAX ≤ 23 | 3.0 | 2.0 |
| 20 ≤ PCMAX < 21 | 2.5 |
| 19 ≤ PCMAX < 20 | 3.5 |
| 18 ≤ PCMAX < 19 | 4.0 |
| 13 ≤ PCMAX < 18 | 5.0 |
| 8 ≤ PCMAX < 13 | 6.0 |
| -40 ≤ PCMAX < 8 | 7.0 |

##### 6.2A.4.1.3 Configured transmitted power for Inter-band CA

For uplink carrier aggregation the UE is allowed to set its configured maximum output power PCMAX,*c* for serving cell *c* and its total configured maximum output power PCMAX.

The configured maximum output power PCMAX,*c* on serving cell *c* shall be set as specified in clause 6.2.4.

For uplink inter-band carrier aggregation, MPR*c* and A-MPR*c* apply per serving cell *c* and are specified in clause 6.2.2 and clause 6.2.3, respectively. P-MPR*c* accounts for power management for serving cell *c*. PCMAX,*c* is calculated under the assumption that the transmit power is increased independently on all component carriers.

The total configured maximum output power PCMAX shall be set within the following bounds:

 PCMAX\_L ≤ PCMAX ≤ PCMAX\_H

For uplink inter-band carrier aggregation with one serving cell c per operating band when same slot symbol pattern is used in all aggregated serving cells,

 PCMAX\_L = MIN {10log10∑ MIN [ pEMAX,c/(tC,c), pPowerClass.c/(MAX(mprc·∆mprc, a-mprc)·tC,c ·tIB,c·tRxSRS,c), pPowerClass,c/pmprc], PEMAX,CA, PPowerClass,CA-ΔPPowerClass, CA}

 PCMAX\_H = MIN{10 log10 ∑ pEMAX,c , PEMAX,CA, PPowerClass,CA-ΔPPowerClass, CA}

where

- pEMAX,c is the linear value of PEMAX, *c* which is given by IE *P-Max* for serving cell *c* in [7];

- PPowerClass,CA is the maximum UE power specified in Table 6.2A.1.3-1 without taking into account the tolerance specified in the Table 6.2A.1.3-1;

- pPowerClass,c is the linear value of the maximum UE power for serving cell *c* specified in Table 6.2.1-1 without taking into account the tolerance;

- ΔPPowerClass,CA = 3 dB for a power class 2 capable UE when the requirements of default power class are applied as specified in sub-clause 6.2.A.1.3; otherwise ΔPPowerClass,CA = 0 dB; - mpr *c* and a-mpr *c* are the linear values of MPR *c* and A-MPR *c* as specified in clause 6.2.2 and clause 6.2.3, respectively;

- ∆mpr *c* is the linear value of ∆MPR *c* as specified in clause 6.2.2;

- pmprc is the linear value of P-MPR*c*;

- ∆tRxSRS,c is the linear value of ∆TRxSRS,c;

- tC,c is the linear value of TC,ctC,c = 1.41 when NOTE 2 in Table 6.2A.1.3-1 applies for a serving cell *c*, otherwise tC,c = 1;

- tIB,c is the linear value of the inter-band relaxation term TIB,c of the serving cell *c* as specified in clause 6.2A.4.2 for NR CA, clause 6.2C.2 for SUL, or TS 38.101-3 clause 6.2B.4.2 for EN-DC; otherwise tIB,c In case the UE supports more than one of band combinations for CA, SUL or DC, and an operating band belongs to more than one band combinations then

a) When the operating band frequency range is ≤ 1 GHz, the applicable additional TIB,c shall be the average value for all band combinations defined in clause 6.2A.4.2, 6.2C.2 in this specification and 6.2B.4.2 in TS 38.101-3 [3], truncated to one decimal place that apply for that operating band among the supported band combinations. In case there is a harmonic relation between low band UL and high band DL, then the maximum ∆TIB,c among the different supported band combinations involving such band shall be applied

b) When the operating band frequency range is > 1 GHz, the applicable additional ∆TIB,c shall be the maximum value for all band combinations defined in clause 6.2A.4.2, 6.2C.2 in this specification and 6.2B.4.2 in TS 38.101-3 [3] for the applicable operating bands.

- PEMAX,CA is the value indicated by *p-NR-FR1* or by *p-UE-FR1* whichever is the smallest if both are present.For uplink inter-band carrier aggregation with one serving cell *c* per operating band when at least one different numerology/slot pattern is used in aggregated cells, the UE is allowed to set its configured maximum output power PCMAX,c(i),i for serving cell c(i) of slot numerology type *i*, and its total configured maximum output power PCMAX.

The configured maximum output power PCMAX,c(i),i (p) in slot p of serving cell c(i) on slot numerology type *i* shall be set within the following bounds:

PCMAX\_L,f,c(i),i (p) ≤ PCMAX,f,c(i), i (p) ≤ PCMAX\_H,f,c(i),i (p)

where PCMAX\_L,f,c (i),i (p) and PCMAX\_H,f,c(i),i (p) are the limits for a serving cell c(i) of slot numerology type i as specified in clause 6.2.4.

The total UE configured maximum output power PCMAX (p,q) in a slot p of slot numerology or symbol pattern *i*, and a slot q of slot numerology or symbol pattern *j* that overlap in time shall be set within the following bounds unless stated otherwise:

PCMAX\_L(p,q) ≤ PCMAX (p,q) ≤ PCMAX\_H (p,q)

When slots p and q have different transmissions lengths and belong to different cells on different bands:

PCMAX\_L (p,q) = MIN {10 log10 [pCMAX\_L,f,c(i),i (p) + pCMAX\_L,f,c(i),j (q)], PPowerClass,CA, PEMAX,CA}

PCMAX\_H (p,q) = MIN {10 log10 [pCMAX\_ H,f,c(i),i (p) + pCMAX\_ H,f,c(i),j (q)], PPowerClass,CA, PEMAX,CA}

where pCMAX\_L,f,c (i),i and pCMAX\_ H,f,c(i),i are the respective limits PCMAX\_L,f,c (i),i and PCMAX\_H,f,c(i),i expressed in linear scale.

For combinations of intra-band and inter-band carrier aggregation with UE configured for transmission on three serving cells (up to two contiguously aggregated carriers per operating band), the following apply:

For the case when p and q belong to the same band and k belongs to a different band, but p, q and k are of the same numerology and slot patterns.

 PCMAX\_L = MIN {10log10∑( pCMAX\_L, Bi), PEMAX,CA, PPowerClass.CA}

 PCMAX\_H = MIN{10 log10 ∑ pEMAX,c , PEMAX,CA, PPowerClass.CA}

Where

- pCMAX\_L, Bi is the linear values of PCMAX\_L specified for the specific operating band *Bi*.

- The linear value of PCMAX\_L specified for uplink intra-band contiguous carrier aggregation in subclause 6.2A.4.1.1 applies for operating band supporting two contiguous serving cells, designated by its band index *Bi*. The linear value of PCMAX\_L specified for single carrier in subclause 6.2.4 applies for operating band *Bj* supporting one serving cell.

For the case when p and q belong to the same band and are of the same numerology *i* and slot patterns (p,q),while k belong to a different band and is of different numerology *j* and/or slot pattern on the 3rd cell then:

PCMAX\_L (p,q,k) = MIN {10 log10 [pCMAX\_L,Bi,i(p,q) + pCMAX\_L,c(3),Bj,j(k)], PEMAX,CA, PPowerClass,CA}

PCMAX\_H (p,q,k) = MIN {10 log10 [pCMAX\_ H,Bi,i (p,q) + pCMAX\_ H,c(3), Bj,j(k)], PEMAX,CA, PPowerClass,CA}

Where

- pEMAX,c is the linear value of PEMAX, *c* which is given by IE *P-Max* for serving cell *c* in [7];

- PEMAX,CA is p-UE-FR1 value signalled by RRC and defined in [38.331];

- PPowerClass,CA is the maximum UE power specified in Table 6.2A.1.3-1 without taking into account the tolerance specified in the Table 6.2A.1.3-1 or Table 6.2F.1A.1-1 for shared spectrum bands;

- pCMAX\_L,c(3),Bj,j(k) and pCMAX\_ H,c(3), Bj,j(k)are the linear values of PCMAX\_L and PCMAX\_H respectively, specified for single carrier in subclause 6.2.4 and applies for operating band supporting one serving cell in the *Bj* band on numerology *j*, using slot pattern k;

- pCMAX\_L,Bi,i(p,q) and pCMAX\_ H,Bi,i (p,q) are the linear values of PCMAX\_L respectively PCMAX\_H for uplink intra-band contiguous carrier aggregation specified in subclause 6.2A.4.1.1 which applies for operating band *Bi* on numerology *i*, supporting two contiguous serving cells, using the same slot pattern (p,q).

TREF and Teval are specified in Table 6.2A.4.1.3-0 when same and different slot patterns are used in aggregated carriers. For each TREF, the PCMAX\_L is evaluated per Teval and given by the minimum value taken over the transmission(s) within the Teval; the minimum PCMAX\_L over the one or more Teval is then applied for the entire TREF. The lesser of PPowerClass,CA and PEMAX,CA shall not be exceeded by the UE during any period of time.

Table 6.2A.4.1.3-0: PCMAX evaluation window for different slot and channel durations

|  |  |  |
| --- | --- | --- |
| TREF | Teval | Teval with frequency hopping |
| TREF of largest slot duration over both UL CCs | Physical channel length | Min(Tno\_hopping, Physical Channel Length) |

If the UE is configured with multiple TAGs and transmissions of the UE on slot *i* for any serving cell in one TAG overlap some portion of the first symbol of the transmission on slot *i* +1 for a different serving cell in another TAG, the UE minimum of PCMAX\_L for slots *i* and *i* + 1 applies for any overlapping portion of slots *i* and *i* + 1. The lesser of PPowerClass,CA and PEMAX,CA shall not be exceeded by the UE during any period of time.

The measured maximum output power PUMAX over all serving cells with same slot pattern shall be within the following range:

 PCMAX\_L – MAX{TL, TLOW(PCMAX\_L) } ≤ PUMAX  ≤ PCMAX\_H + THIGH(PCMAX\_H)

 PUMAX = 10 log10 ∑ pUMAX,c

where pUMAX,c denotes the measured maximum output power for serving cell *c* expressed in linear scale. The tolerances TLOW(PCMAX) and THIGH(PCMAX) for applicable values of PCMAX are specified in Table 6.2A.4.1.3-1. The tolerance TL is the absolute value of the lower tolerance for applicable NR CA configuration as specified in Table 6.2A.1.3-1-2 for inter-band carrier aggregation.

The measured maximum output power PUMAX over all serving cells, when at least one slot has a different transmission numerology or symbol pattern, shall be within the following range:

 P'CMAX\_L– MAX{TL, TLOW (P'CMAX\_L)} ≤ P'UMAX  ≤ P'CMAX\_H + THIGH (P'CMAX\_H)

 P'UMAX = 10 log10 ∑ p'UMAX,c

where p'UMAX,c denotes the average measured maximum output power for serving cell *c* expressed in linear scale over TREF. The tolerances TLOW(P'CMAX) and THIGH(P'CMAX) for applicable values of P'CMAX are specified in Table 6.2A.4.1.3-1 for inter-band carrier aggregation. The tolerance TL is the absolute value of the lower tolerance for applicable NR CA configuration as specified in Table 6.2A.1.3-1 for inter-band carrier aggregation.

where:

 P'CMAX\_L  = MIN{ MIN {10log10∑( pCMAX\_L,f,c(i),i), PPowerClass,CA} over all overlapping slots in TREF}

 P'CMAX\_H = MAX{ MIN{10 log10 ∑ pEMAX,c , PPowerClass,CA} over all overlapping slots in TREF}

Table 6.2A.4.1.3-1: PCMAX tolerance for uplink inter-band CA (two bands)

|  |  |  |
| --- | --- | --- |
| PCMAX(dBm) | ToleranceTLOW(PCMAX)(dB) | ToleranceTHIGH(PCMAX)(dB) |
| 23 ≤ PCMAX ≤ 26 | 3.0 | 2.0 |
| 22 ≤ PCMAX < 23 | 5.0 | 2.0 |
| 21 ≤ PCMAX < 22 | 5.0 | 3.0 |
| 20 ≤ PCMAX < 21 | 6.0 | 4.0 |
| 16 ≤ PCMAX < 20 | 5.0 |
| 11 ≤ PCMAX < 16 | 6.0 |
| -40 ≤ PCMAX < 11 | 7.0 |

<Next changed section>

### 7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA

Sensitivity degradation is allowed for a band in frequency range 1 if it is impacted by UL harmonic interference from another band which belongs to NR band in frequency range 1 of the same downlink CA configuration. Reference sensitivity exceptions due to UL harmonic from a PC3 aggressor NR UL band for either single band uplink or PC3 or PC2 CA are specified in Table 7.3A.4-1 with uplink configuration specified in Table 7.3A.4-2.

Table 7.3A.4-1: Reference sensitivity exceptions due to UL harmonic from a PC3 aggressor NR UL band for NR DL CA FR1

|  |
| --- |
| MSD due to harmonic exception for the DL band |
| UL band | DL band | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | **70**MHz | 80 MHz | 90 MHz | 100 MHz |
|  |  | dB | dB | dB | dB | dB | dB | dB | dB | dB |  | dB | dB | dB |
| n1 | n771,2 |  | 23.9 | 22.1 | 20.9 |  |  | 17.9 | 16.8 | 16.0 |  | 14.8 | 14.3 | 13.8 |
|  | n773 |  | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n2 | n481, 2 | 27.1 | 23.9 | 22.1 | 20.9 |  |  | 17.9 | 16.912 | 16.112 |  | 14.812 | 14.312 | 13.812 |
|  | n483 | 1.9 | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n2 | n771,2 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.0 | 17.9 | 16.8 | 16.0 | 15.5 | 14.8 | 14.3 | 13.8 |
|  | n773 |  | 1.1 | 0.8 | 0.3 | 0.1 |  |  |  |  |  |  |  |  |
| 2 | n781,2 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.0 | 17.9 | 16.8 | 16.0 |  | 14.8 | 14.3 | 13.8 |
|  | n783 |  | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n3 | n771,2 |  | 23.9 | 22.1 | 20.9 |  |  | 17.9 | 16.9 | 16.1 |  | 14.8 | 14.3 | 13.8 |
|  | n773 |  | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
|  | n781,2 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.1 | 17.9 | 16.9 | 16.1 | 15.4 | 14.8 | 14.3 | 13.8 |
|  | n783 |  | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n5 | n774,5,13 |  | 10.5 | 8.9 | 7.8 | 7.2 | 6.5 | 5.1 | 4.2 | 3.5 | 2.8 | 2.3 | 2.1 | 1.4 |
| n5 | n776,7,13 |  | 10.4 | 8.9 | 7.8 | 6.7 | 6.0 | 4.7 | 3.7 | 3 | 2.3 | 1.7 | 1.2 | 0.7 |
| n5 | n784,5 |  | 10.5 | 8.9 | 7.8 | 7.1 | 6.5 | 5.4 | 4.2 | 3.5 | 2.9 | 2.3 | 2.1 | 1.4 |
| n8 | n311 | N/A | N/A | N/A | N/A | N/A | N/A |  |  |  |  |  |  |  |
|  | n78,9 | 10 | 7.5 | 6.2 | 5.5 | 4.4 | 3.6 | 2.4 | 0.8 |  |  |  |  |  |
|  | n418,9 |  | 13.0 | 11.3 | 10.1 |  |  | 7.0 | 6.1 | 5.5 |  | 4.3 | 3.9 | 3.5 |
|  | n774,5 |  | 10.8 | 9.1 | 8.0 | 7.2 | 6.5 | 5.1 | 4.2 | 3.5 | 2.9 | 2.3 | 2.1 | 1.4 |
|  | n784,5 |  | 10.8 | 9.1 | 8.0 | 7.2 | 6.5 | 5.1 | 4.2 | 3.5 |  | 2.3 | 2.1 | 1.4 |
|  | n796,7 |  |  |  |  |  |  | 6.8 | 6.2 | 5.6 |  | 4.9 |  | 4.4 |
| n12 | n486,7 |  | 10.4 | 8.9 | 7.8 |  | 6.5 | 4.7 |  |  |  |  |  |  |
|  | n668,9 | 10 | 7.5 | 6.2 | 5.5 | 4.4 | 3.6 | 2.4 |  |  |  |  |  |  |
|  | n776,7 |  | 10.4 | 8.9 | 7.8 | 6.7 | 6 | 4.7 | 3.7 | 3 | 2.3 | 1.7 | 1.2 | 0.7 |
| n13 | n776,7 |  | 10.4 | 8.9 | 7.8 | 6.7 | 6 | 4.7 | 3.7 | 3 | 2.3 | 1.7 | 1.2 | 0.7 |
| n14 | n776,7 |  | 10.4 | 8.9 | 7.8 | 6.7 | 6 | 4.7 | 3.7 | 3 | 2.3 | 1.7 | 1.2 | 0.7 |
| n18 | n776,7 |  | 10.4 | 8.9 | 7.8 |  |  | 4.7 | 3.7 | 3 |  | 1.7 | 1.2 | 0.7 |
| n20 | n784,5 |  | 10.8 | 9.1 | 8 |  |  | 6 | 4.0 | 3.2 |  | 2.0 | 1.5 | 1.0 |
| n24 | n771,2,13 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.0 | 17.9 | 16.8 | 16.0 | 15.5 | 14.8 | 14.3 | 13.8 |
|  | n773,13 |  | 1.1 | 0.8 | 0.3 | 0.1 |  |  |  |  |  |  |  |  |
| n25 | n481,2 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.0 | 17.9 | 16.8 | 16.0 | 15.5 | 14.812 | 14.312 | 13.812 |
|  | n483 |  | 1.1 | 0.8 | 0.3 | 0.1 |  |  |  |  |  |  |  |  |
| n25 | n771,2 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.0 | 17.9 | 16.8 | 16.0 | 15.5 | 14.8 | 14.3 | 13.8 |
|  | n773 |  | 1.1 | 0.8 | 0.3 | 0.1 |  |  |  |  |  |  |  |  |
| n25 | n781,2 |  | 23.9 | 22.1 | 20.9 |  |  | 17.9 | 16.8 | 16.0 |  | 14.8 | 14.3 | 13.8 |
|  | n783 |  | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n28 | n18,9 | 10.2 | 7.6 | 6.2 | 5.3 |  |  |  |  |  |  |  |  |  |
|  | n501,2 |  | 19.8 | 18.0 | 16.8 |  |  | 13.8 | 12.8 | 12.0 |  | 10.8 |  |  |
|  | n741,2 | 23.1 | 19.8 | 18 | 16.8 |  |  |  |  |  |  |  |  |  |
|  | n751,2 | 28.1 | 25.3 | 24.0 | 22.8 | 21.8 | 21.0 | 19.7 | 18.7 |  |  |  |  |  |
|  | n776,7 |  | 10.4 | 8.9 | 7.8 |  |  | 4.7 | 3.7 | 3 |  | 1.7 | 1.2 | 0.7 |
|  | n786,7 |  | 10.4 | 8.9 | 7.8 | 6.7 | 6 | 4.7 | 3.7 | 3 | 2.3 | 1.7 | 1.2 | 0.7 |
| n66 | n481,2 | 27.1 | 23.9 | 22.1 | 20.9 |  |  | 17.9 | 16.912 | 16.112 |  | 14.812 | 14.312 | 13.812 |
|  | n483 | 1.9 | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n66 | n771,2 |  | 23.9 | 22.1 | 20.9 | 19.8 | 19.0 | 17.9 | 16.8 | 16.0 | 15.5 | 14.8 | 14.3 | 13.8 |
|  | n773 |  | 1.1 | 0.8 | 0.3 | 0.1 |  |  |  |  |  |  |  |  |
| n66 | n781,2 |  | 23.9 | 22.1 | 20.9 |  |  | 17.9 | 16.8 | 16.0 |  | 14.8 | 14.3 | 13.8 |
|  | n783 |  | 1.1 | 0.8 | 0.3 |  |  |  |  |  |  |  |  |  |
| n71 | n2510 | 10 | 7.5 | 6 | 5.1 | 4.1 | 3.0 | 2.1 |  |  |  |  |  |  |
|  | n414,5 |  | 10.8 | 9.1 | 8.0 |  | 6.5 | 5.1 | 4.2 | 3.5 | 2.8 | 2.3 | 2.1 | 1.4 |
|  | n708,9 | 9.9 | 7.1 | 6.7 | 4.9 | 4.1 |  |  |  |  |  |  |  |  |
| n92 | n784,5 |  | 10.8 | 9.1 | 8 |  |  | 6 | 4.0 | 3.2 |  | 2.0 | 1.5 | 1.0 |
| NOTE 1: These requirements apply when there is at least one individual RE within the uplink transmission bandwidth of the aggressor (lower) band for which the 2nd transmitter harmonic is within the downlink transmission bandwidth of a victim (higher) band and a range ∆FHD above and below the edge of this downlink transmission bandwidth. The value ∆FHD depends on the band combination: ∆FHD = 10 MHz for CA\_n1-n77, CA\_n2-n78, CA\_n3-n77, CA\_n3-n78, CA\_n2-n48, CA\_n24-n77, CA\_n25-n48, CA\_n28-n74, CA\_n25-n78, CA\_n48-n66, CA\_n66-n78.NOTE 2: The requirements should be verified for UL NR-ARFCN of the aggressor (lower) band (superscript LB) such that in MHz and  with carrier frequency in the victim (higher) band in MHz and  the channel bandwidth configured in the lower band.NOTE 3: The requirements are only applicable to channel bandwidths no larger than 20 MHz and with a carrier frequency at  MHz offset from  in the victim (higher band) with , whereandare the channel bandwidths configured in the aggressor (lower) and victim (higher) bands in MHz, respectively.NOTE 4: These requirements apply when there is at least one individual RE within the uplink transmission bandwidth of a low band for which the 4th transmitter harmonic is within the downlink transmission bandwidth of a high band.NOTE 5: The requirements should be verified for UL NR‑ARFCN of a low band (superscript LB) such that in MHz and  with the carrier frequency of a high band in MHz and  the channel bandwidth configured in the low band.NOTE 6: These requirements apply when there is at least one individual RE within the uplink transmission bandwidth of a low band for which the 5th transmitter harmonic is within the downlink transmission bandwidth of a high band.NOTE 7: The requirements should be verified for UL NR‑ARFCN of a low band (superscript LB) such that in MHz and  with the carrier frequency of a high band in MHz and  the channel bandwidth configured in the low band.NOTE 8: These requirements apply when there is at least one individual RE within the uplink transmission bandwidth of the aggressor (lower) band for which the 3rd transmitter harmonic is within the downlink transmission bandwidth of a victim (higher) band.NOTE 9: The requirements should be verified for UL NR-ARFCN of the aggressor (lower) band (superscript LB) such that in MHz and  with carrier frequency in the victim (higher) band in MHz and  the channel bandwidth configured in the lower band.NOTE 10: These requirements apply when the lower edge frequency of the 10 MHz, 15 MHz, or 20 MHz uplink channel in Band 71 is located at or below 668 MHz and the downlink channel in Band n25 is located with its upper edge at 1995 MHz.NOTE 11: No requirements apply when there is at least one individual RE within the uplink transmission bandwidth of the low band for which the 2nd transmitter harmonic is within the downlink transmission bandwidth of the high band. The reference sensitivity for all active downlink component carriers is only verified when this is not the case (the requirements specified in clause 7.3.2 apply unless otherwise specified).NOTE 12: For these bandwidths, the minimum requirements are restricted to operation when carrier is configured as a downlink carrier part of CA configuration.NOTE 13: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped. |

Table 7.3A.4-1a: NR-U reference sensitivity measurement exclusion region in MHz.

|  |
| --- |
| NR Band / Harmonic order / Channel BW in UL |
| Band | Harmonic order | 5MHz | 10MHz | 15MHz | 20 MHz | 25 MHz | 30 MHz | 40MHz | 50 MHz |
| n7 | 2 | +/- 10 | +/- 20 | +/- 30 | +/- 40 | +/- 50 | +/- 60 | +/- 80 | +/- 100 |
| NOTE 1: Even though UL harmonic does not fall directly into NR-U band the exclusion region still applies.NOTE 2: The center of the exclusion region is obtained by multiplying the UL channel center frequency by the harmonic order. |

Table 7.3A.4-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for NR CA, FR1

|  |
| --- |
| NR Band / Channel bandwidth of the high band |
| UL band | DL band | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | n77 |  | 25 | 36 | 50 |  |  | 100 | 100 | 100 |  | 100 | 100 | 100 |
| n2 | n48 | 25 | 50 | 50 | 50 |  |  | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n2 | n77 |  | 25 | 36 | 50 | 50 | 50 | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n2 | n78 |  | 25 | 36 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 |
| n3 | n77 |  | 25 | 36 | 50 |  |  | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n3 | n78 |  | 25 | 36 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 |
| n5 | n77 |  | 16 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |
| n5 | n78 |  | 16 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |
| n8 | n7 | 8 | 16 | 25 | 25 | 25 | 25 | 25 | 25 |  |  |  |  |  |
| n8 | n41 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 |  | 25 | 25 | 25 |
| n8 | n77 |  | 16 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |
| n8 | n78 |  | 16 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |  | 25 | 25 | 25 |
| n8 | n79 |  |  |  |  |  |  | 25 | 25 | 25 |  | 25 |  | 25 |
| n12 | n48 |  | 10 | 15 | 20 |  | 25 | 25 |  |  |  |  |  |  |
| n12 | n66 | 8 | 16 | 20 | 20 | 20 | 20 | 20 |  |  |  |  |  |  |
| n12 | n77 |  | 10 | 15 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 |
| n13 | n77 |  | 10 | 15 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 |
| n14 | n77 |  | 10 | 15 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 | 20 |
| n18 | n77 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 |  | 25 | 25 | 25 |
| n20 | n78 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 |  | 25 | 25 | 25 |
| n24 | n77 | 12 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |
| n25 | n48 | 25 | 50 | 50 | 50 |  |  | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n25 | n77 |  | 25 | 36 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | 50 | n2 |
| n25 | n78 |  | 25 | 36 | 50 |  |  | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n28 | n1 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |  |
| n28 | n50 |  | 25 | 25 | 25 |  |  | 25 | 25 | 25 |  | 25 |  |  |
| n28 | n74 | 12 | 25 | 25 | 25 |  |  |  |  |  |  |  |  |  |
| n28 | n75 | 12 | 25 | 36 | 50 | 50 | 50 | 50 | 50 |  |  |  |  |  |
| n28 | n77 |  | 10 | 15 | 20 |  |  | 25 | 25 | 25 |  | 25 | 25 | 25 |
| n28 | n78 |  | 10 | 15 | 20 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |
| n66 | n48 | 12 | 25 | 36 | 50 |  |  | 100 | 128 | 160 |  | 200 | 200 | 200 |
| n66 | n77 |  | 25 | 36 | 50 | 64 | 80 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n66 | n78 |  | 25 | 36 | 50 |  |  | 100 | 100 | 100 |  | 100 | 100 | 100 |
| n71 | n25 | 84 | 84 | 84 | 84 | 84 | 84 | 84 |  |  |  |  |  |  |
| n71 | n41 |  | 16 | 25 | 25 |  | 25 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |
| n71 | n70 | 8 | 16 | 20 | 20 | 20 |  |  |  |  |  |  |  |  |
| n92 | n78 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 |  | 25 | 25 | 25 |
| NOTE 1: 15 kHz SCS is assumed for UL band.NOTE 2: The UL configuration applies regardless of the channel bandwidth of the low band unless the UL resource blocks exceed that specified in Table 7.3.2-3 for the uplink bandwidth in which case the allocation according to Table 7.3.2-3 applies.NOTE 3: Unless stated otherwise, UL resource blocks shall be centred within the transmission bandwidth configuration for the channel bandwidth.NOTE 4: These requirements apply when the lower edge frequency of the uplink channel in Band n71 is located at or below 668 MHz and the downlink channel in Band n25 is located with its upper edge at 1990 MHz. |

Table 7.3A.4-3: Void

Table 7.3A.4-3a: Void

Sensitivity degradation is allowed for a band if it is impacted by receiver harmonic mixing due to another band part which belongs to PC3 NR band or PC2 NR band of the same CA configuration. Reference sensitivity exceptions due to harmonic mixing from a PC3 aggressor NR UL band for either PC3 or PC2 CA are specified in Table 7.3A.4-4 and from a PC2 aggressor NR UL band for PC2 CA are specified in Table 7.3A.4-4a with uplink configuration specified in Table 7.3A.4-5.

Table 7.3A.4-4: Reference sensitivity exceptions due to harmonic mixing from a PC3 aggressor NR UL band for DL NR CA FR1

|  |
| --- |
| NR Band / Channel bandwidth of the affected DL band |
| UL band | DL band | 5 MHz(dB) | 10 MHz(dB) | 15 MHz(dB) | 20 MHz(dB) | 25 MHz(dB) | 30MHz(dB) | 40 MHz(dB) | 50 MHz(dB) | 60 MHz(dB) | 70MHz(dB) | 80 MHz(dB) | 90 MHz(dB) | 100 MHz(dB) |
| n25 | n713,4 | 26.5 | 23.3 | 20.9 | 15.3 |  |  |  |  |  |  |  |  |  |
| n40 | n284 | 37.8 | 34.8 | 33 | 30.3 |  |  |  |  |  |  |  |  |  |
| n40 | n781 |  | 8.3 | 8.0 | 6.9 |  |  | 3.9 | 3 | 2.3 |  | 1.2 |  | 0.4 |
| n413,4 | n18 | [24.3] | [24.3] | [22.5] |  |  |  |  |  |  |  |  |  |  |
| n41 | n481 |  | 8.3 | 8.0 | 6.9 |  |  | 3.9 | 3 | 2.3 |  | 1.2 |  | 0.4 |
| n41 | n781 |  | 8.3 | 8.0 | 6.9 |  |  | 3.9 | 3 | 2.3 |  | 1.2 |  | 0.4 |
| n46 | n71 | 8.3 | 7.1 | 6.4 | 5.5 | 4.3 | 3.1 | 1.5 | 0.6 |  |  |  |  |  |
| n46 | n781 |  | 19.5 | 17.8 | 16.6 | 15.6 | 14.8 | 14 | 13.1 | 12.6 | 12 | 12 | 12 | 12 |
| n77 | n2 | 6.7 | 5.0 | 4.0 | 3.7 |  |  |  |  |  |  |  |  |  |
| n77 | n5 | 5.7 | 4.0 | 3.0 | 2.7 |  |  |  |  |  |  |  |  |  |
| n77 | n125 | 31 | 28 | 26.2 |  |  |  |  |  |  |  |  |  |  |
| n77 | n135 | 31 | 28 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n145 | 31 | 28 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n25 | 6.7 | 5.0 | 4.0 | 3.7 |  |  |  |  |  |  |  |  |  |
| n776 | n295 | 31 | 28 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n302 | 10.4 | 8.0 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | 412 |  | 10.4 | 10.4 | 10.4 |  | 10.4 | 10.4 | 10.4 | 10.4 |  | 10.4 | 10.4 | 10.4 |
| n78 | n402 | 10.4 | 10.4 | 10.4 | 10.4 |  |  | 7.2 | 6.2 | 5.5 |  | 4.5 |  |  |
| n78 | n412 |  | 10.4 | 10.4 | 10.4 |  |  | 8.2 | 7.6 | 7.3 |  | 6.6 | 6.4 | 6.3 |
| NOTE 1: The requirements should be verified for UL NR-ARFCN of the aggressor (lower) band (superscript LB) such that in MHz and  with carrier frequency in the victim (higher) band in MHz and  the channel bandwidth configured in the lower band.NOTE 2: The requirements should be verified for UL NR-ARFCN of the aggressor (high) band (superscript HB) such that in MHz and  with carrier frequency in the victim (lower) band in MHz and  the channel bandwidth configured in the higher band.NOTE 3: These requirements apply when there is at least one individual RE within the downlink transmission bandwidth of the victim (lower) band for which the 3rd harmonic is within the uplink transmission bandwidth or the uplink adjacent channel's transmission bandwidth of an aggressor (higher) band.NOTE 4: The requirements should be verified for UL NR-ARFCN of the aggressor (higher) band (superscript HB) such that  in MHz and  with  the carrier frequency in the victim (lower) band and  the channel bandwidth configured in the higher band.NOTE 5: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and $f\_{UL}^{HB}$ the UL carrier frequency in the higher band, both in MHz.NOTE 6: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped. |

Table 7.3A.4-4a: Reference sensitivity exceptions due to harmonic mixing from a PC2 aggressor NR UL band for NR DL CA FR1

|  |
| --- |
| NR Band / Channel bandwidth of the affected DL band |
| UL band | DL band | 5 MHz(dB) | 10 MHz(dB) | 15 MHz(dB) | 20 MHz(dB) | 25 MHz(dB) | 30MHz(dB) | 40 MHz(dB) | 50 MHz(dB) | 60 MHz(dB) | 70MHz(dB) | 80 MHz(dB) | 90 MHz(dB) | 100 MHz(dB) |
| n77 | n2 | 9.1 | 8.0 | 7.0 | 6.7 |  |  |  |  |  |  |  |  |  |
| n77 | n121 | 34 | 31 | 29.2 |  |  |  |  |  |  |  |  |  |  |
| n77 | n141 | 34 | 31 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n25 | 9.1 | 8.0 | 7.0 | 6.7 |  |  |  |  |  |  |  |  |  |
| n78 | n3 | 8.1 | 6.1 | 4.8 | 4.3 | 3.8 | 3.4 | 1 |  |  |  |  |  |  |
| NOTE 1: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and $f\_{UL}^{HB}$ the UL carrier frequency in the higher band, both in MHz. |

Table 7.3A.4-5: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for DL CA in NR FR1

|  |
| --- |
| NR Band / SCS / Channel bandwidth of the affected DL band |
| UL band | DL band | SCS(kHz) | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30MHz | 40 MHz | 50 MHz | 60 MHz | 70MHz | 80 MHz | 90 MHz | 100 MHz |
| n25 | n71 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |  |
| n40 | n28 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |  |
| n40 | n78 | 30 |  | 24 | 24 | 24 |  |  | 24 | 24 | 24 |  | 24 |  | 24 |
| n41 | n18 | 15 | 25 | 50 | 75 |  |  |  |  |  |  |  |  |  |  |
| n41 | n48 | 30 |  | 24 | 24 | 24 |  |  | 24 | 24 | 24 |  | 24 |  | 24 |
| n41 | n78 | 30 |  | 24 | 24 | 24 |  |  | 24 | 24 | 24 |  | 24 |  | 24 |
| n46 | n7 | 15 | 12 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |  |  |  |  |  |
| n46 | n78 | 15 |  | 25 | 36 | 50 | 75 | 75 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n77 | n2 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |  |
| n77 | n5 | 25 | 25 | 20 | 20 |  |  |  |  |  |  |  |  |  |  |
| n77 | n12 | 15 | 25 | 50 | 75 |  |  |  |  |  |  |  |  |  |  |
| n77 | n13 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n14 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n25 | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 |  |  |  |  |  |  |
| n77 | n29 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n30 | 15 | 12 | 25 |  |  |  |  |  |  |  |  |  |  |  |
| n77 | 41 | 15 |  | 25 | 36 | 50 |  | 50 | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n78 | n3 | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 |  |  |  |  |  |  |
| n78 | n40 | 30 | 50 | 50 | 50 | 50 |  |  | 50 | 50 | 50 |  | 50 |  |  |
| n78 | n41 | 30 |  | 50 | 50 | 50 |  | 50 | 50 | 50 | 50 |  | 50 | 50 | 50 |
| NOTE 1: The UL configuration applies regardless of the channel bandwidth of the UL band unless the UL resource blocks exceed that specified in Table 7.3.2-3 for the uplink bandwidth in which case the allocation according to Table 7.3.2-3 applies. |

<Next changed section>

### 7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA

Sensitivity degradation is allowed for a band if it is impacted by UL of another band part which belongs to NR band of the same NR CA configuration due to cross band isolation issues. Reference sensitivity exceptions for the victim band due to cross band isolation from a PC3 aggressor NR UL band for either PC3 and PC2 NR CA are specified in Table 7.3A.6-1 and from a PC2 aggressor NR UL band for PC2 NR CA are specified in Table 7.3A.6-1a and from a PC1.5 aggressor NR single band uplink are specified in Table 7.3A.6-1b with uplink configuration specified in Table 7.3A.6-2.

Table 7.3A.6-1: Reference sensitivity exceptions (MSD) due to cross band isolation from a PC3 aggressor NR UL band for NR CA FR1

|  |
| --- |
| NR Band / Channel bandwidth of the affected DL band |
| UL band | DL band | 5MHz (dB) | 10MHz (dB) | 15MHz (dB) | 20MHz (dB) | 25MHz (dB) | 30 MHz (dB) | 40 MHz (dB) | 50 MHz (dB) | 60 MHz (dB) | 70MHz(dB) | 80 MHz (dB) | 90 MHz (dB) | 100 MHz (dB) |
| n1 | n3 | 3 | 2.2 | 1.9 | 1.7 | 1.6 | 1.5 | 1.4 |  |  |  |  |  |  |
| n1 | n40 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 |  | 6.6 |  |  |
| n1 | n41 |  | 6.1 | 6.1 | 6.1 |  | 6.1 | 6.1 | 6.1 | 6.1 |  | 6.1 | 6.1 | 6.1 |
| n3 | n41 |  | 0.7 | 0.7 | 0.7 |  | 0.7 | 0.7 | 0.7 | 0.7 |  | 0.7 | 0.7 | 0.7 |
| n3 | n74 | 2.6 | 2.6 | 2.6 | 2.6 |  |  |  |  |  |  |  |  |  |
| n5 | n28 | 8.2 | 6.2 | 5.1 | 3.6 |  | 0.4 |  |  |  |  |  |  |  |
| n7 | n3 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |
| n18 | n28 | [4.5] | [3] |  |  |  |  |  |  |  |  |  |  |  |
| n34 | n3 | 3 | 2.2 | 1.9 | 1.7 | 1.6 | 1.5 |  |  |  |  |  |  |  |
| n38 | n25 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |
| n38 | n78 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 | 4.3 | 4.0 | 3.9 | 3.8 |
| n40 | n1 | 8.3 | 8.3 | 8.3 | 8.3 |  |  |  |  |  |  |  |  |  |
| n41 | n1 | 9.1 | 9.1 | 9.1 | 9.1 | 9.1 | 9.1 | 9.1 | 9.1 |  |  |  |  |  |
| n41 | n3 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |  |
| n41 | n25 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |
| n41 | n48 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 | 4.3 | 4.0 | 3.9 | 3.8 |
| n411 | n66 | 3.5 | 3.5 | 3.5 | 3.5 | 3.5 | 3.5 | 3.5 |  |  |  |  |  |  |
| n41 | n77 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 | 4.3 | 4.0 | 3.9 | 3.8 |
| n41 | n78 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 | 4.3 | 4.0 | 3.9 | 3.8 |
| n46 | n78 |  | 10.4 | 8.8 | 7.8 | 7.8 | 7.8 | 7.8 | 7 | 6.5 | 6.0 | 5.7 | 5.4 | 5.1 |
| n48 | n411 |  | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 |
| n77 | n411 |  | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 |
| n78 | n71 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 |  |  |  |  |  |
| n78 | n38 | 3.3 | 3.3 | 3.3 | 3.3 | 3.3 | 3.3 | 3.3 |  |  |  |  |  |  |
| n78 | n401 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 |  | 4.5 |  |  |
| n78 | n411 |  | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 |
| n78 | n46 |  |  |  | 13.5 |  |  | 10.9 |  | 9.4 |  | 8.7 |  |  |
| n783 | n79 |  |  |  |  |  |  | 2 | 2 | 2 |  | 2 |  | 2 |
| n79 | n783 |  | 2.6 | 2.6 | 2.6 |  |  | 2.6 | 2.6 | 2.6 |  | 2.6 | 2.6 | 2.6 |
| NOTE 1: Applicable only when harmonic mixing MSD for this combination is not applied.NOTE 2: VoidNOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation.NOTE 4: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation. |

Table 7.3A.6-1a: Reference sensitivity exceptions (MSD) due to cross band isolation from a PC2 aggressor NR UL band for NR CA FR1

|  |
| --- |
| NR Band / Channel bandwidth of the affected DL band |
| UL band | DL band | 5MHz (dB) | 10MHz (dB) | 15MHz (dB) | 20MHz (dB) | 25MHz (dB) | 30 MHz (dB) | 40 MHz (dB) | 50 MHz (dB) | 60 MHz (dB) | 70MHz(dB) | 80 MHz (dB) | 90 MHz (dB) | 100 MHz (dB) |
| n41 | n3 | 2.3 | 2.3 | 2.3 | 2.3 | 2.3 | 2.3 | 2.3 |  |  |  |  |  |  |
| n41 | n25 | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 | 1.6 |  |  |  |  |  |  |
| n41 | n66 | 5.4 | 5.4 | 5.4 | 5.4 | 5.4 | 5.4 | 5.4 |  |  |  |  |  |  |
| n41 | n77 |  | 10.5 | 10.5 | 10.5 | 9.5 | 8.6 | 8.3 | 7.2 | 6.3 | 6.0 | 5.7 | 5.6 | 5.6 |
| n41 | n79 |  |  |  |  |  |  | 3.1 | 3.1 | 3.1 |  | 3.1 |  | 3.1 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n77 | n411 |  | 6.5 | 6.5 | 6.5 |  | 6.5 | 6.5 | 6.5 | 6.5 | 6.5 | 6.5 | 6.5 | 6.5 |
| n77 | n412 |  | 13.2 | 13.2 | 13.2 |  | 13.2 | 13.2 | 13.2 | 13.2 | 13.2 | 13.2 | 13.2 | 13.2 |
| n79 | n41 |  | 3.5 | 3.3 | 3.1 |  |  | 2.6 | 2.5 | 2.5 |  | 2.4 | 2.4 | 2.4 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: Applicable only when harmonic mixing MSD for this combination is not applied.NOTE 2: The requirements should be verified for UL NR-ARFCN of the aggressor (high) band (superscript HB) such that in MHz and  with carrier frequency in the victim (lower) band in MHz and  the channel bandwidth configured in the higher band. |

Table 7.3A.6-1b: Reference sensitivity exceptions (MSD) due to cross band isolation from a PC1.5 aggressor NR single UL band for DL NR CA FR1

|  |
| --- |
| NR Band / Channel bandwidth of the affected DL band |
| UL band | DL band | 5MHz (dB) | 10MHz (dB) | 15MHz (dB) | 20MHz (dB) | 25MHz (dB) | 30 MHz (dB) | 40 MHz (dB) | 50 MHz (dB) | 60 MHz (dB) | 70MHz(dB) | 80 MHz (dB) | 90 MHz (dB) | 100 MHz (dB) |
| n41 | n25 | 2.8 | 2.8 | 2.8 | 2.8 | 2.8 | 2.8 | 2.8 |  |  |  |  |  |  |
| n41 | n66 | 7.7 | 7.7 | 7.7 | 7.7 | 7.7 | 7.7 | 7.7 |  |  |  |  |  |  |
| n41 | n77 |  | 13.3 | 13.3 | 13.3 | 12.2 | 11.3 | 11.0 | 9.8 | 8.8 | 8.4 | 8.1 | 8.0 | 8.0 |

Table 7.3A.6.2: Uplink configuration for reference sensitivity exceptions due to cross band isolation for NR CA FR1

|  |
| --- |
| NR Band / SCS / Channel bandwidth of the affected DL band |
| UL band | DL band | SCS of UL band (kHz) | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | n3 | 15 | 25 | 25 | 25 | 25 | 25 | 25 | 25 |  |  |  |  |  |  |
| n1 | n40 | 15 | 25 | 50 | 75 | 100 | 100 | 100 | 100 | 100 | 100 |  | 100 |  |  |
| n1 | n41 | 15 |  | 100 | 100 | 100 |  | 100 | 100 | 100 | 100 |  | 100 | 100 | 100 |
| n3 | n41 | 15 |  | 50 | 50 | 50 |  | 50 | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n3 | n74 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |  |
| n5 | n28 | 15 | 20 | 20 | 20 | 20 |  | 20 |  |  |  |  |  |  |  |
| n7 | n3 | 15 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |
| n18 | n28 | 15 | 18 | 18 |  |  |  |  |  |  |  |  |  |  |  |
| n34 | n3 | 15 | 25 | 25 | 25 | 25 | 25 | 25 |  |  |  |  |  |  |  |
| n38 | n25 | 15 | 160 | 160 | 160 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |
| n38 | n78 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n40 | n1 | 30 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |  |
| n41 | n1 | 30 | 128 | 128 | 128 | 128 | 128 | 128 | 128 | 128 |  |  |  |  |  |
| n41 | n3 | 30 | 160 | 160 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |  |
| n41 | n25 | 15 | 160 | 160 | 160 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |
| n41 | n48 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n41 | n66 | 30 | 128 | 128 | 128 | 128 | 128 | 128 | 128 |  |  |  |  |  |  |
| n41 | n77 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n41 | n78 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n41 | n79 | 15 |  |  |  |  |  |  | 100 | 100 | 100 |  | 100 |  | 100 |
| n46 | n78 | 30 |  | 216 | 216 | 216 | 216 | 216 | 216 | 216 | 216 | 216 | 216 | 216 | 216 |
| n48 | n41 | 30 |  | 270 | 270 | 270 |  | 270 | 270 | 270 | 270 |  | 270 | 270 | 270 |
| n77 | n41 | 30 |  | 270 | 270 | 270 |  | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |
| n78 | n7 | 30 | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  |  |  |  |  |
| n78 | n38 | 30 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |
| n78 | n40 | 30 | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  | 270 |  |  |
| n78 | n41 | 30 |  | 270 | 270 | 270 |  | 270 | 270 | 270 | 270 |  | 270 | 270 | 270 |
| n78 | n46 | 15 |  |  |  | 216 |  |  | 216 |  | 216 |  | 216 |  |  |
| n783 | n79 | 30 |  |  |  |  |  | 270 | 270 | 270 | 270 |  | 270 |  | 270 |
| n79 | n41 | 30 |  | 270 | 270 | 270 |  | 270 | 270 | 270 | 270 |  | 270 | 270 | 270 |
| n79 | n783 | 30 |  | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  | 270 | 270 | 270 |
| NOTE 1: The UL configuration applies regardless of the channel bandwidth of the UL band unless the UL resource blocks exceed that specified in Table 7.3.2-3 for the uplink bandwidth in which case the allocation according to Table 7.3.2-3 applies.NOTE 2: Refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth in Table 5.3.2-1.NOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation. |

<End of changes>