**3GPP TSG-RAN4 Meeting #102-e *R4-2205360***

**Electronic Meeting, 21 February – 3 March, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **-** | **rev** | **-** | **Current version:** | **16.10.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR on CSI-RS measurement requirements R16 |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_CSIRS\_L3meas-Core |  | ***Date:*** | 2022-01-29 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In current requirements for intra-frequency CSI-RS measurement, the SFN reading time is defined for both FR1 and FR2. The requirement for FR2 is unclear because the referred “TSSB\_time\_index\_intra in Clause 9.2.5.1” is only defined for FR1. Moreover, it is specified that when deriveSSB-IndexFromCell is true (which is always the case for FR2), the time period for SFN reading is zero. |
|  |  |
| ***Summary of change:*** | Remove the requirements on SFN reading time for FR2. |
|  |  |
| ***Consequences if not approved:*** | It is confusing whether SFN reading time for FR2 is zero or not. |
|  |  |
| ***Clauses affected:*** | 9.10.2.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

#### 9.10.2.5 Intra-frequency measurements without measurement gaps

If a UE is configured with the higher layer parameters *CSI-RS-Resource-Mobility* and *associatedSSB*, the CSI-RS based measurement shall include PSS/SSS detection time of associatedSSB, the time period used to acquire the SFN information and CSI-RS based measurement period without gap.

PSS/SSS detection time of associatedSSB is the intra-frequency TPSS/SSS\_sync\_intra in Clause 9.2.5.1.

The time period used to acquire the SFN information is equal to 0 if the UE is indicated that the neighbour cell is synchronous with the serving cell (*deriveSSB-IndexFromCell* is enabled). Otherwise, the time period used to acquire the SFN information is TCSI-RS\_SFN\_intra as shown in Table 9.10.2.5-3 for FR1. It is assumed that *deriveSSB-IndexFromCell* is always enabled for FR1 TDD and FR2.

If the associatedSSB, which has been detectable at least for the time period Tidentify\_intra\_with\_index defined in clause 9.2.5.1, becomes undetectable for a period ≤ 5 seconds and then the associatedSSB becomes detectable again with the same spatial reception parameter provided the timing to that cell has not changed more than  3200 Tc, PSS/SSS detection time and time period used to acquire the SFN information are equal to 0.

The measurement period for CSI-RS based intra-frequency measurements without gaps is as shown in table 9.10.2.5-1and Table 9.10.2.5-2.

Additionally, for a given CSI-RS resource, if the associated SS/PBCH block is configured but not detected by the UE, or if CSI-RS is configured with associated SSB but not QCL-ed to the associated SSB, the UE is not required to monitor the corresponding CSI-RS resource.

Table 9.10.2.5-1: Measurement period for intra-frequency CSI-RS based measurements without gaps (FR1)

|  |  |
| --- | --- |
| DRX cycle | T CSI-RS\_measurement\_period\_intra  |
| No DRX | max(200ms, ceil( 5 x Kp\_CSI-RS) x CSI-RS period) x CSSFintra |
| DRX cycle≤ 320ms | max(200ms, ceil(1.5x 5 x Kp\_CSI-RS) x max(CSI-RS period, DRX cycle)) x CSSFintra |
| DRX cycle>320ms | ceil( 5 x Kp\_CSI-RS) x DRX cycle x CSSFintra |
| NOTE 1: The requirements apply assuming CSI-RS configuration with {D=3 with PRBs ≥ 48}. D is frequency domain density for the 1-port CSI-RS for L3 mobility defined in clause 7.4.1 of TS38.211 [6]. |

Table 9.10.2.5-2: Measurement period for intra-frequency CSI-RS based measurements without gaps (FR2)

|  |  |
| --- | --- |
| DRX cycle | T CSI-RS\_measurement\_period\_intra  |
| No DRX | max(400ms, ceil(Mmeas\_period\_w/o\_gaps x Kp\_CSI-RS) x CSI-RS period) x CSSFintra |
| DRX cycle≤ 320ms | max(400ms, ceil(1.5x Mmeas\_period\_w/o\_gaps x Kp\_CSI-RS) x max(CSI-RS period,DRX cycle)) x CSSFintra |
| DRX cycle>320ms | Mmeas\_period\_w/o\_gaps x DRX cycle x CSSFintra |
| NOTE 1: The requirements apply assuming CSI-RS configuration with {D=3 with PRBs ≥ 48}. D is frequency domain density for the 1-port CSI-RS for L3 mobility defined in clause 7.4.1 of TS38.211 [6]. |

Table 9.10.2.5-3: Time period for SFN acquisition for intra-frequency CSI-RS based measurements without gaps (FR1)

|  |  |
| --- | --- |
| DRX cycle | TCSI-RS\_SFN\_intra |
| No DRX | max(200ms, ceil(5 x Kp )x SMTC period)Note 1 x CSSFintra |
| DRX cycle≤ 320ms | max(2000ms, ceil (1.5 x 5 x Kp) x max(SMTC period,DRX cycle)) x CSSFintra |
| DRX cycle>320ms | Ceil(5 x Kp) x DRX cycle x CSSFintra |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identified |

Mmeas\_period\_w/o\_gaps : For a UE supporting power class 1, Mmeas\_period\_w/o\_gaps = 40. For a UE supporting FR2 power class 2, Mmeas\_period\_w/o\_gaps = 24. For a UE supporting power class 3, Mmeas\_period\_w/o\_gaps = 24. For a UE supporting power class 4, Mmeas\_period\_w/o\_gaps = 24.

CSSFintra: it is a carrier specific scaling factor and is determined according to CSSFoutside\_gap,i in clause 9.1.5.

- if intra-frequency CSI-RS resource is fully non overlapping with measurement gaps, Kp\_CSI-RS=1;

- if intra-frequency CSI-RS resource is partially overlapping with measurement gaps, Kp\_CSI-RS = 1/(1- (CSI-RS resource period /MGRP)), where CSI-RS resource period < MGRP.

<End of Change 1>