**3GPP TSG-RAN WG4 Meeting # 102-e R4-22XXXX**

**Electronic Meeting, February 21 – March 3, 2022**

**Agenda item:** 5.1.4

**Source:** CATT

**Title:** WF on CSI-RS based L3 measurement requirements

**Document for:** Approval

# Introduction

This is the WF to capture all the agreements and open issues in [102-e][206] Maintenance\_NR\_CSIRS\_L3meas\_NWM email discussion for RAN4#102e meeting.

# Sub-topic 1-1 UE behavior when the timing offset exceeds the threshold with single FFT assumption

**Issue 1-1-1 UE behavior when the timing offset exceeds the threshold with single FFT assumption**

* *Agreement:* 
  + UE is not required to report CSI-RS based L3 measurements. If UE reports CSI-RS based L3 measurement, then the UE **may not meet** CSI-RS based L3 measurement reporting requirements in TS 38.133 section 9.10.2.4 and 9.10.3.4 based on the accuracy requirements for the case when the timing offset is below the threshold
  + Do not define test cases to verify UE behavior for the case when the timing offset is above the threshold

# Reference

1. R4-22XXXX Email discussion summary for [102-e][206] Maintenance\_NR\_CSIRS\_L3meas\_NWM, CATT, RAN4#102e