**3GPP TSG- Meeting #**

**, 21 - 3, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Add the requirements for RLM/BFD for NR high speed train scenario in FR2 |
|  |  |
| ***Summary of change:*** | 1. Specify the requirements of RLM for FR2 HST
2. Specify the requirements of BFD for FR2 HST
 |
|  |  |
| ***Consequences if not approved:*** | The enhanced requirements for RLM/BFD are missing |
|  |  |
| ***Clauses affected:*** | 8.1.2.2 8.5.2.2 8.5.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

========================= First Change Request ===========================

<Unmodified text omitted >

### 8.1.2 Requirements for SSB based radio link monitoring

#### 8.1.2.1 Introduction

The requirements in this clause apply for each SSB based RLM-RS resource configured for PCell or PSCell, provided that the SSB configured for RLM is actually transmitted within UE active DL BWP during the entire evaluation period specified in clause 8.1.2.2.

Table 8.1.2.1-1: PDCCH transmission parameters for out-of-sync evaluation

|  |  |
| --- | --- |
| Attribute | Value for BLER Configuration #0 |
| DCI format | 1-0 |
| Number of control OFDM symbols | 2 |
| Aggregation level (CCE) | 8 |
| Ratio of hypothetical PDCCH RE energy to average SSS RE energy | 4dB |
| Ratio of hypothetical PDCCH DMRS energy to average SSS RE energy | 4dB |
| Bandwidth (PRBs) | 24 |
| Sub-carrier spacing (kHz) | SCS of the active DL BWP |
| DMRS precoder granularity | REG bundle size |
| REG bundle size | 6 |
| CP length | Normal |
| Mapping from REG to CCE | Distributed |

Table 8.1.2.1-2: PDCCH transmission parameters for in-sync evaluation

|  |  |
| --- | --- |
| Attribute | Value for BLER Configuration #0 |
| DCI payload size | 1-0 |
| Number of control OFDM symbols | 2 |
| Aggregation level (CCE) | 4 |
| Ratio of hypothetical PDCCH RE energy to average SSS RE energy | 0dB |
| Ratio of hypothetical PDCCH DMRS energy to average SSS RE energy | 0dB |
| Bandwidth (PRBs) | 24 |
| Sub-carrier spacing (kHz) | SCS of the active DL BWP |
| DMRS precoder granularity | REG bundle size |
| REG bundle size | 6 |
| CP length | Normal |
| Mapping from REG to CCE | Distributed |

#### 8.1.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_out\_SSB [ms] period becomes worse than the threshold Qout\_SSB within TEvaluate\_out\_SSB [ms] evaluation period.

UE shall be able to evaluate whether the downlink radio link quality on the configured RLM-RS resource estimated over the last TEvaluate\_in\_SSB [ms] period becomes better than the threshold Qin\_SSB within TEvaluate\_in\_SSB [ms] evaluation period.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in Table 8.1.2.2-1 for FR1.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in Table 8.1.2.2-2 for FR2 with scaling factor N=8, for FR2 power classes other than power class 6 or for FR2 class 6 when [*highSpeedMeasFlagFR2-r17*] is not configured.

TEvaluate\_out\_SSB and TEvaluate\_in\_SSB are defined in Table 8.1.2.2-3 for FR2 power class 6 UE configured with [*highSpeedMeasFlagFR2-r17*].

For FR1,

- $P=\frac{1}{1-\frac{T\_{SSB}}{MGRP}}$, when in the monitored cell there are measurement gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, and these measurement gaps are overlapping with some but not all occasions of the SSB; and

- P = 1 when in the monitored cell there are no measurement gaps overlapping with any occasion of the SSB.

For FR2,

- $P=\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when RLM-RS resource is not overlapped with measurement gap and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when the RLM-RS resource is not overlapped with measurement gap and RLM-RS resource is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- $P=\frac{1}{1-\frac{T\_{SSB}}{MGRP} - \frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when the RLM-RS resource is partially overlapped with measurement gap and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and

- TSMTCperiod ≠ MGRP or

- TSMTCperiod = MGRP and TSSB < 0.5\*TSMTCperiod

- $P=\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MGRP}}$, when the RLM-RS is partially overlapped with measurement gap and the RLM-RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and TSMTCperiod = MGRP and TSSB = 0.5 × TSMTCperiod

-- $P=\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when the RLM-RS resource is partially overlapped with measurement gap and the RLM-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with measurement gap

- $P=\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MRGP}}$, when the RLM-RS resource is partially overlapped with measurement gap and the RLM-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with measurement gap (TSMTCperiod < MGRP)

- Psharing factor = 1, if the RLM-RS resource outside measurement gap is

* not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,
* not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

where,

 If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.*

Longer evaluation period would be expected if the combination of RLM-RS resource, SMTC occasion and measurement gap configurations does not meet previous conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 8.1.2.2-1: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR1

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms)  | TEvaluate\_in\_SSB (ms)  |
| no DRX | Max(200, Ceil(10 × P) × TSSB) | Max(100, Ceil(5 × P) × TSSB) |
| DRX cycle≤320ms | Max(200, Ceil(15 × P) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P) × Max(TDRX,TSSB)) |
| DRX cycle>320ms | Ceil(10 × P) × TDRX | Ceil(5 × P) × TDRX |
| NOTE: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length. |

Table 8.1.2.2-2: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR2

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms)  | TEvaluate\_in\_SSB (ms)  |
| no DRX | Max(200, Ceil(10 × P × N) × TSSB) | Max(100, Ceil(5 × P × N) × TSSB) |
| DRX cycle≤320ms | Max(200, Ceil(15 × P × N) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P × N) × Max(TDRX,TSSB)) |
| DRX cycle>320ms | Ceil(10 × P × N) × TDRX | Ceil(5 × P × N) × TDRX |
| NOTE: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length. |

Table 8.1.2.2-3: Evaluation period TEvaluate\_out\_SSB and TEvaluate\_in\_SSB for FR2 power class 6 UE configured with [*highSpeedMeasFlagFR2-r17]*

|  |  |  |
| --- | --- | --- |
| Configuration | TEvaluate\_out\_SSB (ms)  | TEvaluate\_in\_SSB (ms)  |
| no DRX | Max(200, Ceil(10 × P × N Note2) × TSSB) | Max(100, Ceil(5 × P × N Note2) × TSSB) |
| DRX cycle≤80ms | Max(200, Ceil(15 × P × N Note2) × Max(TDRX,TSSB)) | Max(100, Ceil(7.5 × P × N Note2) × Max(TDRX,TSSB)) |
| NOTE 1: TSSB is the periodicity of the SSB configured for RLM. TDRX is the DRX cycle length.Note2: scaling factor N=2 when [highSpeedMeasFlagFR2-r17] is configured to [set1] or scaling factor N=6 when [highSpeedMeasFlagFR2-r17] is configured to [set2]. |

#### 8.1.2.3 Measurement restrictions for SSB based RLM

The UE is required to be capable of measuring SSB for RLM without measurement gaps. The UE is required to perform the SSB measurements with measurement restrictions as described in the following scenarios.

For FR1, when the SSB for RLM is in the same OFDM symbol as CSI-RS for RLM, BFD, CBD or L1-RSRP measurement,

- If SSB and CSI-RS have same SCS, UE shall be able to measure the SSB for RLM without any restriction;

- If SSB and CSI-RS have different SCS,

- If UE supports *simultaneousRxDataSSB-DiffNumerology*, UE shall be able to measure the SSB for RLM without any restriction;

- If UE does not support *simultaneousRxDataSSB-DiffNumerology*, UE is required to measure one of but not both SSB for RLM and CSI-RS. Longer measurement period for SSB based RLM is expected, and no requirements are defined.

For FR2, when the SSB for RLM measurement on one CC is in the same OFDM symbol as CSI-RS for RLM, BFD, CBD or L1-RSRP measurement on the same CC or different CCs in the same band, UE is required to measure one of but not both SSB for RLM and CSI-RS. Longer measurement period for SSB based RLM is expected, and no requirements are defined.

For FR2, there is no measurement restriction allowed when the network configures mixed numerology between SSB for RLM measurement on one FR2 band and CSI-RS for RLM, BFD, CBD, L1-RSRP or L1-SINR measurement on the other FR2 band, provided that UE is capable of independent beam management on this FR2 band pair.

========================= Second Change Request ===========================

<Unmodified text omitted >

### 8.5.2 Requirements for SSB based beam failure detection

#### 8.5.2.1 Introduction

The requirements in this clause apply for each SSB resource in the set  configured for a serving cell, provided that the SSB configured for beam failure detection is actually transmitted within the UE active DL BWP during the entire evaluation period specified in clause 8.5.2.2. The requirements in this clause could not be applicable if UE is required to perform beam failure detection on more than 1 serving cell per band.

Table 8.5.2.1-1: PDCCH transmission parameters for beam failure instance

|  |  |
| --- | --- |
| Attribute | Value for BLER |
| DCI format | 1-0 |
| Number of control OFDM symbols | 2 |
| Aggregation level (CCE) | 8 |
| Ratio of hypothetical PDCCH RE energy to average SSS RE energy | 0dB |
| Ratio of hypothetical PDCCH DMRS energy to average SSS RE energy | 0dB |
| Bandwidth (PRBs) | 24 |
| Sub-carrier spacing (kHz) | Same as the SCS of RMSI CORESET |
| DMRS precoder granularity | REG bundle size |
| REG bundle size | 6 |
| CP length | Normal |
| Mapping from REG to CCE | Distributed |

#### 8.5.2.2 Minimum requirement

UE shall be able to evaluate whether the downlink radio link quality on the configured SSB resource in set  estimated over the last TEvaluate\_BFD\_SSB ms period becomes worse than the threshold Qout\_LR\_SSB within TEvaluate\_BFD\_SSB ms period.

The value of TEvaluate\_BFD\_SSB is defined in Table 8.5.2.2-1 for FR1.

The value of TEvaluate\_BFD\_SSB is defined in Table 8.5.2.2-2 for FR2 with scaling factor N=8, for FR2 power classes other than power class 6 or for FR2 class 6 when [*highSpeedMeasFlagFR2-r17*] is not configured.

The value of TEvaluate\_BFD\_SSB is defined in Table 8.5.2.2-3 for FR2 power class 6 UE configured with [*highSpeedMeasFlagFR2-r17*].

For FR1,

- $P=\frac{1}{1-\frac{T\_{SSB}}{MGRP}}$, when in the monitored cell there are measurement gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB.

- P=1 when in the monitored cell there are no measurement gaps overlapping with any occasion of the SSB.

For FR2,

- $P=\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when BFD-RS resource is not overlapped with measurement gap and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P = Psharing factor, when the BFD-RS resource is not overlapped with measurement gap and the BFD-RS resource is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- $P=\frac{1}{1-\frac{T\_{SSB}}{MGRP} - \frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when the BFD-RS resource is partially overlapped with measurement gap and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and

- TSMTCperiod ≠ MGRP or

- TSMTCperiod = MGRP and TSSB < 0.5\*TSMTCperiod

- $P=\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MGRP}}$, when the BFD-RS resource is partially overlapped with measurement gap and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and TSMTCperiod = MGRP and TSSB = 0.5\*TSMTCperiod

- $P=\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when the BFD-RS resource is partially overlapped with measurement gap (TSSB <MGRP) and the BFD-RS resource is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with measurement gap.

- $P=\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MGRP}}$, when the BFD-RS resource is partially overlapped with measurement gap and the BFD-RS resource is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with measurement gap (TSMTCperiod < MGRP)

- Psharing factor = 1, if the BFD-RS resource outside measurement gap is

- not overlapped with the SSB symbols indicated by SSB-ToMeasure and 1 data symbol before each consecutive SSB symbols indicated by SSB-ToMeasure and 1 data symbol after each consecutive SSB symbols indicated by SSB-ToMeasure, given that SSB-ToMeasure is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and;

- not overlapped with the RSSI symbols indicated by ss-RSSI-Measurement and 1 data symbol before each RSSI symbol indicated by ss-RSSI-Measurement and 1 data symbol after each RSSI symbol indicated by ss-RSSI-Measurement, given that ss-RSSI-Measurement is configured.- Psharing factor = 3, otherwise.

where,

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, given the SMTC offset of all CCs in FR2 provided the same offset.

Longer evaluation period would be expected if the combination of BFD-RS resource, SMTC occasion and measurement gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer BFD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 8.5.2.2-1: Evaluation period TEvaluate\_BFD\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms)  |
| no DRX | Max(50, Ceil(5 × P) × TSSB) |
| DRX cycle ≤ 320ms | Max(50, Ceil(7.5 × P) × Max(TDRX,TSSB)) |
| DRX cycle > 320ms | Ceil(5 × P) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

Table 8.5.2.2-2: Evaluation period TEvaluate\_BFD\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms)  |
| no DRX | Max(50, Ceil(5 × P × N) × TSSB) |
| DRX cycle ≤ 320ms | Max(50, Ceil(7.5 × P × N) × Max(TDRX,TSSB)) |
| DRX cycle > 320ms | Ceil(5 × P × N) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

Table 8.5.2.2-3: Evaluation period TEvaluate\_BFD\_SSB for FR2 power class 6 UE configured with [*highSpeedMeasFlagFR2-r17]*

|  |  |
| --- | --- |
| Configuration | TEvaluate\_BFD\_SSB (ms)  |
| no DRX | Max(50, Ceil(5 × P × N Note2) × TSSB) |
| DRX cycle ≤ 80ms | Max(50, Ceil(7.5 × P × N Note2) × Max(TDRX,TSSB)) |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length.Note2: scaling factor N=2 when [highSpeedMeasFlagFR2-r17] is configured to [set1] or scaling factor N=6 when [highSpeedMeasFlagFR2-r17] is configured to [set2]. |

#### 8.5.2.3 Measurement restriction for SSB based beam failure detection

The UE is required to be capable of measuring SSB for BFD without measurement gaps. The UE is required to perform the SSB measurements with measurement restrictions as described in the following scenarios.

For FR1, when the SSB for BFD measurement is in the same OFDM symbol as CSI-RS for RLM, BFD, CBD or L1-RSRP measurement,

- If SSB and CSI-RS have same SCS, UE shall be able to measure the SSB for BFD measurement without any restriction;

- If SSB and CSI-RS have different SCS,

- If UE supports *simultaneousRxDataSSB-DiffNumerology*, UE shall be able to measure the SSB for BFD measurement without any restriction;

- If UE does not support *simultaneousRxDataSSB-DiffNumerology*, UE is required to measure one of but not both SSB for BFD measurement and CSI-RS. Longer measurement period for SSB based BFD measurement is expected, and no requirements are defined.

For FR2, when the SSB for BFD measurement on one CC is in the same OFDM symbol as CSI-RS for RLM, BFD, CBD or L1-RSRP measurement on the same CC or different CCs in the same band, UE is required to measure one of but not both SSB for BFD measurement and CSI-RS. Longer measurement period for SSB based BFD measurement is expected, and no requirements are defined.

For FR2, if the network configures same or mixed numerology between SSB for BFD measurement on one FR2 band and CSI-RS for RLM, BFD, CBD, L1-RSRP or L1-SINR measurement on the other FR2 band, UE shall be able to perform the related SSB based measurements in one band without any measurement restrictions on the other band, provided that UE is capable of independent beam management on this FR2 band pair.

========================= Second Change Request ===========================

<Unmodified text omitted >

### 8.5.5 Requirements for SSB based candidate beam detection

#### 8.5.5.1 Introduction

The requirements in this clause apply for each SSB resource in the set  configured for a serving cell, provided that the SSBs configured for candidate beam detection are actually transmitted within UE active DL BWP during the entire evaluation period specified in clause 8.5.5.2. The requirements in this clause apply when UE is required to perform beam failure detection on no more than 1 serving cell per band.

#### 8.5.5.2 Minimum requirement

Upon request the UE shall be able to evaluate whether the L1-RSRP measured on the configured SSB resource in set  estimated over the last TEvaluate\_CBD\_SSB ms period becomes better than the threshold Qin\_LR provided SSB\_RP and SSB Ês/Iot are according to Annex Table B.2.4.1 for a corresponding band.

The UE shall monitor the configured SSB resources using the evaluation period in table 8.5.5.2-1 and 8.5.5.2-2 corresponding to the non-DRX mode, if the configured DRX cycle ≤ 320ms.

The value of TEvaluate\_CBD\_SSB is defined in Table 8.5.5.2-1 for FR1.

The value of TEvaluate\_CBD\_SSB is defined in Table 8.5.5.2-2 for FR2 with scaling factor N=8.

where,

For FR1,

- $P=\frac{1}{1-\frac{T\_{SSB}}{MGRP}}$, when in the monitored cell there are measurement gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB,

- P = 1 when in the monitored cell there are no measurement gaps overlapping with any occasion of the SSB.

For FR2,

- $P=\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when candidate beam detection RS is not overlapped with measurement gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when candidate beam detection RS is not overlapped with measurement gap and candidate beam detection RS is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- $P=\frac{1}{1-\frac{T\_{SSB}}{MGRP} - \frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when candidate beam detection RS is partially overlapped with measurement gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and

- TSMTCperiod ≠ MGRP or

- TSMTCperiod = MGRP and TSSB < 0.5 × TSMTCperiod

- $P=\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MGRP}}$, when candidate beam detection RS is partially overlapped with measurement gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and TSMTCperiod = MGRP and TSSB = 0.5 × TSMTCperiod

- $P=\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when candidate beam detection RS is partially overlapped with measurement gap and candidate beam detection RS is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with measurement gap

- $P=\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MGRP}}$, when candidate beam detection RS is partially overlapped with measurement gap and candidate beam detection RS is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with measurement gap (TSMTCperiod < MGRP)

- Psharing factor = 1, if the candidate beam detection RS outside measurement gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and;

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured

- Psharing factor = 3, otherwise.

where,

 If the high layer in TS 38.331 [2] signaling of *smtc2*is present, TSMTCperiod follows *smtc2*; Otherwise TSMTCperiod follows *smtc1.* TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

Longer evaluation period would be expected if the combination of the CBD-RS resource, SMTC occasion and measurement gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer CBD evaluation period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

The values of PCBD used in Table 8.5.5.2-1 and Table 8.5.5.2-2 are defined as

 For each SSB resource in the set  configured for PCell or PSCell in EN-DC or NE-DC or SA; or PCell in NR-DC

- PCBD = 1.

For each SSB resource in the set  configured for PSCell in NR-DC

- PCBD = 2 if UE is configured for candidate beam detection on SCell, 1 otherwise.

 For each SSB resource in the set  configured for a SCell

- PCBD = Z in EN-DC or NE-DC or SA.

- PCBD = 2\* Z in NR-DC.

 Where Z is the number of band(s) on which UE is performing beam failure detection only for SCell

- PCBD is the number of band(s) on which UE is performing candidate beam detection only for SCell.

**Table 8.5.5.2-1: Evaluation period TEvaluate\_CBD\_SSB for FR1**

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_CBD\_SSB (ms)**  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil(3 × P × PCBD) × TSSB) |
| DRX cycle > 320ms | Ceil(3 × P × PCBD) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |

**Table 8.5.5.2-2: Evaluation period TEvaluate\_CBD\_SSB for FR2**

|  |  |
| --- | --- |
| **Configuration** | **TEvaluate\_CBD\_SSB (ms)**  |
| non-DRX, DRX cycle ≤ 320ms | Max(25, Ceil(3 × P × N × PCBD) × TSSB) |
| DRX cycle > 320ms | Ceil(3 × P × N × PCBD) × TDRX |
| Note: TSSB is the periodicity of SSB in the set . TDRX is the DRX cycle length. |