**3GPP TSG-RAN WG4 Meeting #102-e *R4-2204490***

**Electronic Meeting, 21st Feb –3rd Mar, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **-** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR for L1-RSRP measurements for Reporting for HST FR2 |
|  |  |
| ***Source to WG:*** | ZTE |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_HST\_FR2 -Core |  | ***Date:*** | 2022-02-10 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Introduction of requirements enhancements for L1-RSRP measurements for Reporting for NR high speed train scenario in FR2 |
|  |  |
| ***Summary of change:*** | Requirements enhancements for L1-RSRP measurements for Reporting for FR2 with high speed configuration |
|  |  |
| ***Consequences if not approved:*** | No requirements for FR2 in HST scenario |
|  |  |
| ***Clauses affected:*** | 9.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.533 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

< Start of change #1 >

# 9 Measurement Procedure

## 9.5 L1-RSRP measurements for Reporting

### 9.5.4 L1-RSRP measurement requirements

#### 9.5.4.1 SSB based L1-RSRP Reporting

The UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB.

The value of TL1-RSRP\_Measurement\_Period\_SSB is defined in Table 9.5.4.1-1 for FR1. The value of TL1-RSRP\_Measurement\_Period\_SSB is defined in Table 9.5.4.1-2 for FR2 when [*highSpeedMeasFlagFR2-r17*] is not configured or [*highSpeedMeasFlagFR2-r17*] is configured with SMTC period > 40ms for power class 6 UE, and defined in Table 9.5.4.1-3 for FR2 power class 6 UE when [*highSpeedMeasFlagFR2-r17*] is configured with SMTC period <= 40, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- N= 8 in Table 9.5.4.1-2.

For FR1,

- P=$\frac{1}{1-\frac{T\_{SSB}}{MRGP}}$, when in the monitored cell there are measurement gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB; and

- P=1 when in the monitored cell there are no measurement gaps overlapping with any occasion of the SSB.

For FR2,

- P=$\frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when SSB is not overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is Psharing factor, when SSB is not overlapped with measurement gap and SSB is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- P=$\frac{1}{1-\frac{T\_{SSB}}{MGRP}-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when SSB is partially overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and

- TSMTCperiod ≠ MGRP or

- TSMTCperiod = MGRP and TSSB < 0.5\*TSMTCperiod

- P is $\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MGRP}}$, when SSB is partially overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and TSMTCperiod = MGRP and TSSB = 0.5\*TSMTCperiod

- P=$ \frac{1}{1-\frac{T\_{SSB}}{\_{}\_{}}}$, when S SSB is partially overlapped with measurement gap (TSSB <MGRP) and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with measurement gap.

- P is $ \frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{MRGP}}$, when SSB is partially overlapped with measurement gap and SSB is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with measurement gap (TSMTCperiod < MGRP)

- Psharing factor = 1, if the SSB configured for L1-RSRP measurement outside measurement gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured,

- Psharing factor = 3, otherwise.

Where:

- TSSB = ssb-periodicityServingCell

- TSMTCperiod = the configured SMTC period

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and measurement gap configurations does not meet pervious conditions.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer L1 RSRP measurement period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 9.5.4.1-1: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: K = 1 when TSSB ≤ 40 ms and *highSpeedMeasFlag-r16* are configured; otherwise K = 1.5.Note 3: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *[intraRAT-MeasurementEnhancement-r16].* |

Table 9.5.4.1-2: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. |

Table 9.5.4.1-3: Measurement period TL1-RSRP\_Measurement\_Period\_SSB configured with [*highSpeedMeasFlagFR2-r17*] and SMTC period <= 40ms for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*NNote2)\*TSSB) |
| DRX cycle ≤ 80ms | max(TReport, ceil(M\*P\*NNote2\*M2)\*max(TDRX,TSSB))  |
| Note1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: N = 2 when [*highSpeedMeasFlagFR2-r17*] = [set1]; N = 6 when [*highSpeedMeasFlagFR2-r17*] = [set2]. |

### 9.5.6 Scheduling availability of UE during L1-RSRP measurement

Scheduling availability restrictions when the UE is performing L1-RSRP measurement are described in the following clauses.

#### 9.5.6.3 Scheduling availability of UE performing L1-RSRP measurement on FR2

The following scheduling restriction applies due to L1-RSRP measurement.

- For the case where RS for L1-RSRP measurement is CSI-RS which is QCLed with active TCI state for PDCCH/PDSCH and not in a CSI-RS resource set with repetition ON, and N=1 applies as specified in clause 9.5.4.2

- There are no scheduling restrictions due to L1-RSRP measurement performed based on the CSI-RS.

- Otherwise

- In non-HST scenario, ~~T~~the UE is not expected to transmit PUCCH/PUSCH/SRS or receive PDCCH/PDSCH/CSI-RS for tracking/CSI-RS for CQI on

- symbols corresponding to the SSB indexes configured for L1-RSRP measurement, and/or

- symbols corresponding to the periodic CSI-RS resource configured for L1-RSRP measurement, and/or

- symbols corresponding to the semi-perssitent CSI-RS resource configured for L1-RSRP measurement when the resource is activated, and/or

- symbols corresponding to the aperiodic CSI-RS resource configured for L1-RSRP measurement when the reporting is triggered.

- In HST scenario, the UE is not expected to transmit PUCCH/PUSCH/SRS or receive PDCCH/PDSCH/CSI-RS for tracking/CSI-RS for CQI on

- symbols corresponding to the SSB indexes configured for L1-RSRP measurement and 1 data symbol before each consecutive SSB symbols to be measured for L1-RSRP and 1 data symbol after each consecutive SSB symbols to be measured for L1-RSRP, and/or

- symbols corresponding to the periodic CSI-RS resource configured for L1-RSRP measurement and 1 data symbol before each periodic CSI-RS resource to be measured for L1-RSRP and 1 data symbol after each periodic CSI-RS for L1-RSRP measurement symbols to be measured for L1-RSRP , and/or

- symbols corresponding to the semi-perssitent CSI-RS resource configured for L1-RSRP measurement and 1 data symbol before each semi-perssitent CSI-RS resource to be measured for L1-RSRP and 1 data symbol after each semi-perssitent CSI-RS resource to be measured for L1-RSRP when the resource is activated, and/or

- symbols corresponding to the aperiodic CSI-RS resource configured for L1-RSRP measurement and 1 data symbol before each aperiodic CSI-RS resource to be measured for L1-RSRP measurement and 1 data symbol after each aperiodic CSI-RS resource to be measured for L1-RSRP measurement when the reporting is triggered.

When intra-band carrier aggregation in FR2 is performed, the scheduling restrictions on serving cell where L1-RSRP measurement is performed apply to all serving cells in the band on the symbols that fully or partially overlap with restricted symbols.

When inter-band carrier aggregation in FR2 is performed, there are no scheduling restrictions on FR2 serving cells in the bands due to L1-RSRP measurement performed on FR2 serving cell(s) in different band(s), provided that UE is capable of independent beam management on this FR2 band pair. Additionally, there is no scheduling restriction if the UE is configured with different numerology between SSB on one FR2 band and data on the other FR2 band provided the UE is configured for IBM operation for the band pair.

If following conditions are met,

- UE has been notified about system information update through paging,

- The gap between UE’s reception of PDCCH that UE monitors in the Type 2-PDCCH CSS set and that notifies system information update, and the PDCCH that UE monitors in the Type0-PDCCH CSS set, is greater than 2 slots,

For the SSB and CORESET for RMSI scheduling multiplexing patterns 3, UE is expected to receive the PDCCH that UE monitors in the Type0-PDCCH CSS set, and the corresponding PDSCH, on SSB symbols to be measured for L1-RSRP measurement; and

For the SSB and CORESET for RMSI scheduling multiplexing patterns 2, UE is expected to receive PDSCH that corresponds to the PDCCH that UE monitors in the Type0-PDCCH CSS set, on SSB symbols to be measured for L1-RSRP measurement.

< End of change #1 >