**3GPP TSG-<TSG/WG> Meeting # 102-e *<R4-22xxxxx>***

**Electronic Meeting, Feb 21st – Mar 3rd, 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** |  | **rev** | **1** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for Rel-16 TS 38.101-4: Modification on test setup for CSI requirments |
|  |  |
| ***Source to WG:*** | Huawei,HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Perf |  | ***Date:*** | 2022-02-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | There are two set of repeated parameters in table 6.3.3.2.1-1. |
|  |  |
| ***Summary of change:*** | Delete the 1st part of table 6.3.3.2.1-1 |
|  |  |
| ***Consequences if not approved:*** | The parameters in table 6.3.3.2.1-1 will be confusing |
|  |  |
| ***Clauses affected:*** | 6.3.3.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-4 |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### 6.3.3.2 TDD

##### 6.3.3.2.1 Single PMI with 4TX TypeI-SinglePanel Codebook

For the parameters specified in Table 6.3.3.2.1-1, and using the downlink physical channels specified in Annex C.3.1, the minimum requirements are specified in Table 6.3.3.2.1-2.

Table 6.3.3.2.1-1: Test parameters (single layer)

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |
| **Parameter** | **Unit** | **Test 1** |
| Bandwidth | MHz | 40 |
| Subcarrier spacing | kHz | 30 |
| Duplex Mode |  | TDD |
| TDD DL-UL configuration |  | FR1.30-1 as specified in Annex A |
| Propagation channel |  | TDLA30-5 |
| Antenna configuration |  | High XP 4 x 4(N1,N2) = (2,1) |
| Beamforming Model |  | As specified in Annex B.4.1 |
| ZP CSI-RS configuration | CSI-RS resource Type |  | Periodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 5, (4,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (9,-) |
| CSI-RSinterval and offset | slot | 10/1 |
| NZP CSI-RS for CSI acquisition | CSI-RS resource Type |  | Aperiodic |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (ρ) |  | 1 |
| First subcarrier index in the PRB used for CSI-RS (k0, k1 ) |  | Row 4, (0,-) |
| First OFDM symbol in the PRB used for CSI-RS (l0, l1) |  | (13,-) |
| CSI-RSinterval and offset |  | Not configured |
| aperiodicTriggeringOffset |  | 0 |
| CSI-IM configuration | CSI-IM resource Type |  | Aperiodic |
| CSI-IM RE pattern |  | Pattern 0 |
| CSI-IM Resource Mapping(kCSI-IM,lCSI-IM) |  | (4,9) |
| CSI-IM timeConfiginterval and offset | slot | Not configured |
| ReportConfigType |  | Aperiodic |
| CQI-table |  | Table 1 |
| reportQuantity |  | cri-RI-PMI-CQI |
| timeRestrictionForChannelMeasurements |  | Not configured |
| timeRestrictionForInterferenceMeasurements |  | Not configured |
| cqi-FormatIndicator |  | Wideband |
| pmi-FormatIndicator |  | Wideband |
| Sub-band Size | RB | 16 |
| csi-ReportingBand |  | 1111111 |
| CSI-Report interval and offset | slot | Not configured |
| Aperiodic Report Slot Offset |  | 8 |
| CSI request |  | 1 in slots i, where mod(i, 10) = 1, otherwise it is equal to 0 |
| reportTriggerSize |  | 1 |
| CSI-AperiodicTriggerStateList |  | One State with one Associated Report ConfigurationAssociated Report Configuration contains pointers to NZP CSI-RS and CSI-IM |
| Codebook configuration | Codebook Type |  | typeI-SinglePanel |
| Codebook Mode |  | 1 |
| (CodebookConfig-N1,CodebookConfig-N2) |  | (2,1) |
| (CodebookConfig-O1,CodebookConfig-O2) |  | (4,1) |
| CodebookSubsetRestriction |  | 11111111 |
| RI Restriction |  | 00000001 |
| Physical channel for CSI report |  | PUSCH |
| CQI/RI/PMI delay  | ms | 5.5 |
| Maximum number of HARQ transmission |  | 4 |
| Measurement channel |  | R.PDSCH.2-8.1 TDD |
| PDSCH & PDSCH DMRS Precoding configuration for random Precoding |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with Wideband granularity |
| Note 1: When Throughput is measured using random precoder selection, the precoder shall be updated in each slot (0.5 ms granularity) with equal probability of each applicable i1, i2 combination.Note 2: If the UE reports in an available uplink reporting instance at slot#n based on PMI estimation at a downlink slot not later than slot#(n-4), this reported PMI cannot be applied at the gNB downlink before slot#(n+4).Note 3: Randomization of the principle beam direction shall be used as specified in Annex B.2.3.2.3. |

Table 6.3.3.2.1-2: Minimum requirement

|  |  |
| --- | --- |
| **Parameter** | **Test 1** |
| ** | 1.3 |