**3GPP TSG-RAN4 Meeting #102-e *R4-2206616***

**Electronic Meeting, 21 February– 3 March, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-3** | **CR** | **CRNum** | **rev** | **-** | **Current version:** | **15.16.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Big CR for TS 38.101-3 Maintenance (Rel-15) |
|  |  |
| ***Source to WG:*** | MCC, Huawei |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2021-03-07 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…**Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | This big CRs merge the mutiple endorsed draft CRs. The reason for change in each endorsed draft CR is copied below.R4-2205304 Draft CR for 38.101-3 to add spurious response exception for intra-band EN-DC (R15)<Reason for change>The spurious response exception is missing for intra-band EN-DCR4-2206291 Draft CR to correct the output power in EN-DC Rx tests<Reason for change>To prevent and decrease the affect on NR operation by IMD during intra-band EN-DC Rx test, the output power of the E-UTRA uplink shall be set to 29 dB below PCMAX\_L for all intra-band EN-DC tests, not only for intra-band non-contiguous EN-DC.R4-2206293 draft Rel-15 CR 38101-3-fg0 to align spurious emission between R15 and R16<Reason for change>1. Protected E-UTRA band 51 was added to DC\_7\_n28 in the CR in 0042R1 (RP-191241) for Rel-16, but the CR in 0041 (RP-191240) did not add the band for Rel-15. Protected E-UTRA band 51 need also to be added to the Rel-15 version of TS 38.101-3.
2. Protected E-UTRA band 53 was added to DC\_12\_n66 and DC\_30\_n5 in the CR in 0424R1 (RP-202485) for Rel-16, but the CR in 0423R1 (RP-202485) did not add the band for Rel-15. Protected E-UTRA band 53 need also to be added to the Rel-15 version of TS 38.101-3.
3. Protected bands E-UTRA band 28 was added to DC\_39\_n78 and DC\_39\_n78 in the CR in 0184 (RP-201045) for Rel-16, but the band was not added to the Rel-15 version of TS 38.101-3.

Protected E-UTRA bands 48 and 52 was removed from DC\_30\_n5 in the CR in 0423R1 (RP-202485) to the Rel-15 version of 38.101-3 but the bands were not removed when the CR was implemented.R4-2206486 Draft CR for clarification on per band pair simultaneous RxTx capability for TS 38.101-3<Reason for change>In response to the introduction of the new capability signalling of per band pair simultaneous RxTx capability in RAN2#116-e, RAN4#101-bis-e discusses the clarification on mandatory applicaibility for band pairs included in higher order band combinations, and the following proposals were agreed in R4-2202295. *Agreement:** *Proposal 1: For inter-band EN-DC, NE-DC, NR CA, NR DC and SUL configurations,*
	+ *If mandatory simultaneous RxTx capability apply for a band configuration, mandatory simultaneous RxTx capability also apply for the band pair of the configuration when the applicable configuration is a subset of a higher order band configuration.*
* *Proposal 2: Clarification in Proposal 1 should apply from Rel-15 TS 38.101 series.*
* *Proposal 3: FFS how to capture proposal 1 in TS 38.101 series.*
	+ *Option 1: Add NOTEs in band configuration tables including higher order band configuration (more than 2 bands cases).*
	+ *Option 2: Add description in general sections.*

 This CR tries to reflect propsals 1 and 2 into TS 38.101-3. Regarding proposal 3, this CR is based on option 2 since it is redandant to put the same NOTEs into all band configuration tables. |
|  |  |
| ***Summary of change:*** | The summary of change in each endorsed draft CR is copied below.R4-2205304 Draft CR for 38.101-3 to add spurious response exception for intra-band EN-DC (R15)<Summary of change>The declaration of spurious response exception is added for intra-band EN-DC.R4-2206291 Draft CR to correct the output power in EN-DC Rx tests<Summary of change>Apply the general requirement about the output power to all intra-band EN-DC tests.R4-2206293 draft Rel-15 CR 38101-3-fg0 to align spurious emission between R15 and R16<Summary of change>1. Added protected E-UTRA band 51 to DC\_7\_n28.
2. Added protected E-UTRA band 53 to DC\_12\_n66 and DC\_30\_n5.
3. Added protected E-UTRA band 28 to DC\_38\_n78 and DC\_38\_n79.
4. Removed E-UTRA bands 48 and 52 from DC\_30A\_n5A.

R4-2206486 Draft CR for clarification on per band pair simultaneous RxTx capability for TS 38.101-3<Summary of change>The following descriptions are added into section 5.2A.1 and 5.5B.1, respectively:*If the mandatory simultaneous Rx/Tx capability applies for a band combination, the mandatory simultaneous Rx/Tx capability also applies for the band combination when the applicable band combination is a subset of a higher order band combination.**If the mandatory simultaneous Rx/Tx capability applies for a DC configuration, the mandatory simultaneous Rx/Tx capability also applies for the DC configuration when the applicable DC configuration is a subset of a higher order DC configuration.* |
|  |  |
| ***Consequences if not approved:*** | The consequences if not approved for each endorsed draft CR are coppied below.R4-2205304 Draft CR for 38.101-3 to add spurious response exception for intra-band EN-DC (R15)<Consequences if not approved>The spurious response exception is missing for intra-band EN-DC.R4-2206291 Draft CR to correct the output power in EN-DC Rx tests<Consequences if not approved>IMD will affect the test channel, and may cause the incorrect test.R4-2206293 draft Rel-15 CR 38101-3-fg0 to align spurious emission between R15 and R16<Consequences if not approved>1-3: Protected bands will be missing for impacted EN-DC configurations.4: E-UTRA bands 48 and 52 will incorrectly be specified for DC\_30A\_n5A.R4-2206486 Draft CR for clarification on per band pair simultaneous RxTx capability for TS 38.101-3<Consequences if not approved>Mandatory applicaibility for band pairs included in higher order band combinations is unclear considering the existence of per band pair simultaneous RxTx capability signalling of *simultaneousRxTxInterBandCAPer-band-pair/ simultaneousRxTxInterBandENDCPer-band-pair*. |
|  |  |
| ***Clauses affected:*** | 5.2A.1, 5.5B.1, 6.5B.3.3.2, 7.1, 7.4B.1, 7.5B.1, 7.6B.2.1, 7.6B.3.1, 7.6B.4.1, 7.7B.1, 7.8B.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS/TR 38.521-3 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## **<<Start of Change>>**

## 5.2A Operating bands for CA

### 5.2A.1 Inter-band CA between FR1 and FR2

NR carrier aggregation are designed to operate in the operating bands defined in Table 5.2A.1‑1. The band combinations include at least one FR1 operating band and one FR2 operating band.

If the mandatory simultaneous Rx/Tx capability applies for a band combination, the mandatory simultaneous Rx/Tx capability also applies for the band combination when the applicable band combination is a subset of a higher order band combination.

Table 5.2A.1-1: Band combinations for inter-band NR CA between FR1 and FR2

|  |  |
| --- | --- |
| NR CA Band | NR Band |
| CA\_n8-n2581 | n8, n258 |
| CA\_n71-n2571 | n71, n257 |
| CA\_n77-n2571 | n77, n257 |
| CA\_n78-n2571 | n78, n257 |
| CA\_n79-n2571 | n79, n257 |
| NOTE 1: Applicable for UE supporting inter-band carrier aggregation with mandatory simultaneous Rx/Tx capability. |

## **<<Next of Change>>**

## 5.5B Configuration for DC

### 5.5B.1 General

The operating bands and bandwidth classes are specified for operation with EN-DC, NGEN-DC, NE-DC or NR-DC configured. The EN-DC, NGEN-DC or NE-DC band combinations include at least one E-UTRA operating band.

For EN-DC or NE-DC configurations indicated by column "Single Uplink allowed" (e.g., problematic band combinations as defined in TS 38.306 [11]) in tables in this clause the UE may indicate capability of not supporting simultaneous dual and triple uplink operation due to possible intermodulation interference to its own primary downlink channel bandwidth of PCell or PSCell if the intermodulation order is 2 or if the intermodulation order is 3 for the combinations when both operating bands are between 450 MHz – 960 MHz or between 1427 MHz – 2690 MHz.

In the case for EN-DC or NE-DC configurations listed in tables in this clause for which the intermodulation products caused by the dual and triple uplink operation fall into the receive band but do not interfere with its own primary downlink channel bandwidth of PCell or PSCell as defined in Annex I the UE is mandated to operate in dual and triple uplink mode. Single Uplink is also allowed for certain band combinations where intermodulation or reverse intermodulation products could create difficulty for meeting emission requirements.

For EN-DC combinations of order 3 or higher, "Single Uplink allowed" UL configurations captured in Table 5.5B.2-1, Table 5.5B.3-1, and Table 5.5B.4-1 apply.

If multiple UL DC configurations are listed for multiple DL DC configurations, valid uplink configurations are such that uplink does not have more carriers than downlink.

Non‑contiguous resource allocation and almost contiguous allocation are not applicable for E‑UTRA or NR carrier part of intra‑band EN‑DC configuration.

If the mandatory simultaneous Rx/Tx capability applies for a DC configuration, the mandatory simultaneous Rx/Tx capability also applies for the DC configuration when the applicable DC configuration is a subset of a higher order DC configuration.

## **<<Next of Change>>**

##### 6.5B.3.3.2 Spurious emission band UE co-existence

This clause specifies the requirements for the specified EN-DC, for coexistence with protected bands. The requirements in Table 6.5B.3.3.2-1 apply on each component carrier with all component carriers are active.

NOTE: For inter-band EN-DC with uplink assigned to one LTE band and one NR band the requirements in Table 6.5B.3.3.2-1 could be verified by measuring spurious emissions at the specific frequencies where second and third order intermodulation products generated by the two transmitted carriers can occur.

Table 6.5B.3.3.2-1: Requirements

| EN-DC Configuration | Spurious emission  |
| --- | --- |
| Protected band | Frequency range (MHz) | Maximum Level (dBm) | MBW (MHz) | NOTE |
| DC\_1\_n28 | E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 38, 40, 41, 72, 73NR band n79 | FDL\_low  | -  | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 22, 32, 42, 43, 50, 51, 52, 65, 74, 75, 76NR band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 3, 34 | FDL\_low  | -  | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5,16 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 16 |
| DC\_1\_n40 | Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 38, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76NR band n78 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| Band 3, 34 | FDL\_low  | - | FDL\_high | -50 | 1 | 5 |
| NR band n77, n79 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5, 16 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_1\_n51 | E-UTRA Band 7, 12, 13, 17, 20, 22, 27, 28, 29, 31, 38, 44, 48, 67, 68, 69, 72, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5, 2 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 16 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 16 |
| E-UTRA Band 5, 6, 8, 26, 30, 40, 41, 42, 43, 46NR Band n77, n78, n79,  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_1\_n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n78DC\_1\_n84\_ULSUP-TDM\_n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n79 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 21, 26, 28, 34, 40, 41, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_2\_n5 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 28, 29, 30, 42, 48, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 41, 43, 53 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n66 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low  | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 42, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 29, 30, 48, 66 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_2\_n78 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n7 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 40, 43, 44, 50, 51, 65, 67, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 22, 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570  | -  | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_3\_n28 | E-UTRA Band 1, 42, 43, 50, 51, 65, 74, 75, 76NR band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 34, 38, 40, 41, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low  | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 13 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9 |
| DC\_3\_n40 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 33, 34, 38, 39, 41, 43, 44. 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 42, 52NR band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n51 | E-UTRA Band 7, 8, 12, 13, 17, 20, 27, 28, 31, 33, 38, 67, 68, 69, 72, 73 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 1, 5, 6, 22, 26, 30, 34, 36, 40, 41, 42, 43, 44, 46, 48, 65, 71 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n78DC\_3\_n80\_ULSUP-TDM\_n78, | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n79 DC\_3\_n80\_ULSUP-TDM\_n79, | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 28, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n82 | E-UTRA Band 1, 3 7, 8, 20 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 68, 72,74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 22, 38, 42, 69 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_5\_n40 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 21, 28, 31, 34, 38, 42, 43, 45, 65, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 52NR band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_5\_n66 | E-UTRA Band 1, 2, 3, 4, 5, 6, 7, 8, 12, 13, 14, 17, 24, 25, 28, 29, 30, 34, 38, 40, 43, 45, 50, 51, 65, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 42, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_5\_n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 14, 17, 24, 25, 28, 29, 30, 31, 34, 38, 40, 45, 65, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 7, 2 |
| DC\_7\_n28 | E-UTRA Band 2, 3, 5, 7, 8, 20, 26, 27, 31, 34, 40, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 4, 42, 43, 50, 51, 65, 66, 74, 75, 76NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 2570  | -  | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n51 | E-UTRA Band 2, 3, 5, 8, 26, 30, 31, 32, 33, 34, 40, 48, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570  | - | 2575 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5 |
| E-UTRA Band 1, 4, 12, 13, 14, 17, 20, 22, 23, 27, 28, 29, 42, 43, 44, 46, 65, 66, 67, 68NR Band n77, n78, n79, | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_7\_n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 33, 34, 40, 50, 51, 65, 66, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570  | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_8\_n40 | E-UTRA Band 1, 5, 11, 18, 19, 20, 21, 26, 28, 31, 32, 33, 34, 38, 39,, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 22, 41, 42, 43, 52NR band n77, n78, n79 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low  | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_8\_n77 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_8\_n78DC\_8\_n81\_ULSUP-TDM\_n78, | E-UTRA Band 1, 20, 28, 34, 39, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_8\_n79DC\_8\_n81\_ULSUP-TDM\_n79, | E-UTRA Band 1, 8, 28, 34, 39, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3,41,42  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_11\_n77 | E-UTRA Band 1, 3, 18, 19, 28, 34, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_11\_n78 | E-UTRA Band 1, 3, 18, 19, 28, 34, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_11\_n79 | E-UTRA Band 1, 3, 18, 19, 28, 34, 40, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_12\_n5 | E-UTRA Band 2, 5, 13, 14, 17, 24, 25, 26, 30, 43 50, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Bands 4, 41, 42, 48, 51, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_12\_n66 | E-UTRA Band 2, 5, 13, 14, 17, 25, 26, 27, 30, 41, 53, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 48, 50, 51, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_18\_n77 | E-UTRA Band 1, 3, 11, 21, 28, 34, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n78 | E-UTRA Band 1, 3, 11, 21, 28, 34, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n79 | E-UTRA Band 1, 3, 11, 21, 28, 34, 40, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n77 | E-UTRA Band 1, 3, 11, 21, 28, 34, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n78 | E-UTRA Band 1, 3, 11, 21, 28, 34, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n79 | E-UTRA Band 1, 3, 11, 21, 28, 34, 40, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_20\_n8 | E-UTRA Band 1, 28, 31, 32, 34, 65, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 22, 38, 42, 43NR Band n78  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n28DC\_20\_n83 | E-UTRA Band 3, 7, 8, 31, 34 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 22, 32, 38, 42, 43, 65, 75, 76,NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n51 | E-UTRA Band 1, 3, 4, 8, 17, 22, 28, 29, 31, 40, 43, 48, 65, 66, 68, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| E-UTRA Band 2, 7, 25, 32, 33, 34, 35, 36, 37, 38, 39, 41, 42, 46, 69, 70NR Band n77, n78, n79,  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n77 | E-UTRA Band 1, 3, 7, 8, 31, 32, 33, 34, 40, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n78,DC\_20\_n82\_ULSUP-TDM\_n78, | E-UTRA Band 1, 3, 7, 8, 31, 32, 33, 34, 40, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_21\_n77 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_21\_n78 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_21\_n79 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 40, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_25\_n41 | E-UTRA Band 4, 5, 12, 13 , 14, 17, 24, 26, 27, 28, 29, 30, 42, 45, 48, 66, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA/NR Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_26\_n41 | E-UTRA Band 1, 2, 3, 4, 5, 11, 12, 13 , 14, 17, 18, 19, 21, 24, 25, 26, 29, 30, 31, 34, 39, 42, 43, 48, 50, 51, 65, 66, 70, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| DC\_26\_n77 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 | 2 |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_26\_n78 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 | 2 |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_26\_n79 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 | 2 |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_28\_n51 | E-UTRA Band 2, 3, 5, 7, 8, 25, 26, 31, 34, 38, 40, 41, 72 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 20, 22, 24, 32, 42, 43, 45, 46, 65, 66, 71, 73NR band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| DC\_28\_n77 | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3, 9 |
| DC\_28\_n78DC\_28\_n83\_ULSUP-TDM\_n78, | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3, 9 |
| DC\_28\_n79 | E-UTRA Band 3, 5, 8, 18, 19, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3, 9 |
| DC\_30\_n5 | E-UTRA Band 2, 4, 5, 7, 12, 13, 14, 17, 24, 25, 26, 29, 30, 38, 48, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 53, | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_30\_n66 | E-UTRA Band 2, 4, 5, 12, 13, 14, 17, 24, 25, 26, 27, 29, 30, 38, 41, 66, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_38\_n78 | N/A |
| DC\_39\_n78 | E-UTRA Band 1, 8, 28, 34, 40, 41, 44, 45 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 18 |
| DC\_39\_n79 | E-UTRA Band 1, 8, 28, 34, 40, 41, 44, 45  | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 18 |
| DC\_40\_n77 | N/A |
| DC\_41\_n77 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 26, 28, 33, 34, 39, 40, 44, 45, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 3 |
| DC\_41\_n78 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 26, 28, 34, 39, 40, 44, 45, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_41\_n79 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 26, 28, 34, 40, 42, 44, 45, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_42\_n51 | E-UTRA Band 3, 8, 20, 25, 30, 31, 34, 39, 41, 73 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 2, 4, 5, 6, 7, 12, 13, 14, 17, 23, 24, 26, 27, 28, 29, 32, 38, 40, 44, 46, 65, 66, 67, 68, 70, 71 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_42\_n77 | N/A |
| DC\_42\_n78 | N/A |
| DC\_42\_n79 | N/A |
| DC\_66\_n5 | E-UTRA Band 1, 2, 3, 4, 5, 6, 7, 8, 12, 13, 14, 17, 24, 25, 26, 28, 29, 30, 34, 38, 40, 43, 45, 50, 51, 65, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 42, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_66\_n71 | E-UTRA Band 4, 5, 13, 14, 17, 24, 26, 27, 29, 30, 43,50, 51, 66, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 7, 22, 25, 41, 42, 48, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_66\_n78,DC\_66\_n86\_ULSUP-TDM\_n78, | E-UTRA Band 1, 3, 5, 7, 8, 20, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NOTE 1: FDL\_low and FDL\_high refer to each frequency band specified in Table 5.5-1 in 3GPP TS 36.101 [4] or in Table 5.2-1 in 3GPP TS 38.101-1 [2].NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.6.3.1-2 in 3GPP TS 36.101 [4] and Table 6.5.3.1-2 in 3GPP TS 38.101-1 [2] are permitted for each assigned carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x 180 kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.NOTE 3: Applicable when co-existence with PHS system operating in 1884.5 - 1915.7 MHzNOTE 4: VoidNOTE 5: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.6.3.1-1, Table 6.6.3.1A-1 in 3GPP TS 36.101 [4] or in Table 6.5.3.1-1 in 3GPP TS 38.101-1 [2] from the edge of the channel bandwidth.NOTE 6: This requirement is applicable for any channel bandwidths within the range 2500 - 2570 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2560.5 - 2562.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2552 - 2560 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 7: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band.NOTE 8: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplinkNOTE 9: Applicable when the assigned E-UTRA or NR carrier is confined within 718 MHz and 748 MHz and when the channel bandwidth used is 5 or 10 MHz.NOTE 10: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 2nd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 2nd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 11: As exceptions, measurements with a level up to the applicable requirement of -36 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 12: This requirement is applicable only for the following cases: A: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 902.5 MHz ≤ Fc < 907.5 MHz with an uplink transmission bandwidth less than or equal to 20 RB; B: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 907.5 MHz ≤ Fc ≤ 912.5 MHz without any restriction on uplink transmission bandwidth; C: for carriers of 10 MHz channel bandwidth when carrier centre frequency (Fc) is Fc = 910 MHz with an uplink transmission bandwidth less than or equal to 32 RB with RBstart > 3.NOTE 13: VoidNOTE 14: This requirement is applicable for 5 and 10 MHz E-UTRA or NR channel bandwidth allocated within 718-728MHz. For carriers of 10 MHz bandwidth, this requirement applies for an uplink transmission bandwidth less than or equal to 30 RB with RBstart > 1 and RBstart < 48.NOTE 15: VoidNOTE 16: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 17: This requirement is applicable in the case of a 10 MHz E-UTRA or NR carrier confined within 703 MHz and 733 MHz, otherwise the requirement of -25 dBm with a measurement bandwidth of 8 MHz applies.NOTE 18: This requirement is only applicable for E-UTRA carriers with bandwidth confined within 1885 - 1920 MHz (requirement for carriers with at least 1RB confined within 1880 - 1885 MHz is not specified). This requirement applies for an uplink transmission bandwidth less than or equal to 54 RB for E-UTRA carriers of 15 MHz bandwidth when carrier center frequency is within the range 1892.5 - 1894.5 MHz and for E-UTRA carriers of 20 MHz bandwidth when carrier center frequency is within the range 1895 - 1903 MHz.NOTE 19: Void |

NOTE: To simplify the above Table, E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation or both E-UTRA and NR operation. NR band numbers are listed for bands which are specified only for NR operation.

## **<<Next of Change>>**

# 7 Receiver characteristics

## 7.1 General

Unless otherwise stated the receiver characteristics are specified at the antenna connector(s) of the UE for the bands operating on frequency range 1 and over the air of the UE for the bands operating on frequency range 2. The requirements for frequency range 1 and frequency range 2 can be verified separately. For the carrier in frequency range 1, requirements can be verified with NR FR2 link disabled. For the carrier in frequency range 2, requirements can be verified in OTA mode with E-UTRA connecting to the network by OTA without calibration.

The requirements defined in this clause are the extra requirements compared with the single carrier requirements defined in TS 38.101-1 [2] and TS 38.101-2 [3].

Unless otherwise stated, the UL and DL reference measurement channels are the same with the configurations specified in TS 38.101-1 [2] and TS 38.101-2 [3].

Unless otherwise stated, requirements for NR receiver written in TS 38.101-1 [2] and TS 38.101-2 [3] apply and are assumed anchor agnostic. Requirements are verified under conditions where anchor resources do not interfere NR operation.

For intra-band EN-DC, the output power is configured as follows:

- One E-UTRA uplink carrier with the output power set to 29 dB below PCMAX\_L and the NR band whose downlink is being tested has its uplink carrier output power set to 4 dB below PCMAX\_L,f,c.

- One NR uplink carrier with the output power set to 29 dB below PCMAX\_L,f,c and the E-UTRA band whose downlink is being tested has its uplink carrier output power set to 4 dB below PCMAX\_L,c.

For the additional requirements for intra-band non-contiguous EN-DC of two sub-blocks, an in-gap test refers to the case when the interfering signal is located at a negative offset with respect to the assigned lowest channel frequency of the highest sub-block and located at a positive offset with respect to the assigned highest channel frequency of the lowest sub-block.

For the additional requirements for intra-band non-contiguous EN-DC of two sub-blocks, an out-of-gap test refers to the case when the interfering signal(s) is (are) located at a positive offset with respect to the assigned channel frequency of the highest carrier frequency or located at a negative offset with respect to the assigned channel frequency of the lowest carrier frequency.

For the additional requirements for intra-band non-contiguous EN-DC of two sub-blocks with channel bandwidth larger than or equal to 5 MHz, the existing adjacent channel selectivity requirements, in-band blocking requirements (for each case), and narrow band blocking requirements apply for in-gap tests only if the corresponding interferer frequency offsets with respect to the two measured carriers satisfy the following condition in relation to the sub-block gap size Wgap for at least one of the E-UTRA or NR sub-blocks, so that the interferer frequency position does not change the nature of the core requirement tested:

 Wgap ≥ 2∙|FInterferer (offset)| – BWChannel

For the E-UTRA sub-block, the FInterferer (offset), for a sub-block with a single component carrier is the interferer frequency offset with respect to carrier as specified in clause 7.5.1, clause 7.6.1 and clause 7.6.3 for the respective requirement in TS 36.101 [4] and BWChannel. FInterferer (offset) for the E-UTRA sub-block with two or more contiguous component carriers is the interference frequency offset with respect to the carrier adjacent to the gap is specified in clause 7.5.1A, 7.6.1A and 7.6.3A in TS 36.101 [4].

For the NR sub-block, the FInterferer (offset), for a sub-block with a single component carrier is the interferer frequency offset with respect to carrier as specified in clause 7.5.1, clause 7.6.1 and clause 7.6.3 for the respective requirement in TS 38.101-1 [2] and BWChannel.

The interferer frequency offsets for adjacent channel selectivity, each in-band blocking case and narrow-band blocking shall be tested separately with a single in-gap interferer at a time.

For sub-clauses with suffix A or B: the minimum requirements for band combinations including Band n41 also apply for the corresponding band combinations with Band n90 replacing Band n41 but with otherwise identical parameters. For brevity the said band combinations with Band n90 are not listed in the tables below but are covered by this specification.

For the requirements of FR1 in this clause, the UE shall be verified with four Rx antenna ports and skip two Rx antenna ports requirements in operating bands where the UE is equipped with four Rx antenna ports, otherwise, the UE shall be verified with two Rx antenna ports.

## **<<Next of Change>>**

## 7.4B Maximum input level for DC in FR1

### 7.4B.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC maximum input level requirement and parameters are defined in Table 7.4B.1-1.

Table 7.4B.1-1: Maximum Input

|  |  |
| --- | --- |
| **Power in Largest CC, E-UTRA or NR, dBm** | X1 |
| **Power in each other CC, dBm** | X1 – 10\*log10(NxSCSx/NySCSy) |
| NOTE 1: Power in Largest E-UTRA or NR bandwidth CC, listed in Table 7.4-1 [2]NOTE 2: Nx, SCSx is the number of RB's and Sub carrier spacing in the largest carrier bandwidth and could be E-UTRA or NR carrierNOTE 3: Ny, SCSy is the number of RB's in any other carrier.NOTE 4: Void.NOTE 5: Void. |

## **<<Next of Change>>**

## 7.5B Adjacent channel selectivity for DC in FR1

### 7.5B.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC ACS requirement and parameters are defined for test case 1 in Table 7.5B.1-1 and for test case 2 in Table 7.5B.1-2.

Table 7.5B.1-1: ACS test case 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN-DC Aggregated Bandwidth, MHz | <=100 | >100, <=120 | >120, <=140 | >140, <=160 |
| ACS, dB | X1 | 19.2 | 18.5 | 17.9 |
| Pinterferer, dBm | PI 2 | Aggregated power + 17.7 dB | Aggregated power + 17 dB | Aggregated power + 16.4dB |
| Pw in Transmission BW configuration, per CC, dBm | REFSENS +14dB |
| NOTE 1: X is ACS level at the specified EN-DC aggregated bandwidth from Table 7.5.1A-1 in TS 36.101 [4]NOTE 2: PI is from Table 7.5.1A-2 in TS 36.101 [4]NOTE 3: Jammer BW and offset is from Table 7.5.1A-2 [4] and is applied from the lowest edge of the lowest carrier and the highest edge of the highest carrierNOTE 4: Void.NOTE 5: Void. |

Table 7.5B.1-2: ACS test case 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **EN-DC Aggregated Bandwidth, ENBW, MHz** | ≤100 | >100, ≤120 | >120, ≤140 | >140, ≤160 |
| **Pw in Transmission Bandwidth Configuration, perCC, dBm** | PW 1 | -42.7 +10log10(NRB,c/ NRB\_agg) | -42 +10log10(NRB,c/ NRB\_agg) | -41.4 +10log10(NRB,c/ NRB\_agg) |
| **Pinterferer, dBm** | -25 |
| NOTE 1: PW is wanted signal power level at the specified EN-DC aggregated Bandwidth from Table 7.5.1A-3 in TS 36.101 [4]NOTE 2: Jammer BW and offset is from Table 7.5.1A-3 [4] and is applied from the lowest edge of the lowest carrier and the highest edge of the highest carrierNOTE 3: Void.NOTE 4: Void. |

## **<<Next of Change>>**

## 7.6B Blocking characteristics for DC in FR1

### 7.6B.1 General

### 7.6B.2 In-band blocking for DC in FR1

#### 7.6B.2.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC in-band blocking requirement and parameters are defined in Table 7.6B.2.1-1.

Table 7.6B.2.1-1: In-band blocking

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN-DC Aggregated Bandwidth, MHz | ≤100 | >100, ≤120 | >120, ≤140 | >140, ≤160 |
| Pw in Transmission Bandwidth Configuration, perCC, dBm |  | REFSENS + Aggregated BW specific value below |
|  | PW 1 | 16.8 | 17.5 | 18 |
| NOTE 1: PW is wanted signal power level at the specified EN-DC aggregated Bandwidth from Table 7.6.1.1A-1 in TS 36.101 [4]NOTE 2: Interferer values are specified from Table 7.6.1.1A-2 in TS 36.101 [4]NOTE 3: Jammer BW and offset is from Table 7.6.1.1A-1 [4] and is applied from the lowest edge of the lowest carrier and the highest edge of the highest carrierNOTE 4: Void.NOTE 5: Void. |

## **<<Next of Change>>**

### 7.6B.3 Out-of-band blocking for DC in FR1

#### 7.6B.3.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC out-of-band requirement and parameters are defined in Table 7.6B.3.1-1.

Table 7.6B.3.1-1: Out-of-band blocking

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN-DC Aggregated Bandwidth, MHz | ≤100 | >100, ≤120 | >120, ≤140 | >140, ≤160 |
| Pw in Transmission Bandwidth Configuration, perCC, dBm | REFSENS + Aggregated BW specific value below |
|  | 9 |
| NOTE 1: Interferer values and offsets are specified from Table 7.6.2.1A-2 in TS 36.101 [4]NOTE 2: Void.NOTE 3: Void. |

For Table 7.6.2.1A-2 from TS 36.101 [4] in frequency range 1, 2 and 3, up to exceptions are allowed for spurious response frequencies in each assigned frequency channel when measured using a 1MHz step size. For these exceptions the requirements of subclause 7.7B.1 Spurious response are applicable.

## **<<Next of Change>>**

### 7.6B.4 Narrow band blocking for DC in FR1

#### 7.6B.4.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC narrow band blocking requirement and parameters are defined in Table 7.6B.4.1-1.

Table 7.6B.4.1-1: Narrow band blocking parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN-DC Aggregated Bandwidth, MHz | ≤100 | >100, ≤120 | >120, ≤140 | >140, ≤160 |
| Pw in Transmission Bandwidth Configuration, perCC, dBm | REFSENS + Aggregated BW specific value below |
|  | 16 |
| PUW, dBm (CW) | -55 |
| NOTE 1: Jammer offset is from Table 7.6.3.1A-1 [4] and is applied from the lowest edge of the lowest carrier and the highest edge of the highest carrierNOTE 2: Void.NOTE 3: Void.NOTE 4: If NR carrier BW > 40 MHz, no narrow band blocking requirements apply when blocker is applied at the edge of the NR carrier. |

## **<<Next of Change>>**

## 7.7B Spurious response for DC in FR1

### 7.7B.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC spurious response requirement and parameters are defined in Table 7.7B.1-1.

Table 7.7B.1-1: Spurious Response Parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN-DC Aggregated Bandwidth, MHz | ≤100 | >100, ≤120 | >120, ≤140 | >140, ≤160 |
| Pw in Transmission Bandwidth Configuration, perCC, dBm | REFSENS + Aggregated BW specific value below |
|  | 9 |
| Pinterferer, dBm (CW) | -44 |
| NOTE 1: Void.NOTE 2: Void. |

## **<<Next of Change>>**

## 7.8B Intermodulation characteristics for DC in FR1

### 7.8B.1 General

### 7.8B.2 Wide band Intermodulation

#### 7.8B.2.1 Intra-band contiguous EN-DC in FR1

Intra-band contiguous EN-DC wide band intermodulation requirement and parameters are defined in Table 7.8B.2.1-1.

Table 7.8B.2.1-1: Wide band intermodulation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN-DC Aggregated Bandwidth, MHz | <=100 | >100, <=120 | >120, <=140 | >140, <=160 |
| Pw in Transmission Bandwidth Configuration, perCC, dBm | PW 1 | REFSENS + Aggregated BW specific value below |
|  |  | 16.8 | 17.5 | 18.0 |
| Pinterferer 1, dBm (CW)2 | -46 |
| Pinterferer 2, dBm (Modulated)2 | -46 |
| NOTE 1: PW is wanted signal power level from Table 7.8.1A-1 in TS 36.101 [4]NOTE 2: Jammer BW and offsets is from Table 7.8.1A-1 [4] and is applied from the lowest edge of the lowest carrier and the highest edge of the highest carrierNOTE 3: Void.NOTE 4: Void. |

## **<<End of Change>>**