**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Endorced CRs R4-2213995 Correction to NS\_05 frequency range Qualcomm Incorporated, Nokia, Nokia Shanghai Bell Rel-17 38.101-1 17.6.0 NR\_newRAT-Core AR4-2215026 Draft CR for 38.101-1 to improve the wording for simultaneousRxTx clarification(R17) Huawei, HiSilicon Rel-17 38.101-1 17.6.0 NR\_newRAT-Core AR4-2212249 Draft CR to 38101-1-h60 for n41 relevant MSD test frequencies MediaTek Inc. Rel-17 38.101-1 17.6.0 TEI16 NR\_newRAT-Core F　R4-2214975 draft CR to TS38.101-1: 4Rx for inter-band NR CA ZTE Corporation, CHTTL Rel-17 38.101-1 17.6.0 NR\_newRAT-Core FR4-2211577 Update of UL MIMO transmit quality definitions Rohde & Schwarz Rel-17 38.101-1 17.6.0 NR\_newRAT-Core AR4-2212565 Draft CR to TS38.101-1[R17] Corrections on Output power dynamics ZTE Corporation Rel-17 38.101-1 17.6.0 NR\_newRAT-Core A |
|  |  |
| ***Summary of change:*** | Chaanges in endorced CRsR4-2213995 Correction to NS\_05 frequency range Qualcomm Incorporated, Nokia, Nokia Shanghai Bell Rel-17 38.101-1 17.6.0 NR\_newRAT-Core AR4-2215026 Draft CR for 38.101-1 to improve the wording for simultaneousRxTx clarification(R17) Huawei, HiSilicon Rel-17 38.101-1 17.6.0 NR\_newRAT-Core AR4-2212249 Draft CR to 38101-1-h60 for n41 relevant MSD test frequencies MediaTek Inc. Rel-17 38.101-1 17.6.0 TEI16 NR\_newRAT-Core F　R4-2214975 draft CR to TS38.101-1: 4Rx for inter-band NR CA ZTE Corporation, CHTTL Rel-17 38.101-1 17.6.0 NR\_newRAT-Core FR4-2211577 Update of UL MIMO transmit quality definitions Rohde & Schwarz Rel-17 38.101-1 17.6.0 NR\_newRAT-Core AR4-2212565 Draft CR to TS38.101-1[R17] Corrections on Output power dynamics ZTE Corporation Rel-17 38.101-1 17.6.0 NR\_newRAT-Core A |
|  |  |
| ***Consequences if not approved:*** | Specification remains unclear |
|  |  |
| ***Clauses affected:*** | 5.2A.2, 5.2C, 6.2.3.1, 6.3.4.3, 6.3.4.4, 6.4D, 7.3A.1, 7.3A.5, 7.3C.1, 7.3E.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

< Start of changes >

### 5.2A.2 Inter-band CA

NR inter-band carrier aggregation is designed to operate in the operating bands defined in Table 5.2A.2.1-1, 5.2A.2.2-1 and Table 5.2A.2.3-1, where all operating bands are within FR1.

If the mandatory simultaneous Rx/Tx capability applies for a lower order band combination, when the applicable lower order band combination is a band pair in a higher order band combination, the mandatory simultaneous Rx/Tx capability also applies for the band pair in the higher order band combination.

Table 5.2A.2-1: Void

Table 5.2A.2-2: Void

Table 5.2A.2-3: Void

< End of changes >

< Start of changes >

## 5.2C Operating band combination for SUL

NR operation is designed to operate in the operating band combination defined in Table 5.2C-1, Table 5.2C-2, Table 5.2C-3 and Table 5.2C-4, where all operating bands are within FR1.

If the mandatory simultaneous Rx/Tx capability applies for a band combination, when the applicable lower order band combination is a band pair in a higher order band combination, the mandatory simultaneous Rx/Tx capability also applies for the band pair in the higher order band combination.

< End of changes >

< Start of changes >

#### 6.2.3.1 General

Additional emission requirements can be signalled by the network. Each additional emission requirement is associated with a unique network signalling (NS) value indicated in RRC signalling by an NR frequency band number of the applicable operating band and an associated value in the field *additionalSpectrumEmission.* Throughout this specification, the notion of indication or signalling of an NS value refers to the corresponding indication of an NR frequency band number of the applicable operating band, the IE field *freqBandIndicatorNR* and an associated value of *additionalSpectrumEmission* in the relevant RRC information elements [7]*.*

To meet the additional requirements, additional maximum power reduction (A-MPR) is allowed for the maximum output power as specified in Table 6.2.1-1. Unless stated otherwise, the total reduction to UE maximum output power is max(MPR, A-MPR) where MPR is defined in clause 6.2.2. Outer and inner allocation notation used in clause 6.2.3 is defined in clause 6.2.2. Unless stated otherwise, Edge RB allocations get the same AMPR as Outer RB allocations. In absence of modulation and waveform types the A-MPR applies to all modulation and waveform types.

Table 6.2.3.1-1 specifies the additional requirements with their associated network signalling values and the allowed A-MPR and applicable operating band(s) for each NS value. In case of a power class 3 UE, when IE *powerBoostPi2BPSK* is set to 1, power class 2 A-MPR values apply. The mapping of NR frequency band numbers and values of the *additionalSpectrumEmission* to network signalling labels is specified in Table 6.2.3.1-1A.

For almost contiguous allocations in CP-OFDM waveforms in power class 3, the allowed A-MPR defined in clause 6.2.3 is increased by CEIL{ 10 log10(1 + NRB\_gap / NRB\_alloc), 0.5 } dB, where CEIL{x, 0.5} means x rounding upwards to closest 0.5dB, NRB\_gap is the total number of unallocated RBs between allocated RBs and NRB\_alloc is the total number of allocated RBs, and the parameter LCRB is replaced by NRB\_alloc + NRB\_gap in specifying the RB allocation regions.

Unless otherwise specified, pi/2 BPSK in following A-MPR tables refers to both variants of pi/2 BPSK referenced in 6.2.2 tables 6.2.2-1.

Table 6.2.3.1-1: Additional maximum power reduction (A-MPR)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Network signalling label | Requirements (clause) | NR Band | Channel bandwidth (MHz) | Resources blocks (*N*RB) | A-MPR (dB) |
| NS\_01 |  | Table 5.2-1(NOTE 8) | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | Table 5.3.2-1 | N/A |
| NS\_03 | 6.5.2.3.3 | n2, n25, n66,n70, n86 |  |  | Clause 6.2.3.7 |
| NS\_03U | 6.5.2.3.3, 6.5.2.4.2 | n2, n25, n66, n86 |  |  | Clause 6.2.3.7 |
| NS\_04 | 6.5.2.3.2, 6.5.3.3.1 | n41, n90 | 59, 10, 15, 20, 25, 30, 35, 40, 45, 50, 60, 70, 80, 90, 100 |  | Clause 6.2.3.2 |
| NS\_05 | 6.5.3.3.4 | n1, n65, n84 | 5, 10, 15, 20(NOTE 2) |  | Clause 6.2.3.4 (NOTE 7) |
| NS\_05U | 6.5.3.3.4, 6.5.2.4.2 | n1, n65, n84 | 5, 10, 15, 20 |  | Clause 6.2.3.4 (NOTE 7) |
| NS\_06 | 6.5.2.3.4 | n12, n85 | 5, 10, 15 |  | N/A |
|  |  | n14 | 5,10 |  |  |
| NS\_07 | 6.5.3.3.26 | n13 | 5,10 | Table 6.2.3.29-1 | Table6.2.3.29-2 |
| NS\_10 |  | n20, n82 | 15, 20 | Table 6.2.3.3-1 | Table6.2.3.3-1 |
| NS\_12 | 6.5.3.3.17 | n26 | 5,10 | Table 6.2.3.21-1 | Table 6.2.3.21-2 |
| NS\_13 | 6.5.3.3.18 | n26 | 5 | Table 6.2.3.22-1 | Table 6.2.3.22-2 |
| NS\_14 | 6.5.3.3.19 | n26 | 10,15,20 | Table 6.2.3.23-1 | Table 6.2.3.23-2 |
| NS\_15 | 6.5.3.3.20 | n26 | 5,10,15,20 | Table 6.2.3.24-1 | Table 6.2.3.24-2 |
| NS\_17 | 6.5.3.3.2 | n28, n83 | 5,10 | Table 5.3.2-1 | N/A |
| NS\_18 | 6.5.3.3.3 | n28, n83 | 5 |  | Table 6.2.3.13-1, A1 |
|  |  |  | 10, 15, 20 |  | Table 6.2.3.13-1, A2 |
|  |  |  | 25, 30 |  | Table 6.2.3.13-1, A3, A4, A5 |
| NS\_21 | 6.5.3.3.12 | n30 | 5, 10 |  | Clause 6.2.3.14 |
| NS\_24 | 6.5.3.3.13 | n65 (NOTE 4) | 5, 10, 15, 20 | Table 6.2.3.15-1 | Clause 6.2.3.15 |
| NS\_27 | 6.5.2.3.86.5.3.3.14 | n48 | 5, 10, 15, 20, 30, 40 | Table 6.2.3.16-1 | Table 6.2.3.16-2 |
| NS\_35 | 6.5.2.3.1 | n71 | 5, 10, 15, 20 | Table 5.3.2-1 | N/A |
| NS\_37 | 6.5.3.3.6 | n74(NOTE 3) | 10, 15 | Table 6.2.3.8-1 | Table6.2.3.8-1 |
| NS\_38 | 6.5.3.3.7 | n74 | 5, 10, 15, 20 | Table 6.2.3.9-1 | Table6.2.3.9-1 |
| NS\_39 | 6.5.3.3.8 | n74 | 10, 15, 20 | Table 6.2.3.10-1 | Table 6.2.3.10-1 |
| NS\_40 | 6.5.3.3.9 | n51 | 5 |  | Table6.2.3.5-1 |
| NS\_41 | 6.5.3.3.10 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.11-1 |
| NS\_42 | 6.5.3.3.11 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.12-1 |
| NS\_43 | 6.5.3.3.5 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_43U | 6.5.3.3.5, 6.5.2.4.2 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_44 | 6.5.3.3.24 | n38 | 25, 30, 40 | Table 6.2.3.20-1 | Table 6.2.3.20-1 |
| NS\_45 | 6.5.3.3.21 | n53 | 5, 10 |  | Clause 6.2.3.25 |
| NS\_46 | 6.5.3.3.25 | n7 | 25, 30, 35, 40, 50 | Table 6.2.3.17-1 | Table 6.2.3.17-2 |
| NS\_47 | 6.5.3.3.15 | n41 (Note 5) | 30 | Table 6.2.3.18-1 | Table 6.2.3.18-2 |
| NS\_48 | 6.5.3.3.22 | n1 and n84 | 10, 15, 20, 25, 30, 40, 45, 50 | Table 6.2.3.26-1,Table 6.2.3.26-3 | Table 6.2.3.26-2,Table 6.2.3.26-4 (NOTE 7) |
| NS\_49 | 6.5.3.3.23 | n1 and n84 | 10, 15, 20, 25, 30, 40, 45, 50 | Table 6.2.3.27-1,Table 6.2.3.27-3 | Table 6.2.3.27-2,Table 6.2.3.27-4 (NOTE 7) |
| NS\_50 | 6.5.3.3.16 | n39, n98 | 10, 15, 20, 25, 30, 40 |  | Clause 6.2.3.19 |
| NS\_51 | 6.5.3.3.22 | n65 | 50 | Table 6.2.3.28-1 | Table 6.2.3.28-2 |
| NS\_55 | NOTE 6 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  | N/A |
| NS\_56 | 6.5.3.3.27 | n24, n99 | 5, 10 |  | Clause 6.2.3.30 |
| NS\_57 | NOTE 10 | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  | N/A |
| NS\_100 | 6.5.2.4.2 | n1, n2, n3, n5, n8, n18, n25, n26, n65, n66, n80, n81, n84, n86, n89(NOTE 1) |  |  | Table6.2.3.1-2 |
| NOTE 1: This NS can be signalled for NR bands that have UTRA services deployed.NOTE 2: No A-MPR is applied for 5 MHz BWChannel where the upper channel edge is ≥ 1930 MHz,10 MHz BWChannel where the upper channel edge is ≥ 1950 MHz and 15 MHz BWChannel where the upper channel edge is ≥ 1955 MHz and 20 MHz BWChannel where the upper channel edge is ≥ 1970 MHz.NOTE 3: Applicable when the NR carrier is within 1447.9 – 1462.9 MHz.NOTE 4: Applicable when the upper edge of the channel bandwidth frequency is greater than 1980 MHz.NOTE 5: Applicable when the NR carrier is within 2545 – 2575 MHz.NOTE 6: This NS value is applicable for cells in the range 3450 – 3550 MHz for operations in the USA. This NS value does not indicate any additional spurious emission and maximum output power reduction requirements.NOTE 7: The 1Tx architecture is assumed. For power class 2 UE indicating *txDiversity-r16* [TS 38.306], the additional relaxation of [2] dB is applicable.NOTE 8: The NS\_01 label with the field *additionalPmax* [7] absent is default for all NR bands.NOTE 9: 5 MHz only applies to n90, not n41NOTE 10: This NS value is applicable for cells in the range 3650-3980 MHz for operations in Canada. This NS value does not indicate any additional spurious emission and maximum output power reduction requirements. |

< Start of changes >

< End of changes >

#### 6.3.4.3 Relative power tolerance

The relative power tolerance is the ability of the UE transmitter to set its output power in a target sub-frame (1 ms) relatively to the power of the most recently transmitted reference sub-frame (1 ms) if the transmission gap between these sub-frames is less than or equal to 20 ms.

The minimum requirements specified in Table 6.3.4.3-1 apply when the power of the target and reference sub-frames are within the power range bounded by the minimum output power as defined in clause 6.3.1 and the measured PUMAX as defined in clause 6.2.4.

To account for RF Power amplifier mode changes, 2 exceptions are allowed for each of two test patterns. The test patterns are a monotonically increasing power sweep and a monotonically decreasing power sweep over a range bounded by the requirements of minimum power and maximum power specified in clauses 6.3.1 and 6.2.1, respectively. For those exceptions, the power tolerance limit is a maximum of ± 6.0 dB in Table 6.3.4.3-1.

< Start of changes >

< End of changes >

#### 6.3.4.4 Aggregate power tolerance

The aggregate power control tolerance is the ability of the UE transmitter to maintain its power in a sub-frame (1 ms) during non-contiguous transmissions within 21 ms in response to 0 dB commands with respect to the first UE transmission and all other power control parameters as specified in TS 38.213 [8] kept constant.

The minimum requirement specified in Table 6.3.4.4-1 apply in the power range bounded by the minimum output power as specified in clause 6.3.1 and the maximum output power as specified in clause 6.2.1.

< Start of changes >

< End of changes >

## 6.4D Transmit signal quality for UL MIMO

### 6.4D.0 General

For a UE supporting UL MIMO, the requirements in this section are defined per layer or as the sum of emissions from both antennas to account for the UL MIMO scheme.

Alternatively, when applicable, requirements may be verified per antenna connector using an UL MIMO transmission with codebook of and a configuration defined in Table 6.4D.0-1.

Table 6.4D.0-1: UL MIMO configuration for per connector measurements

|  |  |  |
| --- | --- | --- |
| Transmission scheme | DCI format | Codebook Index |
|  Codebook based uplink | DCI format 0\_1 | Codebook index 0 |

### 6.4D.1 Frequency error for UL MIMO

For UE(s) supporting UL MIMO, the basic measurement interval of modulated carrier frequency is 1 UL slot. The mean value of basic measurements of UE modulated carrier frequency per layer shall be accurate to within ± 0.1 PPM observed over a period of 1 ms of cumulated measurement intervals compared to the carrier frequency received from the NR Node B.

### 6.4D.2 Transmit modulation quality for UL MIMO

For UE supporting UL MIMO, the transmit modulation quality requirements are specified based on measurements made at each transmit antenna connector.

If UE is scheduled for single antenna-port PUSCH transmission by DCI format 0\_0 or by DCI format 0\_1 for single antenna port codebook based transmission, the requirements in clause 6.4.2 apply.

The transmit modulation quality is specified in terms of:

- Error Vector Magnitude (EVM) for the allocated resource blocks (RBs)

- EVM equalizer spectrum flatness derived from the equalizer coefficients generated by the EVM measurement process

- Carrier leakage (caused by IQ offset)

- In-band emissions for the non-allocated RB

In case the parameter 3300 or 3301 is reported from UE via the parameter *txDirectCurrentLocation* in *UplinkTxDirectCurrentList* IE (as defined in TS 38.331 [7]), carrier leakage measurement requirement in clause 6.4D.2.2 and 6.4D.2.3 shall be waived, and the RF correction with regard to the carrier leakage and IQ image shall be omitted during the calculation of transmit modulation quality.

#### 6.4D.2.1 Error Vector Magnitude

For UE with two transmit antenna connectors in closed-loop spatial multiplexing scheme, the Error Vector Magnitude requirements specified in clause 6.4.2.1 apply per layer. The requirements shall be met with the UL MIMO configurations specified in Table 6.2D.1-2.

#### 6.4D.2.2 Carrier leakage

For UE with two transmit antenna connectors in closed-loop spatial multiplexing scheme, the Relative Carrier Leakage Power requirements specified in Table 6.4.2.2-1 which is defined in clause 6.4.2.2 apply per layer. The requirements shall be met with the UL MIMO configurations specified in Table 6.2D.1-2.

< Start of changes >

< End of changes >

### 7.3A.1 General

The reference sensitivity power level REFSENS is the minimum mean power applied to each one of the UE antenna ports for all UE categories, at which the throughput shall meet or exceed the requirements for the specified reference measurement channel. For operations with 4 Rx antenna ports, the MSD in the applicable bands shall be increased by the absolute value of ΔRIB,4R in Table 7.3.2-2 when MSD > 0.

For reference sensitivity exception test points where the specified carrier frequency does not correspond to a valid NR-ARFCN, the closest NR-ARFCN as specified in clause 5.4.2 applies.

< Start of changes >

< End of changes >

### 7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA

For inter-band carrier aggregation with uplink assigned to two NR bands given in Table 7.3A.5-1, Table 7.3A.5-1a, Table 7.3A.5-2 and Table 7.3A.5-2a the reference sensitivity is defined only for the specific uplink and downlink test points specified in Table 7.3A.5-1, Table 7.3A.5-1a, Table 7.3A.5-2 and Table 7.3A.5-2a. For these test points the reference sensitivity requirement specified in Table 7.3.2-1a, Table 7.3.2-1b and Table 7.3.2-2 are relaxed by the amount of the corresponding parameter MSD given in Table 7.3A.5-1, Table 7.3A.5-1a, Table 7.3A.5-2 and Table 7.3A.5-2a.

Table 7.3A.5-1: 2DL/2UL inter-band Reference sensitivity QPSK PREFSENS and uplink/downlink configurations for PC3 CA

|  |  |
| --- | --- |
| Band / Channel bandwidth / NRB / Duplex mode | Source of IMD |
| NR CA band combination | NR band | UL Fc (MHz) | UL/DL BW (MHz) | UL CLRB | DL Fc (MHz) | MSD (dB) | Duplex mode |  |
| CA\_n1-n3 | n1 | 1950 | 5 | 25 | 2140 | 23 | FDD | IMD3 |
|  | n3 | 1760 | 5 | 25 | 1855 | N/A | TDD | N/A |
| CA\_n1-n8 | n1 | 1965 | 5 | 25 | 2155 | 6.0 | FDD | IMD4 |
|  | n8 | 887.5 | 5 | 25 | 932.5 | N/A | FDD | N/A |
| CA\_n1-n77 | 1 | 1950 | 5 | 25 | 2140 | 29.8 | FDD | IMD24 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 4090 | 10 | 50 | 4090 | N/A | TDD | N/A |
|  | 1 | 1950 | 5 | 25 | 2140 | 8.0 | FDD | IMD44 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
| CA\_n1-n78 | n1 | 1950 | 5 | 25 | 2140 | 8.0 | FDD | IMD4 |
|  |  |  |  |  |  |  |  |  |
|  | n78 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
| CA\_n2-n48 | n2 | 1852.5 | 5 | 25 | 1932.5 | 12 | FDD | IMD4 |
|  | n48 | 3625 | 20 | 100 | 3625 | N/A | TDD | N/A |
| CA\_n2-n66 | n2 | 1855 | 5 | 25 | 1935 | 20 | FDD | IMD3 |
|  | n66 | 1775 | 5 | 25 | 2175 | N/A | FDD | N/A |
|  | n2 | 1883.3 | 5 | 25 | 1963.3 | N/A | FDD | N/A |
|  | n66 | 1750 | 5 | 25 | 2150 | 4 | FDD | IMD5 |
| CA\_n2-n77 | n2 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD2 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n2 | 1900 | 5 | 25 | 1980 | 8.0 | FDD | IMD4 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
|  | n2 | 1885 | 5 | 25 | 1965 | 5 | FDD | IMD5 |
|  | n77 | 3810 | 10 | 50 | 3810 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1987.5 | 2.7 | FDD | IMD7 |
|  | n7712 | 3455 | 10 | 1 RBSTART=10 | 3455 | N/A | TDD | N/A |
|  |  | 3945 | 10 | 1 RBSTART=0 | 3945 |  |  |  |
| CA\_n2-n78 | n2 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD24 |
|  |  |  |  |  |  |  |  |  |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| CA\_n3-n5 | n3 | 1771 | 10 | 50 | 1866 | 4 | FDD | IMD4 |
|  | n5 | 838 | 5 | 25 | 883 | N/A | FDD | N/A |
|  | n3 | 1721 | 10 | 50 | 1816 | N/A | FDD | N/A |
|  | n5 | 838 | 5 | 25 | 883 | 24 | FDD | IMD23 |
| CA\_n3-n7 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n7 | 2535 | 10 | 50 | 2655 | 10.2 | FDD | IMD4 |
| CA\_n3-n8 | n3 | 1755 | 10 | 50 | 1850 | N/A | FDD | N/A |
|  | n8 | 900 | 5 | 25 | 945 | 8 | FDD | IMD44 |
|  | n3 | 1747.5 | 10 | 50 | 1842.5 | 6.4 | FDD | IMD5 |
|  | n8 | 897.5 | 5 | 25 | 942.5 | N/A | FDD | N/A |
| CA\_n3-n18 | n18 | 818 | 5 | 25 | 863 | N/A | FDD | N/A |
|  | n3 | 1731 | 5 | 25 | 1826 | 4 | FDD | IMD4 |
| CA\_n3-n20 | 3 | 1775 | 5 | 25 | 1870 | 4 | FDD | IMD4 |
|  | 20 | 840 | 5 | 25 | 799 | N/A | FDD | N/A |
|  | 3 | 1735 | 5 | 25 | 1830 | N/A | FDD | N/A |
|  | 20 | 847 | 5 | 25 | 806 | 9 | FDD | IMD4 |
| CA\_n3-n38 | n3 | 1713 | 5 | 25 | 1808 | 8.2 | FDD | IMD4 |
| n38 | 2617 | 5 | 25 | 2617 | N/A | TDD | N/A |
| CA\_n3-n41 | n3 | 1740 | 5 | 25 | 1835 | 8.2 | FDD | IMD4 |
|  | n41 | 2657.5 | 10 | 50 | 2657.5 | N/A | TDD | N/A |
| CA\_n3-n77 | n3 | 1740 | 5 | 25 | 1835 | 26 | FDD | IMD24 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3575 | 10 | 50 | 3575 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 8.0 | FDD | IMD44 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3435 | 10 | 50 | 3435 | N/A | TDD | N/A |
|  | n3 | N/A | N/A | N/A | N/A | N/A6 | FDD | IMD5 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1877.5 | [2.2] | FDD | IMD7 |
|  | n77 | 3455 | 10 | 1 (RBstart=10) | 3455 | N/A | TDD | N/A |
|  |  | 3945 | 10 | 1 (RBstart=0) | 3945 |  |  |  |
| CA\_n3-n78 | n3 | 1740 | 5 | 25 | 1835 | 26 | FDD | IMD24 |
|  |  |  |  |  |  |  |  |  |
|  | n78 | 3575 | 10 | 25 | 3575 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 8.0 | FDD | IMD44 |
|  |  |  |  |  |  |  |  |  |
|  | n78 | 3435 | 10 | 25 | 3435 | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1877.5 | 2.2 | FDD | IMD7 |
|  | n78 | 33053780 | 1010 | 1 (RBstart=3)1 (RBstart=0) | 33053780 | N/A | TDD | N/A |
| CA\_n5-n7 | n5 | 834 | 5 | 25 | 879 | 12 | FDD | IMD34 |
|  | n7 | 2547 | 10 | 50 | 2667 | N/A | FDD | N/A |
| CA\_n5-n14 | n5 | 836 | 5 | 25 | 881 | 25 | FDD | IMD34 |
|  | n14 | 791 | 5 | 25 | 761 | N/A | FDD | N/A |
|  | n5 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n14 | 795.5 | 5 | 25 | 765.5 | 25 | FDD | IMD3 |
| CA\_n5-n66 | n5 | 838 | 5 | 25 | 883 | 30 | FDD | IMD24 |
|  | n66 | 1721 | 5 | 25 | 2121 | N/A | FDD | N/A |
| CA\_n5-n7713 | n5 | N/A | N/A | N/A | N/A | N/A | FDD | IMD27 |
|  | n7712 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
|  | n5 | 844 | 5 | 25 | 889 | 8.3 | FDD | IMD4 |
|  | n77 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
|  | n5 | 829 | 5 | 25 | 874 | 5.5 | FDD | IMD5 |
|  | n77 | 4190 | 10 | 50 | 4190 | N/A | TDD | N/A |
| CA\_n5-n78 | n5 | 844 | 5 | 25 | 889 | 8.3 | FDD | IMD4 |
|  | n78 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
| CA\_n7-n40 | n7 | 2510 | 5 | 25 | 2630 | 23 | FDD | IMD3 |
|  | n40 | 2390 | 5 | 25 | 2390 | N/A | TDD | N/A |
| CA\_n7-n46 | n7 | 2550 | 10 | 50 | 2670 | 26.8 | FDD | IMD24 |
|  | n46 | 5220 | 20 | 50 | 5220 | N/A | TDD | N/A |
| CA\_n7-n66 | n7 | 2535 | 10 | 50 | 2655 | 15 | FDD | IMD4 |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| CA\_n7-n77 | n7 | 2540 | 5 | 25 | 2660 | 7.1 | FDD | IMD4 |
|  | n77 | 3870 | 10 | 50 | 3870 | N/A | TDD | N/A |
| CA\_n8-n41 | n8 | 882.5 | 5 | 25 | 927.5 | 12.1 | FDD | IMD34 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
| CA\_n8-n78 | n8 | 897.5 | 5 | 25 | 942.5 | 8.3 | FDD | IMD4 |
|  | n78 | 3635 | 10 | 50 | 3635 | N/A | TDD | N/A |
| CA\_n8-n79 | n8 | 897.5 | 5 | 25 | 942.5 | 4.8 | FDD | IMD5 |
|  | n79 | 4532.5 | 40 | 216 | 4532.5 | N/A | TDD | N/A |
| CA\_n12-n66 | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n66 | 1765 | 5 | 25 | 2115 | 5.0 | FDD | IMD4 |
| CA\_n12-n77 | n12 | 702 | 5 | 20 | 732 | 5.5 | FDD | IMD5 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n13-n77 | n13 | 782 | 5 | 20 | 751 | 5.5 | FDD | IMD5 |
|  | n77 | 3880 | 10 | 50 | 3880 | N/A | TDD | N/A |
| CA\_n14-n77 | n14 | 793 | 5 | 20 | 763 | 5.5 | FDD | IMD5 |
|  | n77 | 3935 | 10 | 50 | 3935 | N/A | TDD | N/A |
| CA\_n18-n778 | n18 | N/A | N/A | N/A | N/A | N/A | FDD | IMD4/5 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n18-n789 | n18 | N/A | N/A | N/A | N/A | N/A | FDD | IMD4 |
|  | n78 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n20-n78 | n20 | 850 | 5 | 25 | 809 | 11 | FDD | IMD4 |
|  | n78 | 3359 | 10 | 50 | 3359 | N/A | TDD | N/A |
| CA\_n24-n7710 | n24 | N/A | N/A | N/A | N/A | N/A | FDD | IMD4 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n25-n41 | n25 | N/A | 5 | N/A | 1992.5 | 8.5 | FDD | IMD7 |
|  | n41 | 2545 | 90 | 1 (RBstart=0) | 2545 | N/A | TDD | N/A |
|  |  | 2640 | 100 | 1 (RBstart=221) | 2640 |  |  |  |
| CA\_n25-n48 | n25 | 1852.5 | 5 | 25 | 1932.5 | 12 | FDD | IMD4 |
|  | n48 | 3625 | 20 | 100 | 3625 | N/A | TDD | N/A |
| CA\_n25-n66 | n66 | 1775 | 5 | 25 | 2175 | N/A | FDD | N/A |
|  | n25 | 1855 | 5 | 25 | 1935 | 20 | FDD | IMD3 |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | 23 | FDD | IMD3 |
|  | n25 | 1912.5 | 5 | 25 | 1992.5 | N/A | FDD | N/A |
|  | n66 | 1750 | 5 | 25 | 2150 | 4 | FDD | IMD5 |
|  | n25 | 1883.3 | 5 | 25 | 1963.3 | N/A | FDD | N/A |
| CA\_n25-n77 | n25 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD2 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | 8.0 | FDD | IMD4 |
|  | n77 | 3690 | 10 | 50 | 3690 | N/A | TDD | N/A |
|  | n25 | 1885 | 5 | 25 | 1965 | 5 | FDD | IMD5 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| CA\_n25-n78 | n25 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD24 |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| CA\_n26-n66 | n26 | 838 | 5 | 25 | 883 | 30 | FDD | IMD24 |
|  | n66 | 1721 | 5 | 25 | 2121 | N/A | FDD | N/A |
| CA\_n26-n70 | n26 | 838 | 5 | 25 | 883 | 30 | FDD | IMD24 |
|  | n70 | 1710 | 5 | 25 | 2020 | N/A | FDD | N/A |
| CA\_n28-n50 | n28 | 730 | 10 | 50 | 775 | 15.3 | FDD | IMD2 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | TDD | N/A |
|  | n28 | 740 | 10 | 50 | 785 | 6.0 | FDD | IMD44 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | TDD | N/A |
| CA\_n28-n74 | n28 | 705.5 | 5 | 25 | 760.5 | 24.6 | FDD | IMD2 |
|  | n74 | 1466 | 5 | 25 | 1514 | N/A | FDD | N/A |
|  | n28 | 743 | 5 | 25 | 798 | 11.3 | FDD | IMD411 |
|  | n74 | 1431 | 5 | 25 | 1479 | N/A | FDD | N/A |
|  | n28 | 709 | 5 | 25 | 764 | N/A | FDD | N/A |
|  | n74 | 1466 | 5 | 25 | 1514 | 14.6 | FDD | IMD4 |
|  | n28 | 735.5 | 5 | 25 | 790.5 | N/A | FDD | N/A |
|  | n74 | 1450.4 | 5 | 25 | 1498.4 | 2.5 | FDD | IMD5 |
| CA\_n28-n77 | n28 | N/A | N/A | N/A | N/A | N/A | FDD | IMD27 |
|  | n7712 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n28-n77 | n28 | 705.5 | 5 | 25 | 760.5 | 5.5 | FDD | IMD5 |
|  | n77/n78 | 3582.5 | 10 | 50 | 3582.5 | N/A | TDD | N/A |
| CA\_n30-n77 | n30 | 2310 | 5 | 25 | 2355 | 8.0 | FDD | IMD4 |
|  | n77 | 3487.5 | 10 | 50 | 3487.5 | N/A | TDD | N/A |
|  | n30 | N/A | 5 | N/A | 2352.5 | 3.2 | FDD | IMD7 |
|  | n7712 | 3455 | 10 | 1 (RBstart=17) | 3455 | N/A | TDD | N/A |
|  |  | 3825 | 10 | 1 (RBstart=0) | 3825 |  |  |  |
| CA\_n41-n66 | n4112 | 2545 | 90 | 1 (RBstart=0) | 2545 | N/A | TDD | N/A |
|  |  | 2640 | 100 | 1 (RBstart=171) | 2640 |  |  |  |
|  | n66 | N/A | 5 | N/A | 2197.5 | 32.5 | FDD | IMD5 |
| CA\_n41-n71 | n41 | 2614 | 5 | 25 | 2614 | N/A | TDD | N/A |
|  | n71 | 665 | 5 | 25 | 619 | 11 | FDD | IMD4 |
| CA\_n41-n77 | n4112 | 2545 | 60 | 1 (RBstart=0) | 2545 | N/A | TDD | N/A |
|  |  | 2625 | 100 | 1 (RBstart=272) | 2625 |  |  |  |
|  | n77 | N/A | 10 | N/A | 3305 | 2.7 | FDD | IMD9 |
| CA\_n48-n66 | n48 | 3660 | 5 | 25 | 3660 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | 5.0 | FDD | IMD5 |
| CA\_n48-n70 | n70 | 1697.5 | 25/15 | 25 | 1997.5 | 26 | FDD | IMD24 |
|  |
|  | n48 | 3695 | 10 | 50 | 3695 | N/A | TDD | N/A |
| CA\_n66-n71 | n66 | 1750 | 5 | 25 | 2150 | 5 | FDD | IMD4 |
|  | n71 | 675 | 5 | 25 | 629 | N/A | FDD | N/A |
| CA\_n66-n77 | n66 | 1775 | 5 | 25 | 2175 | 31 | FDD | IMD2 |
|  | n77 | 3950 | 10 | 50 | 3950 | N/A | TDD | N/A |
|  | n66 | 1760 | 5 | 25 | 2160 | 5.0 | FDD | IMD5 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | 1.7 | FDD | IMD7 |
|  | n7712 | 3455 | 10 | 1 (RBstart=10) | 3455 | N/A | TDD | N/A |
|  |  | 3875 | 10 | 1 (RBstart=0) | 3875 |  |  |  |
| CA\_n66-n78 | n66 | 1730 | 5 | 25 | 2130 | 5.0 | FDD | IMD5 |
|  | n78 | 3660 | 10 | 50 | 3660 | N/A | TDD | N/A |
| CA\_n70-n71 | n70 | 1697.5 | 5 | 25 | 1997.5 | 5 | FDD | IMD4 |
|  | n71 | 695.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
| CA\_n70-n78 | n70 | 1705 | 5 | 25 | 2005 | 31 | FDD | IMD2 |
|  | n78 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
|  | n70 | 1705 | 5 | 25 | 2005 | 5.0 | FDD | IMD5 |
|  | n78 | 3560 | 10 | 50 | 3560 | N/A | TDD | N/A |
| CA\_n71-n7713 | n71 | 671 | 5 | 25 | 625 | 5.5 | FDD | IMD5 |
|  | n77 | 3309 | 10 | 50 | 3309 | N/A | TDD | N/A |
| CA\_n71-n78 | n71 | 681.5 | 5 | 25 | 635.5 | 5.5 | FDD | IMD5 |
|  | n78 | 3361.5 | 10 | 50 | 3361.5 | N/A | TDD | N/A |
| NOTE 1: Both of the transmitters shall be set min(+20 dBm, PCMAX\_L,f,c) as defined in clause 6.2A.4NOTE 2: RBSTART = 0, 15 kHz SCS is assumed.NOTE 3: No requirements apply when there is at least one individual RE within the intermodulation generated by the dual uplink is within the downlink transmission bandwidth of the FDD band. The reference sensitivity should only be verified when this is not the case (the requirements specified in clause 7.3 apply).NOTE 4: This band is subject to IMD5 also which MSD is not specified.NOTE 5: Void.NOTE 6: Considering the spectrum holdings of the operator for CA\_n77(2A) (when one uplink sub block is assigned within 3300-3400MHz, the other uplink sub block is not assigned within 4000-4200MHz or vice versa), no IMD5 result will fall in Rx frequency range of band n3. Therefore, no MSD requirement apply for this CA configuration when two uplink sub blocks are assigned within CA\_77(2A).NOTE 7: In current release the maximum separation bandwidth class is 600MHz, therefore, no IMD2 MSD requirement apply for this CA configuration when two uplink sub blocks are assigned within CA\_77(2A).NOTE8: There is no IMD4/5 products in band n18 downlink for n77 operating in 3520 – 3560 MHz, 3700 – 3800MHz and 4000 - 4100MHz frequency range.NOTE 9: There is no IMD4 product in band n18 downlink for n78 operating in 3520 – 3560MHz and 3700-3800MHz frequency range.NOTE 10: There is no IMD4 product in band n24 downlink for n77 operating in 3450 – 3980 MHz and n24 uplink restricted to between 1627.5 – 1637.5 MHz and between 1646.5 – 1656.5 MHz.NOTE 11: This band is subject to IMD5 also which MSD is not specified..NOTE 12: This band supports intra-band non-contiguous uplink configuration.NOTE 13: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped. |

Table 7.3A.5-1a: 2DL/2UL inter-band Reference sensitivity QPSK PREFSENS and uplink/downlink configurations for PC2 CA

|  |  |
| --- | --- |
| Band / Channel bandwidth / NRB / Duplex mode | Source of IMD |
| NR CAConfiguration | NR band | UL Fc (MHz) | UL/DL BW (MHz) | UL CLRB | DL Fc (MHz) | MSD (dB) | Duplex mode |  |
| CA\_n1-n78 | n1 | 1950 | 5 | 25 | 2140 | [17.8] | FDD | IMD4 |
|  | n78 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
| CA\_n3-n41 | n3 | 1740 | 5 | 25 | 1835 | 18.4 | FDD | IMD4 |
|  | n41 | 2657.5 | 10 | 50 | 2657.5 | N/A | TDD | N/A |
| CA\_n3-n78 | n3 | 1740 | 5 | 25 | 1835 | 31.9 | FDD | IMD2 |
|  | n78 | 3575 | 10 | 50 | 3575 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 18.5 | FDD | IMD4 |
|  | n78 | 3435 | 10 | 50 | 3435 | N/A | TDD | N/A |
| CA\_n2-n774 | n2 | 1855 | 5 | 25 | 1935 | 32.10 | FDD | IMD2 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n2 | 1900 | 5 | 25 | 1980 | 19.10 | FDD | IMD4 |
|  |  |  |  |  |  |  |  |  |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n5-n774,6 | 5 | 844 | 5 | 25 | 889 | 18.6 | FDD | IMD4 |
|  | n77 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
| CA\_n5-n78 | n5 | 844 | 5 | 25 | 889 | 18.6 | FDD | IMD4 |
|  | n78 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
| CA\_n12-n77 | 12 | 702 | 5 | 20 | 732 | 11.7 | FDD | IMD5 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | TDD | N/A |
| CA\_n13-n77 | 13 | 782 | 5 | 20 | 751 | 20.5 | FDD | IMD5 |
|  | n77 | 3880 | 10 | 50 | 3880 | N/A | TDD | N/A |
| CA\_n14-n77 | 14 | 795.5 | 5 | 15 | 765.5 | 11.7 | FDD | IMD5 |
|  | n77 | 3947.5 | 10 | 50 | 3947.5 | N/A | TDD | N/A |
| CA\_n25-n774 | n25 | 1855 | 5 | 25 | 1935 | 32.1 | FDD | IMD2 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n25 | 1900 | 5 | 25 | 1980 | 19.1 | FDD | IMD4 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n30-n77 | 30 | 2310 | 5 | 25 | 2355 | 17.6 | FDD | IMD4 |
|  | n77 | 3487.5 | 10 | 50 | 3487.5 | N/A | TDD | N/A |
| CA\_n41-n71 | n41 | 2614 | 5 | 25 | 2614 | N/A | TDD | N/A |
|  | n71 | 665 | 5 | 25 | 619 | 16.3 | FDD | IMD4 |
| CA\_n66-n77 | n66 | 1730 | 5 | 25 | 2130 | 34.33 | FDD | IMD2 |
|  | n77 | 3860 | 10 | 50 | 3860 | N/A | TDD | N/A |
|  | n66 | 1760 | 5 | 25 | 2160 | 11.27 | FDD | IMD5 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | TDD | N/A |
| CA\_n71-n776 | n71 | 681.5 | 5 | 25 | 635.5 | 11.4 | FDD | IMD5 |
|  | n77 | 3361.5 | 10 | 50 | 3361.5 | N/A | TDD | N/A |
| NOTE 1: Both of the transmitters shall be set min(+23 dBm, PCMAX\_L,f,c) as defined in clause 6.2A.4NOTE 2: RBSTART = 0, 15 kHz SCS is assumed.NOTE 3: No requirements apply when there is at least one individual RE within the intermodulation generated by the dual uplink is within the downlink transmission bandwidth of the FDD band. The reference sensitivity should only be verified when this is not the case (the requirements specified in clause 7.3 apply).NOTE 4: This band is subject to IMD5 also which MSD is not specified.NOTE 5: Void.NOTE 6: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped. |

< Start of changes >

< End of changes >

### 7.3C.1 General

The reference sensitivity power level REFSENS is the minimum mean power applied to each one of the UE antenna ports for all UE categories, at which the throughput shall meet or exceed the requirements for the specified reference measurement channel.

For reference sensitivity exception test points where the specified carrier frequency does not correspond to a valid NR-ARFCN, the closest NR-ARFCN as specified in clause 5.4.2 applies.

< Start of changes >

< End of changes >

### 7.3E.3 Reference sensitivity power level for V2X con-current operation

When UE is configured for NR V2X reception on V2X carrier con-current with NR uplink and downlink, NR V2X sidelink throughput for the carrier shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in Annexes A.7.2 with parameters specified in Table 7.3E.2-1 and 7.3E.2-2. Also the NR downlink throughput shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in Annexes A.3 with parameters specified in table 7.3.2-1a, 7.3.2-1b, 7.3.2-2 and 7.3.2-3. The reference sensitivity is defined to be met with all downlink component carriers active. The REFSENS of Uu downlink and PC5 sidelink will be tested at the same time. Exceptions to reference sensitivity with different transmission and reception configurations are allowed for the combinations of aggressor and victim bands specified in table 7.3E.3-3 and 7.3E.3-4. The limited test configurations are specified in table 7.3E.3-3 and 7.3E.3-4 to verify MSD requirements.

For the intra-band con-current NR V2X operation, the reference sensitivity power level shall be applied per carrier. The requirements in clause 7.3.2 shall be appled for NR downlink carrier and the requirements in clause 7.3E.2 shall be applied for NR sidelink carrier. NR V2X sidelink throughput for the carrier shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in Annexes A.7.2. Also the NR downlink throughput shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in Annexes A.3.2 in TS38.101-1.

For reference sensitivity exception test points where the specified carrier frequency does not correspond to a valid NR-ARFCN, the closest NR-ARFCN as specified in clause 5.4.2 applies.

< End of changes >