|  |
| --- |
| 3GPP TR 38.774 V0.2.0 (2025-02) |
| Technical Report |
| 3rd Generation Partnership Project;Technical Specification Group Radio Access Networks;Radio Frequency (RF) requirements for Low-Power Wake-up Signal and Receiver (Release 19) |
|   |
|  |  |
|  |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. |

|  |
| --- |
|  |
| ***3GPP***Postal address3GPP support office address650 Route des Lucioles - Sophia AntipolisValbonne - FRANCETel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16Internethttp://www.3gpp.org |
| ***Copyright Notification***No part may be reproduced except as authorized by written permission.The copyright and the foregoing restriction extend to reproduction in all media.© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).All rights reserved.UMTS™ is a Trade Mark of ETSI registered for the benefit of its members3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersLTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersGSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

1 Scope 6

2 References 6

3 Definitions of terms, symbols and abbreviations 6

3.1 Terms 6

3.2 Symbols 6

3.3 Abbreviations 7

4 Background 7

5 System parameters 7

5.1 General 7

5.2 Operating bands 8

5.3 Channel raster 8

6 Simulation assumptions and evaluation 8

6.1 Performance metric 8

6.2 Simulation assumption 8

6.2.1 General 8

6.2.2 Simulation parameters 8

6.3 Simulation evaluation results 8

7 RF requirements 8

7.1 UE RF 8

7.1.1 General 9

7.1.2 Rx SNR evaluations 9

7.1.3 Architecture and NF considerations 9

7.1.4 REFSENS requirements 9

7.1.5 ASCS requirements 9

7.1.6 ACS requirements 9

7.1.7 IBB requirements 9

7.1.8 OBB requirements 9

7.1.9 other Rx requirements 9

7.2 BS RF 9

7.2.1 General 9

7.2.2 LP-WUS power boosting 9

7.2.3 Regulation relevant spectrum requirements 9

7.2.4 Transmitted signal quality 10

7.2.4 other RF requirements 10

8 Testability 10

8.1 Testability for UE Performance verification 10

8.1.1 General Framework 10

8.1.2 other 10

Annex A (informative): Change history 12

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document is a Technical Report for Rel-19 Radio Frequency (RF) requirements for Low-Power Wake-up Signal and Receiver (LP-WUS/WUR). The purpose is to gather the relevant background information and analysis to address RF requirements for LP-WUS/WUR.

This TR contains discussions and agreements for LP-WUS/WUR RF. The actual RF requirements are added to the corresponding technical specifications.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TR 38.869: "Study on low-power Wake-up Signal and Receiver for NR".

[3] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone".

[4] 3GPP TS 38.101-2: "NR; User Equipment (UE) radio transmission and reception; Part 2: Range 2 Standalone"

[5] 3GPP TS 38.104: “NR; Base Station (BS) radio transmission and reception”.

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**Main radio (MR)**: the Tx/Rx module operating for NR signals/channels apart from signals/channel related to low-power wake-up.

**LP-WUR (LR)**: The Rx module operating for receiving/processing signals/channel related to low-power wake-up.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

<ABBREVIATION> <Expansion>

ACS Adjacent Channel Selectivity

ADC Analog to Digital Converter

ASCS Adjacent Subcarrier selectivity

BB Base Band

BLER Block Error Rate

BPF Band Pass Filter

BS Base Station

CFO Center frequency offset

FAR False Alarm Rate

FR1 Frequency range 1

FR2 Frequency range 2

ICS In-channel Selectivity

IF Intermediate Frequency

LP-WUS Low Power-Wake Up Signal

LP-WUR Low Power-Wake Up Receiver

LP-SS Low Power- Synchronization Signal

LO Local Oscillator

LNA Low Noise Amplifier

LPF Low Pass Filter

LR LP-WUR

MDR Miss Detection Rate

MR Main Radio

NF Noise Figure

OOB Out-of-band

OOK On-Off keying

OFDM Orthogonal Frequency Division Multiplexing

RE Resource Element

REFSENS Reference Sensitivity

RF Radio Frequency

SINR Signal to Interference plus Noise Ratio

SNR Signal to Noise Ratio

UE User Equipment

Tx Transmitter

# 4 Background

<Editor’s note: general background and considerations, details TBD. >

The present document is a technical report for Rel-19 Radio Frequency (RF) requirements for Low-Power Wake-up Signal and Receiver (LP-WUS/WUR). It covers RF requirements analysis for both UE and BS side. Some initial analysis of RF aspects for LP-WUS/WUR were captured in TR 38.869 [2].

# 5 System parameters

## 5.1 General

The channel arrangements presented in this clause for LP-WUS are based on the operating bands and channel raster defined in sub-clause 5.2 and 5.3 below.

## 5.2 Operating bands

LP-WUS is designed to operate in the operating bands defined in Table 5.2-1 of TS 38.101-1 [3] and TS 38.101-2 [4].

## 5.3 Channel raster

The PRB grid between LR and MR is aligned and the LP-WUS RBs can be flexibly allocated within the wider NR carrier. How to make sure the RB alignment between LP-WUS RB and MR RB grid is aligned is UE implementation specific.

# 6 Simulation assumptions and evaluation

## 6.1 Performance metric

<Editor’s note: performance metric to specify RF requirements. >

For RF requirements and conformance testing, the performance metric is 1% MDR. Meanwhile, the FAR assumption for MDR evaluation is </=1%.

## 6.2 Simulation assumption

### 6.2.1 General

To evaluate the RF performance of LP-WUS/WUR, the link level simulation is performed in this WI. This clause captures the simulation assumption for LP-WUS UE RF and BS RF analysis.

### 6.2.2 Simulation parameters

For RF performance analysis, the following simulation assumptions are considered.

**Table 6.2.2-1 Link level simulation assumption for FR1 LP-WUS**

|  |  |
| --- | --- |
| Attributes | Assumptions |
| Case name (waveform) | OOK-1 waveform | OOK-4 waveform |
| Center frequency | 900MHz, 2.6GHz and 3.5GHz |
| Channel structure  | Total 8/16 bits |
| Chip rate | M=1 | M=1/2/4 |
| Coding | 1/2 rate Manchester coding |
| Time error | 0 |
| Residual Frequency error | 0/10/20 ppm |
| SCS | 30kHz |
| UE Channel BW  | 20MHz (51 RB)-case 110MHz (24 RB)-case 25MHz (11 RB)-case 3 |
| WUS RB | * Fixed 11RB ~ 3.96MHz for 10MHz and 20MHz cases
 |
| Position within channel | * For 10/20MHz CBW, Center for ASCS, edge for ACS [assume no ASCS impact]
* For 5MHz CBW, fixed center of channel
 |
| Guardband of NR channel, both wanted cell and interfer cell (ACS) | * For wanted signal: 505kHz for 5MHz, 665kHz for 10MH, 805kHz for 20Mhz
* For interference cell2 5MHz: fixed 505kHz
 |
| Guard RB | * For ASCS: 0 or 1RB on each side of LP-WUS bandwidth
* For ACS: 1/2/3/4 RB
 |
| Filter  | * 3th/5th Order lowpass Butterworth matching fixed 3.96MHz RF bandwidth for 10MHz/20MHz case
	+ Other order lowpass filter is not precluded
* The filter bandwidth is adapted with actual WUS RBs, for 5MHz case
 |
| ASCS | PDSCH mapped on RBs not used for LP-WUS and Guard RB;EPRE of PDSCH /EPRE of LP-WUS = 0 dBSame PSD with WUS signal |
| ACS | PDSCH mapped on interference RBs (11RB for 5MHz CBW), one side;EPRE of PDSCH /EPRE of in-band LP-WUS = [20~33] dBNOTE: decide the interference level depending on SNR |
| Wanted signal level | For ACS, REFSENS + 14 dB for LP-WUS |
| Sampling rate | 7.68MHz |
| ADC bit width | 4/8 bits ADC for ASCS/ACSEncourage companies to provide simulation results with both options for comparison |
| Non-linearities | Not modelled |
| Power boosting | EPRE ratio: 0dB/3dB for OOK-1/OOK-4NOTE: 3dB is optional for simulation |
| Channel Model | Option 1: TDL-C 300 Option 2: AWGNNote: encourage companies to provide simulation results with both options |
| Performance metric | * 1% MDR/BLER as baseline and 5% MDR/BLER as optional
* The following false alarm rate can be considered
	+ 1%

Providing the information whether the false alarm rate is considered or not |
| Note: the detailed Channel structure for LP-WUS is under discussion in RAN1, some parameters may be updated accordingly. |

## 6.3 Simulation evaluation results

<Editor’s note: detailed simulations from each company. FFS detailed structure for each RF requirement>

# 7 RF requirements

## 7.1 UE RF

<Editor’s note: discussions and analysis for UE RF requirements related. Mainly focus on key aspects and conclusions, rather than detailed simulations from each company>

### 7.1.1 General

### 7.1.2 Rx SNR evaluations

### 7.1.3 Architecture and NF considerations

The basic architecture considered for the LP\_WUR is a zero-IF architecture for both envelope and sequence based detectors. This assumption is common for both FR1 and FR2. This is just an assumption made to derive parameters which dictate the requirements. This assumption does not preclude any other RF implementations.

In case of FR1, only single RX is assumed. For FR2 requirement derivation, the baseline assumption is an OFDM based receiver with two receiver chains with mutually orthogonally polarized antennas.

### 7.1.4 REFSENS requirements

### 7.1.5 ASCS requirements

### 7.1.6 ACS requirements

### 7.1.7 IBB requirements

### 7.1.8 OBB requirements

### 7.1.9 other Rx requirements

## 7.2 BS RF

<Editor’s note: discussions and analysis for BS RF requirements related. Mainly focus on key aspects and conclusions, rather than detailed simulations from each company.>

### 7.2.1 General

### 7.2.2 LP-WUS power boosting

### 7.2.3 Regulation relevant spectrum requirements

### 7.2.4 Transmitted signal quality

### 7.2.4 other RF requirements

# 8 Testability

<Editor’s note: discussions and analysis for testability solutions>

## 8.1 Testability for UE Performance verification

### 8.1.1 General Framework

It has been agreed that same LP-WUS RF requirements will apply to all three RRC states. Further the metric used for conformance testing is going to be the same as for defining the requirements i.e., 1% MDR. For demodulation requirements FAR will also be used.

### 8.1.2 other

Annex A (informative):
Change history

|  |
| --- |
| Change history |
| Date | Meeting | TDoc | CR | Rev | Cat | Subject/Comment | New version |
| 2024-10 | RAN4#112bis | R4-2415778 |  |  |  | draft TR skeleton | 0.0.0 |
| 2024-11 | RAN4#113 | R4-2418215 |  |  |  | TR skeletonUpdated structure | 0.0.1 |
| 2024-11 | RAN4#113 | R4-2418234 |  |  |  | R4-2420392 TP to TR 38.774 on Clause 5 (System parameters)R4-2420393 TP to TR 38.774 on LP-WUS | 0.1.0 |
| 2025-02 | RAN4#114 | R4-2500753 |  |  |  | R4-2501381 TP for TR 38.774 on LP-WUSR4-2503027 TP to TR 38.774 on LP-WUS | 0.2.0 |