**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft BigCR Rel-19 BS MMSE-IRC in 38.141-2 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Introducing new requirements for Rel-19 NR BS MMSE-IRC on 38.141-2 |
|  |  |
| ***Summary of change:*** | The following changes are made for 38.141-2:* Introduction of the manufacturer declaration in Section 4.6 (source: R4-2508615 Introduction of manufacturer and applicability rules for MMSE-IRC receiver)
* Introduction of the demodulation requirements for Rel-19 BS MMSE-IRC in Section 8.2.x and the interference model in Annex B.x (source: R4-2508614 Draft CR on 38.141-2 for BS demodulation performance requirements for MMSE-IRC)
* Introduction of the measurement of performance requirements in Annex C.3 and the measurement set up in Annex E.3 (source: R4-2508613 (NR\_demod\_Ph5-Perf) Draft CR for 38.141-2 on Base Station supporting enhanced performance requirements)
* Introduction of applicability rules for enhanced performance requirements in Section 8.1.2.1.x
 |
|  |  |
| ***Consequences if not approved:*** | No requirements for Rel-19 NR BS MMSE-IRC on 38.141-2 |
|  |  |
| ***Clauses affected:*** | 4.6, 8.1.2.1.x, 8.2.x, B.x, C.3, E.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.141-1 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**<Start of Change 1>**

## 4.6 Manufacturer's declarations

The following BS manufacturer's declarations listed in table 4.6-1, when applicable to the BS under test, are required to be provided by the manufacturer for radiated requirements testing for *BS type 1-H,* *BS type 1-O* and *BS type 2-O*.

For the *BS type 1-H* declarations required for the conducted requirements testing, refer to TS 38.141-1 [3], clause 4.6.

Table 4.6-1 Manufacturers declarations for *BS type 1-H, BS type 1-O* and *BS type 2-O* radiated test requirements

| Declaration identifier | Declaration | Description | Applicability(Note 1) |
| --- | --- | --- | --- |
|  |  |  | BS type 1-H(Note 2) | BS type 1-O | BS type 2-O |
| D.1 | Coordinate system reference point | Location of coordinated system reference point in reference to an identifiable physical feature of the BS enclosure. | x | x | x |
| D.2 | Coordinate system orientation | Orientation of the coordinate system in reference to an identifiable physical feature of the BS enclosure. | x | x | x |
| D.3 | Beam identifier | A unique title to identify a beam, e.g. a, b, c or 1, 2, 3. The vendor may declare any number of beams with unique identifiers. The minimum set to declare for conformance, corresponds to the beams at the reference beam direction with the highest intended EIRP, and covering the properties listed below:1) A beam with the narrowest intended BeWθ and narrowest intended BeWϕ possible when narrowest intended BeWθ is used.2) A beam with the narrowest intended BeWϕ and narrowest intended BeWθ possible when narrowest intended BeWϕ is used.3) A beam with the widest intended BeWθ and widest intended BeWϕ possible when widest intended BeWθ is used.4) A beam with the widest intended BeWϕ and widest intended BeWθ possible when widest intended BeWϕ is used.5) A beam which provides the highest intended EIRP of all possible beams.When selecting the above five beam widths for declaration, all beams that the BS is intended to produce shall be considered, including beams that during operation may be identified by any kind of cell or UE specific reference signals, with the exception of any type of beam that is created from a group of transmitters that are not all phase synchronised.(Note 3) | x | x | x |
| D.4 | *Operating bands* and frequency ranges | List of NR *operating band(s)* supported by the BS and if applicable, frequency range(s) within the *operating band(s)* that the BS can operate in. Supported bands declared for every beam (D.3).(Note 4) | c | x | x |
| D.5 | BS requirements set | Declaration of one of the NR base station *requirement*'*s set* as defined for *BS type 1-H*, *BS type 1-O*, *or BS type 2-O*. | c | x | x |
| D.6 | BS class | Declared as Wide Area BS, Medium Range BS, or Local Area BS. | c | x | x |
| D.7 | BS channel band width and SCS support | BS supported SCS and channel bandwidth per supported SCS. Declared for each beam (D.3) and each *operating band* (D.4). | c | x | x |
| D.8 | *OTA peak directions set* reference beam direction pair | The beam direction pair, describing the reference beam peak direction and the reference beam centre direction. Declared for every beam (D.3). | x | x | x |
| D.9 | OTA peak directions set | The OTA peak directions set for each beam. Declared for every beam (D.3). | x | x | x |
| D.10 | *OTA peak directions set* maximum steering direction(s) | The *beam direction pair(s)* corresponding to the following points:1) Φmax: The beam peak direction corresponding to the maximum steering from the reference beam centre direction in the positive Φ direction, while the θ value being the closest possible to the reference beam centre direction.2) Φmin: The beam peak direction corresponding to the maximum steering from the reference beam centre direction in the negative *Φ* direction, while the *θ value being the closest possible to the* reference beam centre direction*.*3) *θ*max: The beam peak direction corresponding to the maximum steering from the reference beam centre direction in the positive *θ* direction, while the *Φ value being the closest possible to the* reference beam centre direction.4) *θ*min: The beam peak direction corresponding to the maximum steering from the reference beam centre direction in the negative *θ* direction, while the *Φ value being the closest possible to the* reference beam centre direction*.*The maximum steering direction(s) may coincide with *the reference beam centre direction*.Declared for every beam (D.3).For the EEIRP requirement in subclause 6.9, the OTA peak direction set maximum steering direction(s) describes the BS steering range(s) for a declared mechanical tilt range (D.64). | x | x | x |
| D.11 | Rated beam EIRP | The rated EIRP level per carrier (Prated,c,EIRP) at the *beam peak direction* associated with a particular *beam direction pair* for each of the declared maximum steering directions (D.10), as well as the reference *beam direction pair* (D.8). Declared for every beam (D.3).(Note 12, 14, 18, 20) | x | x | x |
| D.12 | Beamwidth | The *beamwidth* for the reference *beam direction pair* and the four maximum steering directions. Declared for every beam (D.3). | x | x | x |
| D.13 | Equivalent beams | List of beams which are declared to be equivalent.Equivalent beams imply that the beams are expected to have identical *OTA peak directions sets* and intended to have identical spatial properties at all steering directions within the *OTA peak directions set* when presented with identical signals. All declarations (D.4 – D.12) made for the beams are identical and the transmitter unit*,* RDN and antenna array responsible for generating the beam are of identical design. | x | x | x |
| D.14 | Parallel beams | List of beams which have been declared equivalent (D.13) and can be generated in parallel using independent RF power resources.Independent power resources mean that the beams are transmitted from mutually exclusive transmitter units. | x | x | x |
| D.15 | Number of carriers at maximum TRP | The number of carriers per operating band the BS is capable of generating at maximum TRP declared for every beam (D.3). | n/a | x | x |
| D.16 | Operating bands with multi-band dependencies | List of *operating bands* which are generated using transceiver units supporting operation in multiple *operating bands* through common active RF components. Declared for each *operating band* for which multi-band transceiver is used. | c | x | n/a |
| D.17 | Maximum radiated Base Station RF Bandwidth | Maximum *Base Station RF Bandwidth* in the *operating band*, declared for each supported operating band (D.4).(Note 15) | c | x | x |
| D.18 | Maximum *Radio Bandwidth* of the *operating band* with multi-band dependencies | Largest *Radio Bandwidth* that can be supported by the *operating bands* with multi-band dependencies.Declared for each supported *operating band* which has multi-band dependencies (D.16). | c | x | n/a |
| D.19 | Total RF bandwidth (BWtot) | Total RF bandwidth BWtot of transmitter and receiver, declared per the band combinations (D.52).  | c | x | x |
| D.20 | CA-only operation | Declared of CA-only (with equal power spectral density among carriers) but not multiple carriers operation, declared per *operating band* (D.4) and per beam (D.3). | c | x | x |
| D.21 | Maximum number of supported carriers per *operating band* in multi-band operations  | Maximum number of supported carriers per supported *operating band* declared to have multi-band dependencies (D.16). | c | x | n/a |
| D.22 | Contiguous or non-contiguous spectrum operation support | Ability of BS to support contiguous or non-contiguous (or both) frequency distribution of carriers when operating multi-carrier in an operating band. | c | x | x |
| D.23 | OSDD identifier | A unique identifier for the OSDD. | x | x | n/a |
| D.24 | OSDD operating band support | Operating band supported by the OSDD, declared for every OSDD (D.23).(Note 5) | x | x | n/a |
| D.25 | OTA sensitivity supported BS channel bandwidth and SCS | The *BS* supported SCS and channel bandwidth per supported SCS by each OSDD. | x | x | n/a |
| D.26 | Redirection of receiver target support | Ability to redirect the receiver target related to the OSDD. | x | x | n/a |
| D.27 | Minimum EIS for FR1 (EISminSENS) | The minimum EISminSENS requirement (i.e. maximum allowable EIS value) applicable to all sensitivity RoAoA per OSDD.Declared per NR supported channel BW for the OSDD (D.30).The lowest EIS value for all the declared OSDD's is called minSENS, while its related range of angles of arrival is called *minSENS RoAoA*.(Note 6) | x | x | n/a |
| D.28 | EIS REFSENS for FR2 (EISREFSENS\_50M) | The EISREFSENS\_50M level applicable in the OTA REFSENS RoAoA, (used as a basis for the derivation of the FR2 EISREFSENS for other channel bandwidths supported by BS).(Note 7) | n/a | n/a | x |
| D.29 | Receiver target reference direction Sensitivity Range of Angle of Arrival | The sensitivity RoAoA associated with the receiver target reference direction (D.31) for each OSDD. | x | x | n/a |
| D.30 | Receiver target redirection range | For each OSDD the associated union of all the sensitivity RoAoA achievable through redirecting the receiver target related to the OSDD.(Note 8) | x | x | n/a |
| D.31 | Receiver target reference direction | For each OSDD an associated direction inside the receiver target redirection range (D.30).(Note 9) | x | x | n/a |
| D.32 | Conformance test directions sensitivity RoAoA | For each OSDD that includes a receiver target redirection range, four sensitivity RoAoA comprising the conformance test directions (D.33). | x | x | n/a |
| D.33 | Conformance test directions | For each OSDD four conformance test directions.If the OSDD includes a receiver target redirection range the following four directions shall be declared:1) The direction determined by the maximum φ value achievable inside the receiver target redirection range, while θ value being the closest possible to the receiver target reference direction.2) The direction determined by the minimum φ value achievable inside the receiver target redirection range, while θ value being the closest possible to the receiver target reference direction.3) The direction determined by the maximum θ value achievable inside the receiver target redirection range, while φ value being the closest possible to the receiver target reference direction.4) The direction determined by the minimum θ value achievable inside the receiver target redirection range, while φ value being the closest possible to the receiver target reference direction.If an OSDD does not include a receiver target redirection range the following 4 directions shall be declared:1) The direction determined by the maximum φ value achievable inside the sensitivity RoAoA, while θ value being the closest possible to the receiver target reference direction.2) The direction determined by the minimum φ value achievable inside the sensitivity RoAoA, while θ value being the closest possible to the receiver target reference direction.3) The direction determined by the maximum θ value achievable inside the sensitivity RoAoA, while φ value being the closest possible to the receiver target reference direction.4) The direction determined by the minimum θ value achievable inside the sensitivity RoAoA, while φ value being the closest possible to the receiver target reference direction. | x | x | n/a |
| D.34 | OTA coverage range | Declared as a single range of directions within which selected TX OTA requirements are intended to be met.(Note 10) | x | x | x |
| D.35 | *OTA coverage range* reference direction | The direction describing the reference direction of the *OTA converge range* (D.34).(Note 11) | x | x | x |
| D.36 | OTA coverage range maximum directions | The directions corresponding to the following points:1) The direction determined by the maximum φ value achievable inside the *OTA coverage range*, while θ value being the closest possible to the *OTA coverage range* reference direction.2) The direction determined by the minimum φ value achievable inside the *OTA coverage range*, while θ value being the closest possible to the *OTA coverage range* reference direction.3) The direction determined by the maximum θ value achievable inside the *OTA coverage range*, while φ value being the closest possible to the *OTA coverage range* reference direction.4) The direction determined by the minimum θ value achievable inside the OTA coverage range, while φ value being the closest possible to the OTA coverage range reference direction. | x | x | x |
| D.37 | The rated carrier OTA BS power, Prated,c,TRP | Prated,c,TRP is declared as TRP OTA power per carrier, declared per supported operating band.(Note 12, 14, 18, 20) | n/a | x | x |
| D.38 | Rated transmitter TRP, Prated,t,TRP | Rated total radiated output power*.*Declared per supported *operating band*.(Note 12,14, 18, 20) | n/a | x | x |
| D.39 | CLTA placement for co-location test | The manufacturer shall declare the side of EUT where radiating elements are placed closest to the edge of EUT when applicable. The CLTA shall be placed at the EUT side where radiating elements are placed closest. | n/a | x | n/a |
| D.40 | Spurious emission category | Declare the BS spurious emission category as either category A or B with respect to the limits for spurious emissions, as defined in Recommendation ITU-R SM.329 [5]. | c | x | x |
| D.41 | Additional operating band unwanted emissions | The manufacturer shall declare whether the BS under test is intended to operate in geographic areas where the additional operating band unwanted emission limits defined in clause 6.7.4 apply.(Note 16, Note 19) | c | x | x |
| D.42 | Co-existence with other systems | The manufacturer shall declare whether the BS under test is intended to operate in geographic areas where one or more of the systems GSM850, GSM900, DCS1800, PCS1900, UTRA FDD, UTRA TDD, E-UTRA, PHS and/or NR operating in another operating band are deployed. | c | x | x |
| D.43 | Co-location with other base stations | The manufacturer shall declare whether the BS under test is intended to operate co-located with Base Stations of one or more of the systems GSM850, GSM900, DCS1800, PCS1900, UTRA FDD, UTRA TDD, E-UTRA and/or NR operating in another operating band. | c | x | n/a |
| D.44 | Single-band RIB or multi-band RIB | List of single-band RIB and/or multi-band RIB for the supported operating bands (D.4).  | c | x | n/a |
| D.45 | Single or multiple carrier | BS capability to operate with a single carrier (only) or multiple carriers. Declared per supported operating band, per RIB. (Note 17) | c | x | x |
| D.46 | Maximum number of supported carriers per *operating band* | Maximum number of supported carriers. Declared per supported operating band, per RIB.(Note 15) | c | x | x |
| D.47 | Total maximum number of supported carriers | Maximum number of supported carriers for all supported operating bands. Declared per RIB. | c | x | x |
| D.48 | Other band combination multi-band restrictions | Declare any other limitation under simultaneous operation in the declared band combinations (D.16), which have any impact on the test configuration generation. | c | x | n/a |
| D.49 | Ncells | Number corresponding to the minimum number of cells that can be transmitted by a BS in a particular *operating band*. Declared per *operating band* (D.4). | c | n/a | n/a |
| D.50 | Maximum supported power difference between carriers | Maximum supported power difference between carriers in each supported *operating band*. Declared per *operating band* (D.4). | c | x | x |
| D.51 | Maximum supported power difference between carriers is different *operating bands* | Maximum supported power difference between any two carriers in any two different supported *operating bands*. Declared per operating bands combination (D.52). | c | x | n/a |
| D.52 | Operating band combination support | List of *operating bands* combinations supported by *single-band RIB(s)* and/or *multi-band RIB(s)* of the BS.  | c | x | n/a |
| D.53 | OTA REFSENS RoAoA | Range of angles of arrival associated with the OTA REFSENS.  | n/a | x | x |
| D.54 | OTA REFSENS receiver target reference direction | Reference direction inside the OTA REFSENS RoAoA (D.53). | n/a | x | x |
| D.55 | OTA REFSENS conformance test directions | The following four OTA REFSENS conformance test directions shall be declared:1) The direction determined by the maximum φ value achievable inside the OTA REFSENS RoAoA, while θ value being the closest possible to the OTA REFSENS receiver target reference direction.2) The direction determined by the minimum φ value achievable inside the OTA REFSENS RoAoA, while θ value being the closest possible to the OTA REFSENS receiver target reference direction.3) The direction determined by the maximum θ value achievable inside the OTA REFSENS RoAoA, while φ value being the closest possible to the OTA REFSENS receiver target reference direction.4) The direction determined by the minimum θ value achievable inside the OTA REFSENS RoAoA, while φ value being the closest possible to the OTA REFSENS receiver target reference direction. | n/a | x | x |
| D.56 | Supported frequency range of the NR *operating band* | List of supported frequency ranges representing *fractional bandwidths* (FBW) of *operating bands* with FBW larger than 6%. | x | x | x |
| D.57 | Rated beam EIRP at lower end of the *fractional bandwidth* (Prated,c,FBWlow) | The rated EIRP level per carrier at lower frequency range of the *fractional bandwidth* (Prated,c,FBWlow), at the *beam peak direction* associated with a particular *beam direction pair* for each of the declared maximum steering directions (D.10), as well as the reference *beam direction pair* (D.8).Declared per beam for all supported frequency ranges (D.56).(Note 12, 13, 14, 15, 18, 20) | x | x | x |
| D.58 | Rated beam EIRP at higher frequency range of the *fractional bandwidth* (Prated,c,FBWhigh) | The rated EIRP level per carrier at higher frequency range of the *fractional bandwidth* (Prated,c,FBWhigh), at the *beam peak direction* associated with a particular *beam direction pair* for each of the declared maximum steering directions (D.10), as well as the reference *beam direction pair* (D.8).Declared per beam for all supported frequency ranges in (D.56).(Note 12, 13, 14 ,15, 18, 20) | x | x | x |
| D.59 | Relation between supported maximum RF bandwidth, number of carriers and Rated maximum TRP  | If the rated transmitter TRP and total number of supported carriers are not simultaneously supported, the manufacturer shall declare the following additional parameters:- The reduced number of supported carriers at the rated transmitter TRP;- The reduced total output power at the maximum number of supported carriers. | n/a | x | x |
| D.60 | Inter-band CA  | Declaration of operating band(s) combinations supporting inter‑band CA. Declared per operating band combination (D.52).  | c | x | x |
| D.61 | Intra-band contiguous CA  | Declaration of operating band(s) supporting intra-band contiguous CA. Declared per *operating band* with CA support. | c | x | x |
| D.62 | Intra-band non-contiguous CA  | Declaration of operating band(s) supporting intra-band non‑contiguous CA. Declared per operating band with CA support.  | c | x | x |
| D.63 | Total maximum number of supported carriers in multi-band operation | Maximum number of supported carriers for all supported *operating bands* declared to have multi-band dependencies (D.16)*.*  | c | x | n/a |
| D.64 | The mechanical tilt for EEIRP | The declaration of mechanical tilt together with D.10.(NOTE 21)  | x | x | n/a |
| D.100 | PUSCH mapping type | Declaration of the supported PUSCH mapping type for FR1 as specified in TS 38.211 [20], i.e., type A, type B or both. | c | x | n/a |
| D.101 | PUSCH additional DM-RS positions | Declaration of the supported additional DM-RS position(s) for FR2, i.e., pos0, pos1, or both. | n/a | n/a | x |
| D.102 | PUCCH format | Declaration of the supported PUCCH format(s) as specified in TS 38.211 [20], i.e., format 0, format 1, format 2, format 3, format 4. | c | x | x |
| D.103 | PRACH format and SCS | Declaration of the supported PRACH format(s) as specified in TS 38.211 [20], i.e., format: 0, A1, A2, A3, B4, C0, C2.Declaration of the supported SCS(s) per supported PRACH format with short sequence, as specified in TS 38.211 [20], i.e.: - For *BS type 1-O*: 15 kHz, 30 kHz or both.- For *BS type 2-O*: 60 kHz, 120 kHz or both. | c | x | x |
| D.104 | Additional DM-RS for PUCCH format 3 | Declaration of the supported additional DM-RS for PUCCH format 3: without additional DM-RS, with additional DM-RS or both. | c | x | x |
| D.105 | Additional DM-RS for PUCCH format 4 | Declaration of the supported additional DM-RS for PUCCH format 4: without additional DM-RS, with additional DM-RS or both. | c | x | x |
| D.106 | PUSCH PT-RS  | Declaration of PT-RS in PUSCH support: without PT-RS, with PT-RS or both. | n/a | n/a | x |
| D.107 | PUCCH multi-slot  | Declaration of multi-slot PUCCH support. | c | x | n/a |
| D.108 | UL CA | For the highest supported SCS, declaration of the carrier combination with the largest aggregated bandwidth. If there is more than one combination, the carrier combination with the largest number of carriers shall be declared. | c | x | x |
| D.109 | High speed train | Declaration of high speed train scenario support, i.e. HST support or no HST support | c | x | x |
| D.110 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h. This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if BS declares to support high speed train in D.109. | c | x | n/a |
| D.111 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.This declaration is applicable to PRACH for high speed train only if BS declares to support high speed train in D.109. | c | x | x |
| D.112 | Interlaced formats | Declaration of support of interlaced PUSCH and PUCCH formats, i.e. interlaced format support or no interlaced format support.  | c | x | n/a |
| D.113 | PRACH format with LRA = 1151 for 15 kHz SCS and LRA = 571 for 30 kHz SCS | Declaration of the supported PRACH format(s) as specified in TS 38.211 [17], i.e., format: A2, B4, C2. Declaration of the supported SCS(s) per supported PRACH format as specified in TS 38.211 [17], i.e., 15 kHz, 30 kHz or both. | c | x | n/a |
| D.114 | CG-UCI | Declaration of support of GC-UCI multiplexed on PUSCH as specified in TS 38.211 [17].  | c | x | n/a |
| D.115 | 2-step RA | Declaration of support of 2-step RA type.  | c | x | x |
| D.116 | PUSCH 256QAM | Declaration of PUSCH 256QAM support | c | x | x |
| D.117 | Additional DM-RS for FR2 high speed train | Declaration of supported additional DM-RS position(s) for FR2 high speed train scenario for PUSCH and UL timing adjustment, i.e., pos0, pos1, pos2, or any combination | n/a | n/a | x |
| D.118 | PUCCH sub-slot based repetition formats | Declaration of PUCCH sub-slot based repetition formats. | c | x | n/a |
| D.119 | PUSCH TB over multi-slots | BS support TBoMS over physical consecutive UL slots | c | x | x |
| D.120 | PUSCH TB over multi-slots | BS support TBoMS over physical non-consecutive UL slots | c | x | x |
| D.121 | Supported SCS for TDD PUSCH DM-RS bundling and PUCCH DM-RS bundling | Declaration of supported SCS for TDD PUSCH DM-RS bundling and and PUCCH DM-RS bundling and, i.e. {15 kHz, 30 kHz, 60 kHz 120 kHz} | c | x | x |
| D.122 | Supported FDD PUSCH DM-RS bundling and and PUCCH DM-RS bundling and | Declaration of supporting FDD PUSCH DM-RS bundling and PUCCH DM-RS bundling | c | x | x |
| D.123 | MCS index table 3 | Declaration of support MCS index table 3 as specified in TS 38.214 [18].  | c | x | n/a |
| D.124 | PUSCH repetition type A | Declaration of support PUSCH repetition type A | c | x | x |
| D.125 | Air-to-ground scenario | Declaration of air-to-ground scenario support, i.e. ATG support or no ATG support | c | x | n/a |
| D.126 | PRACH format and SCS for Multiple PRACH transmission | Declaration of the supported PRACH format(s) as specified in TS 38.211 [20] for Multiple PRACH transmission, i.e., format: A2, B4, C2.Declaration of the supported SCS(s) per supported PRACH format with short sequence for Multiple PRACH transmission, as specified in TS 38.211 [20], i.e.: - For BS type 2-O: 120 kHz. | c | n/a | x |
| D.127 | PUSCH with enhanced DM-RS type | Declaration of support enhanced DM-RS typeas specified in TS 38.211 [17]. | x | x | n/a |
| D.128 | PRACH format for HAPS scenario | Declaration of supported PRACH format(s) for HAPS scenario, i.e., format 1. | x | x | n/a |
| D.129 | Enhanced performance requirements  | Declaration of BS supporting enhanced performance requirements  | c | n/a | n/a |
| NOTE 1: Manufacturer declarations applicable per BS *requirement set* were marked as "x". Manufacturer declarations not applicable per BS *requirement set* were marked as "n/a".NOTE 2: For *BS type 1-H*, the only radiated declarations are related to EIRP and EIS requirements. For *BS type 1-H* declarations required for the conducted requirements testing, refer to TS 38.141-1 [3]. For declarations marked as 'c', related conducted declarations in TS 38.141-1 [3] apply. When separately declared, they shall still use the same declaration identifier.NOTE 3: Depending on the capability of the system some of these beams may be the same. For those same beams, testing is not repeated.NOTE 4: These *operating bands* are related to their respective single‑band RIBs.NOTE 5: As each identified OSDD has a declared minimum EIS value (D.27), multiple operating band can only be declared if they have the same minimum EIS declaration.NOTE 6: If the *BS type 1-H* or *BS type 1-O* is not capable of redirecting the receiver target related to the OSDD then there is only one RoAoA applicable to the OSDD.NOTE 7: Although EISREFSENS\_50M level is based on a reference measurement channel with BWChannel = 50 MHz, it does not imply that BS has to support 50 MHz channel bandwidth.NOTE 8: Not applicable for *BS type 2-O*.NOTE 9: For an OSDD without receiver target redirection range, this is a direction inside the sensitivity RoAoA.NOTE 10: *OTA coverage range* is used for conformance testing of such TX OTA requirements as occupied bandwidth, frequency error, TAE or EVM.NOTE 11: The *OTA coverage reference* direction may be the same as the Reference beam direction pair (D.8) but does not have to be.NOTE 12: If a *BS type 2-O* is capable of 64QAM DL operation but not capable of 256QAM DL operation, then up to two rated output power declarations may be made. One declaration is applicable when configured for 64QAM transmissions and the other declaration is applicable when not configured for 64QAM transmissions.NOTE 13: If D.57 and D.58 are declared for certain frequency range (D.56), there shall be no "Rated beam EIRP" declaration (D.11) for the *operating band* containing that particular frequency range.NOTE 14: If a BS is capable of 1024QAM DL operation then up to three rated output power declarations may be made. One declaration is applicable when configured for 1024QAM transmissions, a different declaration is applicable when configured 256QAM transmissions and the other declaration is applicable when configured neither for 256QAM nor 1024QAM transmissions.NOTE 15: Parameters for contiguous or non-contiguous spectrum operation in the operating band are assumed to be the same unless they are separately declared.NOTE 16: If BS is declared to support Band n20 (D.4), the manufacturer shall declare if the BS may operate in geographical areas allocated to broadcasting (DTT). Additionally, related declarations of the emission levels and maximum output power shall be declared. NOTE 17: In case of BS type 1-H, this declaration applies per *TAB connector*. NOTE 18: If a *BS type 2-O* is capable of 256QAM DL operation, then up to three rated output power declarations may be made. One declaration is applicable when configured for 256QAM transmissions, a different declaration is applicable when configured for 64QAM transmissions and the other declaration is applicable when not configured neither for 256QAM nor 64QAM transmissions.NOTE 19: If BS is declared to support Band n24 (D.4), the manufacturer shall declare if the BS may operate in geographical areas where FCC regulations apply. Additionally, related declarations of the emission levels and maximum output power shall be declared.NOTE 20: If a BS is capable of 256QAM DL operation but not capable of 1024QAM DL operation then up to two rated output power declarations may be made. One declaration is applicable when configured for 256QAM transmissions, and the other declaration is applicable when not configured for 256QAM transmissionsNOTE 21: The minimum mechanical down tilt and the maximum electrical steering range shall be declared. If the maximum steering range and the minimum mechanical down tilt are not simultaneously supported, the manufacturer shall declare and test the following two instances: One instance is minimum mechanical down tilt and the reduced electrical steering range, and the other instance is maximum electrical steering range and increased mechanical down tilt. |

**<End of Change 1>**

**<Start of Change 2>**

### 8.1.2 Applicability rule

#### 8.1.2.0 General

Unless otherwise stated, for a BS declared to support more than 2 demodulation branches (for *BS type 1-O* and *BS type 2-O*), the performance requirement tests for 2 demodulation branches shall apply, and the mapping between connectors and demodulation branches is up to BS implementation.

The tests requiring more than [20] dB SNR level are set to N/A in the test requirements.

#### 8.1.2.1 Applicability of PUSCH performance requirements

<***Removed unchanged part***>

##### 8.1.2.1.10 Applicability of requirements with 256QAM

Unless otherwise stated, PUSCH with 256QAM requirements shall apply only for a BS declaring support of 256QAM (see D.116 in table 4.6-1).

##### 8.1.2.1.11 Applicability of PUSCH with enhanced DM-RS requirements

Unless otherwise stated, a BS declares to support PUSCH enhanced DM-RS type (see [D.127] in table 4.6-1) and pass the requirements defined in section 8.2.14, can also consider the tests defined in section 8.2.1 with same configurations except the DM-RS ports as passed.

##### 8.1.2.1.xx Applicability of enhanced performance requirements

Unless otherwise stated, enhanced performance requirements shall apply only for a BS declaring support of enhanced performance requirements (see D.129 in table 4.6-1).

**<End of Change 2>**

**<Start of Change 3>**

### 8.2.X Performance requirements for PUSCH with inter-cell interference

#### 8.2.x.1 Definition and applicability

The performance requirement of PUSCH is determined by a minimum required throughput for a given SNR. The required throughput is expressed as a fraction of maximum throughput for the FRCs listed in annex A. The performance requirements assume HARQ re-transmissions.

Which specific test(s) are applicable to BS is based on the test applicability rules defined in clause 8.1.x.1.

#### 8.2.x.2 Minimum Requirement

For *BS type 1-O*, the minimum requirement is in TS 38.104 [2], clause 11.2.1.x.

#### 8.2.x.3 Test purpose

The test shall verify the receiver's ability to achieve throughput under multipath fading propagation conditions for a given SNR.

#### 8.2.x.4 Method of test

##### 8.2.x.4.1 Initial conditions

Test environment: Normal, see annex B.2.

RF channels to be tested for single carrier: M, see clause 4.9.1.

RF channels to be tested for carrier aggregation: MBW Channel CA; see clause 4.9.1.

Direction to be tested: OTA REFSENS *receiver target reference direction* (see D.54 in table 4.6-1).

##### 8.2.x.4.2 Procedure

1) Place the BS with its manufacturer declared coordinate system reference point in the same place as calibrated point in the test system, as shown in annex E.3.

2) Align the manufacturer declared coordinate system orientation of the BS with the test system.

3) Set the BS in the declared direction to be tested.

4) Connect the BS tester generating the wanted signal, multipath fading simulators and AWGN generators to a test antenna via a combining network in OTA test setup, as shown in annex E.3. Each of the demodulation branch signals should be transmitted on one polarization of the test antenna(s).

5) The characteristics of the wanted signal shall be configured according to the corresponding UL reference measurement channel defined in annex A, and according to additional test parameters listed in table 8.2.x.4.2-1.

Table 8.2.x.4.2-1: Test parameters for testing PUSCH

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Tested signal | Interferer 1 (Note 1 ) | Interferer 2 (Note 1 ) |
| Transform precoding | Disabled | Disabled | Disabled |
| Default TDD UL-DL pattern (Note 2)  | FDD | N/A |
| TDD | 30 kHz SCS:7D1S2U, S=6D:4G:4U |
| Physical cell ID | 0 | 1 | 2 |
| Interference Model | N/A | As specified in clause B.x |
| INR (Note 3) | Set 1 with 1 interferer | N/A | 5.35 dB | N/A |
| Set 1 with 2 interferer | N/A | 7.28 dB | -2.52dB |
| Set 2 with 1 interferer |  | 9.82 dB | N/A |
| Set 2 with 2 interferer |  | 12.38dB | -0.97dB |
| MCS for interferer cell |  | 16QAM  | 16QAM  |
| HARQ | Maximum number of HARQ transmissions | 4 | N/A | N/A |
|  | RV sequence | 0, 2, 3, 1 | N/A | N/A |
| DM-RS | DM-RS configuration type | 1 |
|  | DM-RS duration | single-symbol DM-RS |
|  | Additional DM-RS position | pos1 |
|  | Number of DM-RS CDM group(s) without data | 2 |
|  | Ratio of PUSCH EPRE to DM-RS EPRE | -3 dB |
|  | DM-RS port(s) | {0} |
|  | DM-RS sequence generation | NID0=0, nSCID=0 |
| Time | PUSCH mapping type | A,B |
| domain | Start symbol | 0 |
| resource assignment | Allocation length | 14 |
| Frequency | RB assignment | Full applicable test bandwidth |
| domain resource assignment | Frequency hopping | Disabled |
| Code block group based PUSCH transmission | Disabled |
| Note 1: One explicit interferer, i.e., interferer 1, is modelled for tests with 2 RX antennas. Two explicit interferers are modelled for tests with 4 or 8 RX antennas.Note 2: The same requirements are applicable to FDD and TDD with different UL-DL pattern.Note 3: The respective received energy of each interferer relative to is defined by its associated INR value as specified in clause B.X.1. INR set 1 and set 2 are derived respectively in homogeneous and heterogeneous network scenarios.Note 4: All cells are time-synchronous. |

6) The multipath fading emulators shall be configured according to the corresponding channel model defined in annex J.

7) Adjust the test signal mean power so the calibrated radiated SNR value at the BS receiver is as specified in clause 8.2.x.5.1 *BS type 1-O*  respectively, and that the SNR at the BS receiver is not impacted by the noise floor.

 The power level for the transmission may be set such that the AWGN level at the RIB is equal to the AWGN level in table 8.2.x.4.2-2.

Table 8.2.x.4.2-2: AWGN power level at the BS input

|  |  |  |  |
| --- | --- | --- | --- |
| BS type | Sub-carrier spacing (kHz) | Channel bandwidth (MHz) | AWGN power level |
| BS type 1-O(Note 4) | 15  | 5 | -86.5 - ΔOTAREFSENS dBm / 4.5 MHz |
|  |  | 20 | -80.2 - ΔOTAREFSENS dBm / 19.08 MHz |
|  | 30  | 10 | -83.6 - ΔOTAREFSENS dBm / 8.64 MHz |
|  |  | 100 | -73.1 - ΔOTAREFSENS dBm / 98.28 MHz |
| NOTE 1: ΔOTAREFSENS as declared in D.53 in table 4.6-1 and clause 7.1.NOTE 2: ΔFR2\_REFSENS = -3 dB as described in clause 7.1, since the OTA REFSENS reference direction (as declared in D.54 in table 4.6-1) is used for testing.NOTE 3: EISREFSENS\_50M as declared in D.28 in table 4.6-1.NOTE 4: The AWGN power level contains an AWGN offset of 16dB by default. If needed for test purposes, the AWGN level can be reduced from the default by any value in the range 0dB to 16dB. Changing the AWGN level does not impact the validity of the test, as it reduces the effective base band SNR level. |

8) For reference channels applicable to the BS, measure the throughput.

#### 8.2.x.5 Test Requirement

##### 8.2.x.5.1 Test requirement for *BS type 1-O*

The throughput measured according to clause 8.2.x.4.2 shall not be below the limits for the SNR levels specified in table 8.2.x.5.1-1 to table 8.2.x.5.1-8 for 1Tx transmission.

Table 8.2.x.5.1-1: Test requirements for PUSCH with 70% of maximum throughput, Type A, 5 MHz channel bandwidth, 15 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\* with 1 interferer | G-FR1-A4-8 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\* with 1 interferer | G-FR1-A4-8 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-2: Test requirements for PUSCH with 70% of maximum throughput, Type A, 20 MHz channel bandwidth, 15 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\* with 1 interferer | G-FR1-A4-10 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\* with 1 interferer | G-FR1-A4-10 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-3: Test requirements for PUSCH with 70% of maximum throughput, Type A, 10 MHz channel bandwidth, 30 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\*with 1 interferer | G-FR1-A4-11 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\*with 1 interferer | G-FR1-A4-11 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-4: Test requirements for PUSCH with 70% of maximum throughput, Type A, 100 MHz channel bandwidth, 30 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\*with 1 interferer | G-FR1-A4-14 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\*with 1 interferer | G-FR1-A4-14 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-5: Test requirements for PUSCH with 70% of maximum throughput, Type B, 5 MHz channel bandwidth, 15 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\*with 1 interferer | G-FR1-A4-8 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\*with 1 interferer | G-FR1-A4-8 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-8 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-6: Test requirements for PUSCH with 70% of maximum throughput, Type B, 20 MHz channel bandwidth, 15 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\*with 1 interferer | G-FR1-A4-10 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\*with 1 interferer | G-FR1-A4-10 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-10 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-7: Test requirements for PUSCH with 70% of maximum throughput, Type B, 10 MHz channel bandwidth, 30 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\*with 1 interferer | G-FR1-A4-11 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\*with 1 interferer | G-FR1-A4-11 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-11 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

Table 8.2.x.5.1-8: Test requirements for PUSCH with 70% of maximum throughput, Type B, 100 MHz channel bandwidth, 30 kHz SCS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas(Note 1) | Number of demodulation branches(Note 2) | Propagation conditions and correlation matrix (annex J) (Note 2) | INR set | FRC(Annex A) | Fraction of maximum throughput |  SNR(dB) |
| Tested signal | Interferer 1 | Interferer 2 |
| 1 | 2 | TDLC300-100 | TDLC300-100 | N/A | Set 1\*with 1 interferer | G-FR1-A4-14 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | N/A | Set 2\*with 1 interferer | G-FR1-A4-14 | 70% | TBD |
| 4 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| 8 | TDLC300-100 | TDLC300-100 | TDLC300-100 | Set 1with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| TDLA30-10 | TDLC300-100 | TDLC300-100 | Set 2with 2 interferer | G-FR1-A4-14 | 70% | TBD |
| Note\*: Not applicable for Local Area BS and Home BS. |
| Note 1: Antenna configuration applies for each of the tested signal, interferer 1 and interferer 2.Note 2: The propagation conditions for the tested signal, interferer 1and interferer 2 are statistically independent. |

NOTE: If the above Test Requirement differs from the Minimum Requirement then the Test Tolerance applied for this test is non-zero. The Test Tolerance for this test and the explanation of how the Minimum Requirement has been relaxed by the Test Tolerance is given in annex C.

**<End of Change 3>**

**<Start of Change 4>**

# B.X Interference model for PUSCH requirement with inter-cell interference

## B.x.1 Interference to Noise ratio (INR)

Each interfering cell involved in PUSCH performance requirements with intercell interference is characterized by its associated interferer to noise ratio (INR) value:

where is the received energy from the *i*-th strongest inter-cell interferer involved in the requirement scenario is the the energy of the white noise source consistent with the definition provided in clause xx.

## B.X.2 Interference model for synchronous scenario

This clause provides synchronous network deployment interference model for each explicitly modelled interfering cell in the requirement scenario where the inter-cell interferer (s) are time-synchronous with the tested signal.

In each subframe, each interferer shall transmit 16QAM randomly modulated data over the entire PUSCH region and the same resource blocks as the tested signal. Demodulation reference signal (DM-RS), configured according to Table xxx for enhanced performance requirements is transmitted associated with the transmission of PUSCH.

**<End of Change 4>**

**<Start of Change 5>**

# C.3 Measurement of performance requirements

Table C.3-1: Derivation of test requirements (FR1 OTA performance tests)

|  |  |  |  |
| --- | --- | --- | --- |
| Test  | Minimum Requirement in TS 38.104 [2] | Test Tolerance(TTOTA) | Test requirement in the present document |
| 8.2.1 Performance requirements for PUSCH with transform precoding disabled | See clause 11.2.1.1 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.2 Performance requirements for PUSCH with transform precoding enabled | See clause 11.2.1.2 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.3 Performance requirements for UCI multiplexed on PUSCH  | See clause 11.2.1.3 | 0.6 dB | Formula: SNR + TTOTABLER limit unchanged |
| 8.2.4 Performance requirements for PUSCH for high speed train | SNRs as specified | 0.3 dB | Formula: SNR + TTT-put limit unchanged |
| 8.2.6 Performance requirements for PUSCH with 0.001% BLER | SNRs as specified | 0.3 dB | Formula: SNR + TT + 1dB1dB is added to the test requirement to facilitate early test pass. The BLER delivered by the device during the test will be lower than the test requirement, which enables compliance to the requirement to be demonstrated with a number of observed block errors lower than a certain threshold. |
| 8.2.7 Performance requirements for PUSCH repetition Type A | See clause 11.2.1.7 | 0.6 dB | Formula: SNR + TTOTABLER limit unchanged |
| 8.2.8 Performance requirements for PUSCH mapping type B with non-slot transmission | See clause 11.2.1.8 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.12 Performance requirements for PUSCH TB over Multi-Slots | See clause 11.2.1.12 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.13 Performance requirements for PUSCH with DM-RS bundling | See clause 11.2.1.13 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.14 Performance requirements for PUSCH for ATG | See clause 11.2.1.14 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.15 Performance requirements for PUSCH with enhanced DM-RS | See clause 11.2.1.15 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.x Performance requirements for PUSCH with inter-cell interference | See clause 11.2.1.x | [0.6 dB] | Formula: SNR + TTOTAT-put limit unchanged |
| 8.3.1 Performance requirements for PUCCH format 0 | See clause 11.3.1.2 | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchangedCorrect ACK limit unchanged |
| 8.3.2 Performance requirements for PUCCH format 1 | See clause 11.3.1.3  | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchanged False NACK limit unchangedCorrect ACK limit unchanged |
| 8.3.3 Performance requirements for PUCCH format 2 | See clause 11.3.1.4  | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchangedCorrect ACK limit unchangedUCI BLER limit unchanged |
| 8.3.4 Performance requirements for PUCCH format 3 | See clause 11.3.1.5  | 0.6 dB | Formula: SNR + TTOTAUCI BLER limit unchanged |
| 8.3.5 Performance requirements for PUCCH format 4 | See clause 11.3.1.6  | 0.6 dB | Formula: SNR + TTOTAUCI BLER limit unchanged |
| 8.3.6 Performance requirements for multi-slot PUCCH | See clause 11.3.1.7 | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchangedFalse NACK limit unchangedCorrect ACK limit unchanged |
| 8.3.11 Performance requirements for PUCCH sub-slot based repetition format 0 | See clause 11.3.1.10 | 0.6dB | Formula: SNR + TTOTAFalse ACK limit unchangedCorrect ACK limit unchanged |
| 8.3.12 Performance requirements for PUCCH format 1 with DM-RS bundling | See clause 11.3.1.8 | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchangedFalse NACK limit unchangedCorrect ACK limit unchanged |
| 8.3.13 Performance requirements for PUCCH format 3 with DM-RS bundling | See clause 11.3.1.9 | 0.6 dB | Formula: SNR + TTOTAUCI BLER limit unchanged |
| 8.4.1 PRACH false alarm probability and missed detection | See clause 11.4.1 | 0.6 dB for fading cases0.3 dB for AWGN cases | Formula: SNR + TTOTAPRACH False detection limit unchangedPRACH detection limit unchanged  |
| 8.4.2 Performance requirements for PRACH for high speed train | SNRs as specified | 0.6 dB for fading cases0.3 dB for AWGN cases | Formula: SNR + TTPRACH False detection limit unchangedPRACH detection limit unchanged |
| 8.2.5 Performance requirements for UL timing adjustment | See clause 11.2.1.5 | 0.3 dB for AWGN cases | Formula: SNR + TTOTAT-put limit unchanged |
| NOTE: TT values are applicable for normal condition unless otherwise stated. |

Table C.3-2: Derivation of test requirements (FR2 OTA performance tests)

|  |  |  |  |
| --- | --- | --- | --- |
| Test  | Minimum requirement in TS 38.104 [2] | Test Tolerance(TTOTA) | Test requirement in the present document |
| 8.2.1 Performance requirements for PUSCH with transform precoding disabled | See clause 11.2.2.1 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.2 Performance requirements for PUSCH with transform precoding enabled | See clause 11.2.2.2 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.3 Performance requirements for UCI multiplexed on PUSCH  | See clause 11.2.2.3 | 0.6 dB | Formula: SNR + TTOTABLER limit unchanged |
| 8.2.7 Performance requirements for PUSCH repetition Type A | See clause 11.2.2.4 | 0.6 dB | Formula: SNR + TTOTABLER limit unchanged |
| 8.2.8 Performance requirements for PUSCH mapping Type B with non-slot transmission | See clause 11.2.2.5 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.12 Performance requirements for PUSCH TB over Multi-Slots | See clause 11.2.2.9 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.2.13 Performance requirements for PUSCH with DM-RS bundling | See clause 11.2.2.10 | 0.6 dB | Formula: SNR + TTOTAT-put limit unchanged |
| 8.3.1 Performance requirements for PUCCH format 0 | See clause 11.3.2.2 | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchangedCorrect ACK limit unchanged |
| 8.3.2 Performance requirements for PUCCH format 1 | See clause 11.3.2.3  | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchanged False NACK limit unchangedCorrect ACK limit unchanged |
| 8.3.3 Performance requirements for PUCCH format 2 | See clause 11.3.2.4  | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchangedCorrect ACK limit unchangedUCI BLER limit unchanged |
| 8.3.4 Performance requirements for PUCCH format 3 | See clause 11.3.2.5  | 0.6 dB | Formula: SNR + TTOTAUCI BLER limit unchanged |
| 8.3.5 Performance requirements for PUCCH format 4 | See clause 11.3.2.6  | 0.6 dB | Formula: SNR + TTOTAUCI BLER limit unchanged |
| 8.3.12 Performance requirements for PUCCH format 1 with DM-RS bundling | See clause 11.3.2.7  | 0.6 dB | Formula: SNR + TTOTAFalse ACK limit unchanged False NACK limit unchangedCorrect ACK limit unchanged |
| 8.3.13 Performance requirements for PUCCH format 3 with DM-RS bundling | See clause 11.3.2.8  | 0.6 dB | Formula: SNR + TTOTAUCI BLER limit unchanged |
| 8.4.1 PRACH false alarm probability and missed detection | See clause 11.4.2 | 0.6 dB for fading cases0.3 dB for AWGN cases | Formula: SNR + TTOTAPRACH False detection limit unchangedPRACH detection limit unchanged  |
| NOTE: TT values are applicable for normal condition unless otherwise stated. |

**<End of Change 5>**

**<Start of Change 6>**

# E.3 Performance requirements



Figure E.3-5: Measurement set up for enhanced performance requirements, single TX, dual polarization radiated performance requirements

The OTA chambers shown in figures E.3-1, E.3-2, E.3-3, E.3-4 and E.3-5 are intended to be generic and can be replaced with any suitable OTA chamber (e.g. far field anechoic chamber, CATR, etc.). The PA(s) depicted in figures E.3-1, E.3-2, E.3-3, E.3-4 and E.3-5 is optional. Fading channel emulators are included when needed according to the requirement description.

NOTE: The HARQ Feedback (only for PUSCH) could be done as an RF feedback or as a digital feedback. The HARQ Feedback should be error free.

**<End of Change 6>**