3GPP TSG-RAN WG4 Meeting #94-e R4-2002067

Electronic Meeting, 24th February – 6th March, 2020

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.4* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-3** | **CR** | **Draft** | **rev** | **-** | **Current version:** | **16.2.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR for 38.101-3: to correct editoral errors for spurious emissions for UE co-existence | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | DC\_R16\_1BLTE\_1BNR\_2DL2UL-Core | | | | |  | | ***Date:*** | | 2020-01-15 |
|  |  | | | |  | | |  | |  |
| ***Category:*** | **F** |  | | | | | | ***Release:*** | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | There are some editoral errors in table 6.5B.3.3.2-1.  ULSUP FDM combinations are thus incomplete and must be removed from the specification based on R4-2001697. | | | | | | | | |
| ***Summary of change:*** | | Some editoral errors in table 6.5B.3.3.2-1 are corrected.  The FDM mode of ULSUP combination is removed in the combination tables. | | | | | | | | |
| ***Consequences if not approved:*** | | There are still some editoral errors in table 6.5B.3.3.2-1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.5B.3.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | |  | | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | TS/TR ... CR ... | | | |
| ***affected:*** | |  | **x** | Test specifications | | | TS/TR ... CR ... | | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | TS/TR ... CR ... | | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

## **<Start of Changes>**

##### 6.5B.3.3.2 Spurious emission band UE co-existence

This clause specifies the requirements for the specified EN-DC, for coexistence with protected bands. The requirements in Table 6.5B.3.3.2-1 apply on each component carrier with all component carriers are active.

NOTE: For inter-band EN-DC with uplink assigned to one LTE band and one NR band the requirements in Table 6.5B.3.3.2-1 could be verified by measuring spurious emissions at the specific frequencies where second and third order intermodulation products generated by the two transmitted carriers can occur;

Table 6.5B.3.3.2-1: Requirements

| EN-DC Configuration | Spurious emission | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| DC\_1\_n3 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 38, 40, 41, 43, 44, 50, 51, 65, 67, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 22, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 16 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5,17 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 17 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 17 |
| DC\_1\_n5 | E-UTRA Band 1, 5, 7, 8, 22, 26, 28, 31, 38, 40, 42, 43, 50, 51, 65, 73, 74  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3,34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 41, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_1\_n7 | E-UTRA Band 1, 5, 7, 8, 20, 22, 26, 27, 28, 31,32, 40, 42, 43, 50, 51, 52, 65, 67, 72, 74, 75, 76  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5,16 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_1\_n8 | E-UTRA Band 20, 28, 31, 32, 38, 40, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41, 42, 43, 52  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1, 8, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 12, 15 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5, 16 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 16 |
| DC\_1\_n28 | E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 32, 38, 40, 41, 50, 51, 72, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 43, 75, 76  NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5,16 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 1839.9 | - | 1879.9 | -50 | 1 | 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 9, 15 |
| DC\_1\_n38 | E-UTRA Band 1, 3, 5, 8, 20, 22, 27, 28, 31, 32, 33, 34, 40, 42, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_1\_n40 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 38, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5, 17 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 17 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 17 |
| DC\_1\_n41 | E-UTRA Band 3, 4, 5, 8, 12, 13, 14, 17, 19, 20, 21, 24, 26, 27, 28, 29, 30, 31, 32, 40, 42, 43, 44, 45, 50, 51, 52, 66, 67, 68, 71, 72, 73, 75, 76, 85  NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 8, 20 |
| E-UTRA Band 9, 11, 18, 19, 21, 74 | FDL\_low | - | FDL\_high | -50 | 1 | 20 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 20 |
| DC\_1\_n50 | E-UTRA Band 3, 4, 5, 7, 8, 12, 13, 17, 18, 19, 20, 26, 27, 28, 29, 31, 38, 40, 41, 42, 43, 44, 48, 52, 66, 67, 68, 69, 72, 73, 85  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5,16 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 1400 |  | 1427 | -32 | 27 |  |
| DC\_1\_n51 | E-UTRA Band 7, 12, 13, 17, 20, 22, 27, 28, 29, 31, 38, 44, 48, 67, 68, 69, 72, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5, 2 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 16 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 16 |
| E-UTRA Band 5, 6, 8, 26, 30, 40, 41, 42, 43, 46  NR Band n77, n78, n79, | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_1\_n77  DC\_1\_n84\_ULSUP-TDM\_n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n78  DC\_1\_n84\_ULSUP-TDM\_n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n79  DC\_1\_n84\_ULSUP-TDM\_n79 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 21, 26, 28, 34, 40, 41, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n80 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 38, 40, 41, 43, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73,74, 75, 76,  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 42,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 13 |
| DC\_2\_n5 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 28, 29, 30, 42, 48, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 41, 43 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_2\_n7 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 26, 27, 28, 29, 30, 42, 50, 51, 66, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | 1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_2\_n38 | E-UTRA Band 4, 5, 10, 12, 13, 14,17, 27, 28, 29, 30, 42, 50, 51, 66, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n41 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 42, 48, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n48 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_2\_n66 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 42, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 29, 30, 48, 66 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_2\_n78 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 48, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n1 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 38, 40, 41, 43, 44, 50, 51, 65, 67, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 22, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 16 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5,17 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 17 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 17 |
| DC\_3\_n5 | E-UTRA Band 1, 5, 7, 8, 22, 26, 28, 31, 38, 40, 42, 43, 50, 51, 65, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3,34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n7 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 40, 43, 44, 50, 51, 65, 67, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 22, 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_3\_n20 | E-UTRA Band 1, 7, 8, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3  NR band n20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 38, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| DC\_3\_n28 | E-UTRA Band 1, 42, 43, 50, 51, 65, 74, 75, 76  NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 5, 7, 8, 20, 26, 27, 31, 34, 38, 40, 41, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 13 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 13 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9 |
| DC\_3\_n34 | E-UTRA Band 1, 7, 8, 11, 18, 19, 20, 21, 26, 28, 31, 32, 33, 38, 39, 40, 41, 43, 44, 45, 50, 51, 65, 67, 69,72, 73, 74, 75, 76, 79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 22, 42, 52  NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_3\_n38 | E-UTRA Band 1, 5, 8, 20, 27, 28, 31, 32, 33, 34, 40, 42, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 22, 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n40 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 38, 39, 41, 43, 44. 45, 50, 51, 65, 67, 68, 69, 72, 73, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_3\_n41  DC\_3\_n80\_ULSUP-TDM\_n41, | E-UTRA Band 1, 5, 8, 20, 26, 27, 28, 34, 39, 40, 44, 45, 50, 51, 65, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 14, 20 |
| E-UTRA Band 42,  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 20 |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| DC\_3\_n50 | E-UTRA Band 5, 7, 8, 12, 13, 17, 18, 19, 20, 26, 27, 28, 29, 31, 32, 38, 40, 41, 43, 44, 48, 52, 67, 68, 69, 72, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 2, 4, 33, 34, 39, 42, 65, 66  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 |  |
| Frequency range | 1400 | - | 1427 | -42 | 27 |  |
| DC\_3\_n51 | E-UTRA Band 7, 8, 12, 13, 17, 20, 27, 28, 31, 33, 38, 48, 67, 68, 69, 72, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 1, 5, 6, 22, 26, 30, 34, 36, 40, 41, 42, 43, 44, 46, 65, 71 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n77  DC\_3\_n80\_ULSUP-TDM\_n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_3\_n78  DC\_3\_n80\_ULSUP-TDM\_n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_3\_n79 DC\_3\_n80\_ULSUP-TDM\_n79 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_3\_n82 | E-UTRA Band 1, 3 7, 8, 20，22, 31, 32, 33, 34, 38, 40, 43, 50, 51, 65, 67, 68, 69, 72,74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n84 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 38, 40, 41, 43, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73,74, 75, 76  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_4\_n38 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 27, 28, 29, 30, 43, 50, 51, 66, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_4\_n41 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 24, 25, 26, 27, 28, 29, 30, 48, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_4\_n78 | E-UTRA Band 5, 7, 26, 28, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_5\_n2 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 28, 29, 30, 42, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n2 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_5\_n7 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 28, 29, 30, 31, 34, 40, 42, 43, 65, 66, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 52  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 26 | 859 | - | 869 | -27 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 7, 6 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 7, 6 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 14 |
| DC\_5\_n40 | E-UTRA Band 1, 3, 5, 7, 8, 28, 31, 34, 38, 42, 43, 45, 65, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 52 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_5A\_n48A | E-UTRA Band 2, 4, 5, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_5\_n66 | E-UTRA Band 1, 2, 3, 4, 5, 6, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 34, 38, 40, 43, 45, 50, 51, 65, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 42, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 18, 19 | FDL\_low | - | FDL\_high | -40 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_5\_n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 30, 48, 66, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 5 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_5\_n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 31, 34, 38, 40, 45, 48, 65, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 4 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 7 |
| E-UTRA Band 18, 19 | FDL\_low | - | FDL\_high | -40 | 1 | 4 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| DC\_5\_n79 | Bands 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 31, 34, 38, 40, 42, 43, 45, 48, 50, 51, 65, 66, 70, 71, 73, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| Bands 41, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 18, 19 | FDL\_low | - | FDL\_high | -40 | 1 | 4 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 4 |
| NR Band n257 | 26500 | - | 29500 | -5 | 100 |  |
| NR Band n258 | 24250 | - | 27500 | -5 | 100 |  |
| DC\_7\_n1 | Band 1, 5, 7, 8, 20, 22, 26, 27, 28, 31,32, 40, 42, 43, 50, 51, 52, 65, 67, 72, 74, 75, 76, n78,n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5,16 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7,16 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7,16 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n3 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 22, 42, 52  NR band n78, n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n5 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 22, 26, 28, 29, 30, 31, 40, 42, 43, 50, 51, 65, 66, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 52  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 7, 6 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 7, 6 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 14 |
| DC\_7\_n28 | E-UTRA Band 2, 3, 5, 7, 8, 20, 26, 27, 31, 34, 40, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 4, 10, 42, 43, 50, 51, 65, 66, 74, 75, 76  NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n51 | E-UTRA Band 2, 3, 5, 8, 26, 30, 31, 32, 33, 34, 40, 48, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5 |
| E-UTRA Band 1, 4, 10, 12, 13, 14, 17, 20, 22, 23, 27, 28, 29, 42, 43, 44, 46, 65, 66, 67, 68  NR Band n77, n78, n79, | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_7\_n66 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 26, 27, 28, 29, 30, 43, 50, 51, 66, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 26, 30, 66, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 5 |
| Frequency range | 2570 | - | 2575 | 1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n77 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 33, 34, 40, 50, 51, 65, 66, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 33, 34, 40, 50, 51, 65, 66, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_8\_n1 | E-UTRA Band 20, 28, 31, 32, 38, 40, 50, 51, 65, 67, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41, 42, 43, 52  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1, 8, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 12, 15 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5, 16 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 16 |
| DC\_8\_n3 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 44, 50, 51, 65, 67, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 8 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 5 |
| E-UTRA band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| E-UTRA band 7, 22, 41, 42, 43, 52  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3.12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5. 12 |
| DC\_7\_n80 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 40, 42, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76.  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 42,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_8\_n28 | E-UTRA Band 20, 31, 34, 38, 40, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41, 42, 43, 50, 51, 65, 73, 74, 75, 76  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 9, 10 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11, 12 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9, 12 |
| DC\_8\_n34 | E-UTRA Band 1, 20, 28, 31, 32, 33, 38, 39, 40, 45, 50, 51, 65, 67, 69,72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 22, 41, 42, 43, 52  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| DC\_8\_n39 | E-UTRA Band 1, 34, 40, 45, 50, 51, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| 1. UTRA Band 22, 41, 42, 52   NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_8\_n40 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39,, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 22, 41, 42, 43, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | ３, 12 |
| DC\_8\_n41  DC\_8\_n81\_ULSUP-TDM\_n41, | E-UTRA Band 1, 28, 34, 39, 40, 45, 50, 51, 65, 73, 74, n77,78,79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| DC\_8\_n77 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_8\_n78  DC\_8\_n81\_ULSUP-TDM\_n78 | E-UTRA Band 1, 8, 20, 28, 34, 39, 40,65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_8\_n79  DC\_8\_n81\_ULSUP-TDM\_n79 | E-UTRA Band 1, 8, 28, 34, 39, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3,41,42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_8\_n80 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 3, 7, 22, 41, 42, 43, 52  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 13 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_8A\_n93A\_ULSUP-TDM,  DC\_8A\_n94A\_ULSUP-TDM | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low  FDL\_low | -  - | FDL\_high  FDL\_high | -50  -50 | 1  1 | 2 |
| E-UTRA band 3, 7, 22, 41, 42, 43, 52,  NR Band n77, n78 | FDL\_low  FDL\_low | -  - | FDL\_high  FDL\_high | -50  -50 | 1  1 | 5 |
| E-UTRA 8 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_11\_n77 | E-UTRA Band 1, 3, 18, 19, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_11\_n78 | E-UTRA Band 1, 3, 18, 19, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_11\_n79 | E-UTRA Band 1, 3, 18, 19, 28, 34, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_12\_n2 | E-UTRA Band 5, 13, 14, 17, 24, 26, 27, 30, 41, 50, 53, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 12, 25, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 3 |
| E-UTRA Band 2 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 4, 10, 51, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_12\_n5 | E-UTRA Band 2, 5, 12, 13, 14, 17, 24, 25, 26, 30, 42, 43 50, 51, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Bands 4, 10, 41, 48, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_12\_n66 | E-UTRA Band 2, 4, 5, 13, 14, 17, 24, 25, 26, 27, 29, 30, 41, 50, 51, 70, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 2, 5, 12, 13, 14, 17, 24, 25, 30, 42, 43 50, 51, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_12\_n7 | E-UTRA Band 2, 5, 7, 13, 14, 17, 26, 27, 30, 74,  NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 50, 51,66 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_12\_n71 | E-UTRA Band 5, 13, 14, 17, 24, 26, 27, 30, 48, 50, 51, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 4, 25, 41, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_12\_n78 | E-UTRA Band 2, 5, 7. 13, 17, 25, 26, 41, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 66 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 12 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_13\_n48 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 25, 26, 27, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 14 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 24, 30 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 769 | - | 775 | -35 | 0.00625 | 5 |
| Frequency range | 799 | - | 805 | -35 | 0.00625 | 5 |
| DC\_13\_n66 | Bands 2, 4, 5, 7, 10, 12, 13, 17, 25, 26, 27, 29, 41, 53, 66, 70, 71, 85 and | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 14 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 769 | - | 775 | -35 | 0.00625 | 5 |
| Frequency range | 799 | - | 805 | -35 | 0.00625 | 5, 21 |
| Bands 24, 30, 46, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_13\_n71 | E-UTRA Band 4, 5, 12, 13, 17, 26, 48, 66, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 24, 25, 30, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 5 |
| E-UTRA Band 14, 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 769 | - | 775 | -35 | 0.00625 | 5 |
| Frequency range | 799 | - | 805 | -35 | 0.00625 | 5, 21 |
| DC\_18\_n3 | E-UTRA Band 1, 3, 11, 18, 19, 21, 28, 34, 42, 65  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n77 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n78 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n79 | E-UTRA Band 1, 3, 11, 21, 28, 34, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n77 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n78 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n79 | E-UTRA Band 1, 3, 11, 21, 28, 34, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_20\_n1 | E-UTRA Band 1, 3, 7, 8, 20, 22, 31, 32, 33, 34, 40, 42, 43, 50, 51, 65, 67, 68, 72, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| DC\_20\_n3 | E-UTRA Band 1, 7, 8, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20  E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 38, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| DC\_20\_n7 | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 52 NR band n78, n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_20\_n8 | E-UTRA Band 1, 3, 7, 22, 28, 31, 32, 34, 38, 42, 43, 65, 75, 76  NR bandn78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_20\_n38 | E-UTRA Band 1, 3, 8, 22, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_20\_n28  DC\_20\_n83 | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 34, 38, 42, 43, 65, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_20\_n50 | E-UTRA Band 2, 3, 7, 12, 17, 31, 33, 38, 39, 41, 43, 48, 52, 65, 66, 67, 68, 69, 72, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1400 | - | 1427 | -42 | 27 |  |
| E-UTRA Band 1, 4, 5, 8, 13, 34, 38, 40, 42, 43, 65, 66, 67, 68  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| DC\_20\_n51 | E-UTRA Band 1, 3, 4, 8, 17, 22, 28, 29, 31, 40, 43, 48, 65, 66, 68, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| E-UTRA Band 2, 7, 25, 32, 33, 34, 35, 36, 37, 38, 39, 41, 42, 46, 69, 70  NR Band n77, n78, n79, | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n77 | E-UTRA Band 1, 3, 7, 8, 31, 32, 33, 34, 40, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n78,  DC\_20\_n82\_ULSUP-TDM\_n78 | E-UTRA Band 1, 3, 7, 8, 31, 32, 33, 34, 40, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n80 | E-UTRA Band 1, 7, 8, 27, 28, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76.  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 42,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20A\_n91A\_ULSUP-TDM,  DC\_20A\_n92A\_ULSUP-TDM | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 33, 34, 40, 42, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 42, 69,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| DC\_21\_n77 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_21\_n78 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_21\_n79 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_25\_n41 | E-UTRA Band 4, 5, 10, 12, 13 , 14, 17, 24, 26, 27, 28, 29, 30, 42, 45, 48, 66, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_26\_n25 | 4, 5, 10, 12, 13, 14, 17, 24, 26, 29, 30, 42, 48, 53, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| 41, 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_26\_n41 | E-UTRA Band 1, 2, 3, 4, 5, 10, 11, 12, 13 , 14, 17, 18, 19, 21, 24, 25, 26, 29, 30, 31, 34, 39, 42, 43, 48, 50, 51, 65, 66, 70, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 9, 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 19 |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 3, 19 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| DC\_26\_n77 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 41, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_26\_n78 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 41, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_26\_n79 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 41, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_28\_n3 | E-UTRA Band 1, 22, 42, 43, 50, 51, 65, 74, 75, 76,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 27, 31, 34, 38, 40, 41, 72, 73  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9 |
| DC\_28\_n5 | E-UTRA Band 2, 3, 5, 7, 8, 12, 13, 14, 17, 18, 19, 24, 25, 26, 28, 29, 30, 31, 34, 38, 40, 45, 48, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 |  |  |
| E-UTRA Band 1, 4, 10, 22, 32, 41, 42, 43, 50, 51, 52, 65, 66, 73, 74, 75, 76 NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 4 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| DC\_28\_n7 | E-UTRA Band 2, 3, 5, 8, 20, 26, 27, 31, 34, 40, 72 NR band n7 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 22, 32, 42, 43, 50, 51, 52, 65, 66, 74, 75, 76  NR band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_28\_n8 | E-UTRA Band 20, 31, 34, 38, 40, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41, 42, 43, 50, 51, 52, 65, 73, 74, 75, 76  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_28\_n41 | E-UTRA Band 4, 10, 12, 13, 14, 17, 18, 19, 20, 26, 27, 29, 39, 42, 43, 50, 51, 52, 65, 66, 71, 73, 85  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA Band 2, 3, 5, 8, 24, 25, 30, 31, 34, 40, 44, 48, 70, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 21, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9 |
| DC\_28\_n50 | E-UTRA Band 4, 10, 29, 40, 42, 43, 52, 65, 66, 73, 85  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA Band 2, 3, 5, 7, 8, 18, 19, 25, 26, 27, 31, 34, 38, 39, 41, 48, 52, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9 |
| Frequency range | 1400 |  | 1427 | -32 | 27 |  |
| DC\_28\_n51 | E-UTRA Band 2, 3, 5, 7, 8, 25, 26, 31, 34, 38, 40, 41, 66, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 20, 22, 24, 32, 42, 43, 45, 46, 65, 66, 71, 73  NR band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| DC\_28\_n77 | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_28\_n78  DC\_28\_n83\_ULSUP-TDM\_n78 | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_28\_n79 | E-UTRA Band 3, 5, 8, 18, 19, 34, 39, 40, 41, 42 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_30\_n2 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 42, 48, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 2 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_30\_n5 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 24, 25, 26, 28, 29, 30, 31, 34, 38, 40, 42, 43, 45, 48, 50, 51, 65, 66, 70, 71, 73, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 18, 19 | FDL\_low | - | FDL\_high | -40 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_30\_n66 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 24, 25, 26, 27, 29, 30, 38, 41, 66, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Band 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_38\_n78 | N/A | | | | | | |
| DC\_39\_n40 | E-UTRA Band 1, 8, 22, 26, 34, 41, 42, 44, 45, 50, 51, 52, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1805 |  | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 |  | 1880 | -15.5 | 5 | 5, 7, 18 |
| DC\_39\_n41 | E-UTRA Band 1, 8, 26, 34, 40, 42, 44, 45, 50, 51, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 5 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 5, 7, 19 |
| DC\_39\_n78 | E-UTRA Band 1, 8, 34, 40, 41, 44, 45 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 18 |
| DC\_39\_n79 | E-UTRA Band 1, 8, 34, 40, 41, 44, 45 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 18 |
| DC\_40\_n1 | E-UTRA Band 1, 3, 5, 7, 8, 20, 22, 26, 27, 28, 31, 32, 38, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76  NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_40\_n41 | Bands 1, 3, 5, 8, 26, 27, 28, 34, 39, 42, 44, 45, 50, 51, 65, 73, 74, NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 19 |
| DC\_40\_n77 | N/A | | | | | | |
| DC\_40\_n78 | E-UTRA Band 1, 3, 5, 7, 8, 20, 22, 26, 27, 28, 31, 32, 33, 34, 38, 39, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_40\_n79 | Bands 1, 3, 5, 8, 28, 34, 39, 41, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 19 |
| DC\_41\_n77 | E-UTRA Band 1, 3, 5, 8, 26, 28, 33, 34, 39, 40, 44, 45, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 9, 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 19 |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 3, 19 |
| DC\_41\_n78 | E-UTRA Band 1, 3, 8, 34, 39, 40, 44, 45 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 19 |
| DC\_41\_n79 | E-UTRA Band 1, 3, 5, 8, 9, 11, 18, 19, 21, 28, 34, 40, 42, 44, 45, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_42\_n51 | E-UTRA Band 3, 8, 20, 25, 30, 31, 34, 39, 41, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 2, 4, 5, 6, 7, 10, 12, 13, 14, 17, 23, 24, 26, 27, 28, 29, 32, 38, 40, 44, 46, 65, 66, 67, 68, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_42\_n77 | N/A | | | | | | |
| DC\_42\_n78 | N/A | | | | | | |
| DC\_42\_n79 | N/A | | | | | | |
| DC\_66\_n2 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 22, 24, 26, 27, 28, 29, 30, 41, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 2 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 42, 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_66\_n5 | E-UTRA Band 1, 2, 3, 4, 5, 6, 7, 8, 10, 12, 13, 14, 17, 24, 25, 26, 28, 29, 30, 34, 38, 40, 43, 45, 50, 51, 65, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 42, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 18, 19 | FDL\_low | - | FDL\_high | -40 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_66\_n7 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 26, 27, 28, 29, 30, 43, 50, 51, 66, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_66\_n25 | E-UTRA Band 4, 5, 7, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 38, 41, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 2 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_66\_n41 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 24, 25, 26, 27, 28, 29, 30, 43, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_66\_n48 | E-UTRA Band 2, 4, 5, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_66\_n71 | E-UTRA Band 4, 5, 7,10, 13, 14, 17, 22, 24, 26, 27, 29, 30, 43,50, 51, 66, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 42, 48, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_66\_n78,  DC\_66\_n86\_ULSUP-TDM\_n78 | E-UTRA Band 1, 3, 5, 7, 8, 20, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_71\_n5 | E-UTRA Band 4, 12, 13, 14, 17, 24, 26, 30, 48, 66, 85  NR Band n5 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 5 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NOTE 1: FDL\_low and FDL\_high refer to each E-UTRA frequency band specified in Table 5.5-1 in TS 36.101 [4].  NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.6.3.1-2 are permitted for each assigned E-UTRA carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x 180 kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.  NOTE 3: Applicable when co-existence with PHS system operating in 1884.5 - 1915.7 MHz  NOTE 4: Applicable only when the assigned E-UTRA carrier is confined within 824 MHz and 849 MHz for UE category M1, M2 and UE category NB1 and NB2.  NOTE 5: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.6.3.1-1 and Table 6.6.3.1A-1 from the edge of the channel bandwidth.  NOTE 6: This requirement is applicable for any channel bandwidths within the range 2500 - 2570 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2560.5 - 2562.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2552 - 2560 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.  NOTE 7: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band.  NOTE 8: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplink  NOTE 9: Applicable when the assigned E-UTRA carrier is confined within 718 MHz and 748 MHz and when the channel bandwidth used is 5 or 10 MHz.  NOTE 10: As exceptions, measurements with a level up to the applicable requirement of -36 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 2nd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 2nd harmonic totally or partially overlaps the measurement bandwidth (MBW).  NOTE 11: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).  NOTE 12: This requirement is applicable only for the following cases: A: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 902.5 MHz ≤ Fc < 907.5 MHz with an uplink transmission bandwidth less than or equal to 20 RB; B: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 907.5 MHz ≤ Fc ≤ 912.5 MHz without any restriction on uplink transmission bandwidth; C: for carriers of 10 MHz channel bandwidth when carrier centre frequency (Fc) is Fc = 910 MHz with an uplink transmission bandwidth less than or equal to 32 RB with RBstart > 3.  NOTE13: This requirement applies for 5, 10, 15 and 20 MHz E-UTRA channel bandwidth allocated within 1744.9MHz and 1784.9MHz.  NOTE 14: This requirement is applicable for 5 and 10 MHz E-UTRA channel bandwidth allocated within 718-728MHz. For carriers of 10 MHz bandwidth, this requirement applies for an uplink transmission bandwidth less than or equal to 30 RB with RBstart > 1 and RBstart < 48.  NOTE 15: Applicable when NS\_05 in clause 6.6.3.3.1 is signalled by the network.  NOTE 16: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.  NOTE 17: This requirement is applicable in the case of a 10 MHz E-UTRA carrier confined within 703 MHz and 733 MHz, otherwise the requirement of -25 dBm with a measurement bandwidth of 8 MHz applies.  NOTE 18: This requirement is only applicable for E-UTRA carriers with bandwidth confined within 1885 - 1920 MHz (requirement for carriers with at least 1RB confined within 1880 - 1885 MHz is not specified). This requirement applies for an uplink transmission bandwidth less than or equal to 54 RB for E-UTRA carriers of 15 MHz bandwidth when carrier center frequency is within the range 1892.5 - 1894.5 MHz and for E-UTRA carriers of 20 MHz bandwidth when carrier center frequency is within the range 1895 - 1903 MHz.  NOTE 19: This requirement applies when the E-UTRA and NR carriers are confined within 2545 – 2575 MHz or 2595 - 2645 MHz and the channel bandwidth is 10 or 20 MHz  NOTE 20: For category NB1 and NB2 UE when carrier centre frequency is 1920.1 MHz, in case of single-tone uplink transmission the requirement is applicable only for sub-carrier index > 2.  NOTE 21: Whether the applicable frequency range should be 793 – 805 MHz instead of 799 – 805 MHz is TBD | | | | | | | |

NOTE: To simplify the above Table, E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation or both E-UTRA and NR operation. NR band numbers are listed for bands which are specified only for NR operation.

## **<End of Changes>**