**3GPP TSG-RAN WG4 Meeting #94-e R4-20xxxxx**

**Electronic Meeting, Feb.24th – Mar.6th 2020**

**Agenda item:** 8.16.1.3 /8.16.1.4 /8.16.1.5

**Source:** OPPO

**Title:** Email discussion summary for RAN4#94e\_#66\_NR\_CSIRS\_L3meas\_RRM\_Part\_2

**Document for:** Information

# Introduction

*Briefly introduce background, the scope of this email discussion and provide some guidelines for email discussion if necessary.*

In order to make progress on CSI-RS L3 measurement, we would like to discuss the following topics/issues and try to get some agreements in this meeting.

* + Topic #1:Measurement capability (sub-agenda 8.16.1.3)

Sub-topic 1-1: Applicability and assumption for CSI-RS based measurement capability

* + - Issue 1-1-1:Applicability for CSI-RS based measurement capability
		- Issue 1-1-2:Measurement capabilities per MO or per layer

Sub-topic 1-2: Requirements for measurement capability

* + - Issue 1-2-1:Number of frequency layers to be monitored
		- Issue 1-2-2:Number of cells to be monitored
		- Issue 1-2-3:Number of CSI-RS resource/beams to be monitored
		- Issue 1-2-4:UE capability to indicate maximum number of CSI-RS resources in a slot per MO
	+ Topic #2: Measurement requirements for intra and inter-frequency measurement (sub-agenda 8.16.1.4/.5)

 Sub-topic 2-1: Framework of CSI-RS based measurement requirements

* + - Issue 2-1-1: Components of CSI-RS based measurement requirements
		- Issue 2-1-2: Specification structure of CSI-RS L3 intra-f/inter-f measurement requirement

Sub-topic 2-: Key open issues

* + - Issue 2-2-1: CSSF
		- Issue 2-2-2: Scaling factor for RX beam sweeping
		- Issue 2-2-3: Factors to consider for scheduling restriction
		- Issue 2-2-4: Requirements for scheduling restriction
		- Issue 2-2-5: Whether to restrict CSI-RS resources outside of DRX/MG duration
		- Issue 2-2-6: Others

*List of candidate target of email discussion for 1st round and 2nd round*

* **1st round**: Collect views from companies, and try to achieve agreements on the two sub-agenda:
	+ Measurement capability
	+ Measurement requirement for intra/inter-frequency measurement
* **2nd round**: Discuss the remaining issues and propose a way forward for next meeting

Note: Since some issues are highly related to definition of CSI-RS intra/inter-frequency measurement, we try to recognize these and suggest to collect views in 1st round and try to get agreements in 1st/2nd round.

# Topic #1: Measurement capability

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [**R4-2000464**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000464.zip) | MediaTek inc. | Observation 1: SSB-based cell detection is still required for CSI-RS based L3 measurement. Proposal 1: Requirement is only defined when • the CSI-RS based measurement is configured with SSB based measurement within the same MO,• UE can perform CSI-RS and SSB measurement with overlapped bandwidth in the same time duration Proposal 2: Given proposal 1 is agreed, CSI-RS based L3 measurement does not add additional frequency layers to be monitored on top of the number specified for SSB based measurement.Observation 2: If proposal 1 is not agreed, CSI-RS based L3 measurement will add additional frequency layers to be monitored on top of the number specified for SSB based measurement, resulting the extended measurement delay of every frequency layer.Observation 3: If RAN4 allows some CSI-RS resources in the same MO to be intra-frequency and the other to be inter-frequency, the total number of frequency layers to be monitored will be increased further.Proposal 3: There is no need to introduce additional number of cells to be monitored per layer based on L3 CSI-RS on top of the requirements already specified for SSB.Proposal 4: Regarding the number of CSI-RS (beams) to be monitored per layer based on L3 CSI-RS, requirements defined the same requirements as those for SSB. Proposal 5: If network configures more CSI-RS resources in an MO than the UE measurement capability, the UE behavior is undefined. |
| [**R4-2000585**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000585.zip) | CATT | Proposal 1: CSI-RS based UE measurement capabilities shall specified in terms of:- Number of carrier to be monitored if CSI-RS resources are configured- Number of cell to be monitored per MO- Number of CSI-RS resources to be monitored per MOProposal 2: UE shall be able to measure at least 3 CSI-RS frequency layers.Proposal 3: UE shall be able to measure at least 8 NR frequency layers in total, including SSB frequency layers and CSI-RS frequency layers.Proposal 4: UE shall be able to measure at least 14 carriers of all RATs in total.Proposal 5: For the number of CSI-RS resource, UE shall monitor at least 32 CSI-RS resources per frequency layer considering mobility performance and UE’s complexity. |
| [**R4-2000995**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000995.zip) | OPPO | Observation 1：CSI-RS resource for mobility is beneficial to be configured with associated SSB, which can reduce the complexity of both network and UE implementation.Proposal 1: Share the current number of frequency layers to be monitored for both SSB based measurement and CSI-RS frequency layers.• UE shall be able to measure at least 7 NR frequency layers in total, including SSB frequency layers and CSI-RS frequency layers.• UE shall be able to measure at least 13 carriers of all RATs in total, including SSB frequency layers and CSI-RS frequency layers.Proposal 2: No need to introduce additional number of cells to be monitored per layer based on L3 CSI-RS on top of the requirements already specified for SSB.Proposal 3: 32 CSI-RS resources can be as baseline for discussion, and RAN4 can further decide the value based on more vendors’ input. |
| [**R4-2001276**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2001276.zip) | ZTE | Proposal 1. A UE shall be capable of monitoring at least 7 NR inter frequency layers configured by serving cell. The UE shall be capable of performing measurements including (SS-RSRP, SS-RSRQ, SS-SINR, CSI-RSRP, CSI-RSRQ, CSI-SINR, E-UTRAN RSRP, E-UTRAN RSRQ, E-UTRAN RS-SINR measurements, etc.) of detected cells on all the layers. Proposal 2. UE capability of number of cells and number of CSI-RS resources that the UE shall be capable of performing CSI-RS based measurement for L3 mobility should be specified. Proposal 3. UE shall be capable of performing CSI-RS based measurements for at least [8] identified cells in FR1 for intra frequency measurement and at least [4] identified cells in FR1 for inter frequency measurement.Proposal 4. UE shall be capable of performing CSI-RS based measurements for at least [6] identified cells in FR2 for intra frequency measurement and at least [4] identified cells in FR2 for inter frequency measurement.Proposal 5. FFS the requirements for total number of cells the UE shall be capable of performing SSB based and CSI-RS based measurements.Proposal 6. Number of CSI-RS resources shall be monitored by UE,- [24] CSI-RS resources for intra frequency measurements in FR1- [48] CSI-RS resources for intra frequency measurements in FR2,- [16] CSI-RS resources for inter frequency measurements in FR1,- [24] CSI-RS resources for inter frequency measurements in FR2. |
| [**R4-2001647**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2001647.zip) | Huawei, HiSilicon | Proposal 1: UE shall be able to measure at least 3 CSI-RS frequency layers for CSI-RS based mobility. Proposal 2: UE shall be able to measure at least 7 SSB frequency layers, including MO with SSB as mobility RS, and MO with CSI-RS as mobility RS with associated SSB.Proposal 3: UE shall be able to measure at least 8 NR frequency layers in total, including SSB frequency layers and CSI-RS frequency layers.Proposal 4: UE shall be able to measure at least 14 carriers of all RATs in total.Proposal 5: RAN4 should discuss the total number of cells and CSI-RS resources UE should measure per MO.Proposal 6: Update existing UE capability maxNumberCSI-RS-RRM-RS-SINR or define another capability for UE to indicate maximum number of CSI-RS resources in a slot per MO.Proposal 7: The UE capability on UE buffering and processing time RAN1 defined for PRS is re-used for CSI-RS. Alternatively, define UE capability on the minimum separation between two slots with CSI-RS resources. |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 1-1: Assumption and applicability

*Sub-topic description*

In this section, we discuss assumption and applicability of CSI-RS based measurement capability.

*Open issues and candidate options before e-meeting:*

**Issue 1-1-1: Applicability of CSI-RS based measurement capability**

* Proposals
	+ Option 1: Only define the requirements when the CSI-RS based measurement is configured with SSB based measurement within the same MO, and UE can perform CSI-RS and SSB measurement with overlapped bandwidth in the same time duration
	+ Option 2: No restriction on MO configurations
* Recommended WF
	+ Collect the views from companies and try to achieve agreement in 1st round discussion
	+ If Option 1 is agreed, CSI-RS based L3 measurement does not add additional frequency layers to be monitored on top of the number specified for SSB based measurement.
	+ If Option 1 is not agreed, FFS measurement capability on top of the number specified for SSB based measurement, including
		- frequency layers to be monitored
		- cells to be monitored
		- CSI-RS resource/beams to be monitored

**Issue 1-1-2: Measurement capabilities per MO or per layer**

* Proposals
	+ Option 1: RAN4 should discuss the total number of cells and CSI-RS resources UE should measure per MO
	+ Option 2: RAN4 should discuss the total number of cells and CSI-RS resources UE should measure per layer
* Recommended WF
	+ RAN4 design shall not contradict RAN2 agreements on MO signalling
		- the same MO can configure more than one frequency layer
	+ Tentative agreement:

RAN4 would reuse the rules for SSB based measurement, which means number of cells and CSI-RS resources to be discussed per layer.

### Sub-topic 1-2: Requirements of measurement capabilities

*Sub-topic description*

In this section, we discuss measurement capabilities for CSI-RS based L3 measurement including:

* number of frequency layers to be monitored
* number of cells to be monitored per layer
* number of CSI-RS resource/beams to be monitored per layer

*Open issues and candidate options before e-meeting:*

**Issue 1-2-1: number of frequency layers to be monitored**

* Proposals
	+ Option 1 (MediaTek, OPPO, ZTE):

No need to introduce additional frequency layer, reusing the current UE measurement requirements defined in TS38.133

* + - UE shall be able to measure at least 7 NR frequency layers in total, including SSB frequency layers and CSI-RS frequency layers.
		- UE shall be able to measure at least 13 carriers of all RATs in total, including SSB frequency layers and CSI-RS frequency layers.
	+ Option 2 (CATT, Huawei):
		- UE shall be able to measure at least 3 CSI-RS frequency layers.
		- UE shall be able to measure at least 8 NR frequency layers in total, including SSB frequency layers and CSI-RS frequency layers.
		- UE shall be able to measure at least 14 carriers of all RATs in total.
* Recommended WF
	+ Tentative agreement: Option 1
	+ Collect the views from companies and try to achieve agreement in 1st round discussion

**Issue 1-2-2: number of cells to be monitored per layer/MO**

* Proposals
	+ Option 1 (MediaTek, OPPO): No need to introduce additional number of cells to be monitored per layer based on L3 CSI-RS on top of the requirements already specified for SSB.
	+ Option 2 (ZTE): UE shall be capable of performing CSI-RS based measurements for at least [8] identified cells in FR1 for intra frequency measurement and at least [4] identified cells in FR1 for inter frequency measurement, at least [6] identified cells in FR2 for intra frequency measurement and at least [4] identified cells in FR2 for inter frequency measurement.
	+ Option 3 (Huawei): RAN4 should discuss the total number of cells and CSI-RS resources UE should measure per MO.
	+ Recommended WF
	+ Tentative agreement: Option 1
	+ Collect the views from companies and try to achieve agreement in 1st round discussion

**Issue 1-2-3: number of CSI-RS resource/beams to be monitored per layer/MO**

* Proposals
	+ Option 1: UE shall monitor at least 32 CSI-RS resources per frequency layer
	+ Option 2: Number of CSI-RS resources shall be monitored by UE,
		- [24] CSI-RS resources for intra frequency measurements in FR1
		- [48] CSI-RS resources for intra frequency measurements in FR2,
		- [16] CSI-RS resources for inter frequency measurements in FR1,
		- [24] CSI-RS resources for inter frequency measurements in FR2.
	+ Option 3: Requirements defined the same requirements as those for SSB.
	+ Recommended WF
	+ Collect the views from companies and try to achieve agreement in 1st round discussion
		- FFS on UE behaviour if network configures more CSI-RS resources in an MO than the UE measurement capability

**Issue 1-2-4: UE capability to indicate maximum number of CSI-RS resources in a slot per MO**

* Proposals
	+ Option 1: Reuse existing UE capability *maxNumberCSI-RS-RRM-RS-SIN*R and update the value.
	+ Option 2: Define another capability for UE to indicate maximum number of CSI-RS resources per MO in a slot.
	+ Recommended WF
	+ Collect the views from companies and try to achieve agreement in 2nd round discussion
		- FFS on UE capability
		- FFS how to account the UE buffering and processing capability in the requirements
		- Send LS and ask for RAN1/2’s view if needed

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Sub topic 1-1: Assumption and applicabilityIssue 1-1-1: Support Option 1. Regarding the definition of CSI-RS intra-frequency and inter-frequency, the restriction of MO configuration is beneficial to specify requirements for the limited or selected scenarios. In this case, CSI-RS based L3 measurement does not add additional frequency layers to be monitored on top of the number specified for SSB based measurement.Issue 1-1-2: Prefer capability as per layer, which follows the similar rules for SSB based measurement.Sub topic 1-2: Requirements of measurement capabilities Issue 1-2-1: support Option 1. The reason is similar as issue 1-1-1.Issue 1-2-2: support Option 1Issue 1-2-3: support Option 1Issue 1-2-4: support Option 1 |
| Apple | Issue 1-1-1: It is not very clear of us on option 1. Does that mean CSI-RS and SSB not only share the same center frequency but also share the same OFDM symbol? In general, we think this restriction is quite strong. Issue 1-1-2:Option 2 seems more reasonable than option 1. Depend on the conclusion of MO definition/restriction, there can be multiple MO per frequency layer and multiple frequency layer per MO. If we limit all bandwidth in the same MO to be the same, we then eliminate the case of multiple frequency layer per MO. The situation becomes clear that we only need to focus on number of cells and CSI-RS resources per frequency layer, which can include multiple MO. Issue 1-2-1: Option 1….Issue 1-2-2: option 1Others: |
| QC | Issue 1-1-1: Applicability of CSI-RS based measurement capabilityNot clear on why the restriction is needed to be in the same MO. It is understood that in order to do CSI-RS measurement either there will be an associated SSB that UE is racking for timing or that sync to serving cell is indicated in some fashion. Why is the restriction important?Issue 1-2-1: number of frequency layers to be monitoredWhat does a frequency layer for CSI-RS mean. Is it just the same center frequency of CSI-RS resource or same center frequency and BW, With SSB it is simpler definition since BW is always the same. Issue 1-2-3: number of CSI-RS resource/beams to be monitored per layer/MOThe total number of CSI resources that UE can monitor should come from the UE capability maxNumberCSI-RS-RRM-RS-SINR. How to split that up per layer would or MO would depend on resolution of Issue 1-1-1 and Issue 1-2-1Issue 1-2-4: UE capability to indicate maximum number of CSI-RS resources in a slot per MOWe agree with option 1, but we shouldn’t need to update the value since it is UE capability.  |
| Ericsson | Issue 1-1-1: option 2 (no restriction)Issue 1-1-2: option 2 (per frequency layer)Issue 1-2-1: option 1Issue 1-2-2: option 1Issue 1-2-3: option 2Issue 1-2-4: option 1 |
| CATT | Issue 1-1-1: Applicability of CSI-RS based measurement capabilitySame view as QC, the restriction is not needed, and both associated SSB case and non-associated case shall be considered. For non-associated SSB case, the target cell is synchronized to the serving cell, e.g. in TDD network scenarios, UE is not required to detect the target SSB for tracking timing. From our perspective, this is more useful case.**Issue 1-1-2: Measurement capabilities per MO or per layer**According to RAN1/RAN2’s agreement, frequency layer is Measurement object (MO), so not very clear the intention for this issue. In RAN4, according to my understanding, the capability should be defined per frequency layer.**Issue 1-2-1: number of frequency layers to be monitored**At least 3 CSI-RS frequency layer;At least 8 NR frequency layers in total, including SSB frequency layers and CSI-RS frequency layersAt least 14 carriers of all RATs in totalFor associated SSB case, UE is required to detect SSB on target cell firstly, then the configured CSI-RS can be measured. So, the measurement capability can be considered as SSB based measurement capability. For non-associated SSB case, It is required UE capable to perform CSI-RS based layers.**Issue 1-2-2: number of cells to be monitored per layer/MO**Support option 3, need more discussion on the number.**Issue 1-2-3: number of CSI-RS resource/beams to be monitored per layer/MO**Option 1 can be discussed as start point. Option 2 is also fine for us.**Issue 1-2-4: UE capability to indicate maximum number of CSI-RS resources in a slot per MO**Support option 1. |
| Intel | Sub topic 1-1: Issue 1-1-2: Before discussing the UE capability requirement, prefer to discuss MO configuration, intra-frequency measurement definition and layer definition first. There may be some new scenarios, it’s hard to decide which one is simpler. If there are both intra and inter frequency measurement in one MO, can we still define the UE capability requirement based on MO? In one MO, if there several bandwidths, do they belong to same layer or different layer? If the intra-frequency measurement is defined without fixing the center-frequency, there may be several MOs for intra-frequency. Whether to define the MO number for intra-frequency? Sub topic 1-2: same as the comment about Sub topic 1-1. |
| CMCC | Issue 1-1-1: option 2 (no restriction on MO configuration)Issue 1-1-2: not clear with this issue, what is the difference between MO and layer? According to the RAN1 LS (R4-1905310), it is agreed in RAN1 agreed that ‘frequency layer’ used in RAN1 specification should be changed to ‘measurement object’.Issue 1-2-1: we do not agree to reuse the measurement capability specified for SSB based measurement. More discussion is neededIssue 1-2-2: we do not agree to reuse the measurement capability specified for SSB based measurement. More discussion is needed Issue 1-2-3: more discussion is neededIssue 1-2-4: for option 1, we are OK to reuse existing UE capability on the number of CSI-RS resources, but we need clarification on the wording “update the value”  |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| YYY | Company A |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #2: Measurement requirements for CSI-RS intra-frequency and inter-frequency measurements

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [**R4-2000465**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000465.zip) | MediaTek inc. | Observation 1: SSB-based cell detection is still required for CSI-RS based cell identification.Observation 2: According to TS38.331, if associatedSSB is configured, the timing reference of the CSI-RS follows the target cell. • If deriveSSB-IndexFromCell is not indicated, UE has to decode the PBCH of the target cell to get SFN, frame boundary and symbol-level timing with remaining error within CP before measuring the CSI-RS.• If deriveSSB-IndexFromCell is indicated, UE can resolve the remaining symbol-level timing ambiguity of deriveSSB-IndexFromCell through the timing estimated from SSB.Observation 3: If associatedSSB is not configured, UE has to measure up to 96 CSI-RS resources per MO. This is a huge waste of UE’s computation power.Observation 4: UE has to maintain a separate AGC control for CSI-RS measurement.Proposal 1: RAN4 does not specify requirements for the case that associatedSSB is not configured.Proposal 2: The AGC control for L3 CSI-RS is more challenging than SSB and should be considered in the requirements.Proposal 3: The requirement of CSI-RS based cell identification consists of the following 3 components: 1) Cell search via SSB with AGC margin, 2) PBCH decoding and 3) CSI-RS measurement with AGC margin.Proposal 4: RAN4 should avoid to create new definition of CSI-RS specific CSSF or change the framework of CSSF in this WI and should try to re-use the existing requirement as much as possible.Proposal 5: The CSI-RS resource configured for L3 measurement is not shared with other L1 measurement.Proposal 6: The FFT window timing for intra frequency measurement always follows the serving cell timing.Proposal 7: Scheduling restriction for CSI-RS based L3 measurement is still needed to address the issues of 1) collision with UL transmission and DL measurement on TDD carrier and 2) the need of Rx beam sweeping in FR2.Proposal 8: The scheduling restriction on the additional OFDM symbols before and after SSB is not needed for CSI-RS based L3 measurement. |
| [**R4-2000586**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000586.zip) | CATT | Proposal 1: If associated SSB is not configured for CSI-RS resources, the CSI-RS identification time can be expressed as: TCSI-RS\_identification\_without\_associatedSSB = TCSI-RS\_measurement\_period.Proposal 2: If associated SSB is configured for CSI-RS resources, the CSI-RS identification time can be expressed as: TCSI-RS\_identification\_with\_associatedSSB = TPSS/SSS\_sync + TCSI-RS\_measurement\_period.Proposal 3: If the CSI-RS resource is configured with associated SSB and QCLed to the associated SSB, the CSI-RS based measurement requirement does not need to consider the scaling factor due to Rx beam sweeping.Proposal 4: the scheduling restriction for CSI-RS based measurement shall be introduced for the following cases:1. Mix-numerology between data/SSB of serving cell and CSI-RS of neighbour cell2. RX beam sweeping in FR23. Collision between UL transmission and DL measurement for TDD carrierProposal 5: the CSSFwithin\_gap specified in 38.133 should be updated by considering the CSI-RS based measurement within the active BWP, and the CSSFoutside\_gap specified in 38.133 should be updated by considering the CSI-RS based measurement outside the active BWP.Proposal 6: For CSI-RS based measurement, the following options can be considered to define the corresponding requirements:• Option 1: UE is allowed not to measure the CSI-RS resources that are not within DRX on-duration or measurement gap;• Option 2: No UE performance requirement is defined for the CSI-RS resources that are not within DRX on-duration or measurement gap;• Option 3: the network needs to make sure the configured CSI-RS resources falls within the configured measurement gaps |
| [**R4-2000947**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000947.zip) | NTT DOCOMO, INC. | Observation 1: The method of identify timing synchronization is not related to measurement requirements directly. Proposal 1: RRM requirements should be specified based on the configuration of associatedSSB, e.g., if both ssbIndex and isQuasiColocated are provided, Rx beam sweeping is not needed. |
| [**R4-2000996**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2000996.zip) | OPPO | Proposal 1: If associatedSSB is not configured, two options are to be down selected for CSI-RS L3 measurement.Option 1: No requirements specified for CSI-RS L3 measurementOption 2: CSI-RS identification time is the CSI-RS measurement periodicityProposal 2: If associated SSB is configured for CSI-RS resources, CSI-RS based cell identification consists: 1) Cell search via SSB, 2) PBCH decoding and 3) CSI-RS measurement.Proposal 3: Study the impact of AGC control and if any define AGC margin additionally.Observation 1: From specification’s perspective, the structure of CSI-RS L3 measurement can be more concise than those of SSB.Proposal 4: Intra-frequency measurement can all be configured without gaps if the definition of intra-frequency includes the bandwidth of the CSI-RS on the neighbor cell is within the active BWP of the UE. Otherwise, all others are inter-frequency measurement with gaps.Proposal 5: RAN4 try to re-use the existing requirement of CSSF as much as possible, and the framework of CSSF can be shared by SSB and CSI-RS based L3 measurement. Observation 2: RAN4 to consider the collision with UL transmission and DL measurement for TDD band on FR1, and Rx beam sweeping and intra-band carrier aggregation on FR2, for scheduling restriction of CSI-RS based L3 measurement without gaps.Proposal 6: If CSI-RS based L3 measurement is configured without gaps, the requirements of scheduling restriction can be chosen from two options:• Option 1: the scheduling restriction on the additional OFDM symbols before and after SSB is not needed for CSI-RS based L3 measurement.• Option 2: define scheduling restriction on CSI-RS to be measurement and additional X OFDM symbol before and after consecutive CSI-RS symbols to be measured, FFS on X value.Proposal 7: If CSI-RS is configured with associated SSB and QCL-ed to the associated SSB, no Rx sweeping is needed, and do not define any scaling factor due to Rx beam sweeping.Proposal 8: If CSI-RS configured with associated SSB but not QCL-ed to the associated SSB, Rx sweeping is needed and FFS on the scaling factor N. |
| [**R4-2001658**](http://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_94_e/Docs/R4-2001658.zip) | Huawei, HiSilicon | Proposal 1: CSI-RS measurement requirement is the CSI-RS measurement periodicity when associatedSSB is not configured.Proposal 2: The above requirement is applicable assuming that the timing between serving cell and the neighbour cell is frame boundary synchronized.Proposal3:If the MO includes the serving CSI-RS resource with associated SSB, for the cells in the same MO,o For FR1 FDD cell, UE can perform PSS/SSS detection and DMRS matching to acquire time index of each cell in the MO.o For TDD cell or FR2 cells, UE can perform PSS/SSS detection to acquire symbol level timing of each cell in the MO.o If the MO doesn’t include the serving CSI-RS resource and the CSI-RS resource associated SSB is configured, UE needs to perform PSS/SSS detection, DMRS matching and PBCH decoding to acquire SFN, frame boundary timing, slot timing and symbol level timing of one cell. For the other cells in the same MO, o For FR1 FDD cell, UE can perform PSS/SSS detection and DMRS matching to acquire time index of each cell in the MO.o For FR1 TDD cell or FR2 cells, UE can perform PSS/SSS detection to acquire symbol level timing of each cell in the MO.Proposal 4: If CSI-RS is not QCL-ed to the associated SSB, UE needs to sweep the RX beam. If the CSI-RS is QCL-ed to the associated SSB, no Rx sweeping is needed.Proposal 5: If UE is not able to support mixed numerology of data and CSI-RS L3 mobility, the following scheduling restrictions apply due to CSI-RS based L3 intra-frequency measurement:-if the associatedSSB is configured, UE is not expected to transmit or receive on 2 data OFDM symbols impacted by CSI-RS resource symbol to be measured.-if the associatedSSB is not configured, UE is not expected to transmit or receive on the data OFDM symbol impacted by the CSI-RS resource symbol to be measured, provided timing difference between the CSI-RS resource and the serving cell should be less than half CP corresponding to the SCS of the CSI-RS.Proposal 6: When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit and receive on 2 data OFDM symbols impacted by CSI-RS resource symbol to be measured.Proposal 7: Scheduling restriction shall be considered when UE performs RX beam sweeping. |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 2-1: Framework of CSI-RS based measurement requirements

*Sub-topic description*

As guideline, framework of CSI-RS based measurement requirements is to be discussed firstly, including:

* Components of CSI-RS based measurement requirements
* Specification structure of CSI-RS L3 intra-f/inter-f measurement requirement

Note: according to whether CSI-RS configured with associatedSSB or not, the requirements could be defined for two cases.

*Open issues and candidate options before e-meeting:*

**Issue 2-1-1: Components of CSI-RS based measurement requirements**

* Proposals

***Case1: if associatedSSB is not configured***

* + Option 1: No requirements specified for CSI-RS L3 measurement
	+ Option 2: CSI-RS identification time is the CSI-RS measurement periodicity

***Case 2: if associatedSSB is configured for CSI-RS***

* + Option 1: CSI-RS based cell identification consists:
		- 1) Cell search via SSB,
		- 2) PBCH decoding
		- 3) CSI-RS measurement.
	+ FFS AGC margin.
* Recommended WF
	+ Collect the views from companies and try to agree on the framework for the measurement delay
	+ Tentative agreement:
	+ For Case1: if associatedSSB is not configured
		- No requirements specified for CSI-RS L3 measurement
	+ For Case 2: if associatedSSB is configured for CSI-RS
		- CSI-RS based cell identification consists:
			* 1) Cell search via SSB,
			* 2) PBCH decoding
			* 3) CSI-RS measurement.
		- AGC margin should be considered.

**Issue 2-1-2: Specification structure of CSI-RS L3 intra-f/inter-f measurement requirement**

* Proposals
	+ Option 1:

Intra-frequency measurement can all be configured without gaps if the definition of intra-frequency includes the bandwidth of the CSI-RS on the neighbour cell is within the active BWP of the UE. Otherwise, all others are inter-frequency measurement with gaps.

* Recommended WF
	+ Wait for the conclusion of NR\_CSIRS\_L3meas\_RRM\_Part\_1

### Sub-topic 2-2: Key open issues

*Sub-topic description*

According to companies’ inputs, we suggest to discuss the following key open issues for intra/inter-frequency measurement, including

* CCSF
* Scaling factor for Rx beam sweeping
* Scheduling restriction
	+ Factors to consider for scheduling restriction
	+ Requirements for scheduling restriction
* Whether to restrict CSI-RS resources outside of DRX/MG duration
* Others

*Open issues and candidate options before e-meeting:*

**Issue 2-2-1: CSSF**

* Proposals
	+ Option 1:

RAN4 to re-use the existing requirement of CSSF as much as possible, and the framework of CSSF can be shared by SSB and CSI-RS based L3 measurement.

* + Option 2:

The CSSFwithin\_gap specified in 38.133 should be updated by considering the CSI-RS based measurement within the active BWP, and the CSSFoutside\_gap specified in 38.133 should be updated by considering the CSI-RS based measurement outside the active BWP.

* Recommended WF
	+ Collect the views from companies and try to achieve agreement in 1st or 2nd round discussion

**Issue 2-2-2: Scaling factor for RX beam sweeping**

* Proposals
	+ Option 1:
	+ If CSI-RS is not QCL-ed to the associated SSB, UE needs to sweep the RX beam.
		- FFS on the scaling factor N
	+ If the CSI-RS is QCL-ed to the associated SSB, no Rx sweeping is needed.
* Recommended WF
	+ Tentative Agreement:
	+ If CSI-RS is not QCL-ed to the associated SSB, UE needs to sweep the RX beam.
		- FFS on the scaling factor N
	+ If the CSI-RS is QCL-ed to the associated SSB, no Rx sweeping is needed.

**Issue 2-2-3: Factors to consider for scheduling restriction**

* Proposals
	+ Option 1:
	+ Scheduling restriction for CSI-RS based L3 measurement is still needed to address the issues of
		- 1) collision with UL transmission and DL measurement on TDD carrier and
		- 2) the need of Rx beam sweeping in FR2.
	+ Option 2:
	+ the scheduling restriction for CSI-RS based measurement shall be introduced for the following cases:
		- 1. Mix-numerology between data/SSB of serving cell and CSI-RS of neighbour cell
		- 2. RX beam sweeping in FR2
		- 3. Collision between UL transmission and DL measurement for TDD carrier
* Recommended WF
	+ Tentative Agreement:
		- RAN4 agree to consider for scheduling restriction for CSI-RS L3 measurement
			* 1) collision with UL transmission and DL measurement on TDD carrier and

2) the need of Rx beam sweeping in FR2.

* + - FFS the impact of mix-numerology in 1st round and try to achieve agreement in 2nd round

**Issue 2-2-4: Requirements for scheduling restriction**

* Proposals
	+ Option 1:
	+ If UE is not able to support mixed numerology of data and CSI-RS L3 mobility, the following scheduling restrictions apply due to intra-frequency CSI-RS based L3 measurement:
		- if the associatedSSB is configured, UE is not expected to transmit or receive on 2 data OFDM symbols impacted by CSI-RS resource symbol to be measured.
		- if the associatedSSB is not configured, UE is not expected to transmit or receive on the data OFDM symbol impacted by CSI-RS resource symbol to be measured, provided timing difference between the CSI-RS resource and the serving cell should be less than half CP corresponding to the SCS of the CSI-RS.
	+ When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit and receive on 2 data OFDM symbols impacted by CSI-RS resource symbol to be measured.
	+ Scheduling restriction shall be considered when UE performs RX beam sweeping.
	+ Option 2:
	+ The scheduling restriction on the additional OFDM symbols before and after SSB is not needed for CSI-RS based L3 measurement.
	+ Option 3:
	+ Define scheduling restriction on CSI-RS to be measurement and additional X OFDM symbol before and after consecutive CSI-RS symbols to be measured. FFS on X value.
* Recommended WF
	+ Tentative Agreement: the requirements are only discussed for CSI-RS based L3 measurement without gaps
	+ Collect views from companies
		- FFS on additional X OFDM symbol before and after consecutive CSI-RS symbols to be measured
		- FFS on additional Y OFDM symbols before and after SSB

**Issue 2-2-5: Whether to restrict CSI-RS resources outside of DRX/MG duration**

* Proposals
	+ Option 1: UE is allowed not to measure the CSI-RS resources that are not within DRX on-duration or measurement gap;
	+ Option 2: No UE performance requirement is defined for the CSI-RS resources that are not within DRX on-duration or measurement gap;
	+ Option 3: the network needs to make sure the configured CSI-RS resources falls within the configured measurement gaps
* Recommended WF
	+ Tentative Agreement: Option 2

**Issue 2-2-6: Others**

* Proposal 1:
	+ Option1: The CSI-RS resource configured for L3 measurement is not shared with other L1 measurement.
* Proposal 2:
	+ Option1: The FFT window timing for intra frequency measurement always follows the serving cell timing.
* Recommended WF
	+ Tentative Agreement :
		- Agreement: The FFT window timing for intra frequency measurement always follows the serving cell timing.
		- FFS CSI-RS resource configured for L3 measurement is not shared with other L1 measurement.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| OPPO | Sub-topic 2-1: Framework of CSI-RS based measurement requirementsIssue 2-1-1: Agree with tentative agreement.Issue 2-1-2: Wait for the conclusion of NR\_CSIRS\_L3meas\_RRM\_Part\_1.Sub-topic 2-2: Key open issuesIssue 2-2-1: support option 1. Re-use the existing requirement of CSSF as much as possible, and the framework of CSSF can be shared by SSB and CSI-RS based L3 measurement.Issue 2-2-2: Agree with tentative agreement.* If CSI-RS is not QCL-ed to the associated SSB, UE needs to sweep the RX beam.
* If the CSI-RS is QCL-ed to the associated SSB, no Rx sweeping is needed.

Issue 2-2-3: Agree with tentative agreement. RAN4 agree to consider for scheduling restriction for CSI-RS L3 measurement1) collision with UL transmission and DL measurement on TDD carrier and 2) the need of Rx beam sweeping in FR2.Issue 2-2-4: Prefer Option 3. As we can agree firstly, the requirements are only discussed for CSI-RS based L3 measurement without gaps. And whether it applies to intra-frequency or/and inter-frequency depends on the conclusion of email discussion of NR\_CSIRS\_L3meas\_RRM\_Part\_1.As for intra-frequency CSI-RS based L3 measurement, majority companies support SCSs of CSI-RS for serving cell and neighbour cell are the same. If this is the case, the mix-numerology between data/SSB of serving cell and CSI-RS of neighbour cell would not exist. Issue 2-2-5: Prefer Option 2.Issue 2-2-6: Agree with tentative agreement. The FFT window timing for intra-frequency measurement always follows the serving cell timing. |
| Apple | Issue 2-1-1: in Case 1, the synchronization level between serving and target cell needs to be clarified. If sufficient synchronization can be guaranteed, option 2 is OK. In case 2, option 1 is OK.Issue 2-1-2: it seems the title of issue and proposal are not fully aligned. If spec structure is the concern, we should have a dedicated section for CSI-RS based L3 measurement. If the discussion is about gap or gapless based measurement, I agree we should hold this until the definition of inter-/intra-frequency becomes clear.  |
| QC | Issue 2-1-1: Components of CSI-RS based measurement requirementsFor Case1, for option 2 what is the sync assumption between serving cell and CSI-RS resource from other cellsIssue 2-2-2: Scaling factor for RX beam sweepingFor the case where CSI-RS is QCL’d to SSB, no beam sweeping needed only **after** SSB has been detected. SSB detection would still need beam sweeping. Issue 2-2-4: Requirements for scheduling restrictionWe agree with WF. IF we can restrict to specifying requirements only for cases where no gaps are needed that will simplify the requirements quite a lot. The overhead for doing CSI-RS measurements with gaps really gives no benefit over SSB. Issue 2-2-5: Whether to restrict CSI-RS resources outside of DRX/MG durationAgree with option 2 in terms of DRx. As said in 2-2-4 we should restrict to defining requirements without gaps. Issue 2-2-6: OthersFor proposal 1, need more clarification as to why the restriction is needed. For proposal 2, we assume that this means that performance requirements will be defined based on serving cell timing.  |
| Ericsson | Issue 2-1-1: support the proposed WFIssue 2-1-2: the proposed WF is fineIssue 2-2-1: option 1Issue 2-2-2: the proposed WF is acceptableIssue 2-2-3: the proposed WF looks okIssue 2-2-4: needs further discussionIssue 2-2-5: needs further discussionIssue 2-2-6: needs further discussion |
| CATT | **Issue 2-1-1: Components of CSI-RS based measurement requirements**Do not agree the recommended WF. Non-associated SSB case shall be supported, and we can further discuss the synchronization assumption, as Apple mentioned above. In our understanding, if the target cell and the serving cell are synchronized, there is no need to detect SSB. And for case 2, why UE should decode PBCH? SSN index will configured to UE is associated SSB is configured.**Issue 2-2-1: CSSF**The CSSF need to be updated by considering the CSI-RS based measurement. It depends on the conclusion on intra-frequency and inter-frequency measurement definition. We can refer the discussion and conclusion on inter-frequency measurement without gap in RRM enhancement WI.**Issue 2-2-2: Scaling factor for RX beam sweeping**Agree with QC**Issue 2-2-3: Factors to consider for scheduling restriction**My understanding is that the SCS of CSI-RS for RRM is configured independently of the PDSCH/PDCCH SCS. CSI-RS for RRM is in general configured for serving all UEs, while PDSCH/PDCCH is more related to individual UEs. So there is not necessary to restrict that the SCS of CSI-RS is always the same as PDCCH/PDSCH.**Issue 2-2-4: Requirements for scheduling restriction**Need more discussion.**Issue 2-2-5: Whether to restrict CSI-RS resources outside of DRX/MG duration**Either option is OK for us. |
| Intel | Issue 2-1-1: For case 1, clarify how UE do measurement if associatedSSB is not configured. If the timing of serving cell can be used, then the requirement can be defined. For case 2, we can agree on option 1.Issue 2-1-2: agree with Recommended WF.Issue 2-2-1: agree with option 1.Issue 2-2-2: agree with recommended WF.Issue 2-2-3: agree with option 2.Issue 2-2-4: agree with recommended WF.Issue 2-2-5: agree with recommended WF. |
| CMCC | Issue 2-1-1: We are not OK with the recommended WF. It is preferred to specify requirements for the case with *associatedSSB* and the case without *associatedSSB*Issue 2-1-2: it is related to the definition of intra-frequency measurementIssue 2-2-1: it is related to the definition of intra-frequency measurementIssue 2-2-2: only the case with *associatedSSB is considered. The case* without *associatedSSB* configured also needs to be studied.Issue 2-2-3: Mix-numerology between data of serving cell and target CSI-RS need to be consideredIssue 2-2-4: needs further discussionIssue 2-2-5: needs further discussionIssue 2-2-6: needs further discussion |

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| YYY | Company A |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |