{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Basic_Para","PUSCH","PRACH"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":12,"n_cols":10,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #94-e",null,null,null,null,null,null,null,"R4-2000309"]
[null,"Online 24th February– 6th March,  2020"]
[]
[null,"Source: Samsung"]
[null,"Title:  Simulation results summary of BS demodulation requirement for LTE Rel-16 HST"]
[null,"Agenda : 7.13.4.1"]
[null,"Document for: Information"]
[]
[]
[null,"Simualtion assumptions"]
[null,"R4-1912777, WF on LTE BS demodulation requirements"]

{"sheet":"Basic_Para","index":1,"n_rows":43,"n_cols":9,"rows_kept":43,"cut":false,"hidden":false,"merged":[[30,4,31,4],[30,5,30,8],[32,1,34,1],[30,3,31,3],[1,1,3,1],[1,2,1,3],[7,1,10,1],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[15,1,16,1],[15,2,15,3],[24,1,25,1],[26,1,26,3],[30,1,31,1],[30,2,31,2]]}
[]
[null," Parameter","Value"]
[null,null,"Open space","Tunnel for multi-antennas"]
[null,null,"Bi-directional","Bi-directional"]
[null,"Ds","1000 m","300 m"]
[null,"Dmin","50 m","2 m"]
[null,"v","500 km/h","500 km/h"]
[null,"fd","1944Hz"]
[null,null,"If 70%ile of the max. throughput is not achievable with 1944Hz:"]
[null,null,"Case 1: fallback to 1750Hz, or "]
[null,null,"Case 2: accept %ile of max. throughput lower than 70%ile with 1944Hz    "]
[]
[]
[]
[]
[null,"Parameters","Value"]
[null,null,"Scenario 1 (Open space)","Scenario 3 (Tunnel)"]
[null,"CBW","1.4/3/5/10/15/20 MHz","1.4/3/5/10/15/20 MHz"]
[null,"CP","Normal","Normal"]
[null,"FRC","A.3-2 to A.3-7 (QPSK 1/3)","A.3-2 to A.3-7 (QPSK 1/3)"]
[null,"Antenna configuration ","1Tx2Rx","1Tx1Rx"]
[null,"Reference receiver","MRC","MRC"]
[null,"Noise estimation","Practical","Practical"]
[null,"Time and frequency track","Practical","Practical"]
[null,"Test metric","70%ile of the max. throughput","70%ile of the max. throughput"]
[null,null,"30%ile of the max. throughput","30%ile of the max. throughput"]
[null,"NOTE: The configuration of PUCCH (format 2) is optional"]
[]
[]
[]
[null,"Number of TX antennas","Number of RX antennas","Propagation conditions and correlation matrix ","Frequency offset","SNR [dB]"]
[null,null,null,null,null,"Burst format 0","Burst format 1","Burst format 2","Burst format 3"]
[null,1,2,"AWGN","1944Hz"]
[null,null,4,"AWGN","1944Hz"]
[null,null,8,"AWGN","1944Hz"]
[]
[]
[]
[null,"Burst format","Ncs","Logical sequence index","v"]
[null,0,15,30,30]
[null,1,100,168,20]
[null,2,118,204,10]
[null,3,137,264,0]

{"sheet":"PUSCH","index":2,"n_rows":50,"n_cols":29,"rows_kept":50,"cut":false,"hidden":false,"merged":[[0,27,0,28],[42,1,43,1],[42,2,43,2],[42,3,43,3],[40,3,41,3],[2,27,13,27],[26,27,37,27],[14,27,25,27],[38,27,49,27],[32,3,33,3],[28,1,29,1],[28,2,29,2],[36,1,37,1],[36,2,37,2],[36,3,37,3],[38,3,39,3],[40,1,41,1],[40,2,41,2],[26,4,37,4],[38,4,49,4],[48,1,49,1],[48,2,49,2],[48,3,49,3],[46,1,47,1],[46,2,47,2],[46,3,47,3],[44,1,45,1],[44,2,45,2],[44,3,45,3],[32,1,33,1],[32,2,33,2],[22,1,23,1],[22,2,23,2],[22,3,23,3],[28,3,29,3],[26,0,49,0],[26,1,27,1],[26,2,27,2],[26,3,27,3],[30,1,31,1],[30,2,31,2],[30,3,31,3],[34,1,35,1],[34,2,35,2],[34,3,35,3],[38,1,39,1],[38,2,39,2],[20,1,21,1],[20,2,21,2],[20,3,21,3],[18,1,19,1],[18,2,19,2],[18,3,19,3],[2,0,25,0],[0,18,0,19],[0,6,0,7],[0,8,0,9],[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[4,1,5,1],[6,1,7,1],[6,2,7,2],[6,3,7,3],[2,4,13,4],[2,1,3,1],[2,2,3,2],[4,2,5,2],[2,3,3,3],[4,3,5,3],[10,1,11,1],[8,2,9,2],[10,2,11,2],[12,1,13,1],[12,2,13,2],[8,1,9,1],[14,4,25,4],[8,3,9,3],[12,3,13,3],[10,3,11,3],[16,1,17,1],[16,2,17,2],[16,3,17,3],[14,1,15,1],[14,2,15,2],[14,3,15,3],[24,1,25,1],[24,2,25,2],[24,3,25,3]]}
[null,null,null,null,null,null,"Samsung",null,"Ericcson",null,"Nokia",null,"Huawei",null,"XXXX",null,"SPAN",null,"AVERAGE",null,36.103999999999999,36.140999999999998,null,"For imformation\n\n[0.5]dB additional margin","For imformation\n\n[1.0]dB additional margin","For imformation\n\n[1.5]dB additional margin",null,"Reference\nHST Senario 1\nHST Senario 3"]
["Scenario","BW","MCS","Antenna configuration","Doppler Value","Test  metric","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment",null,null,null,36.103999999999999,36.103999999999999,36.103999999999999,null,"Doppler Value",36.103999999999999]
["Open space","15kHz, 1.4MHz","MCS6 QPSK 1/3","1x2","1944Hz","30% TP",-7.2,{"$f":"G3+2","v":-5.2},-8.32,-5.82,null,null,-7.21,-5.21,null,null,{"$f":"MAX(G3,I3,K3,M3,O3)-MIN(G3,I3,K3,M3,O3)","v":1.1200000000000001},{"$f":"MAX(H3,J3,L3,N3)-MIN(H3,J3,L3,N3)","v":0.62000000000000011},{"$f":"AVERAGE(G3,I3,K3,M3,O3)","v":-7.5766666666666671},{"$f":"AVERAGE(H3,J3,L3,N3)","v":-5.41},{"$f":"T3","v":-5.41},{"$f":"T3+0.3","v":-5.1100000000000003},null,{"$f":"U3+0.5","v":-4.91},{"$f":"U3+1","v":-4.41},{"$f":"U3+1.5","v":-3.91},null,1340,-3.9]
[null,null,null,null,null,"70% TP",-2.5,{"$f":"G4+2","v":-0.5},-3.76,-1.2599999999999998,null,null,-3.86,-1.8599999999999999,null,null,{"$f":"MAX(G4,I4,K4,M4,O4)-MIN(G4,I4,K4,M4,O4)","v":1.3599999999999999},{"$f":"MAX(H4,J4,L4,N4)-MIN(H4,J4,L4,N4)","v":1.3599999999999999},{"$f":"AVERAGE(G4,I4,K4,M4,O4)","v":-3.3733333333333331},{"$f":"AVERAGE(H4,J4,L4,N4)","v":-1.2066666666666666},-1.2066666666666666,{"$f":"T4+0.3","v":-0.90666666666666651},null,{"$f":"U4+0.5","v":-0.70666666666666655},{"$f":"U4+1","v":-0.20666666666666655},{"$f":"U4+1.5","v":0.29333333333333345},null,null,-0.6]
[null,"15kHz, 3MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.1,-5.0999999999999996,-8.6300000000000008,-6.1300000000000008,null,null,-7.8,-5.8,null,null,1.5300000000000011,{"$f":"MAX(H5,J5,L5,N5)-MIN(H5,J5,L5,N5)","v":1.0300000000000011},-7.8433333333333337,{"$f":"AVERAGE(H5,J5,L5,N5)","v":-5.6766666666666667},-5.6766666666666667,-5.3766666666666669,null,-5.1766666666666667,-4.6766666666666667,-4.1766666666666667,null,null,-4.5]
[null,null,null,null,null,"70% TP",-3,-1,-3.88,-1.38,null,null,-3.85,-1.85,null,null,0.87999999999999989,0.85000000000000009,-3.5766666666666667,-1.4100000000000001,-1.4100000000000001,-1.1100000000000001,null,-0.91000000000000014,-0.41000000000000014,8.9999999999999858E-2,null,null,-1]
[null,"15KHz, 5MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.8000000000000007,-5.8000000000000007,-9.24,-6.74,null,null,-9.09,-7.09,null,null,1.4399999999999995,1.2899999999999991,-8.7099999999999991,-6.5433333333333339,-6.5433333333333339,-6.2433333333333341,null,-6.0433333333333339,-5.5433333333333339,-5.0433333333333339,null,null,-5.0999999999999996]
[null,null,null,null,null,"70% TP",-3.5,-1.5,-4.71,-2.21,null,null,-4.6100000000000003,-2.6100000000000003,null,null,1.21,1.1100000000000003,-4.2733333333333334,-2.1066666666666669,-2.1066666666666669,-1.8066666666666669,null,-1.6066666666666669,-1.1066666666666669,-0.60666666666666691,null,null,-1.4]
[null,"15KHz, 10MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.8000000000000007,-5.8000000000000007,-8.69,-6.1899999999999995,null,null,-8.32,-6.32,null,null,0.88999999999999879,0.51999999999999957,-8.2700000000000014,-6.1033333333333344,-6.1033333333333344,-5.8033333333333346,null,-5.6033333333333344,-5.1033333333333344,-4.6033333333333344,null,null,-5.4]
[null,null,null,null,null,"70% TP",-3.3,-1.2999999999999998,-3.9,-1.4,null,null,-3.97,-1.9700000000000002,null,null,0.67000000000000037,0.67000000000000037,-3.7233333333333332,-1.5566666666666666,-1.5566666666666666,-1.2566666666666666,null,-1.0566666666666666,-0.55666666666666664,-5.6666666666666643E-2,null,null,-1.5]
[null,"15KHz, 15MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.9,-5.9,-9.1999999999999993,-6.6999999999999993,null,null,-9.1999999999999993,-7.1999999999999993,null,null,1.2999999999999989,1.2999999999999989,-8.7666666666666675,-6.5999999999999988,-6.5999999999999988,-6.2999999999999989,null,-6.0999999999999988,-5.5999999999999988,-5.0999999999999988,null,null,-5.2]
[null,null,null,null,null,"70% TP",-3.45,-1.4500000000000002,-4.6900000000000004,-2.1900000000000004,null,null,-4.5999999999999996,-2.5999999999999996,null,null,1.2400000000000002,1.1499999999999995,-4.246666666666667,-2.08,-2.08,-1.78,null,-1.58,-1.08,-0.58000000000000007,null,null,-1.4]
[null,"15KHz, 20MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.9,-5.9,-8.68,-6.18,null,null,-8.4,-6.4,null,null,0.77999999999999936,0.5,-8.3266666666666662,-6.16,-6.16,-5.86,null,-5.66,-5.16,-4.66,null,null,-5.3]
[null,null,null,null,null,"70% TP",-3.75,-1.75,-3.84,-1.3399999999999999,null,null,-3.74,-1.7400000000000002,null,null,9.9999999999999645E-2,0.41000000000000014,-3.7766666666666668,-1.61,-1.61,-1.31,null,-1.1100000000000001,-0.6100000000000001,-0.1100000000000001,null,null,-1.4]
[null,"15kHz, 1.4MHz","MCS6 QPSK 1/3","1x2","1750Hz","30% TP",-7.2,-5.2,-8.35,-5.85,-7,-5,-7.11,-5.1100000000000003,null,null,1.3499999999999996,0.84999999999999964,-7.415,-5.29,-5.29,-4.99,null,-4.79,-4.29,-3.79,null,1340,-3.9]
[null,null,null,null,null,"70% TP",-2.75,-0.75,-3.79,-1.29,-2.5,-0.5,-3.86,-1.8599999999999999,null,null,1.3599999999999999,1.3599999999999999,-3.2249999999999996,-1.1000000000000001,-1.1000000000000001,-0.8,null,-0.60000000000000009,-0.10000000000000009,0.39999999999999991,null,null,-0.6]
[null,"15kHz, 3MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.2,-5.2,-8.6300000000000008,-6.1300000000000008,-7.5,-5.5,-7.8,-5.8,null,null,1.4300000000000006,0.9300000000000006,-7.7825000000000006,-5.6575000000000006,-5.6575000000000006,-5.3575000000000008,null,-5.1575000000000006,-4.6575000000000006,-4.1575000000000006,null,null,-4.5]
[null,null,null,null,null,"70% TP",-3.15,-1.1499999999999999,-3.87,-1.37,-2.4,-0.4,-3.85,-1.85,null,null,1.4700000000000002,1.4500000000000002,-3.3174999999999999,-1.1924999999999999,-1.1924999999999999,-0.89249999999999985,null,-0.69249999999999989,-0.19249999999999989,0.30750000000000011,null,null,-1]
[null,"15KHz, 5MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.8000000000000007,-5.8000000000000007,-9.23,-6.73,-7.4,-5.4,-9.16,-7.16,null,null,1.83,1.7599999999999998,-8.3975000000000009,-6.2725,-6.2725,-5.9725000000000001,null,-5.7725,-5.2725,-4.7725,null,null,-5.0999999999999996]
[null,null,null,null,null,"70% TP",-3.7,-1.7000000000000002,-4.71,-2.21,-2,0,-4.6100000000000003,-2.6100000000000003,null,null,2.71,2.6100000000000003,-3.7549999999999999,-1.6300000000000001,-1.6300000000000001,-1.33,null,-1.1300000000000001,-0.63000000000000012,-0.13000000000000012,null,null,-1.4]
[null,"15KHz, 10MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.8000000000000007,-5.8000000000000007,-8.6999999999999993,-6.1999999999999993,-7.4,-5.4,-8.24,-6.24,null,null,1.2999999999999989,0.83999999999999986,-8.0350000000000001,-5.91,-5.91,-5.61,null,-5.41,-4.91,-4.41,null,null,-5.4]
[null,null,null,null,null,"70% TP",-3.4,-1.4,-3.89,-1.3900000000000001,-2,0,-3.98,-1.98,null,null,1.98,1.98,-3.3174999999999999,-1.1924999999999999,-1.1924999999999999,-0.89249999999999985,null,-0.69249999999999989,-0.19249999999999989,0.30750000000000011,null,null,-1.5]
[null,"15KHz, 15MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.9,-5.9,-9.18,-6.68,-7.5,-5.5,-9.26,-7.26,null,null,1.7599999999999998,1.7599999999999998,-8.4599999999999991,-6.3349999999999991,-6.3349999999999991,-6.0349999999999993,null,-5.8349999999999991,-5.3349999999999991,-4.8349999999999991,null,null,-5.2]
[null,null,null,null,null,"70% TP",-3.5,-1.5,-4.6900000000000004,-2.1900000000000004,-2,0,-4.5999999999999996,-2.5999999999999996,null,null,2.6900000000000004,2.5999999999999996,-3.6975000000000002,-1.5725,-1.5725,-1.2725,null,-1.0725,-0.57250000000000001,-7.2500000000000009E-2,null,null,-1.4]
[null,"15KHz, 20MHz","MCS6 QPSK 1/3","1x2",null,"30% TP",-7.9,-5.9,-8.67,-6.17,-8,-6,-8.3699999999999992,-6.3699999999999992,null,null,0.76999999999999957,0.46999999999999886,-8.2349999999999994,-6.1099999999999994,-6.1099999999999994,-5.81,null,-5.6099999999999994,-5.1099999999999994,-4.6099999999999994,null,null,-5.3]
[null,null,null,null,null,"70% TP",-4.0999999999999996,-2.0999999999999996,-3.84,-1.3399999999999999,-2,0,-3.74,-1.7400000000000002,null,null,2.0999999999999996,2.0999999999999996,-3.42,-1.2949999999999999,-1.2949999999999999,-0.99499999999999988,null,-0.79499999999999993,-0.29499999999999993,0.20500000000000007,null,null,-1.4]
["Tunnel for multi-antenna","15kHz, 1.4MHz","MCS6 QPSK 1/3","1x1","1944Hz","30% TP",-3.7,-1.7000000000000002,-5.14,-2.6399999999999997,null,null,-4.97,-2.9699999999999998,null,null,1.4399999999999995,{"$f":"MAX(H27,J27,L27,N27)-MIN(H27,J27,L27,N27)","v":1.2699999999999996},-4.6033333333333326,-2.4366666666666665,-2.4366666666666665,-2.1366666666666667,null,-1.9366666666666665,-1.4366666666666665,-0.93666666666666654,null,1150,-1.5]
[null,null,null,null,null,"70% TP",0.6,2.6,-0.77,1.73,null,null,-0.85,1.1499999999999999,null,null,1.45,{"$f":"MAX(H28,J28,L28,N28)-MIN(H28,J28,L28,N28)","v":1.4500000000000002},-0.34,1.8266666666666669,1.8266666666666669,2.1266666666666669,null,2.3266666666666671,2.8266666666666671,3.3266666666666671,null,null,1.9]
[null,"15kHz, 3MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.3,-2.2999999999999998,-5.57,-3.0700000000000003,null,null,-5.1100000000000003,-3.1100000000000003,null,null,1.2700000000000005,0.8100000000000005,-4.9933333333333332,-2.8266666666666667,-2.8266666666666667,-2.5266666666666668,null,-2.3266666666666667,-1.8266666666666667,-1.3266666666666667,null,null,-2.1]
[null,null,null,null,null,"70% TP",0.6,2.6,-0.88,1.62,null,null,-0.79,1.21,null,null,1.48,1.3900000000000001,-0.35666666666666669,1.8100000000000003,1.8100000000000003,2.1100000000000003,null,2.3100000000000005,2.8100000000000005,3.3100000000000005,null,null,1.6]
[null,"15KHz, 5MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.8,-2.8,-6.18,-3.6799999999999997,null,null,-6.16,-4.16,null,null,1.38,1.3600000000000003,-5.7133333333333338,-3.5466666666666669,-3.5466666666666669,-3.246666666666667,null,-3.0466666666666669,-2.5466666666666669,-2.0466666666666669,null,null,-2.6]
[null,null,null,null,null,"70% TP",-0.4,1.6,-1.7,0.8,null,null,-1.57,0.42999999999999994,null,null,1.2999999999999998,1.1700000000000002,-1.2233333333333334,0.94333333333333336,0.94333333333333336,1.2433333333333334,null,1.4433333333333334,1.9433333333333334,2.4433333333333334,null,null,1.3]
[null,"15KHz, 10MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.8,-2.8,-5.65,-3.1500000000000004,null,null,-5.29,-3.29,null,null,0.85000000000000053,0.49000000000000021,-5.2466666666666661,-3.08,-3.08,-2.7800000000000002,null,-2.58,-2.08,-1.58,null,null,-2.7]
[null,null,null,null,null,"70% TP",0.5,2.5,-0.87,1.63,null,null,-0.89,1.1099999999999999,null,null,1.3900000000000001,1.3900000000000001,-0.42,1.7466666666666668,1.7466666666666668,2.0466666666666669,null,2.246666666666667,2.746666666666667,3.246666666666667,null,null,1.2]
[null,"15KHz, 15MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.8,-2.8,-6.15,-3.6500000000000004,null,null,-6.24,-4.24,null,null,1.4400000000000004,1.4400000000000004,-5.7299999999999995,-3.5633333333333339,-3.5633333333333339,-3.2633333333333341,null,-3.0633333333333339,-2.5633333333333339,-2.0633333333333339,null,null,-2.7]
[null,null,null,null,null,"70% TP",-0.35,1.65,-1.66,0.84000000000000008,null,null,-1.55,0.44999999999999996,null,null,1.31,1.2,-1.1866666666666665,0.98000000000000009,0.98000000000000009,1.28,null,1.48,1.98,2.48,null,null,1.2]
[null,"15KHz, 20MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.9000000000000004,-2.9000000000000004,-5.63,-3.13,null,null,-5.27,-3.2699999999999996,null,null,0.72999999999999954,0.36999999999999922,-5.2666666666666666,-3.1,-3.1,-2.8000000000000003,null,-2.6,-2.1,-1.6,null,null,-2.7]
[null,null,null,null,null,"70% TP",-0.4,1.6,-0.83,1.67,null,null,-0.67,1.33,null,null,0.42999999999999994,0.33999999999999986,-0.6333333333333333,1.5333333333333332,1.5333333333333332,1.8333333333333333,null,2.0333333333333332,2.5333333333333332,3.0333333333333332,null,null,1.2]
[null,"15kHz, 1.4MHz","MCS6 QPSK 1/3","1x1","1750Hz","30% TP",-3.9000000000000004,-1.9000000000000004,-5.3,-2.8,-5,-3,-5.16,-3.16,null,null,1.3999999999999995,1.2599999999999998,-4.84,-2.7149999999999999,-2.7149999999999999,-2.415,null,-2.2149999999999999,-1.7149999999999999,-1.2149999999999999,null,1150,-1.5]
[null,null,null,null,null,"70% TP",0.55000000000000004,2.5499999999999998,-0.8,1.7,-0.46,1.54,-0.85,1.1499999999999999,null,null,1.4,1.4,-0.39,1.7349999999999999,1.7349999999999999,2.0349999999999997,null,2.2349999999999999,2.7349999999999999,3.2349999999999999,null,null,1.9]
[null,"15kHz, 3MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.5,-2.5,-5.57,-3.0700000000000003,-5.0999999999999996,-3.1,-5.07,-3.0700000000000003,null,null,1.0700000000000003,0.60000000000000009,-5.0600000000000005,-2.9350000000000001,-2.9350000000000001,-2.6350000000000002,null,-2.4350000000000001,-1.9350000000000001,-1.4350000000000001,null,null,-2.1]
[null,null,null,null,null,"70% TP",0.35,2.35,-0.87,1.63,-0.35,1.65,-0.8,1.2,null,null,1.22,1.1500000000000001,-0.41749999999999998,1.7075,1.7075,2.0074999999999998,null,2.2075,2.7075,3.2075,null,null,1.6]
[null,"15KHz, 5MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.8,-2.8,-6.16,-3.66,-6,-4,-6.22,-4.22,null,null,1.42,1.42,-5.7949999999999999,-3.67,-3.67,-3.37,null,-3.17,-2.67,-2.17,null,null,-2.6]
[null,null,null,null,null,"70% TP",-0.5,1.5,-1.7,0.8,-0.34,1.66,-1.57,0.42999999999999994,null,null,1.3599999999999999,1.23,-1.0275000000000001,1.0974999999999999,1.0974999999999999,1.3975,null,1.5974999999999999,2.0975000000000001,2.5975000000000001,null,null,1.3]
[null,"15KHz, 10MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.8,-2.8,-5.64,-3.1399999999999997,-5,-3,-5.3,-3.3,null,null,0.83999999999999986,0.5,-5.1849999999999996,-3.0599999999999996,-3.0599999999999996,-2.76,null,-2.5599999999999996,-2.0599999999999996,-1.5599999999999996,null,null,-2.7]
[null,null,null,null,null,"70% TP",0,2,-0.88,1.62,-0.1,1.9,-0.87,1.1299999999999999,null,null,0.88,0.87000000000000011,-0.46250000000000002,1.6624999999999999,1.6624999999999999,1.9624999999999999,null,2.1624999999999996,2.6624999999999996,3.1624999999999996,null,null,1.2]
[null,"15KHz, 15MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.8,-2.8,-6.14,-3.6399999999999997,-6.2,-4.2,-6.24,-4.24,null,null,1.4400000000000004,1.4400000000000004,-5.8450000000000006,-3.72,-3.72,-3.4200000000000004,null,-3.22,-2.72,-2.2200000000000002,null,null,-2.7]
[null,null,null,null,null,"70% TP",-0.4,1.6,-1.67,0.83000000000000007,0.1,2.1,-1.56,0.43999999999999995,null,null,1.77,1.6600000000000001,-0.88249999999999995,1.2425000000000002,1.2425000000000002,1.5425000000000002,null,1.7425000000000002,2.2425000000000002,2.7425000000000002,null,null,1.2]
[null,"15KHz, 20MHz","MCS6 QPSK 1/3","1x1",null,"30% TP",-4.9000000000000004,-2.9000000000000004,-5.63,-3.13,-5.4,-3.4,-5.27,-3.2699999999999996,null,null,0.72999999999999954,0.49999999999999956,-5.3000000000000007,-3.1749999999999998,-3.1749999999999998,-2.875,null,-2.6749999999999998,-2.1749999999999998,-1.6749999999999998,null,null,-2.7]
[null,null,null,null,null,"70% TP",-0.8,1.2,-0.83,1.67,0.9,2.9,-0.67,1.33,null,null,1.73,1.7,-0.35,1.7749999999999999,1.7749999999999999,2.0749999999999997,null,2.2749999999999999,2.7749999999999999,3.2749999999999999,null,null,1.2]

{"sheet":"PRACH","index":3,"n_rows":14,"n_cols":30,"rows_kept":14,"cut":false,"hidden":false,"merged":[[2,28,13,28],[0,28,0,29],[2,6,13,6],[0,20,0,21],[0,8,0,9],[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19]]}
[null,null,null,null,null,null,null,null,"Samsung",null,"Ericcson",null,"Nokia",null,"Huawei",null,"XXXX",null,"SPAN",null,"AVERAGE",null,36.103999999999999,36.140999999999998,null,"Option 1\n\nSNR values that are smaller or far greater than for 1875Hz are excluded","Option 2\n\n [0.5]dB additional margin",null,"Reference\nRestricted set type B with 1875Hz frequency offset"]
["Format","Propagation channel","Ncs","Logical sequence index","v","Antenna configuration","Frequency offset","Test  metric","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment",null,null,null,36.103999999999999,36.103999999999999,null,"Frequency offset",36.103999999999999]
["Format0","AWGN",15,30,30,"1x2","1944Hz","1% miss detection",-13.78,-11.78,-14.76,-12.26,-14.4,-11.8,-11.5,-9.15,null,null,{"$f":"MAX(I3,K3,M3,O3)-MIN(I3,K3,M3,O3)","v":3.26},{"$f":"MAX(J3,L3,N3,P3)-MIN(J3,L3,N3,P3)","v":3.1099999999999994},{"$f":"AVERAGE(I3,K3,M3,O3)","v":-13.61},{"$f":"AVERAGE(J3,L3,N3,P3)","v":-11.2475},{"$f":"V3","v":-11.2475},{"$f":"V3+0.3","v":-10.9475},null,-10.909999999999998,{"$f":"W3+0.5","v":-10.7475},null,"1875Hz",-11.8]
["Format0","AWGN",15,30,30,"1x4",null,"1% miss detection",-16.22,-14.22,-17.22,-14.719999999999999,-16.8,-14.2,-13.5,-11.5,null,null,{"$f":"MAX(I4,K4,M4,O4)-MIN(I4,K4,M4,O4)","v":3.7199999999999989},{"$f":"MAX(J4,L4,N4,P4)-MIN(J4,L4,N4,P4)","v":3.2199999999999989},{"$f":"AVERAGE(I4,K4,M4,O4)","v":-15.934999999999999},{"$f":"AVERAGE(J4,L4,N4,P4)","v":-13.66},{"$f":"V4","v":-13.66},{"$f":"V4+0.3","v":-13.36},null,-12.85,{"$f":"W4+0.5","v":-13.16},null,null,-14.2]
["Format0","AWGN",15,30,30,"1x8",null,"1% miss detection",-18.48,-16.48,-19.5,-17,-18.899999999999999,-16.100000000000001,-16.48,-14.68,null,null,3.0199999999999996,2.3200000000000003,-18.34,-16.065000000000001,-16.065000000000001,-15.765000000000001,null,-15.39,-15.565000000000001,null,null,-16.3]
["Format1","AWGN",100,168,20,"1x2",null,"1% miss detection",-13.43,-11.43,-14.5,-12,-14.4,-11.4,-13.7,-11.7,null,null,1.0700000000000003,0.59999999999999964,-14.0075,-11.6325,-11.6325,-11.3325,null,-11.4,-11.1325,null,null,-11.4]
["Format1","AWGN",100,168,20,"1x4",null,"1% miss detection",-15.89,-13.89,-16.97,-14.469999999999999,-16.8,-13.8,-15.81,-13.81,null,null,1.1599999999999984,0.66999999999999815,-16.3675,-13.9925,{"$f":"V7","v":-13.9925},-13.692499999999999,null,-13.8,-13.4925,null,null,-13.8]
["Format1","AWGN",100,168,20,"1x8",null,"1% miss detection",-18.190000000000001,-16.190000000000001,-19.239999999999998,-16.739999999999998,-19.100000000000001,-15.9,-17.93,-15.93,null,null,1.3099999999999987,0.83999999999999808,-18.615000000000002,-16.189999999999998,-16.189999999999998,-15.889999999999997,null,-15.914999999999999,-15.689999999999998,null,null,-16]
["Format2","AWGN",118,204,10,"1x2",null,"1% miss detection",-16.04,-14.04,-16.91,-14.41,-17,-13.8,-16.14,-14.14,null,null,0.96000000000000085,0.60999999999999943,-16.522500000000001,-14.0975,-14.0975,-13.797499999999999,null,-13.8,-13.5975,null,null,-13.8]
["Format2","AWGN",118,204,10,"1x4",null,"1% miss detection",-18.34,-16.34,-19.22,-16.72,-19.2,-16,-18.79,-16.760000000000002,null,null,0.87999999999999901,0.76000000000000156,-18.887500000000003,-16.455000000000002,-16.455000000000002,-16.155000000000001,null,"N/A",-15.955000000000002,null,null,-15.9]
["Format2","AWGN",118,204,10,"1x8",null,"1% miss detection",-20.49,-18.489999999999998,-21.2,-18.7,-21.6,-18,-20.86,-18.86,null,null,1.110000000000003,0.85999999999999943,-21.037500000000001,-18.512499999999999,-18.512499999999999,-18.212499999999999,null,-18,-18.012499999999999,null,null,-18]
["Format3","AWGN",137,264,0,"1x2",null,"1% miss detection",-16.04,-14.04,-17.149999999999999,-14.649999999999999,-16.8,-14.1,-16.45,-14.45,null,null,1.1099999999999994,0.60999999999999943,-16.61,-14.309999999999999,-14.309999999999999,-14.009999999999998,null,"N/A",-13.809999999999999,null,null,-14]
["Format3","AWGN",137,264,0,"1x4",null,"1% miss detection",-18.32,-16.32,-19.420000000000002,-16.920000000000002,-19,-16.399999999999999,-18.86,-16.86,null,null,1.1000000000000014,0.60000000000000142,-18.899999999999999,-16.625,-16.625,-16.324999999999999,null,"N/A",-16.125,null,null,-16.3]
["Format3","AWGN",137,264,0,"1x8",null,"1% miss detection",-20.49,-18.489999999999998,-21.54,-19.04,-21.6,-18.399999999999999,-21.03,-19.03,null,null,1.110000000000003,0.64000000000000057,-21.164999999999999,-18.740000000000002,-18.740000000000002,-18.440000000000001,null,-18.399999999999999,-18.240000000000002,null,null,-18.399999999999999]