{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Cover","Parameters","PUSCH 350kmph","PUSCH 500kmph","PUSCH UL timing adjustment","PRACH 1.25kHz SCS Type A","PRACH 1.25kHz SCS Type B","PRACH 15kHz SCS","PRACH 30kHz SCS"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #94-e",null,null,null,null,null,null,null,"R4-2000613"]
[null,"Online,  24th February - 6th March, 2020"]
[]
[null,"Source: CATT"]
[null,"Title: Summary of ideal and impairment results for NR HST demodulation requirements"]
[null,"Agenda: 8.17.2.2"]
[null,"Document for: Information"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH 350kmph","index":2,"n_rows":18,"n_cols":31,"rows_kept":18,"cut":false,"hidden":false,"merged":[[2,0,17,0],[2,1,9,1],[10,1,17,1],[0,11,1,11],[0,1,1,1],[0,3,1,3],[0,5,1,5],[0,6,1,6],[0,9,1,9],[0,10,1,10],[0,0,1,0],[2,2,5,2],[6,2,9,2],[10,2,13,2],[14,2,17,2],[2,3,5,3],[0,2,1,2],[0,4,1,4],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,8,1,8],[0,7,1,7],[12,6,13,6],[14,6,15,6],[16,6,17,6],[2,6,3,6],[4,6,5,6],[10,6,11,6],[6,6,7,6],[8,6,9,6],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,17,0,18],[0,19,0,20],[0,21,0,22],[6,3,9,3],[10,3,13,3],[14,3,17,3],[14,5,17,5],[14,4,17,4],[2,4,5,4],[6,4,9,4],[2,5,5,5],[6,5,9,5],[10,5,13,5],[10,4,13,4]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Maximum Doppler shift","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["AWGN","Tunnel",2.1,"15KHz","10MHz","1340Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,{"$f":"DerivingPerfReq(N3:AA3)","v":-100},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-100},null,null,null,null,null,null,-3.47,-1.4700000000000002,null,null,null,null,null,null,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":0},0,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-3.47},-1.4700000000000002]
[null,null,null,"15KHz","10MHz","1340Hz","1T1R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,8.65,10.65,null,null,null,null,null,null,0,0,8.65,10.65]
[null,null,null,"15KHz","10MHz","1340Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.2,-4.2,-5.93,-3.4299999999999997,null,null,null,null,0.27000000000000046,0.77000000000000046,-6.0649999999999995,-3.8149999999999999]
[null,null,null,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,5.68,7.68,5.75,8.25,null,null,null,null,7.0000000000000284E-2,0.57000000000000028,5.7149999999999999,7.9649999999999999]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-3.37,-1.37,null,null,null,null,null,null,0,0,-3.37,-1.37]
[null,null,null,"30KHz","40MHz","2334Hz","1T1R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,8.73,10.73,null,null,null,null,null,null,0,0,8.73,10.73]
[null,null,null,"30KHz","40MHz","2334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.11,-4.1100000000000003,-5.97,-3.4699999999999998,null,null,null,null,0.14000000000000057,0.64000000000000057,-6.04,-3.79]
[null,null,null,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,5.79,7.79,5.74,8.24,null,null,null,null,4.9999999999999822E-2,0.45000000000000018,5.7650000000000006,8.0150000000000006]
[null,"Open space",2.1,"15KHz","10MHz","1340Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.21,-4.21,-6,-3.5,null,null,null,null,0.20999999999999996,0.71,-6.1050000000000004,-3.855]
[null,null,2.1,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 [FFS]",16,{"$f":"DerivingPerfReq(N12:AA12)","v":-100},{"$f":"IF(L12>-100,L12+0.3,L12)","v":-100},null,null,null,null,null,null,5.67,7.67,5.73,8.23,null,null,null,null,{"$f":"MAX(N12,P12,R12,T12,V12,X12,Z12)-MIN(N12,P12,R12,T12,V12,X12,Z12)","v":6.0000000000000497E-2},{"$f":"MAX(O12,Q12,S12,U12,W12,Y12,AA12)-MIN(O12,Q12,S12,U12,W12,Y12,AA12)","v":0.5600000000000005},{"$f":"AVERAGE(N12,P12,R12,T12,V12,X12,Z12)","v":5.7},{"$f":"AVERAGE(O12,Q12,S12,U12,W12,Y12,AA12)","v":7.95}]
[null,null,2.1,"15KHz","10MHz","1340Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-11.2,-9.1999999999999993,null,null,null,null,null,null,0,0,-11.2,-9.1999999999999993]
[null,null,2.1,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,-0.24,1.76,null,null,null,null,null,null,0,0,-0.24,1.76]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.12,-4.12,-6.01,-3.51,null,null,null,null,0.11000000000000032,0.61000000000000032,-6.0649999999999995,-3.8149999999999999]
[null,null,3.6,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,5.76,7.76,5.72,8.2199999999999989,null,null,null,null,4.0000000000000036E-2,0.45999999999999908,5.74,7.9899999999999993]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-11.05,-9.0500000000000007,null,null,null,null,null,null,0,0,-11.05,-9.0500000000000007]
[null,null,3.6,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,-0.11,1.89,null,null,null,null,null,null,0,0,-0.11,1.89]

{"sheet":"PUSCH 500kmph","index":3,"n_rows":18,"n_cols":31,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,29,0,30],[2,0,17,0],[2,1,9,1],[10,1,17,1],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,6,1,6],[0,9,1,9],[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,7,1,7],[0,8,1,8],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[6,2,9,2],[6,3,9,3],[6,4,9,4],[6,5,9,5],[10,5,13,5],[10,4,13,4],[10,3,13,3],[10,2,13,2],[14,2,17,2],[14,3,17,3],[14,4,17,4],[14,5,17,5],[12,6,13,6],[14,6,15,6],[16,6,17,6],[2,6,3,6],[4,6,5,6],[6,6,7,6],[8,6,9,6],[10,6,11,6]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Maximum Doppler shift","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["AWGN","Tunnel",1.8,"15KHz","10MHz","1740Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,{"$f":"DerivingPerfReq(N3:AA3)","v":-100},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-100},null,null,null,null,null,null,-3.46,-1.46,null,null,null,null,null,null,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":0},0,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-3.46},-1.46]
[null,null,null,"15KHz","10MHz","1740Hz","1T1R","Type A","1+1+1","2 [FFS]","16 [FFS]",-100,-100,null,null,null,null,null,null,8.67,10.67,null,null,null,null,null,null,0,0,8.67,10.67]
[null,null,null,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.2,-4.2,-5.8,-3.3,null,null,null,null,0.40000000000000036,0.90000000000000036,-6,-3.75]
[null,null,null,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]","16 [FFS]",-100,-100,null,null,null,null,null,null,5.7,7.7,6.46,8.9600000000000009,null,null,null,null,0.75999999999999979,1.2600000000000007,6.08,8.33]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-3.37,-1.37,null,null,null,null,null,null,0,0,-3.37,-1.37]
[null,null,3.6,null,"40MHz","3334Hz","1T1R","Type A","1+1+1","2 [FFS]","16 [FFS]",-100,-100,null,null,null,null,null,null,8.77,10.77,null,null,null,null,null,null,0,0,8.77,10.77]
[null,null,3.6,null,"40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.11,-4.1100000000000003,-5.91,-3.41,null,null,null,null,0.20000000000000018,0.70000000000000018,-6.01,-3.7600000000000002]
[null,null,3.6,null,"40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]","16 [FFS]",-100,-100,null,null,null,null,null,null,5.83,7.83,5.81,8.3099999999999987,null,null,null,null,2.0000000000000462E-2,0.47999999999999865,5.82,8.07]
[null,"Open space",1.8,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.21,-4.21,-5.97,-3.4699999999999998,null,null,null,null,0.24000000000000021,0.74000000000000021,-6.09,-3.84]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,5.68,7.68,5.75,8.25,null,null,null,null,7.0000000000000284E-2,0.57000000000000028,5.7149999999999999,7.9649999999999999]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-11.2,-9.1999999999999993,null,null,null,null,null,null,0,0,-11.2,-9.1999999999999993]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T8R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-6.12,-4.12,-5.98,-3.4800000000000004,null,null,null,null,0.13999999999999968,0.63999999999999968,-6.0500000000000007,-3.8000000000000003]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,5.79,7.79,5.74,8.24,null,null,null,null,4.9999999999999822E-2,0.45000000000000018,5.7650000000000006,8.0150000000000006]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-11.04,-9.0399999999999991,null,null,null,null,null,null,0,0,-11.04,-9.0399999999999991]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T8R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,-0.1,1.9,null,null,null,null,null,null,0,0,-0.1,1.9]

{"sheet":"PUSCH UL timing adjustment","index":4,"n_rows":18,"n_cols":33,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,9,1,9],[0,13,1,13],[0,14,1,14],[0,15,0,16],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,4,1,4],[0,5,1,5],[0,7,1,7],[0,12,1,12],[0,29,0,30],[0,31,0,32],[2,0,17,0],[0,10,1,10],[0,11,1,11],[0,3,1,3],[2,1,5,1],[6,1,9,1],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,6,1,6],[0,8,1,8],[10,1,13,1],[14,1,17,1],[2,2,3,2],[4,2,5,2],[6,2,7,2],[8,2,9,2],[10,2,11,2],[12,2,13,2],[14,2,15,2],[16,2,17,2]]}
["Scenario","PUSCH transmission","SRS transmission","CBW","SCS","Waveform","Tx/Rx","DMRS","l0","MCS","A","Δω","PUSCH mapping type","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Scenario Y","FDD","Enabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",{"$f":"DerivingPerfReq(P3:AC3)","v":-100},{"$f":"IF(N3>-100,N3+0.3,N3)","v":-100},null,null,null,null,null,null,null,null,5.74,8.24,null,null,null,null,{"$f":"MAX(P3,R3,T3,V3,X3,Z3,AB3)-MIN(P3,R3,T3,V3,X3,Z3,AB3)","v":0},0,{"$f":"AVERAGE(P3,R3,T3,V3,X3,Z3,AB3)","v":5.74},8.24]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.74,8.24,null,null,null,null,0,0,5.74,8.24]
[null,null,"Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.74,8.24,null,null,null,null,0,0,5.74,8.24]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.74,8.24,null,null,null,null,0,0,5.74,8.24]
[null,"TDD","Enabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,null,null,null,null,0,0,5.71,8.2100000000000009]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,null,null,null,null,0,0,5.71,8.2100000000000009]
[null,null,"Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,null,null,null,null,0,0,5.71,8.2100000000000009]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,null,null,null,null,0,0,5.71,8.2100000000000009]
[null,"FDD","Enabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.7,8.1999999999999993,null,null,null,null,0,0,5.7,8.1999999999999993]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.69,8.1900000000000013,null,null,null,null,0,0,5.69,8.1900000000000013]
[null,null,"Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.7,8.1999999999999993,null,null,null,null,0,0,5.7,8.1999999999999993]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.69,8.1900000000000013,null,null,null,null,0,0,5.69,8.1900000000000013]
[null,"TDD","Enabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.67,8.17,null,null,null,null,0,0,5.67,8.17]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.67,8.17,null,null,null,null,0,0,5.67,8.17]
[null,null,"Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.67,8.17,null,null,null,null,0,0,5.67,8.17]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.67,8.17,null,null,null,null,0,0,5.67,8.17]

{"sheet":"PRACH 1.25kHz SCS Type A","index":5,"n_rows":11,"n_cols":31,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,27,0,28],[0,29,0,30],[0,8,1,8],[0,9,1,9],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,13,0,14],[0,12,1,12],[0,0,1,0],[0,1,1,1],[0,6,1,6],[0,7,1,7],[0,11,1,11],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,2,1,2],[0,10,1,10]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"AWGN",625,"1.04us",{"$f":"DerivingPerfReq(N3:AA3)","v":-100},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-100},null,null,null,null,null,null,-13.75,-11.75,-14.56,-12.06,null,null,null,null,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":0.8100000000000005},0.3100000000000005,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-14.155000000000001},-11.905000000000001]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"AWGN",1340,"1.04us",-100,-100,null,null,null,null,null,null,-16.350000000000001,-14.350000000000001,-15.2,-12.7,null,null,null,null,1.1500000000000021,1.6500000000000021,-15.775,-13.525]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"TDLC300-100",400,"2.55us",-100,-100,null,null,null,null,null,null,-6.67,-4.67,-7.52,-5.0199999999999996,null,null,null,null,0.84999999999999964,0.34999999999999964,-7.0949999999999998,-4.8449999999999998]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"AWGN",625,"1.04us",-100,-100,null,null,null,null,null,null,-16.079999999999998,-14.079999999999998,-16.87,-14.370000000000001,null,null,null,null,{"$f":"MAX(N6,P6,R6,T6,V6,X6,Z6)-MIN(N6,P6,R6,T6,V6,X6,Z6)","v":0.7900000000000027},{"$f":"MAX(O6,Q6,S6,U6,W6,Y6,AA6)-MIN(O6,Q6,S6,U6,W6,Y6,AA6)","v":0.2900000000000027},{"$f":"AVERAGE(N6,P6,R6,T6,V6,X6,Z6)","v":-16.475000000000001},{"$f":"AVERAGE(O6,Q6,S6,U6,W6,Y6,AA6)","v":-14.225}]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"AWGN",1340,"1.04us",-100,-100,null,null,null,null,null,null,-18.760000000000002,-16.760000000000002,-17.510000000000002,-15.010000000000002,null,null,null,null,1.25,1.75,-18.135000000000002,-15.885000000000002]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"TDLC300-100",400,"2.55us",-100,-100,null,null,null,null,null,null,-12.51,-10.51,-12.67,-10.17,null,null,null,null,0.16000000000000014,0.33999999999999986,-12.59,-10.34]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"AWGN",625,"1.04us",-100,-100,null,null,null,null,null,null,-18.12,-16.12,-18.96,-16.46,null,null,null,null,{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":0.83999999999999986},{"$f":"MAX(O9,Q9,S9,U9,W9,Y9,AA9)-MIN(O9,Q9,S9,U9,W9,Y9,AA9)","v":0.33999999999999986},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-18.54},{"$f":"AVERAGE(O9,Q9,S9,U9,W9,Y9,AA9)","v":-16.29}]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"AWGN",1340,"1.04us",-100,-100,null,null,null,null,null,null,-20.53,-18.53,-19.62,-17.12,null,null,null,null,0.91000000000000014,1.4100000000000001,-20.075000000000003,-17.825000000000003]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"TDLC300-100",400,"2.55us",{"$f":"DerivingPerfReq(N11:AA11)","v":-100},{"$f":"IF(L11>-100,L11+0.3,L11)","v":-100},null,null,null,null,null,null,-14.79,-12.79,-16.63,-14.129999999999999,null,null,null,null,{"$f":"MAX(N11,P11,R11,T11,V11,X11,Z11)-MIN(N11,P11,R11,T11,V11,X11,Z11)","v":1.8399999999999999},{"$f":"MAX(O11,Q11,S11,U11,W11,Y11,AA11)-MIN(O11,Q11,S11,U11,W11,Y11,AA11)","v":1.3399999999999999},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11,Z11)","v":-15.709999999999999},{"$f":"AVERAGE(O11,Q11,S11,U11,W11,Y11,AA11)","v":-13.459999999999999}]

{"sheet":"PRACH 1.25kHz SCS Type B","index":6,"n_rows":11,"n_cols":31,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,10,1,10],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,12,1,12],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,11,1,11],[0,5,1,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",2.1,"AWGN",625,"1.04us",{"$f":"DerivingPerfReq(N3:AA3)","v":-100},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-100},null,null,null,null,null,null,-12.86,-10.86,-14.16,-11.66,null,null,null,null,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":1.3000000000000007},0.80000000000000071,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-13.51},-11.26]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",2.1,"AWGN",2334,"1.04us",-100,-100,null,null,null,null,null,null,-15.51,-13.51,-14.61,-12.11,null,null,null,null,0.90000000000000036,1.4000000000000004,-15.059999999999999,-12.809999999999999]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",2.1,"TDLC300-100",400,"2.55us",-100,-100,null,null,null,null,null,null,-5.38,-3.38,-6.89,-4.3899999999999997,null,null,null,null,1.5099999999999998,1.0099999999999998,-6.1349999999999998,-3.8849999999999998]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",2.1,"AWGN",625,"1.04us",-100,-100,null,null,null,null,null,null,-15.33,-13.33,-16.34,-13.84,null,null,null,null,{"$f":"MAX(N6,P6,R6,T6,V6,X6,Z6)-MIN(N6,P6,R6,T6,V6,X6,Z6)","v":1.0099999999999998},{"$f":"MAX(O6,Q6,S6,U6,W6,Y6,AA6)-MIN(O6,Q6,S6,U6,W6,Y6,AA6)","v":0.50999999999999979},{"$f":"AVERAGE(N6,P6,R6,T6,V6,X6,Z6)","v":-15.835000000000001},{"$f":"AVERAGE(O6,Q6,S6,U6,W6,Y6,AA6)","v":-13.585000000000001}]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",2.1,"AWGN",2334,"1.04us",-100,-100,null,null,null,null,null,null,-18.010000000000002,-16.010000000000002,-16.72,-14.219999999999999,null,null,null,null,1.2900000000000027,1.7900000000000027,-17.365000000000002,-15.115]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",2.1,"TDLC300-100",400,"2.55us",-100,-100,null,null,null,null,null,null,-11.81,-9.81,-12.12,-9.6199999999999992,null,null,null,null,0.30999999999999872,0.19000000000000128,-11.965,-9.7149999999999999]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",2.1,"AWGN",625,"1.04us",-100,-100,null,null,null,null,null,null,-17.34,-15.34,-18.32,-15.82,null,null,null,null,{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":0.98000000000000043},{"$f":"MAX(O9,Q9,S9,U9,W9,Y9,AA9)-MIN(O9,Q9,S9,U9,W9,Y9,AA9)","v":0.48000000000000043},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-17.829999999999998},{"$f":"AVERAGE(O9,Q9,S9,U9,W9,Y9,AA9)","v":-15.58}]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",2.1,"AWGN",2334,"1.04us",-100,-100,null,null,null,null,null,null,-19.78,-17.78,-18.73,-16.23,null,null,null,null,1.0500000000000007,1.5500000000000007,-19.255000000000003,-17.005000000000003]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",2.1,"TDLC300-100",400,"2.55us",{"$f":"DerivingPerfReq(N11:AA11)","v":-100},{"$f":"IF(L11>-100,L11+0.3,L11)","v":-100},null,null,null,null,null,null,-14.06,-12.06,-15.93,-13.43,null,null,null,null,{"$f":"MAX(N11,P11,R11,T11,V11,X11,Z11)-MIN(N11,P11,R11,T11,V11,X11,Z11)","v":1.8699999999999992},{"$f":"MAX(O11,Q11,S11,U11,W11,Y11,AA11)-MIN(O11,Q11,S11,U11,W11,Y11,AA11)","v":1.3699999999999992},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11,Z11)","v":-14.995000000000001},{"$f":"AVERAGE(O11,Q11,S11,U11,W11,Y11,AA11)","v":-12.745000000000001}]

{"sheet":"PRACH 15kHz SCS","index":7,"n_rows":20,"n_cols":30,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,22,0,23],[0,24,0,25],[0,26,0,27],[0,28,0,29],[0,11,1,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9]]}
["Format","SCS","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M3:Z3)","v":-100},{"$f":"IF(K3>-100,K3+0.3,K3)","v":-100},null,null,null,null,null,null,-13.29,-11.29,-11.48,-8.98,null,null,null,null,{"$f":"MAX(M3,O3,Q3,S3,U3,W3,Y3)-MIN(M3,O3,Q3,S3,U3,W3,Y3)","v":1.8099999999999987},2.3099999999999987,{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3,Y3)","v":-12.385},-10.135]
["Format A2","15kHz",23,0,0,"1T2R",1.8,"TDLC300-100",400,"2.03us ",-100,-100,null,null,null,null,null,null,-6.57,-4.57,-7.22,-4.72,null,null,null,null,0.64999999999999947,0.14999999999999947,-6.8949999999999996,-4.6449999999999996]
["Format B4","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",-100,-100,null,null,null,null,null,null,-16.510000000000002,-14.510000000000002,-15.58,-13.08,null,null,null,null,0.93000000000000149,1.4300000000000015,-16.045000000000002,-13.795000000000002]
["Format B4","15kHz",23,0,0,"1T2R",1.8,"TDLC300-100",400,"2.03us ",{"$f":"DerivingPerfReq(M6:Z6)","v":-100},{"$f":"IF(K6>-100,K6+0.3,K6)","v":-100},null,null,null,null,null,null,-9.82,-7.82,-11.24,-8.74,null,null,null,null,{"$f":"MAX(M6,O6,Q6,S6,U6,W6,Y6)-MIN(M6,O6,Q6,S6,U6,W6,Y6)","v":1.42},{"$f":"MAX(N6,P6,R6,T6,V6,X6,Z6)-MIN(N6,P6,R6,T6,V6,X6,Z6)","v":0.91999999999999993},{"$f":"AVERAGE(M6,O6,Q6,S6,U6,W6,Y6)","v":-10.530000000000001},{"$f":"AVERAGE(N6,P6,R6,T6,V6,X6,Z6)","v":-8.2800000000000011}]
["Format C2","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",-100,-100,null,null,null,null,null,null,-13.31,-11.31,-11.51,-9.01,null,null,null,null,1.8000000000000007,2.3000000000000007,-12.41,-10.16]
["Format C2","15kHz",23,0,0,"1T2R",1.8,"TDLC300-100",400,"2.03us ",-100,-100,null,null,null,null,null,null,-6.81,-4.8099999999999996,-7.13,-4.63,null,null,null,null,0.32000000000000028,0.17999999999999972,-6.97,-4.72]
["Format A2","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M9:Z9)","v":-100},{"$f":"IF(K9>-100,K9+0.3,K9)","v":-100},null,null,null,null,null,null,-15.32,-13.32,-13.89,-11.39,null,null,null,null,{"$f":"MAX(M9,O9,Q9,S9,U9,W9,Y9)-MIN(M9,O9,Q9,S9,U9,W9,Y9)","v":1.4299999999999997},{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":1.9299999999999997},{"$f":"AVERAGE(M9,O9,Q9,S9,U9,W9,Y9)","v":-14.605},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-12.355}]
["Format A2","15kHz",23,0,0,"1T4R",1.8,"TDLC300-100",400,"2.03us ",-100,-100,null,null,null,null,null,null,-11.22,-9.2200000000000006,-12.17,-9.67,null,null,null,null,0.94999999999999929,0.44999999999999929,-11.695,-9.4450000000000003]
["Format B4","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-100,-100,null,null,null,null,null,null,-18.489999999999998,-16.489999999999998,-17.600000000000001,-15.100000000000001,null,null,null,null,0.88999999999999702,1.389999999999997,-18.045000000000002,-15.795]
["Format B4","15kHz",23,0,0,"1T4R",1.8,"TDLC300-100 ",400,"2.03us ",-100,-100,null,null,null,null,null,null,-14.24,-12.24,-15.23,-12.73,null,null,null,null,0.99000000000000021,0.49000000000000021,-14.734999999999999,-12.484999999999999]
["Format C2","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-100,-100,null,null,null,null,null,null,-15.34,-13.34,-13.89,-11.39,null,null,null,null,1.4499999999999993,1.9499999999999993,-14.615,-12.365]
["Format C2","15kHz",23,0,0,"1T4R",1.8,"TDLC300-100",400,"2.03us ",-100,-100,null,null,null,null,null,null,-11.23,-9.23,-12.21,-9.7100000000000009,null,null,null,null,0.98000000000000043,0.48000000000000043,-11.72,-9.4700000000000006]
["Format A2","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M15:Z15)","v":-100},{"$f":"IF(K15>-100,K15+0.3,K15)","v":-100},null,null,null,null,null,null,-17.350000000000001,-15.350000000000001,-15.51,-13.01,null,null,null,null,{"$f":"MAX(M15,O15,Q15,S15,U15,W15,Y15)-MIN(M15,O15,Q15,S15,U15,W15,Y15)","v":1.8400000000000016},{"$f":"MAX(N15,P15,R15,T15,V15,X15,Z15)-MIN(N15,P15,R15,T15,V15,X15,Z15)","v":2.3400000000000016},{"$f":"AVERAGE(M15,O15,Q15,S15,U15,W15,Y15)","v":-16.43},{"$f":"AVERAGE(N15,P15,R15,T15,V15,X15,Z15)","v":-14.18}]
["Format A2","15kHz",23,0,0,"1T8R",1.8,"TDLC300-100",400,"2.03us ",-100,-100,null,null,null,null,null,null,-14.29,-12.29,-15.26,-12.76,null,null,null,null,0.97000000000000064,0.47000000000000064,-14.774999999999999,-12.524999999999999]
["Format B4","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-100,-100,null,null,null,null,null,null,-20.260000000000002,-18.260000000000002,-19.22,-16.72,null,null,null,null,1.0400000000000027,1.5400000000000027,-19.740000000000002,-17.490000000000002]
["Format B4","15kHz",23,0,0,"1T8R",1.8,"TDLC300-100 ",400,"2.03us ",-100,-100,null,null,null,null,null,null,-17.27,-15.27,-19.02,-16.52,null,null,null,null,1.75,1.25,-18.145,-15.895]
["Format C2","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-100,-100,null,null,null,null,null,null,-17.329999999999998,-15.329999999999998,-15.5,-13,null,null,null,null,1.8299999999999983,2.3299999999999983,-16.414999999999999,-14.164999999999999]
["Format C2","15kHz",23,0,0,"1T8R",1.8,"TDLC300-100",400,"2.03us ",-100,-100,null,null,null,null,null,null,-14.26,-12.26,-15.5,-13,null,null,null,null,1.2400000000000002,0.74000000000000021,-14.879999999999999,-12.629999999999999]

{"sheet":"PRACH 30kHz SCS","index":8,"n_rows":20,"n_cols":30,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,22,0,23],[0,24,0,25],[0,26,0,27],[0,28,0,29],[0,11,1,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9]]}
["Format","SCS","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M3:Z3)","v":-100},{"$f":"IF(K3>-100,K3+0.3,K3)","v":-100},null,null,null,null,null,null,-13.19,-11.19,-13.54,-11.04,null,null,null,null,{"$f":"MAX(M3,O3,Q3,S3,U3,W3,Y3)-MIN(M3,O3,Q3,S3,U3,W3,Y3)","v":0.34999999999999964},0.15000000000000036,{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3,Y3)","v":-13.364999999999998},-11.114999999999998]
["Format A2","30kHz",46,0,0,"1T2R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-7.03,-5.03,-7.55,-5.05,null,null,null,null,0.51999999999999957,1.9999999999999574E-2,-7.29,-5.04]
["Format B4","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",-100,-100,null,null,null,null,null,null,-16.41,-14.41,-17.309999999999999,-14.809999999999999,null,null,null,null,0.89999999999999858,0.39999999999999858,-16.86,-14.61]
["Format B4","30kHz",46,0,0,"1T2R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-10.09,-8.09,-11.21,-8.7100000000000009,null,null,null,null,1.120000000000001,0.62000000000000099,-10.65,-8.4]
["Format C2","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",-100,-100,null,null,null,null,null,null,-13.19,-11.19,-13.55,-11.05,null,null,null,null,0.36000000000000121,0.13999999999999879,-13.370000000000001,-11.120000000000001]
["Format C2","30kHz",46,0,0,"1T2R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-7.02,-5.0199999999999996,-7.46,-4.96,null,null,null,null,0.44000000000000039,5.9999999999999609E-2,-7.24,-4.99]
["Format A2","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M9:Z9)","v":-100},{"$f":"IF(K9>-100,K9+0.3,K9)","v":-100},null,null,null,null,null,null,-15.25,-13.25,-15.68,-13.18,null,null,null,null,{"$f":"MAX(M9,O9,Q9,S9,U9,W9,Y9)-MIN(M9,O9,Q9,S9,U9,W9,Y9)","v":0.42999999999999972},{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":7.0000000000000284E-2},{"$f":"AVERAGE(M9,O9,Q9,S9,U9,W9,Y9)","v":-15.465},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-13.215}]
["Format A2","30kHz",46,0,0,"1T4R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-11.32,-9.32,-11.43,-8.93,null,null,null,null,0.10999999999999943,0.39000000000000057,-11.375,-9.125]
["Format B4","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-100,-100,null,null,null,null,null,null,-18.329999999999998,-16.329999999999998,-19.260000000000002,-16.760000000000002,null,null,null,null,0.93000000000000327,0.43000000000000327,-18.795000000000002,-16.545000000000002]
["Format B4","30kHz",46,0,0,"1T4R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-14.14,-12.14,-14.84,-12.34,null,null,null,null,0.69999999999999929,0.19999999999999929,-14.49,-12.24]
["Format C2","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-100,-100,null,null,null,null,null,null,-15.25,-13.25,-15.7,-13.2,null,null,null,null,0.44999999999999929,5.0000000000000711E-2,-15.475,-13.225]
["Format C2","30kHz",46,0,0,"1T4R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-11.1,-9.1,-11.45,-8.9499999999999993,null,null,null,null,0.34999999999999964,0.15000000000000036,-11.274999999999999,-9.0249999999999986]
["Format A2","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M15:Z15)","v":-100},{"$f":"IF(K15>-100,K15+0.3,K15)","v":-100},null,null,null,null,null,null,-17.27,-15.27,-17.43,-14.93,null,null,null,null,{"$f":"MAX(M15,O15,Q15,S15,U15,W15,Y15)-MIN(M15,O15,Q15,S15,U15,W15,Y15)","v":0.16000000000000014},{"$f":"MAX(N15,P15,R15,T15,V15,X15,Z15)-MIN(N15,P15,R15,T15,V15,X15,Z15)","v":0.33999999999999986},{"$f":"AVERAGE(M15,O15,Q15,S15,U15,W15,Y15)","v":-17.350000000000001},{"$f":"AVERAGE(N15,P15,R15,T15,V15,X15,Z15)","v":-15.1}]
["Format A2","30kHz",46,0,0,"1T8R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-14.26,-12.26,-14.25,-11.75,null,null,null,null,9.9999999999997868E-3,0.50999999999999979,-14.254999999999999,-12.004999999999999]
["Format B4","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-100,-100,null,null,null,null,null,null,-20.2,-18.2,-20.8,-18.3,null,null,null,null,0.60000000000000142,0.10000000000000142,-20.5,-18.25]
["Format B4","30kHz",46,0,0,"1T8R",3.6,"TDLC300-100",400,"1.77us",-100,-100,null,null,null,null,null,null,-17.23,-15.23,-17.670000000000002,-15.170000000000002,null,null,null,null,0.44000000000000128,5.9999999999998721E-2,-17.450000000000003,-15.200000000000001]
["Format C2","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-100,-100,null,null,null,null,null,null,-17.239999999999998,-15.239999999999998,-17.39,-14.89,null,null,null,null,0.15000000000000213,0.34999999999999787,-17.314999999999998,-15.065]
["Format C2","30kHz",46,0,0,"1T8R",3.6,"TDLC300-100 ",400,"1.77us",{"$f":"DerivingPerfReq(M20:Z20)","v":-100},{"$f":"IF(K20>-100,K20+0.3,K20)","v":-100},null,null,null,null,null,null,-14.32,-12.32,-14.29,-11.79,null,null,null,null,{"$f":"MAX(M20,O20,Q20,S20,U20,W20,Y20)-MIN(M20,O20,Q20,S20,U20,W20,Y20)","v":3.0000000000001137E-2},{"$f":"MAX(N20,P20,R20,T20,V20,X20,Z20)-MIN(N20,P20,R20,T20,V20,X20,Z20)","v":0.53000000000000114},{"$f":"AVERAGE(M20,O20,Q20,S20,U20,W20,Y20)","v":-14.305},{"$f":"AVERAGE(N20,P20,R20,T20,V20,X20,Z20)","v":-12.055}]