{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Cover","Parameters","PUSCH 350kmph","PUSCH 500kmph","PUSCH UL timing adjustment","PRACH 1.25kHz SCS Type A","PRACH 1.25kHz SCS Type B","PRACH 15kHz SCS","PRACH 30kHz SCS"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #94-e",null,null,null,null,null,null,null,"R4-2000613"]
[null,"Online,  24th February - 6th March, 2020"]
[]
[null,"Source: CATT"]
[null,"Title: Summary of ideal and impairment results for NR HST demodulation requirements"]
[null,"Agenda: 8.17.2.2"]
[null,"Document for: Information"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH 350kmph","index":2,"n_rows":18,"n_cols":31,"rows_kept":18,"cut":false,"hidden":false,"merged":[[2,0,17,0],[2,1,9,1],[10,1,17,1],[0,11,1,11],[0,1,1,1],[0,3,1,3],[0,5,1,5],[0,6,1,6],[0,9,1,9],[0,10,1,10],[0,0,1,0],[2,2,5,2],[6,2,9,2],[10,2,13,2],[14,2,17,2],[2,3,5,3],[0,2,1,2],[0,4,1,4],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,8,1,8],[0,7,1,7],[12,6,13,6],[14,6,15,6],[16,6,17,6],[2,6,3,6],[4,6,5,6],[10,6,11,6],[6,6,7,6],[8,6,9,6],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,17,0,18],[0,19,0,20],[0,21,0,22],[6,3,9,3],[10,3,13,3],[14,3,17,3],[14,5,17,5],[14,4,17,4],[2,4,5,4],[6,4,9,4],[2,5,5,5],[6,5,9,5],[10,5,13,5],[10,4,13,4]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Maximum Doppler shift","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["AWGN","Tunnel",2.1,"15KHz","10MHz","1340Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,{"$f":"DerivingPerfReq(N3:AA3)","v":-100},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-100},null,null,null,null,null,null,-3.47,-1.4700000000000002,null,null,null,null,"-3,0","-0,9",{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":0},0,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-3.47},-1.4700000000000002]
[null,null,null,"15KHz","10MHz","1340Hz","1T1R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,8.65,10.65,null,null,null,null,"9,7","12,1",0,0,8.65,10.65]
[null,null,null,"15KHz","10MHz","1340Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4.0999999999999996,-3.8,null,null,null,null,null,null,-6.2,-4.2,-5.93,-3.4299999999999997,-6.6,-4.5999999999999996,"-6,0","-3,6",0.66999999999999993,1.17,-6.2433333333333323,-4.0766666666666671]
[null,null,null,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 [FFS]",16,7.8,8.1,null,null,null,null,null,null,5.68,7.68,5.75,8.25,5.41,7.41,"6,6","9,1",0.33999999999999986,0.83999999999999986,5.6133333333333333,7.78]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-3.37,-1.37,null,null,null,null,"-3,0","-1,0",0,0,-3.37,-1.37]
[null,null,null,"30KHz","40MHz","2334Hz","1T1R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,8.73,10.73,null,null,null,null,"9,5","11,7",0,0,8.73,10.73]
[null,null,null,"30KHz","40MHz","2334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4.0999999999999996,-3.8,null,null,null,null,null,null,-6.11,-4.1100000000000003,-5.97,-3.4699999999999998,-6.59,-4.59,"-6,0","-3,6",0.62000000000000011,1.1200000000000001,-6.2233333333333336,-4.0566666666666666]
[null,null,null,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 [FFS]",16,7.8,8.1,null,null,null,null,null,null,5.79,7.79,5.74,8.24,5.42,7.42,"6,5","9,0",0.37000000000000011,0.82000000000000028,5.6500000000000012,7.8166666666666673]
[null,"Open space",2.1,"15KHz","10MHz","1340Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4.0999999999999996,-3.8,null,null,null,null,null,null,-6.21,-4.21,-6,-3.5,-6.6,-4.5999999999999996,"-6,1","-4,0",0.59999999999999964,1.0999999999999996,-6.2700000000000005,-4.1033333333333326]
[null,null,2.1,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 [FFS]",16,{"$f":"DerivingPerfReq(N12:AA12)","v":7.8},{"$f":"IF(L12>-100,L12+0.3,L12)","v":8.1},null,null,null,null,null,null,5.67,7.67,5.73,8.23,5.4,7.4,"6,3","8,5",{"$f":"MAX(N12,P12,R12,T12,V12,X12,Z12)-MIN(N12,P12,R12,T12,V12,X12,Z12)","v":0.33000000000000007},{"$f":"MAX(O12,Q12,S12,U12,W12,Y12,AA12)-MIN(O12,Q12,S12,U12,W12,Y12,AA12)","v":0.83000000000000007},{"$f":"AVERAGE(N12,P12,R12,T12,V12,X12,Z12)","v":5.6000000000000005},{"$f":"AVERAGE(O12,Q12,S12,U12,W12,Y12,AA12)","v":7.7666666666666666}]
[null,null,2.1,"15KHz","10MHz","1340Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-102,-102,null,null,null,null,null,null,-11.2,-9.1999999999999993,null,null,-12.57,-10.57,-12,"-9,9",1.370000000000001,1.370000000000001,-11.923333333333332,-9.8849999999999998]
[null,null,2.1,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 [FFS]",16,-103,-103,null,null,null,null,null,null,-0.24,1.76,null,null,0.4,2.4,"0,3","2,6",0.64,0.6399999999999999,8.0000000000000016E-2,2.08]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4.0999999999999996,-3.8,null,null,null,null,null,null,-6.12,-4.12,-6.01,-3.51,-6.63,-4.63,"-6,0","-3,6",0.62000000000000011,1.1200000000000001,-6.253333333333333,-4.0866666666666669]
[null,null,3.6,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 [FFS]",16,7.8,8.1,null,null,null,null,null,null,5.76,7.76,5.72,8.2199999999999989,5.4,7.4,"6,2","8,5",0.35999999999999943,0.81999999999999851,5.6266666666666678,7.793333333333333]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-103,-103,null,null,null,null,null,null,-11.05,-9.0500000000000007,null,null,-12.6,-10.6,"-12,0","-9,5",1.5499999999999989,1.5499999999999989,-11.824999999999999,-9.8249999999999993]
[null,null,3.6,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 [FFS]",16,-103,-103,null,null,null,null,null,null,-0.11,1.89,null,null,0.4,2.4,"0,3","2,4",0.51,0.51,0.14500000000000002,2.145]

{"sheet":"PUSCH 500kmph","index":3,"n_rows":18,"n_cols":31,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,29,0,30],[2,0,17,0],[2,1,9,1],[10,1,17,1],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,6,1,6],[0,9,1,9],[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,7,1,7],[0,8,1,8],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[6,2,9,2],[6,3,9,3],[6,4,9,4],[6,5,9,5],[10,5,13,5],[10,4,13,4],[10,3,13,3],[10,2,13,2],[14,2,17,2],[14,3,17,3],[14,4,17,4],[14,5,17,5],[12,6,13,6],[14,6,15,6],[16,6,17,6],[2,6,3,6],[4,6,5,6],[6,6,7,6],[8,6,9,6],[10,6,11,6]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Maximum Doppler shift","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["AWGN","Tunnel",1.8,"15KHz","10MHz","1740Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,{"$f":"DerivingPerfReq(N3:AA3)","v":-100},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-100},null,null,null,null,null,null,-3.46,-1.46,null,null,null,null,-3,-0.8,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":0.45999999999999996},0.65999999999999992,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-3.23},-1.1299999999999999]
[null,null,null,"15KHz","10MHz","1740Hz","1T1R","Type A","1+1+1","2 [FFS]","16 [FFS]",-100,-100,null,null,null,null,null,null,8.67,10.67,null,null,null,null,10.5,12.6,1.83,1.9299999999999997,9.5850000000000009,11.635]
[null,null,null,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4,-3.7,null,null,null,null,null,null,-6.2,-4.2,-5.8,-3.3,-6.6,-4.5999999999999996,-6,-3.9,0.79999999999999982,1.2999999999999998,-6.15,-4]
[null,null,null,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]","16 [FFS]",8,8.3000000000000007,null,null,null,null,null,null,5.7,7.7,6.46,8.9600000000000009,5.41,7.41,7.5,10,2.09,2.59,6.2675000000000001,8.5175000000000001]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T1R [FFS]","Type A","1+1+1","2 [FFS]",2,-100,-100,null,null,null,null,null,null,-3.37,-1.37,null,null,null,null,-3,-0.8,0.37000000000000011,0.57000000000000006,-3.1850000000000001,-1.085]
[null,null,3.6,null,"40MHz","3334Hz","1T1R","Type A","1+1+1","2 [FFS]","16 [FFS]",-100,-100,null,null,null,null,null,null,8.77,10.77,null,null,null,null,10.4,12.4,1.6300000000000008,1.6300000000000008,9.5850000000000009,11.585000000000001]
[null,null,3.6,null,"40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-3.9,-3.6,null,null,null,null,null,null,-6.11,-4.1100000000000003,-5.91,-3.41,-6.59,-4.59,-6,-3.5,0.67999999999999972,1.1799999999999997,-6.1524999999999999,-3.9024999999999999]
[null,null,3.6,null,"40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]","16 [FFS]",7.9,8.2000000000000011,null,null,null,null,null,null,5.83,7.83,5.81,8.3099999999999987,5.42,7.42,7.5,9.8000000000000007,2.08,2.3800000000000008,6.1400000000000006,8.34]
[null,"Open space",1.8,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4.0999999999999996,-3.8,null,null,null,null,null,null,-6.21,-4.21,-5.97,-3.4699999999999998,-6.6,-4.5999999999999996,-6.1,-4.0999999999999996,0.62999999999999989,1.1299999999999999,-6.2200000000000006,-4.0949999999999998]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 [FFS]",16,8,8.3000000000000007,null,null,null,null,null,null,5.68,7.68,5.75,8.25,5.4,7.4,6.5,8.6,1.0999999999999996,1.1999999999999993,5.8324999999999996,7.9824999999999999]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-9.1999999999999993,-8.8999999999999986,null,null,null,null,null,null,-11.2,-9.1999999999999993,null,null,-10.28,-8.2799999999999994,-12,-10,1.7200000000000006,1.7200000000000006,-11.159999999999998,-9.1599999999999984]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T8R","Type A","1+1+1","2 [FFS]",16,-100,-100,null,null,null,null,null,null,null,null,null,null,0.4,2.4,0.5,2.5,9.9999999999999978E-2,0.10000000000000009,0.45,2.4500000000000002]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]",2,-4,-3.7,null,null,null,null,null,null,-6.12,-4.12,-5.98,-3.4800000000000004,-6.61,-4.6100000000000003,-6,-3.8,0.62999999999999989,1.1299999999999999,-6.1775000000000002,-4.0025000000000004]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T2R","Type A","1+1+1","2 [FFS]",16,8.1,8.4,null,null,null,null,null,null,5.79,7.79,5.74,8.24,5.4,7.4,6.5,8.9,1.0999999999999996,1.5,5.8574999999999999,8.0824999999999996]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T8R","Type A","1+1+1","2 [FFS]",2,-9.8000000000000007,-9.5,null,null,null,null,null,null,-11.04,-9.0399999999999991,null,null,-12.6,-10.6,-12,-9.9,1.5600000000000005,1.5600000000000005,-11.88,-9.8466666666666658]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T8R","Type A","1+1+1","2 [FFS]",16,2.4,2.6999999999999997,null,null,null,null,null,null,-0.1,1.9,null,null,0.4,2.4,0.5,2.8,0.6,0.89999999999999991,0.26666666666666666,2.3666666666666667]

{"sheet":"PUSCH UL timing adjustment","index":4,"n_rows":18,"n_cols":33,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,9,1,9],[0,13,1,13],[0,14,1,14],[0,15,0,16],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,4,1,4],[0,5,1,5],[0,7,1,7],[0,12,1,12],[0,29,0,30],[0,31,0,32],[2,0,17,0],[0,10,1,10],[0,11,1,11],[0,3,1,3],[2,1,5,1],[6,1,9,1],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,6,1,6],[0,8,1,8],[10,1,13,1],[14,1,17,1],[2,2,3,2],[4,2,5,2],[6,2,7,2],[8,2,9,2],[10,2,11,2],[12,2,13,2],[14,2,15,2],[16,2,17,2]]}
["Scenario","PUSCH transmission","SRS transmission","CBW","SCS","Waveform","Tx/Rx","DMRS","l0","MCS","A","Δω","PUSCH mapping type","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Scenario Y","FDD","Enabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",{"$f":"DerivingPerfReq(P3:AC3)","v":-100},{"$f":"IF(N3>-100,N3+0.3,N3)","v":-100},null,null,null,null,null,null,null,null,5.74,8.24,5.88,{"$f":"Z3+2","v":7.88},null,null,{"$f":"MAX(P3,R3,T3,V3,X3,Z3,AB3)-MIN(P3,R3,T3,V3,X3,Z3,AB3)","v":0.13999999999999968},0.36000000000000032,{"$f":"AVERAGE(P3,R3,T3,V3,X3,Z3,AB3)","v":5.8100000000000005},8.06]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.74,8.24,6.08,{"$f":"Z4+2","v":8.08},null,null,0.33999999999999986,0.16000000000000014,5.91,8.16]
[null,null,"Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",8.1,8.4,null,null,null,null,null,null,null,null,5.74,8.24,5.88,7.88,6,8.3000000000000007,0.25999999999999979,0.42000000000000082,5.873333333333334,8.14]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",8.1999999999999993,8.5,null,null,null,null,null,null,null,null,5.74,8.24,6.08,8.08,6,8.1999999999999993,0.33999999999999986,0.16000000000000014,5.94,8.1733333333333338]
[null,"TDD","Enabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,5.87,7.87,null,null,0.16000000000000014,0.34000000000000075,5.79,8.0400000000000009]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,6.08,8.08,null,null,0.37000000000000011,0.13000000000000078,5.8949999999999996,8.1449999999999996]
[null,null,"Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",8.1999999999999993,8.5,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,6.01,8.01,6,8.3000000000000007,0.29999999999999982,0.29000000000000092,5.9066666666666663,8.1733333333333338]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type B",8.1999999999999993,8.5,null,null,null,null,null,null,null,null,5.71,8.2100000000000009,6.25,8.25,6,8.1999999999999993,0.54,5.0000000000000711E-2,5.9866666666666672,8.2200000000000006]
[null,"FDD","Enabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.7,8.1999999999999993,null,null,null,null,0,0,5.7,8.1999999999999993]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.69,8.1900000000000013,null,null,null,null,0,0,5.69,8.1900000000000013]
[null,null,"Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.7,8.1999999999999993,null,null,6,8.3000000000000007,0.29999999999999982,0.10000000000000142,5.85,8.25]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.69,8.1900000000000013,null,null,6,8.1,0.30999999999999961,9.0000000000001634E-2,5.8450000000000006,8.1449999999999996]
[null,"TDD","Enabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",-100,-100,null,null,null,null,null,null,null,null,5.67,8.17,6.04,8.0399999999999991,null,null,0.37000000000000011,0.13000000000000078,5.8550000000000004,8.1050000000000004]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",-100,-100,null,null,null,null,null,null,null,null,5.67,8.17,6.25,8.25,null,null,0.58000000000000007,8.0000000000000071E-2,5.96,8.2100000000000009]
[null,null,"Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",8.1999999999999993,8.5,null,null,null,null,null,null,null,null,5.67,8.17,6.04,8.0399999999999991,6,8.3000000000000007,0.37000000000000011,0.26000000000000156,5.9033333333333333,8.17]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type B",8.1999999999999993,8.5,null,null,null,null,null,null,null,null,5.67,8.17,6.26,8.26,6,8.1,0.58999999999999986,0.16000000000000014,5.9766666666666666,8.1766666666666676]

{"sheet":"PRACH 1.25kHz SCS Type A","index":5,"n_rows":11,"n_cols":31,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,27,0,28],[0,29,0,30],[0,8,1,8],[0,9,1,9],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,13,0,14],[0,12,1,12],[0,0,1,0],[0,1,1,1],[0,6,1,6],[0,7,1,7],[0,11,1,11],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,2,1,2],[0,10,1,10]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"AWGN",625,"1.04us",{"$f":"DerivingPerfReq(N3:AA3)","v":-12},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-11.7},null,null,null,null,null,null,-13.75,-11.75,-14.56,-12.06,-14.11,-12.11,"-14,3","-12,0",{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":0.8100000000000005},0.35999999999999943,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-14.14},-11.973333333333334]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"AWGN",1340,"1.04us",-13.9,-13.6,null,null,null,null,null,null,-16.350000000000001,-14.350000000000001,-15.2,-12.7,-16.55,-14.55,"-15,5","-13,4",1.3500000000000014,1.8500000000000014,-16.033333333333335,-13.866666666666667]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"TDLC300-100",400,"2.55us",-5.2,-4.9000000000000004,null,null,null,null,null,null,-6.67,-4.67,-7.52,-5.0199999999999996,-7.9,-5.9,"-7,6","-5,1",1.2300000000000004,1.2300000000000004,-7.3633333333333333,-5.1966666666666663]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"AWGN",625,"1.04us",-14.5,-14.2,null,null,null,null,null,null,-16.079999999999998,-14.079999999999998,-16.87,-14.370000000000001,-17.02,-15.02,"-16,7","-14,5",{"$f":"MAX(N6,P6,R6,T6,V6,X6,Z6)-MIN(N6,P6,R6,T6,V6,X6,Z6)","v":0.94000000000000128},{"$f":"MAX(O6,Q6,S6,U6,W6,Y6,AA6)-MIN(O6,Q6,S6,U6,W6,Y6,AA6)","v":0.94000000000000128},{"$f":"AVERAGE(N6,P6,R6,T6,V6,X6,Z6)","v":-16.656666666666666},{"$f":"AVERAGE(O6,Q6,S6,U6,W6,Y6,AA6)","v":-14.49}]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"AWGN",1340,"1.04us",-16.399999999999999,-16.099999999999998,null,null,null,null,null,null,-18.760000000000002,-16.760000000000002,-17.510000000000002,-15.010000000000002,-19.41,-17.41,"-17,9","-15,4",1.8999999999999986,2.3999999999999986,-18.560000000000002,-16.393333333333334]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"TDLC300-100",400,"2.55us",-10.7,-10.399999999999999,null,null,null,null,null,null,-12.51,-10.51,-12.67,-10.17,-13.37,-11.37,"-13,0","-10,6",0.85999999999999943,1.1999999999999993,-12.85,-10.683333333333332]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"AWGN",625,"1.04us",-16.5,-16.2,null,null,null,null,null,null,-18.12,-16.12,-18.96,-16.46,-18.82,-16.82,"-18,9","-16,4",{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":0.83999999999999986},{"$f":"MAX(O9,Q9,S9,U9,W9,Y9,AA9)-MIN(O9,Q9,S9,U9,W9,Y9,AA9)","v":0.69999999999999929},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-18.633333333333333},{"$f":"AVERAGE(O9,Q9,S9,U9,W9,Y9,AA9)","v":-16.466666666666665}]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"AWGN",1340,"1.04us",-18.399999999999999,-18.099999999999998,null,null,null,null,null,null,-20.53,-18.53,-19.62,-17.12,-21.41,-19.41,"-20,1","-17,7",1.7899999999999991,2.2899999999999991,-20.52,-18.353333333333335]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"TDLC300-100",400,"2.55us",{"$f":"DerivingPerfReq(N11:AA11)","v":-103},{"$f":"IF(L11>-100,L11+0.3,L11)","v":-103},null,null,null,null,null,null,-14.79,-12.79,-16.63,-14.129999999999999,-17.5,-15.5,"-17,3","-15,0",{"$f":"MAX(N11,P11,R11,T11,V11,X11,Z11)-MIN(N11,P11,R11,T11,V11,X11,Z11)","v":2.7100000000000009},{"$f":"MAX(O11,Q11,S11,U11,W11,Y11,AA11)-MIN(O11,Q11,S11,U11,W11,Y11,AA11)","v":2.7100000000000009},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11,Z11)","v":-16.306666666666668},{"$f":"AVERAGE(O11,Q11,S11,U11,W11,Y11,AA11)","v":-14.14}]

{"sheet":"PRACH 1.25kHz SCS Type B","index":6,"n_rows":11,"n_cols":31,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,10,1,10],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,12,1,12],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,11,1,11],[0,5,1,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",2.1,"AWGN",625,"1.04us",{"$f":"DerivingPerfReq(N3:AA3)","v":-11.6},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-11.299999999999999},null,null,null,null,null,null,-12.86,-10.86,-14.16,-11.66,-14.27,-12.27,"-15,7","-13,6",{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3)-MIN(N3,P3,R3,T3,V3,X3,Z3)","v":1.4100000000000001},1.4100000000000001,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3)","v":-13.763333333333334},-11.596666666666666]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",2.1,"AWGN",2334,"1.04us",-12.8,-12.5,null,null,null,null,null,null,-15.51,-13.51,-14.61,-12.11,-14.87,-12.87,"-14,4","-11,9",0.90000000000000036,1.4000000000000004,-14.996666666666664,-12.829999999999998]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",2.1,"TDLC300-100",400,"2.55us",-102,-102,null,null,null,null,null,null,-5.38,-3.38,-6.89,-4.3899999999999997,-8.1999999999999993,-6.2,-8.3000000000000007,"-5,8",2.9200000000000008,2.8200000000000003,-7.1924999999999999,-4.6566666666666663]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",2.1,"AWGN",625,"1.04us",-13.9,-13.6,null,null,null,null,null,null,-15.33,-13.33,-16.34,-13.84,-16.649999999999999,-14.65,"-17,9","-15,7",{"$f":"MAX(N6,P6,R6,T6,V6,X6,Z6)-MIN(N6,P6,R6,T6,V6,X6,Z6)","v":1.3199999999999985},{"$f":"MAX(O6,Q6,S6,U6,W6,Y6,AA6)-MIN(O6,Q6,S6,U6,W6,Y6,AA6)","v":1.3200000000000003},{"$f":"AVERAGE(N6,P6,R6,T6,V6,X6,Z6)","v":-16.106666666666666},{"$f":"AVERAGE(O6,Q6,S6,U6,W6,Y6,AA6)","v":-13.94}]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",2.1,"AWGN",2334,"1.04us",-15.3,-15,null,null,null,null,null,null,-18.010000000000002,-16.010000000000002,-16.72,-14.219999999999999,-17.63,-15.63,"-16,7","-14,6",1.2900000000000027,1.7900000000000027,-17.453333333333333,-15.286666666666667]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",2.1,"TDLC300-100",400,"2.55us",-10,-9.6999999999999993,null,null,null,null,null,null,-11.81,-9.81,-12.12,-9.6199999999999992,-12.5,-10.5,"-13,7","-11,2",0.6899999999999995,0.88000000000000078,-12.143333333333333,-9.9766666666666666]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",2.1,"AWGN",625,"1.04us",-15.9,-15.6,null,null,null,null,null,null,-17.34,-15.34,-18.32,-15.82,-18.63,-16.63,"-20,1","-17,7",{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":1.2899999999999991},{"$f":"MAX(O9,Q9,S9,U9,W9,Y9,AA9)-MIN(O9,Q9,S9,U9,W9,Y9,AA9)","v":1.2899999999999991},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-18.096666666666664},{"$f":"AVERAGE(O9,Q9,S9,U9,W9,Y9,AA9)","v":-15.93}]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",2.1,"AWGN",2334,"1.04us",-17.3,-17,null,null,null,null,null,null,-19.78,-17.78,-18.73,-16.23,-19.89,-17.89,"-18,9","-16,9",1.1600000000000001,1.6600000000000001,-19.466666666666669,-17.3]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",2.1,"TDLC300-100",400,"2.55us",{"$f":"DerivingPerfReq(N11:AA11)","v":-103},{"$f":"IF(L11>-100,L11+0.3,L11)","v":-103},null,null,null,null,null,null,-14.06,-12.06,-15.93,-13.43,-17.25,-15.25,"-17,7","-15,2",{"$f":"MAX(N11,P11,R11,T11,V11,X11,Z11)-MIN(N11,P11,R11,T11,V11,X11,Z11)","v":3.1899999999999995},{"$f":"MAX(O11,Q11,S11,U11,W11,Y11,AA11)-MIN(O11,Q11,S11,U11,W11,Y11,AA11)","v":3.1899999999999995},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11,Z11)","v":-15.746666666666668},{"$f":"AVERAGE(O11,Q11,S11,U11,W11,Y11,AA11)","v":-13.58}]

{"sheet":"PRACH 15kHz SCS","index":7,"n_rows":20,"n_cols":30,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,22,0,23],[0,24,0,25],[0,26,0,27],[0,28,0,29],[0,11,1,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9]]}
["Format","SCS","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M3:Z3)","v":-103},{"$f":"IF(K3>-100,K3+0.3,K3)","v":-103},null,null,null,null,null,null,-13.29,-11.29,-11.48,-8.98,-13.66,-11.66,"-13,8","-11,4 ",{"$f":"MAX(M3,O3,Q3,S3,U3,W3,Y3)-MIN(M3,O3,Q3,S3,U3,W3,Y3)","v":2.1799999999999997},2.6799999999999997,{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3,Y3)","v":-12.81},-10.643333333333333]
["Format A2","15kHz",23,0,0,"1T2R",1.8,"TDLC300-100",400,"2.03us ",-103,-103,null,null,null,null,null,null,-6.57,-4.57,-7.22,-4.72,null,null,"-6,8","-4,7  ",0.64999999999999947,0.14999999999999947,-6.8949999999999996,-4.6449999999999996]
["Format B4","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",-14.2,-13.899999999999999,null,null,null,null,null,null,-16.510000000000002,-14.510000000000002,-15.58,-13.08,-17.149999999999999,-15.15,"-16,4","-14,1 ",1.5699999999999985,2.0700000000000003,-16.413333333333334,-14.246666666666668]
["Format B4","15kHz",23,0,0,"1T2R",1.8,"TDLC300-100",400,"2.03us ",{"$f":"DerivingPerfReq(M6:Z6)","v":-103},{"$f":"IF(K6>-100,K6+0.3,K6)","v":-103},null,null,null,null,null,null,-9.82,-7.82,-11.24,-8.74,null,null,"-8,9","-6,8  ",{"$f":"MAX(M6,O6,Q6,S6,U6,W6,Y6)-MIN(M6,O6,Q6,S6,U6,W6,Y6)","v":1.42},{"$f":"MAX(N6,P6,R6,T6,V6,X6,Z6)-MIN(N6,P6,R6,T6,V6,X6,Z6)","v":0.91999999999999993},{"$f":"AVERAGE(M6,O6,Q6,S6,U6,W6,Y6)","v":-10.530000000000001},{"$f":"AVERAGE(N6,P6,R6,T6,V6,X6,Z6)","v":-8.2800000000000011}]
["Format C2","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",-103,-103,null,null,null,null,null,null,-13.31,-11.31,-11.51,-9.01,-13.63,-11.63,"-13,1","-10,6",2.120000000000001,2.620000000000001,-12.816666666666668,-10.65]
["Format C2","15kHz",23,0,0,"1T2R",1.8,"TDLC300-100",400,"2.03us ",-103,-103,null,null,null,null,null,null,-6.81,-4.8099999999999996,-7.13,-4.63,null,null,"-6,8","-4,7",0.32000000000000028,0.17999999999999972,-6.97,-4.72]
["Format A2","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M9:Z9)","v":-12.9},{"$f":"IF(K9>-100,K9+0.3,K9)","v":-12.6},null,null,null,null,null,null,-15.32,-13.32,-13.89,-11.39,-15.89,-13.89,"-16,1","-13,6 ",{"$f":"MAX(M9,O9,Q9,S9,U9,W9,Y9)-MIN(M9,O9,Q9,S9,U9,W9,Y9)","v":2},{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":2.5},{"$f":"AVERAGE(M9,O9,Q9,S9,U9,W9,Y9)","v":-15.033333333333333},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-12.866666666666667}]
["Format A2","15kHz",23,0,0,"1T4R",1.8,"TDLC300-100",400,"2.03us ",-103,-103,null,null,null,null,null,null,-11.22,-9.2200000000000006,-12.17,-9.67,null,null,"-11,5","-9,1 ",0.94999999999999929,0.44999999999999929,-11.695,-9.4450000000000003]
["Format B4","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-16.3,-16,null,null,null,null,null,null,-18.489999999999998,-16.489999999999998,-17.600000000000001,-15.100000000000001,-19.309999999999999,-17.309999999999999,"-18,7","-16,5 ",1.7099999999999973,2.2099999999999973,-18.466666666666669,-16.3]
["Format B4","15kHz",23,0,0,"1T4R",1.8,"TDLC300-100 ",400,"2.03us ",-103,-103,null,null,null,null,null,null,-14.24,-12.24,-15.23,-12.73,null,null,"-13,4","-11,0  ",0.99000000000000021,0.49000000000000021,-14.734999999999999,-12.484999999999999]
["Format C2","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-12.8,-12.5,null,null,null,null,null,null,-15.34,-13.34,-13.89,-11.39,-15.82,-13.82,"-15,5","-13,2",1.9299999999999997,2.4299999999999997,-15.016666666666666,-12.85]
["Format C2","15kHz",23,0,0,"1T4R",1.8,"TDLC300-100",400,"2.03us ",-103,-103,null,null,null,null,null,null,-11.23,-9.23,-12.21,-9.7100000000000009,null,null,"-11,6","-9,2",0.98000000000000043,0.48000000000000043,-11.72,-9.4700000000000006]
["Format A2","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M15:Z15)","v":-103},{"$f":"IF(K15>-100,K15+0.3,K15)","v":-103},null,null,null,null,null,null,-17.350000000000001,-15.350000000000001,-15.51,-13.01,-17.96,-15.96,"-18,3","-16,0 ",{"$f":"MAX(M15,O15,Q15,S15,U15,W15,Y15)-MIN(M15,O15,Q15,S15,U15,W15,Y15)","v":2.4500000000000011},{"$f":"MAX(N15,P15,R15,T15,V15,X15,Z15)-MIN(N15,P15,R15,T15,V15,X15,Z15)","v":2.9500000000000011},{"$f":"AVERAGE(M15,O15,Q15,S15,U15,W15,Y15)","v":-16.940000000000001},{"$f":"AVERAGE(N15,P15,R15,T15,V15,X15,Z15)","v":-14.773333333333333}]
["Format A2","15kHz",23,0,0,"1T8R",1.8,"TDLC300-100",400,"2.03us ",-103,-103,null,null,null,null,null,null,-14.29,-12.29,-15.26,-12.76,null,null,"-15,2","-12,8 ",0.97000000000000064,0.47000000000000064,-14.774999999999999,-12.524999999999999]
["Format B4","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-18,-17.7,null,null,null,null,null,null,-20.260000000000002,-18.260000000000002,-19.22,-16.72,-21.12,-19.12,"-20,9","-18,6 ",1.9000000000000021,2.4000000000000021,-20.200000000000003,-18.033333333333335]
["Format B4","15kHz",23,0,0,"1T8R",1.8,"TDLC300-100 ",400,"2.03us ",-103,-103,null,null,null,null,null,null,-17.27,-15.27,-19.02,-16.52,null,null,"-17,1","-14,7 ",1.75,1.25,-18.145,-15.895]
["Format C2","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-103,-103,null,null,null,null,null,null,-17.329999999999998,-15.329999999999998,-15.5,-13,-17.89,-15.89,"-17,6","-15,5",2.3900000000000006,2.8900000000000006,-16.906666666666666,-14.74]
["Format C2","15kHz",23,0,0,"1T8R",1.8,"TDLC300-100",400,"2.03us ",-103,-103,null,null,null,null,null,null,-14.26,-12.26,-15.5,-13,null,null,"-15,3","-13,3",1.2400000000000002,0.74000000000000021,-14.879999999999999,-12.629999999999999]

{"sheet":"PRACH 30kHz SCS","index":8,"n_rows":20,"n_cols":30,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,22,0,23],[0,24,0,25],[0,26,0,27],[0,28,0,29],[0,11,1,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9]]}
["Format","SCS","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M3:Z3)","v":-11.2},{"$f":"IF(K3>-100,K3+0.3,K3)","v":-10.899999999999999},null,null,null,null,null,null,-13.19,-11.19,-13.54,-11.04,-13.42,-11.42,"-13,7","-11,2 ",{"$f":"MAX(M3,O3,Q3,S3,U3,W3,Y3)-MIN(M3,O3,Q3,S3,U3,W3,Y3)","v":0.34999999999999964},0.38000000000000078,{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3,Y3)","v":-13.383333333333333},-11.216666666666667]
["Format A2","30kHz",46,0,0,"1T2R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-7.03,-5.03,-7.55,-5.05,null,null,"-7,2","-4,7  ",0.51999999999999957,1.9999999999999574E-2,-7.29,-5.04]
["Format B4","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",-14.9,-14.6,null,null,null,null,null,null,-16.41,-14.41,-17.309999999999999,-14.809999999999999,-17.43,-15.43,"-16,4","-14,4 ",1.0199999999999996,1.0199999999999996,-17.05,-14.883333333333333]
["Format B4","30kHz",46,0,0,"1T2R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-10.09,-8.09,-11.21,-8.7100000000000009,null,null,"-8,7","-6,4  ",1.120000000000001,0.62000000000000099,-10.65,-8.4]
["Format C2","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",-11.3,-11,null,null,null,null,null,null,-13.19,-11.19,-13.55,-11.05,-13.66,-11.66,"-13,0","-10,5",0.47000000000000064,0.60999999999999943,-13.466666666666669,-11.300000000000002]
["Format C2","30kHz",46,0,0,"1T2R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-7.02,-5.0199999999999996,-7.46,-4.96,null,null,"-7,3","-4,8",0.44000000000000039,5.9999999999999609E-2,-7.24,-4.99]
["Format A2","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M9:Z9)","v":-13.4},{"$f":"IF(K9>-100,K9+0.3,K9)","v":-13.1},null,null,null,null,null,null,-15.25,-13.25,-15.68,-13.18,-15.76,-13.76,"-16,1","-13,9 ",{"$f":"MAX(M9,O9,Q9,S9,U9,W9,Y9)-MIN(M9,O9,Q9,S9,U9,W9,Y9)","v":0.50999999999999979},{"$f":"MAX(N9,P9,R9,T9,V9,X9,Z9)-MIN(N9,P9,R9,T9,V9,X9,Z9)","v":0.58000000000000007},{"$f":"AVERAGE(M9,O9,Q9,S9,U9,W9,Y9)","v":-15.563333333333333},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9,Z9)","v":-13.396666666666667}]
["Format A2","30kHz",46,0,0,"1T4R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-11.32,-9.32,-11.43,-8.93,null,null,"-11,4","-9,3  ",0.10999999999999943,0.39000000000000057,-11.375,-9.125]
["Format B4","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-16.899999999999999,-16.599999999999998,null,null,null,null,null,null,-18.329999999999998,-16.329999999999998,-19.260000000000002,-16.760000000000002,-19.510000000000002,-17.510000000000002,"-18,6","-16,1 ",1.1800000000000033,1.1800000000000033,-19.033333333333335,-16.866666666666671]
["Format B4","30kHz",46,0,0,"1T4R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-14.14,-12.14,-14.84,-12.34,null,null,"-12,4","-9,9  ",0.69999999999999929,0.19999999999999929,-14.49,-12.24]
["Format C2","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-13.4,-13.1,null,null,null,null,null,null,-15.25,-13.25,-15.7,-13.2,-15.87,-13.87,"-15,5","-13,5",0.61999999999999922,0.66999999999999993,-15.606666666666667,-13.44]
["Format C2","30kHz",46,0,0,"1T4R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-11.1,-9.1,-11.45,-8.9499999999999993,null,null,"-11,5","-9,0",0.34999999999999964,0.15000000000000036,-11.274999999999999,-9.0249999999999986]
["Format A2","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M15:Z15)","v":-15.4},{"$f":"IF(K15>-100,K15+0.3,K15)","v":-15.1},null,null,null,null,null,null,-17.27,-15.27,-17.43,-14.93,-17.86,-15.86,"-18,2","-15,8 ",{"$f":"MAX(M15,O15,Q15,S15,U15,W15,Y15)-MIN(M15,O15,Q15,S15,U15,W15,Y15)","v":0.58999999999999986},{"$f":"MAX(N15,P15,R15,T15,V15,X15,Z15)-MIN(N15,P15,R15,T15,V15,X15,Z15)","v":0.92999999999999972},{"$f":"AVERAGE(M15,O15,Q15,S15,U15,W15,Y15)","v":-17.52},{"$f":"AVERAGE(N15,P15,R15,T15,V15,X15,Z15)","v":-15.353333333333333}]
["Format A2","30kHz",46,0,0,"1T8R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-14.26,-12.26,-14.25,-11.75,null,null,"-14,4","-12,2 ",9.9999999999997868E-3,0.50999999999999979,-14.254999999999999,-12.004999999999999]
["Format B4","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-18.7,-18.399999999999999,null,null,null,null,null,null,-20.2,-18.2,-20.8,-18.3,-21.49,-19.489999999999998,"-20,8","-18,7 ",1.2899999999999991,1.2899999999999991,-20.83,-18.66333333333333]
["Format B4","30kHz",46,0,0,"1T8R",3.6,"TDLC300-100",400,"1.77us",-103,-103,null,null,null,null,null,null,-17.23,-15.23,-17.670000000000002,-15.170000000000002,null,null,"-15,3","-13,3 ",0.44000000000000128,5.9999999999998721E-2,-17.450000000000003,-15.200000000000001]
["Format C2","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-15.3,-15,null,null,null,null,null,null,-17.239999999999998,-15.239999999999998,-17.39,-14.89,-17.89,-15.89,"-17,6","-15,6",0.65000000000000213,1,-17.506666666666664,-15.339999999999998]
["Format C2","30kHz",46,0,0,"1T8R",3.6,"TDLC300-100 ",400,"1.77us",{"$f":"DerivingPerfReq(M20:Z20)","v":-103},{"$f":"IF(K20>-100,K20+0.3,K20)","v":-103},null,null,null,null,null,null,-14.32,-12.32,-14.29,-11.79,null,null,"-14,6","-12,2",{"$f":"MAX(M20,O20,Q20,S20,U20,W20,Y20)-MIN(M20,O20,Q20,S20,U20,W20,Y20)","v":3.0000000000001137E-2},{"$f":"MAX(N20,P20,R20,T20,V20,X20,Z20)-MIN(N20,P20,R20,T20,V20,X20,Z20)","v":0.53000000000000114},{"$f":"AVERAGE(M20,O20,Q20,S20,U20,W20,Y20)","v":-14.305},{"$f":"AVERAGE(N20,P20,R20,T20,V20,X20,Z20)","v":-12.055}]