**3GPP TSG-RAN WG4 Meeting # 97-e R4-201XXXX**

**Electronic Meeting, 2 – 13 Nov., 2020**

**Agenda item:** 7.9.2 and 7.9.3

**Source:** Moderator (Samsung)

**Title:** Email discussion summary for [97e][216] NR\_eMIMO\_RRM

**Document for:** Information

# Introduction

*Briefly introduce background, the scope of this email discussion and provide some guidelines for email discussion if necessary.*

Rel-16 NR eMIMO WI (i.e., Enhancements on MIMO for NR) is a RAN1 leading WI with below major enhancement in RAN1 area, in which the following items are identified for having RAN4 RRM requirement impact, based on previous RAN4 discussion:

* Enhancements on multi-beam operation
  + DL/UL beam indication with reduced latency and overhead
  + Beam failure recovery for SCell
  + L1-SINR measurement

In last RAN4 meeting (RAN#96e), main tasks within the RRM core work scope have completed. In the subsequent meetings, online discussion will focus on the eMIMO RRM performance requirement of the above aspects for Release-16.

*List of candidate target of email discussion for 1st round and 2nd round*

* 1st round: TBA
* 2nd round: TBA

As the rapporteur company for Rel-16 MIMO enhancement WI, we would like to suggest the following candidate target of 1st and 2nd round email discussion:

* 1st round: Collect more views on all topics and to get progress as much as possible:
* 2nd round: Based on results from 1st round, complete outstanding issues and reach the consensus for the WF.

# Topic #1: RRM Core Remaining Issues

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014244  Discussion on RRM requirements for Multi-TRP | Apple | **Proposal #1: Update in MRTD requirements for NR CA that UE may assume that all signals from all CCs and multi-TRxP will be received within CP in intra-band contiguous CA scenario.** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 1-1

***RRM core requirement maintenance: correction and clarification***

*Open issues and candidate options before e-meeting:*

**Issue 1-1-1: Clarification of multi-TRxP in MRTD requirements (section 7.6.4) for intra-band contiguous CA**

* Proposals (Apple): Update in MRTD requirements for NR CA that UE may assume that all signals from all CCs and multi-TRxP will be received within CP in intra-band contiguous CA scenario. (MediaTek)
* Recommended WF
  + Based on the 1st round discussion. Companies may discuss on the necessity and the wording.

**Issue 1-1-2: Update the definition of PBFD and PCBD in NR-DC case when** **both PCell and PScell configured**

* Proposals (Apple): Update the definition of PBFD and PCBD (section 8.5) for SSB based CBD, CSI-RS based BFD and CBD in NR-DC with SCell.
* Proposals: other solutions. (MediaTek)
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 1-1-3: Clarification of L1-SINR reporting with CSI-RS based CMR and dedicated IMR configured**

* Proposals (Ericsson): update clarification on M=1 case when at least one of the two signalling configured.( MediaTek)
* Recommended WF
  + Based on the 1st round discussion. Companies may discuss on the necessity.

**Issue 1-1-4: Clean up CR for RRM core requirement on L1-RSRP measurement procedure**

* Proposals (Samsung): Add the missing part for L1-RSRP measurement procedure which are previously agreed but missing due to ITU submission. (MediaTek)
* Recommended WF
  + Companies’ views are collected in 1st round discussion. Other corrections may be added.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | Sub topic 1-1:  Issue 1-1-1:  We agree with Apple’s proposal because it is clearer for reader to understand the MRTD applied to different scenarios, i.e., multi-TPxP.  Issue 1-1-2:  More discussion is needed. For Apple’s proposal, the same factor is applied to SCell and PSCell in NR-DC. In our understanding, PSCell is more important than SCell, thus the PSCell’s factor would be different with SCell’s.  Issue 1-1-3:  We agree with Ericsson’s proposal Issue 1-1-4:  We agree with Samsung’s proposal for clearer definition. |
| Nokia | Sub topic 1-1:  Issue 1-1-1:  The agreement captured in the RAN4 RRM chairman report is an assumption (not a requirement):  “UE may assume that all signals from multi-TRxPs of the same serving cell will be received within CP in intra-band contiguous CA scenario”  Thus, it is not necessary to capture such an assumption in the specification.  Issue 1-1-2:  Can you elaborate on why 1 is added to PBFD and PCBD?  Issue 1-1-3:  As the proposed changes in the CR (R4-2015826) alter the meaning of the original text, some clarifications are needed.  Issue 1-1-4  The proposal is OK. |
| **Qualcomm** | Issue 1-1-1:  Agreeable as Apple’s proposal captures the Chairman’s note.  Issue 1-1-2:  Can we pls clarify if the assumption is as below for NRDC?  1 searcher is reserved for PCELL; the other searcher is shared for PSCELL and all of the SCELLs? We agree with MTK if we shall favor PSCELL by equally sharing the searcher with all of the SCELLs. E.g PCBD for PSCELL is (1+numberofbands)/2 and PCBD for SCELLS is (1+numberofbands)/2?  Issue 1-1-3:  Agreeable, to clarify the conditions of M=1  Issue 1-1-4:  Agreeable |
| Apple | Sub topic 1-1:  Issue 1-1-1: We propose to capture the assumption in spec, otherwise its not clear, especially for intra-band contiguous CA where we don’t have MRTD requirement and the assumption with mTRP is not obvious.  Issue 1-1-2: [To Nokia] 1 is added because in NR-DC we have 1 PSCell and could have multiple SCells for BFD/CBD. The earlier scaling factor was just number of SCells, without accounting for PSCell. The assumption is searcher is shared between PSCell and SCells, hence 1+#bands for PScell and SCells for NR-DC.  [To MTK, QC] We have 1 for PCell and 1+PBFD for PScell and SCells assuming shared searcher between PSCell and SCells . If SCell is configured for BFD along with PScell, we are not sure we can prioritize one over the other.  Issue 1-1-3: We don’t see why ‘or’ should be changed to ‘and’. Suggest the following:  …at least one of the higher layer parameters *timeRestrictionForChannelMeasurement* or *timeRestrictionForInterferenceMeasurements* is configured, |
| Huawei | Issue 1-1-1:  The proposal seems different with the agreement captured in chairman notes.   * The agreements in chairman notes: UE may assume that all signals from multi-TRxPs of the same serving cell will be received within CP in intra-band contiguous CA scenarios. * The proposal: UE may assume that all signals from all CCs and multi-TRxP will be received within CP in intra-band contiguous CA scenario   This agreement only mentions that signals from same serving cell will be within CP. But the proposal restricts that signals from all CCs will be within CP.  RAN4 has discussed the impacts of multi-TRxP transmission on MRTD/MTTD requirements for several meeting cycles. It has been agreed in last meeting that no RRM core requirement impact is identified on MRTD/MTTD requirements, which has been captured in WF R4-2012146. It is RAN4 common understanding that MRTD/MTTD requirements in clauses 7.5.3, 7.6.3 and 7.6.4 is sufficient for support the deployment with multi-TRxP transmission. So, there is no need to add the clarification.  Issue 1-1-2:  In NR-DC, if the UE shares BFD/CBD measurement opportunities between PSCell and SCell, it means that the BFD/CBD measurement requirements on PSCell in Rel-16 will be degraded by compared with the requirements in Rel-15. That is the reason why the UE does not share BFD/CBD measurement opportunities between PSCell and SCell in NR-DC.  So, there is no need to update the definition of PBFD and PCBD.  Issue 1-1-3:  From my side, there is no misunderstanding based on the original wording. We need to focus on the technique issues.  Issue 1-1-4:  Agree with Samsung’s proposal. |
| Ericsson | Sub topic 1-1:  Issue 1-1-1:  As we concluded in RAN4#96-e, we don’t need any additional description in TS38.133.  TS38.133 7.6.4 specifies the relation between two carriers, but we think the existing MRTD requirement is applicable for CA with multi-antenna transmission including ‘multi-TRxP deployment’.  RAN1 agreed that all signals from transmission antennas in multi-TRP feature will be received within a CP, and this is same assumption as Rel-15 MIMO. This is the reason RAN1 does not introduce the terminology like ‘multi-TRxP deployment’ in TS38.21x.    Issue 1-1-3:  [To Apple] The relation between M and CMR/IMR measurement restriction configurations are given as follows:   |  |  |  |  | | --- | --- | --- | --- | |  |  | CMR measurement restriction  (timeRestrictionForChannelMeasurement) | | |  |  | Not configured | Configured | | IMR measurement restriction  (timeRestrictionForInterferenceMeasurements) | Not configured | MCMR=3, MIMR=3 | MCMR=1, MIMR=1 | | Configured | MCMR=1, MIMR=1 | MCMR=1, MIMR=1 |   Considering the table, we would like to revise texts as follows:  - M=1 shall be applied if  - aperiodic NZP-CSI-RS as CMR or dedicated IMR, or  - aperiodic CSI-IMR as dedicated IMR, or  - periodic and semi-persistent NZP-CSI-RS as CMR or dedicated IMR and ~~at least one of~~ higher layer parameters *timeRestrictionForChannelMeasurement* and/or *timeRestrictionForInterferenceMeasurements* is configured, or  - periodic and semi-persistent CSI-IM as dedicated IMR and ~~at least one of~~ higher layer parameters *timeRestrictionForChannelMeasurement* and/or *timeRestrictionForInterferenceMeasurements* is configured;  Issue 1-1-4:  We are fine with this proposal. |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014245  Apple | Company A |
| Company B |
|  |
| R4-2014246  Apple | Company A |
| Company B |
|  |
| R4-2015826  Ericsson | Ericsson: Would like to revise it according to the discussion. |
| R4-2016029 Samsung |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #2: eMIMO RRM Performance General

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014756  Discussion on RRM Performance part for Rel-16 NR eMIMO | Samsung | Proposal 1: RAN4 shall study on and complete Rel-16 eMIMO RRM performance part following the work scope in Table 1. |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 2-1

***Work scope of RRM performance requirement***

*Open issues and candidate options before e-meeting:*

**Issue 2-1-1: Work scope of RRM performance part**

* Proposals (Samsung): RAN4 shall study on and complete Rel-16 eMIMO RRM performance part following the work scope in the Table 1. (4756) (MediaTek)



* Recommended WF
  + Companies’ views are collected in 1st round discussion. Companies may discuss on the scope and the impact on the spec.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | Sub topic 2-1:  Issue 2-1-1:  Agree with Samsung’s proposal. |
| Nokia | The proposed work scope is OK. |
| Qualcomm | Recommended WF is agreeable. |
| Apple | We are fine with work plan. |
| Huawei | Issue 2-1-1:  Agree with Samsung’s proposal. |
| Ericsson | Support the moderator’s recommended WF. |

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| YYY | Company A |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #3: L1-SINR Measurement Accuracy

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014247  Simulation results for L1-SINR Measurement accuracy | Apple | **Proposal #1: Define measurement accuracy for CMR based L1-SINR based on results from single shot measurement.**  **Proposal #2: Define measurement accuracy requirement for CMR based L1-SINR measurement as ±5 dB in FR1 and ±6.5 dB in FR2.** |
| R4-2014297  Requirements for L1-SINR measurement accuracy | Qualcomm | **Observation 1: Table 1 shows the statistics of L1-SINR simulation results in different scenarios.**  **Observation 2: Simulation results show +- 1.5 dB accuracy for all CMR + IMR scenarios and roughly +- 3 dB accuracy for CMR only scenarios.**  **Observation 3: The implementation margin for L1-RSRP measurement accuracy in FR2 is 1.5 dB higher than that in FR1.**  **Proposal 1: RAN4 uses following table to define the estimation accuracy requirements of L1-SINR.**   |  |  |  | | --- | --- | --- | |  | **FR1** | **FR2** | | **CMR only** | **+- 5 dB** | **+- 6.5 dB** | | **CMR + IMR** | **+- 3.5 dB** | **+- 5 dB** | |
| R4-2014603  Discussion on L1-SINR measurement accuracy requirement | MediaTek | **Observation 1: For CMR only scenario, the L1-SINR measurement will become less inaccurate if either signal power is low (i.e. high SNR) or noise power is low (i.e. low SNR).**  **Proposal 1: For CMR only scenario, RAN4 need to evaluate L1-SINR accuracy requirement with side condition on Es/Iot = 25 dB, in addition to Es/Iot = -3 dB.**  **Proposal 2: For CMR only scenario L1- SINR for reporting, the absolute measurement accuracy is +/- 4.5 dB for FR1; +/- 4.5 dB for FR2 with side condition on CMR=-3dB.**  **Proposal 3: For SSB based CMR + NZP IMR L1-SINR for reporting, the absolute measurement accuracy is +/- 4 dB for FR1; +/- 4 dB for FR2 with side condition on CMR=-3dB and IMR=-3dB.**  **Proposal 4: For SSB based CMR + ZP-IMR L1-SINR for reporting, the absolute measurement accuracy is +/- 4 dB for FR1; +/- 4 dB for FR2 with side condition on CMR=-3dB and IMR=-3dB.**  **Proposal 5: For CSI-RS based CMR + NZP IMR L1- SINR for reporting, the absolute measurement accuracy is +/- 4 dB for FR1; +/- 4 dB for FR2 with side condition on CMR=-3dB and IMR=-3dB.**  **Proposal 6: For CSI-RS based CMR + ZP-IMR L1- SINR for reporting, the absolute measurement accuracy is +/- 4 dB for FR1; +/- 4 dB for FR2 with side condition on CMR=-3dB and IMR=-3dB.** |
| R4-2014758  Simulation results summary for L1-SINR measurement accuracy | Samsung | **Summary of all submitted simulation results from interested companies for information.**  **It will be shared with companies for reference and submitted after all results updated** |
| R4-2014759  Discussion on L1-SINR measurement accuracy requirement | Samsung | **Observation 1: Basically there are three levels of L1-SINR measurement accuracy for in total 5 scenarios: 1A, (2A, 2B), and (2C, 2D) respectively.**  **Observation 2: Very similar simulation results for L1-SINR measurement accuracy in both FR1 case and FR2 case.**  **Proposal 1: Under the normal condition, L1-SINR measurement accuracy is set to be +/-4.0dB for Scenario 1A; +/-3.5 dB for Scenario 2A and 2B; and +/-3.0dB for Scenario 2C and 2D.**  **Proposal 2: Under the extreme condition, L1-SINR measurement accuracy is set to be +/-5.0dB for Scenario 1A; +/-4.5 dB for Scenario 2A and 2B; and +/-4.0dB for Scenario 2C and 2D.**  **Proposal 3: Discuss on how to simplify the requirements scenarios/subsections in RAN4 for eMIMO performance part.** |
| R4-2015471  Discussion on L1-SINR measurement accuracy requirements | Huawei, HiSilicon | **Proposal 1: It is suggested to define L1-SINR accuracy requirements based on the single shot L1-SINR measurement performance.**  **Proposal 2: It is suggested to define the L1-SINR accuracy requirements based on following five generalizes scenarios:**   * + - **L1-SINR accuracy requirements with CSI-RS based CMR and no dedicated IMR configured**     - **L1-SINR accuracy requirements with SSB based CMR and dedicated ZP-IMR configured**     - **L1-SINR accuracy requirements with CSI-RS based CMR and dedicated NZP-IMR configured**     - **L1-SINR accuracy requirements with SSB based CMR and dedicated ZP-IMR configured**     - **L1-SINR accuracy requirements with CSI-RS based CMR and dedicated NZP-IMR configured**   **Proposal 3: For CMR only and CMR+ZP-IMR scenarios, the L1-SINR absolute accuracy requirements can be defined as +/-3.5dB under the side condition of CMR Es/Iot≥-3dB.**  **Proposal 4: For CMR only and CMR+ZP-IMR scenarios, the L1-SINR absolute accuracy requirements can be defined as +/-3.0dB under the side condition of CMR/IMR Es/Iot≥0dB.** |
| R4-2016239  Simulation results of L1-SINR measurement accuracy | Nokia, Nokia Shanghai Bell | **The document has presented the simulation results of L1-SINR measurement accuracy for CMR-only, SSB+NZP-IMR, SSB+ZP-IMR, CSI-RS+NZP-IMR and CSI-RS+ZP-IMR.** |
| R4-2015827  Simulation results of L1-SINR measurement accuracy | Ericsson | **Proposal 1: Derive L1-SINR measurement accuracy requirements based on the simulation results with M=1.**  **Proposal 2: After taking an average of companies simulation results, adopt the same methodology as L1-RSRP measurement accuracy to derive L1-SINR measurement accuracy requirements.** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 3-1

***Defining L1-SINR measurement accuracy requirement***

*Open issues and candidate options before e-meeting:*

**Issue 3-1-1: Methodology for defining the L1-SINR accuracy requirements**

* Proposals
  + Option 1: Reuse the same methodology of L1-RSRP requirement
  + Option 2: Refer to the methodology of L1-RSRP requirement (MediaTek)
* Recommended WF
  + Companies’ views are collected in 1st round discussion. The difference between defining absolute accuracy requirement and relative accuracy requirement could be discussed.

**Issue 3-1-2: Alignment of companies’ simulation result for L1-SINR accuracy requirement**

* Proposals: Companies could clarify their simulation results and try to align the results based on which the accuracy requirement could be defined.
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 3-1-3: Accuracy requirements of L1-SINR under normal condition**

* Proposals
  + Option 1: For Scenario 1A: ±5 dB in FR1 and ±6.5 dB in FR2; for CMR + IMR: ±3.5 dB in FR1 and ±5 dB in FR2
  + Option 2: For Scenario 1A: ±4.5 dB in FR1 and ±4.5 dB in FR2; for CMR + IMR: ±4 dB in FR1 and ±4 dB in FR2 (MediaTek)
  + Option 3: +/-4.0dB for Scenario 1A; +/-3.5 dB for Scenario 2A and 2B; and +/-3.0dB for Scenario 2C and 2D
  + Option 4: +/-3.5dB for Scenario 1A, 2A and 2B; and +/-3.0dB for Scenario 2C and 2D
* Recommended WF
  + Companies’ views are collected in 1st round discussion. Companies may support one of the options or propose their values in the comments.

**Issue 3-1-4: Difference of accuracy requirements of L1-SINR between FR1 and FR2**

* Proposals
  + Option 1: No obvious difference as it is SINR (MediaTek)
  + Option 2: Consider RF margin 1.5dB higher for FR2 than FR1
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 3-1-5: Accuracy requirements of L1-SINR under extreme condition**

* Proposals
  + Option 1: 1dB higher for extreme condition than normal condition
  + Option 2: Other values
    - Option 2a: 2dB higher for extreme condition than normal condition (MediaTek)
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

### Sub-topic 3-2

***Settings for L1-SINR measurement accuracy requirement***

*Open issues and candidate options before e-meeting:*

**Issue 3-2-1: Measurement samples for defining L1-SINR accuracy requirements**

* Proposals
  + Option 1: L1-SINR accuracy requirements is defined based on the single shot L1-SINR measurement performance, i.e. M = 1. (MediaTek)
  + Option 2: Other values.
* Recommended WF
  + Support M = 1, i.e. L1-SINR accuracy requirements is defined based on the single shot L1-SINR measurement performance.

**Issue 3-2-2: Side condition of Ês/Iot for accuracy requirement**

* Proposals
  + Option 1: -3dB for Scenario 1A, 2A and 2B; 0dB for Scenario 2C and 2D (MediaTek)
  + Option 2: -3dB for all scenarios
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 3-2-3: Io condition of dBm/BWChannel for accuracy requirement**

* Proposals
  + Option 1: Define accuracy requirement for “Max Io -50 dBm” only (MediaTek)
  + Option 2: Define accuracy requirement for “Max Io -70 dBm” and “Min Io -70 dBm + Max Io -50 dBm”
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

### Sub-topic 3-3

***Spec structure for L1-SINR measurement accuracy requirement***

*Open issues and candidate options before e-meeting:*

**Issue 3-3-1: Scenarios for L1-SINR measurement accuracy requirement in the spec**

* Proposals
  + Option 1: Each scenarios (1A, 2A, 2B, 2C, 2D) for one sub-section.
  + Option 2: Simplify the scenarios/subsections for accuracy requirement
    - Option 2a: Combine scenarios with the same requirement and side condition into one subsection ([1A], [2A, 2B], [2C, 2D]). (MediaTek)
    - Option 2b: other spec structures
* Recommended WF
  + Companies’ views are collected in 1st round discussion. Companies may propose their preference and the reason.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | Sub topic 3-1:  Issue 3-1-1:  We prefer to option-2. In option 1, the L1-RSRP measurement accuracy requirement for FR1 and FR2 are different because of RF margin. However, we do not need to consider the RF margin for L1-SINR measurement accuracy requirement in FR2 because the impact of RF modules will be cancelled while signal part divided by noise part.  Issue 3-1-2:  As we mentioned in Issue 3-1-1, for L1-SINR measurement, the impact of RF modules will be cancelled. Thus, the simulation results for FR1 and FR2 in CMR + IMR scenarios are similar.  Issue 3-1-3:  We suggest option-2. The L1-SINR measurement accuracy requirement for FR1 and FR2 shall be the same according to our discussion in Issue 3-1-1. In addition, we convert the simulated value into the nearest ceiling that is an integer multiple of 0.5 dB. Besides, an implementation margin of 2 dB is also added to each scenario.  Issue 3-1-4:  We suggest option 1 and the reason is provided in Issue 3-1-2.  Issue 3-1-5:  We prefer to option 2 and propose 2 dB higher for extreme condition than normal condition. Because, in L1-RSRP and SS-SINR measurement, the accuracy requirement under extreme condition is higher 2 dB and 1 dB than normal condition, respectively. Thus, consider the worst case between these two cases, we can take 2 dB for L1-SINR under extreme condition.Sub topic 3-2:  Issue 3-2-1:  We suggest option 1 because the worst case shall be considered while defining accuracy requirement.  Issue 3-2-2:  We suggest option 1 because we shall define the L1-SINR measurement accuracy based on the simulation assumption which the value of side condition is same as option 1.  Issue 3-2-3:  We slight prefer to option 1 because following the same logic as SS-SINR, the accuracy requirement is defined while Max Io is -50 dBm.  Sub topic 3-3:  Issue 3-3-1:  We slight prefer to option 2a for conciseness. |
| Nokia | Sub topic 3-1:  Issue 3-1-1:  Can you elaborate on what the differences between the two options? L1-SINR is not the same as L-RSRP. Once the differences are known, then it is possible to determine what can be reused from L1-RSRP. The approach for SS-SINR should also be taken into consideration as well.  Issue 3-1-2:  If our simulation results do not align with others shown by the span analysis, an attempt will be made to align our simulation results.  Issue 3-1-3:  This depends on the outcome of Issue 3-1-1 (i.e., the selected methodology used to compute L1-SINR accuracy).  Issue 3-1-4:  This depends on the outcome of Issue 3-1-1. For option 2, the RF margin of 1.5 dB is based on L1-RSRP?  Issue 3-1-5:  This can be further discussed.  Sub topic 3-2:  Issue 3-2-1:  It can adopt the same approach as L1-RSRP, i.e., M =1 (Option 1).  Issue 3-2-2:  Option 1 because the side condition is aligned with the agreed simulation assumptions.  Issue 3-2-3:  No strong preference. This depends on which methodology to use in Issue 3-1-1.  Sub topic 3-3:  Issue 3-3-1:  This can be discussed once other issues are resolved. Based on the structure in CR (R4-2016240), it is Option 1. |
| Qualcomm | **Issue 3-1-1: Methodology for defining the L1-SINR accuracy requirements**  Assume signal and noise are from the same source, the gain imperfection can be cancelled. However, if when the interference presents from a different Tx beam, it is subject to the gain accuracy issue still, which motivates us to adopt different implementation margins for FR1 and FR2.  **Issue 3-1-2: Alignment of companies’ simulation result for L1-SINR accuracy requirement**  We support different accuracy requirements for FR1 v.s FR2.  **Issue 3-1-3: Accuracy requirements of L1-SINR under normal condition**  Option1 is supported.  **Issue 3-1-4: Difference of accuracy requirements of L1-SINR between FR1 and FR2**  As we have established in Issue3-1-2 to allow 1.5dB higher margin in FR2  **Issue 3-1-5: Accuracy requirements of L1-SINR under extreme condition**  Option2 is supported.  **Issue 3-2-1: Measurement samples for defining L1-SINR accuracy requirements**  Option1 is supported for L1 measurement.  **Issue 3-2-2: Side condition of Ês/Iot for accuracy requirement**  Option1 is supported as the simulation results are derived assuming the same side conditions.  **Issue 3-2-3: Io condition of dBm/BWChannel for accuracy requirement**  Option1 is supported.  **Issue 3-3-1: Scenarios for L1-SINR measurement accuracy requirement in the spec**  Agree with Nokia that option1 is supported allowing each scenario can be tested. |
| Apple | Sub topic 3-1:  Issue 3-1-1: We are also not clear about the options. We can have only absolute measurement accuracy requirements for L1-SINR measurement.  Issue 3-1-3: We support option 1 with slight modification to have same reqt for FR1 and FR2. We understand that extra RF margin need not be added for SINR measurement.  Issue 3-1-4: Option 1.  Issue 3-1-5: Option 1.  Sub topic 3-2:  Issue 3-2-1: We support the recommended WF.  Issue 3-2-2: Option 1 is already agreed in simulation assumptions.  Issue 3-2-3: Needs further discussion  Sub topic 3-3:  Issue 3-3-1: We prefer option 2a in order to simplify spec. But the TC split is based on option 1. |
| Huawei | Issue 3-1-3:  We support option 4. The L1-SINR measurement accuracy is mainly related to the value of CMR Es/Iot, We suggest to define the same accuracy requirements for Scenario 1A/2A/2B, and define the same accuracy requirements for Scenario 2C/2D.  Issue 3-1-4:  We agree with option 1. RF margin does not need to be considered for L1-SINR measurement accuracy requirements.  Issue 3-2-1:  We can agree with the recommended WF.  Issue 3-2-2:  For scenario 2C/2D, the side conditions include CMR Ês/Iot and IMR Ês/Iot.  We support option 1A: CMR Ês/Iot = -3dB for Scenario 1A, 2A and 2B; CMR Ês/Iot = 0dB and IMR Ês/Iot = 0dB for Scenario 2C and 2D.  Issue 3-2-3:  We support option 1, since only “Max Io -50 dBm” is defined for SS-SINR in NR and RS-SINR in LTE.  Issue 3-3-1:  In order to align with the structure of core requirements, we can agree with   * Option 2b: [1A], [2A, 2C], [2B, 2D]   For each subsection with IMR is configured, the L1-SINR accuracy requirements with ZP-IMR and NZP-IMR will be separately defined by using separate Tables.  Option 2b will make the reference in core requirements become easier. |
| Ericsson | Sub-topic 3-1  Issue 3-1-1: What we need to decide is the additional margin for each scenario after the taking an average of companies simulation result. So we prefer option 1.  It is straightforward to reuse the same margin when we derived L1-RSRP (R4-1904820). But L1-SINR takes a ratio of power estimates and noise estimates, which is different from L1-RSRP as some company comments. We are open to apply the different margin from L1-RSRP if it is reasonable.    Issue 3-1-2: Our simulation results in R4-2015827 is ideal results. The parameters are listed in the same Tdoc. Set SNR so that the ideal SINR becomes -3dB.  Issue 3-1-3: It depends on the conclusion of 3-1-1.  Issue 3-1-4: L1-RSRP considered RF margin 1.5dB higher for FR2 than FR1 because FR2 cannot compensate the RF impairments. If it is same for L1-SINR, we support option 2. If not, we support option 1. We need more inputs.  Issue 3-1-5: Option 1. In LTE, RS-SINR in extreme condition set 1dB higher than that in normal condition. We can keep the same value.  Sub-topic 3-2  Issue 3-2-1: Support the moderator’s recommended WF, that is M=1.  Issue 3-2-2: Option 1. Set the side condition so that the ideal SINR becomes -3dB.  Issue 3-2-3: Option 2. Try to use the same requirements as L1-RSRP.  Sub-topic 3-3  Issue 3-3-1: Need clarification of proposal. We want to define clauses:   * L1-SINR accuracy requirements with CSI-RS based CMR and no dedicated IMR configured, * L1-SINR accuracy requirements with SSB based CMR and dedicated IMR configured,   + Including NZP-IMR and ZP-IMR * L1-SINR accuracy requirements with CSI-RS based CMR and dedicated IMR configured,   + Including NZP-IMR and ZP-IMR   This is aligned with core requirements in 9.8.4. |
| CMCC | **Issue 3-1-3: Accuracy requirements of L1-SINR under normal condition**  For option 1 and option 2, we have one question for clarification. Does CMR+IMR in these two options includes both CMR+ZP\_IMR and CMR + NZP\_IMR? Measurement accuracy is related to the side condition. Since the side condition is different for scenario2A/2B and scenario2C/2D (also related to Issue 3-2-2), we are wondering why the same accuracy requirements are suggested for CMR+ZP\_IMR and CMR + NZP\_IMR?  **Issue 3-1-4: Difference of accuracy requirements of L1-SINR between FR1 and FR2**  Support Option 1. We also check with SS-SINR, there is no difference between FR1 and FR2, same approach can be used for L1-SINR. |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2016240  Nokia, Nokia Shanghai Bell | Company A |
| Company B |
|  |
|  | Company A |
| Company B |
|  |
|  |  |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #4: Test Case for L1-SINR Measurement

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014604  Discussion on test cases for L1-SINR measurement | MediaTek | **Observation 1: In current TS 38.133 specification, the CSI-RS resources set are configured with “repetition=OFF” in all L1-RSRP measurement test case.**  **Proposal 1: For procedure and performance requirement, to define the NZP CSI-RS based L1-SINR measurement test case as NZP CSI-RS with “repetition=OFF” rather than “repetition=ON”.**  **Proposal 2: Regarding the L1-SINR measurement procedure, to define the test case with NZP CSI-RS as IMR rather than with CSI-IM as IMR.**  **Proposal 3: For CMR only scenario, no need to define the test case for the measurement procedure** |
| R4-2015472  Discussion on L1-SINR measurement tests for NR eMIMO | Huawei, HiSilicon | **Proposal 1: It is suggested to define 5 L1-RSRP measurement test cases in sections A.4.6, A.4.7, A.5.6, A.5.7, A.6.6, A.6.7, A.7.6 and A.7.7. And the structure of L1-RSRP measurement test cases could be defined as follows: see the table in R4-2015472.**  **Proposal 2: The L1-RSRP measurement test setups are proposed as Table 2.**  **Proposal 3: CSI-IM configurations and one type of aperiodic CSI-RS configuration with repetition=off need to be introduced as IMR.** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 4-1

***Spec structure for L1-SINR measurement procedure test cases***

*Open issues and candidate options before e-meeting:*

**Issue 4-1-1: Scenarios defined for L1-SINR measurement procedure test cases in the spec**

* Proposals
  + Option 1: All scenarios are defined follow the same methodology as L1-RSRP, i.e. (5 scenarios x 2 FR x 2 DRX)
  + Option 2: Simplify the test scenarios defined for the test
    - Option 2a: Each scenario (1A, 2A, 2B, 2C, 2D) corresponding to either DRX and non-DRX
    - Option 2b: Define the test case with NZP-CSI-RS as IMR for dedicated IMR scenario and not to define the tests with CSI-IM as IMR.
    - Option 2c: For dedicated IMR scenario, only define (non-DRX x CSI-IM IMR) and (DRX x CSI-RS IMR) test case (MediaTek)
    - Option 2d: other solutions
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 4-1-2: Whether to define test cases for CMR only scenario**

* Proposals
  + Option 1: Define test cases for CMR only scenario
  + Option 2: Do not define test cases for CMR only scenario (MediaTek)
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

### Sub-topic 4-2

***Settings for L1-SINR measurement procedure test cases***

*Open issues and candidate options before e-meeting:*

**Issue 4-2-1: Repetition configuration for NZP-CSI-RS based L1-SINR measurement test case**

* Proposals
  + Option 1: Repetition = off (MediaTek)
* Recommended WF
  + Support Repetition = off for all cases in L1-SINR measurement test case.

**Issue 4-2-2: IMR configuration for L1-SINR measurement test case**

* Proposals
  + Option 1: CSI-IM configurations and one type of aperiodic CSI-RS configuration with repetition=off need to be introduced in 38.133 Annex A (MediaTek)
  + Option 2: Other solutions
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | Sub topic 4-1:  Issue 4-1-1:  We tend to agree with option 2c because it is with the minimum number of test cases, while it select on DRX and on IMR type for each scenario.  Issue 4-1-2:  We suggest option 2, because, the UE’s behavior of CMR ouly are very similar to L1-RSRP, regarding the measurement procedure test case.  Sub topic 4-2:  Issue 4-2-1:  We suggest option 1. Following the same logic as L1-RSRP test case, for L1-SINR measurement, the procedure (delay) test case may be defined while NZP-CSI-RS is only configured with “repetition=OFF”.  Issue 4-2-2  We suggest option 1, where CSI-IM could be used for accuracy test. |
| Nokia | Sub topic 4-1:  Issue 4-1-1:  Option 2 is used to further down select suitable test cases in which L1-RSRP methodology can be used.  Issue 4-1-2:  This depends on the outcome of Issue 4-1-1.  Sub topic 4-2:  Issue 4-2-1:  There is only one option outlined. Should there be another option? |
| Qualcomm | **Issue 4-1-1: Scenarios defined for L1-SINR measurement procedure test cases in the spec**  Option2 in general could be supported for avoiding many test cases.  **Issue 4-1-2: Whether to define test cases for CMR only scenario**  We support option1, as it reflects one category of scenarios which was discussed to support by RAN4.  **Issue 4-2-1: Repetition configuration for NZP-CSI-RS based L1-SINR measurement test case**  Recommended WF can be agreed.  **Issue 4-2-2: IMR configuration for L1-SINR measurement test case**  Recommended WF can be agreed to introduce IMR configuration for RMC. |
| Apple | Sub topic 4-1:  Issue 4-1-1: We prefer option 2 to reduce number of testcases. Option 2c significantly reduces testcases.  Issue 4-1-2: We support option 2 to reduce testcases. Also, CMR only L1-SINR is similar to L1-RSRP.  Sub topic 4-2:  Issue 4-2-1: We are fine with the recommended WF.  Issue 4-2-2: We are fine with adding config that’s needed for the agreed testcases. |
| Huawei | Issue 4-1-1: We support option 2a and option 2d   * Option 2d: define test for CSI-RS CMR only in non-DRX, SSB CMR+CSI-IM IMR in non-DRX and CSI-RS CMR+CSI-RS IMR in DRX   Issue 4-1-2: Support option 1.  Issue 4-2-1: We can agree with the recommended WF.  Issue 4-2-2: Depend on the discussion on issue 4-1-1. But IMR configuration is needed. |
| Ericsson | Sub-topic 4-1  Issue 4-1-1: Option 2. We are ok to reduce the number of test cases in general, but we need to cover all the scenarios (1A, 2A, 2B, 2C, 2D). We need discuss how to reduce the number of test cases.  Issue 4-1-2: Option 1. CMR-only L1-SINR is similar to L1-RSRP, but not the same.  Sub-topic 4-2  Issue 4-2-1: Support the moderator’s recommended WF.  Issue 4-2-2: Support option 1. |
| CMCC | **Issue 4-1-1: Scenarios defined for L1-SINR measurement procedure test cases in the spec**  Our preference is option 1, but we also understand companies’ concern on the number of test cases. We can consider option 2 to move forward, but we are not OK to only test partial scenarios, in our view, all 5 scenarios need to be tested, and we are open not to duplicate each scenario just for DRX and non-DRX.  **Issue 4-1-2: Whether to define test cases for CMR only scenario**  Option 1 |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014291  Qualcomm | Company A |
| Company B |
|  |
| R4-2014757  Samsung | Company A |
| Company B |
|  |
| R4-2015473  Huawei, HiSilicon |  |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014292  Qualcomm | Company A |
| Company B |
|  |
| R4-2015474  Huawei, HiSilicon | Company A |
| Company B |
|  |
|  |  |
|  |  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #5: Test Case for Scell Beam Failure Recovery

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014605  Discussion on test cases for SCell BFR | MediaTek | **Observation 1: Only consider the periodic CSI-RS as BFD-RSs for SCell BFR in test case.**  **Proposal 1: To configure CSI-RS resources as CBD-RSs in FR2**  **Proposal 2: To introduce test cases for Beam Failure Detection and Link Recovery with the following cases:**  **• FR1 SCell configured with CSI-RS based BFD and SSB-based CBD in non-DRX mode**  **• FR2 SCell configured with CSI-RS based BFD and CSI-RS-based CBD in non-DRX mode**  **• FR1 SCell configured with CSI-RS based BFD and SSB-based CBD in DRX mode**  **• FR2 SCell configured with CSI-RS based BFD and CSI-RS-based CBD in DRX mode**  **Observation 2: The test for “BFD and link recovery procedure” and “Link Recovery with Link Recovery Request (LRR)” are ending up with performing random access procedure and PUCCH transmission, respectively.**  **Proposal 3: To check the PRACH transmission as the test requirement in test case “BFD and link recovery procedure”** |
| R4-2015828  Link recovery test with link recovery requests | Ericsson | **Proposal 1: RAN4 defines two test cases for link recovery in SCell.**  **• Scenario 1: Network does not configure PUCCH for SR for BFR MAC CE**  **• Scenario 2: Network configures PUCCH for SR for BFR MAC CE**  **Proposal 2: Test setup of two scenarios, e.g., time duration, q0/q1 configuration, are common for both scenarios.**  **Proposal 3: Scenario 1 does not configure PUCCH as same as the existing BFR tests on PCell/PSCell, although Scenario 2 configures PUCCH for SR for BFR MAC CE. It verifies UE transmits RACH for SR, followed by BFR MAC CE containing a beam associated with the candidate beam set q1.**  **Proposal 4: Scenario 2 verifies UE transmits PUCCH with an LRR, followed by BFR MAC CE containing a beam associated with the candidate beam set q1.** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 5-1

***Spec structure for Scell Beam Failure Recovery test cases***

*Open issues and candidate options before e-meeting:*

**Issue 5-1-1: Scenarios defined for Beam Failure Recovery test cases**

* Proposals
  + Option 1: (MediaTek)
    - Scenario 1: Network does not configure PUCCH for SR for BFR MAC CE
    - Scenario 2: Network configures PUCCH for SR for BFR MAC CE
  + Option 2: Other solutions
* Recommended WF
  + Companies’ views are collected in 1st round discussion. Also the subsection titles for the test should be defined.

**Issue 5-1-2: The setting of cases to be defined for each scenario**

* Proposals
  + Option 1: Define setting combination for each scenario as table below (MediaTek)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Mode** | **BFD-RSs** | **DRX** | **FR** | **CBD-RSs** |
| ED-DC / Standalone (SA) | CSI-RS | non-DRX | FR1 | SSB |
| FR2 | CSI-RS |
| DRX  (40 ms for FR1 and  640 ms for FR2) | FR1 | SSB |
| FR2 | CSI-RS |

* + Option 2: Other combinations
* Recommended WF
  + Companies’ views are collected in 1st round discussion. Maintain the necessary cases and try to reduce the total number.

### Sub-topic 5-2

***Defining Scell Beam Failure Recovery test cases***

*Open issues and candidate options before e-meeting:*

**Issue 5-2-1: Configuration for Beam Failure Recovery test cases**

* Proposals
  + Option 1: Reuse the same test parameters for both scenarios with the same setting (MediaTek)
  + Option 2: Other solutions
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 5-2-2: UE behaviour of BFR for the scenario dedicated PUCCH is not configured**

* Proposals
  + Option 1: UE shall transmit preamble on a beam associated with the candidate beam set q1. (MediaTek)
  + Option 2: UE shall transmit preamble on a beam followed by BFR MAC CE containing a beam associated with the candidate beam set q1.
* Recommended WF
  + Companies’ views are collected in 1st round discussion. This is a somewhat new requirement, UE behaviour should be clarify in the test.

**Issue 5-2-3: UE behaviour of BFR for the scenario dedicated PUCCH is configured**

* Proposals
  + Option 1: UE shall transmit PUCCH with LRR, followed by BFR MAC CE containing a beam associated with the candidate beam set q1.
  + Option 2: Test case only include PUCCH transmission (MediaTek)
* Recommended WF
  + Companies’ views are collected in 1st round discussion. This is a somewhat new requirement, UE behaviour should be clarify in the test.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | Sub topic 5-1:  Issue 5-1-1:  We agree with option 1. In our understanding, the last procedure in SCell BFR test case will depend on whether *schedulingRequestID-BFR-SCell-r16* is configured, i.e. PUCCH for SR for BFR MAC CE is configured or not.   * Scenario 1: Network does not configure PUCCH for SR for BFR MAC CE   According to clause 5.4.4 in TS 38.321 as follows, the random access procedure will be triggered while there is no PUCCH resource, i.e., UE is not provided by *schedulingRequestID-BFR-SCell-r16*.   |  | | --- | | As long as at least one SR is pending, the MAC entity shall for each pending SR:  1>if the MAC entity has no valid PUCCH resource configured for the pending SR:  2>initiate a Random Access procedure (see clause 5.1) on the SpCell and cancel the pending SR. |  * Scenario 2: Network configures PUCCH for SR for BFR MAC CE   According to TS38.213 as follows, the PUCCH transmission will be triggered while UE has PUCCH resource, i.e., UE is provided by *schedulingRequestID-BFR-SCell-r16*.   |  | | --- | | A UE can be provided, by *schedulingRequestID-BFR-SCell-r16*, a configuration for PUCCH transmission with a link recovery request (LRR) as described in Clause 9.2.4. The UE can transmit in a first PUSCH MAC CE providing index(es) for at least corresponding SCell(s) with radio link quality worse than Qout,LR, indication(s) of presence ofqnew for corresponding SCell(s), and index(es)qnew for a periodic CSI-RS configuration or for a SS/PBCH block provided by higher layers, as described in [11, TS 38.321], if any, for corresponding SCell(s). |   Issue 5-1-2:  We suggest option 1. In order to reduce the testing time, the CSI-RS based CBD-RSs are configured in FR2 because the periodicity of CSI-RS resource is short than SSB.  Sub topic 5-2:  Issue 5-2-1:  We suggest option 1 to reuse the same parameter, e.g. the setting of BFD-RSs or CBD-RSs, for both scenario because the difference between these two scenarios is the last procedure in test case only.  Issue 5-2-2:  We agree with option 1 and disagree with option 2 because following the same logic as the existing RLM test case, the test case for scenario 1 shall be ended up with random access procedure.  Issue 5-2-3:  We disagree with option 1. RAN4 only has agreed that to specify requirements of “step 1 of BFRQ” for the PUCCH transmission, but it was not agreed to introduce the requirement of “step 2 of BFRQ” for PUSCH transmission. Thus, we think PUSCH transmission procedure should not be included in this test.  Agreement:   |  | | --- | | Necessity of Requirement of Step-1 of BFRQ on SCell  RAN4 should define the requirement of PUCCH-based link recovery request (LLR), in which UE reports beam failure event through a dedicated SR like PUCCH resources. | |
| Qualcomm | **Issue 5-1-1: Scenarios defined for Beam Failure Recovery test cases**  Since the core requirement doesnot specify scenario1, we can focus on defining test case for scenario2.  **Issue 5-1-2: The setting of cases to be defined for each scenario**  Recommended WF is agreeable.  **Issue 5-2-1: Configuration for Beam Failure Recovery test cases**  This depends on the agreement in issue 5-1-1 because we may not need to test the scenario 1.  **Issue 5-2-2: UE behaviour of BFR for the scenario dedicated PUCCH is not configured**  This depends on the agreement in issue 5-1-1 because we may not need to test the scenario 1.  **Issue 5-2-3: UE behaviour of BFR for the scenario dedicated PUCCH is configured**  Option1 is supported in line with RAN4 agreement as MTK suggested. |
| Ericsson | Sub-topic 5-1  Issue 5-1-1: Support Option 1  Issue 5-1-2: Support Option 1  Sub-topic 5-2  Issue 5-2-1: Support Option 1  Issue 5-2-2: Support Option 1  Issue 5-2-3: Support Option 1. We think Rel-15 BFR tests verify UE reports the found beam index by checking the used PRACH preamble associated to q1. For BFR on Scell, it is also important to verify UE reports the found beam index in MAC CE. |
| Apple | Issue 5-1-1: Option 1/ Scenario 2 The core requirement is defined for Scenario 2, hence test case should be for that. It is unclear why Scenario 1 is discussed. Same view as QC.  Issue 5-1-2: We are fine with recommended WF.  Issue 5-2-1/2: We prefer to define test only for scenario 2. Depends on Issue 5-1-1  Issue 5-2-3: Option 1. We have core requirement for transmission of PUCCH. But BFR MAC-CE with candidate beam can also be tested. |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014606  MediaTek | Company A |
| Company B |
|  |
| R4-2015829  Ericsson | Company A |
| Company B |
|  |
|  |  |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #6: Test Case for Pathloss RS Activation Delay

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014010  Test cases for applicable timing for PL RS activated by MAC-CE | ZTE | **Proposal 1: Test cases for MAC-CE based pathloss RS activation delay shall be defined in TS 38.133.**  **Proposal 2: Endorse draft CR [4]. (R4-2014011)**  **Proposal 3: Define test cases for both FR1 and FR2.** |
|  |  |  |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 6-1

***Defining Pathloss RS Activation Delay Test Case***

*Open issues and candidate options before e-meeting:*

**Issue 6-1-1: Whether to define the test case for MAC-CE based pathloss RS activation delay**

* Proposals
  + Option 1: Define the test case
  + Option 2: Do not define the test case
* Recommended WF
  + Companies’ views are collected in 1st round discussion.

**Issue 6-1-2: How to define the test case for MAC-CE based pathloss RS activation delay**

* Proposals:
  + Option 1: Reflect the RS change by the power headroom report (PHR) from the UE
  + Option 2: Other test methods
* Recommended WF
  + Companies’ views are collected in 1st round discussion. RAN4 could discuss on testability and test method first.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Issue 6-1-1: Option 1. We have the core requirements defined and we need test cases in correspondance. In our view whether we need test cases or not is not a question, we can discuss Issue 6-1-2 directly on how to define such tests.  Issue 6-1-2: Option 1. We have prepared a draft CR to show how to do this through triggering a PHR and we consider this as a simple and straightforward way. |
| MediaTek | Sub topic 6-1:  More discussion is needed.  In ZTE’s TDoc, two methods are provided to discuss the feasibility of PL-RS test case.   * Method 1:let the test equipment (TE) monitor the transmission power of the UE before and after the delay defined in core part * Method 2: UE transmit the power headroom report (PHR) to reflect the change of uplink power.   For method 1, we are not clear the uncertainty on TE receive power measurement, i.e., UE uplink power. Thus, RAN4 need to further study on this method if we agree to define the test case based on method 1.  For method 2, it may be a feasible method for PL-RS test case but we would like to hear other companies view.  Issue 6-1-2:  Wait for the conclusion of Issue 6-1-1. |
| Qualcomm | **Issue 6-1-1: Whether to define the test case for MAC-CE based pathloss RS activation delay**  It is worth further discussing whether PHR based approach can be employed.  **Issue 6-1-2: How to define the test case for MAC-CE based pathloss RS activation delay**  For method2, in R4-2014011,   1. “The UE shall track SSB #1”, does it mean the TCI state has switched from SSB#0 to SSB#1? Or it just means UE detects and measures the SSB#1 with better RSRP? If the latter, we suggest TE to transmit a MAC CE based TCI switch (SSB0🡪SSB1) together with the MAC-CE activation of PL RS for coherence. 2. SSB#0 and SSB#1 shall have larger power difference due to FR1/FR2 relative accuracy |
| Apple | Sub topic 6-1:  Issue 6-1-1: Option 2 – do not define test case for MAC CE based pathloss RX activation delay. This was agreement in previous meetings.  We need more time to understand the suggested PHR based method.  **Update**  [To ZTE] To clarify earlier comments. After I checked that agreement was not to define requirements if testability was an issue, I meant to delete the first comment that we had previous agreement not to define testcase for this. We need some time to understand the proposed method and would suggest defining test case as FFS for now. |
| Huawei | Issue 6-1-1:  Support option 1.  The uplink transmission power is determined by several factors, as defined:    The pathloss-RS activation only will impact the downlink pathloss estimation . How to set the other parameters to implement different power headroom report for two pathloss-RS will be very complicated. Besides, the RSRP measurement inaccuracy on pathloss-RS shall also be considered. Method 2 seems not quite feasible for testing. |
| ZTE | Issue 6-1-1:  A question to Apple: I didn’t find any agreement from the last meeting saying that we wouldn’t define test cases, did I miss anything?  Our suggestion is to agree that we need such test cases, and then study the details of the proposed PHR approach. |
| Ericsson | Issue 6-1-1:  It depends on the testability. If it is testable, it is good to test the requirements. Need to wait for the conclusion of Issue 6-2-2.  Issue 6-1-2:  We need more time to check the feasibility of the suggested PHR based method. |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
|  |  |
|  |
|  |
|  |  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014011  ZTE | Company A |
| Company B |
|  |
|  |  |
|  |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |