**3GPP TSG-RAN WG4 Meeting # 97-e R4-20XXXXX**

**Electronic Meeting, Nov 2 – 13, 2020**

**Agenda item:** 7.11.2, 7.11.3

**Source:** Moderator (Huawei, HiSilicon)

**Title:** Email discussion summary for [97e][217] NR\_RF\_FR1\_RRM

**Document for:** Information

# Introduction

This email thread discusses the RRM core part/ performance part for Tx switching between two uplink carriers in agenda 7.11.2/3.

List of candidate target of email discussion for 1st round and 2nd round:

* 1st round: Invite companies to review the recommended WF in each sub-topic, and provide comments.
* 2nd round: TBA

# Topic #1: Core part

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014505 | China Telecom | (for TS 38.133)  Indicate that for some EN-DC and UL CA configurations, DL interruption is not allowed. |
| R4-2014506 | China Telecom | (for TS 36.133)  Indicate that for some EN-DC and UL CA configurations, DL interruption is not allowed. |
| R4-2015488 | Huawei, HiSilicon | 1. Correct the reference section of TS 38.214;  2. The interruption length on 120Khz victim cell in NR SA for 210us uplink switching period shall be 14. |

## Open issues summary

N/A

## Companies views’ collection for 1st round

### Open issues

N/A

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014505  (China Telecom) | MTK: OK |
| Huawei: ok |
|  |
| R4-2014506  (China Telecom) | MTK: OK |
| Huawei: ok |
|  |
| R4-2015488  (Huawei, HiSilicon) | MTK: OK |
| China Telecom: OK |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #2: Test case

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014503 | China Telecom | Proposal: To verify the symbol-level DL interruption in test:   * Interruption location happens from symbol #[14-(Interruption length+2)] to the end of last GP symbol assuming 2 symbols for SRS transmission in special slot. * Not consider MRTD in the test. * Two options can be considered for PDCCH/PDSCH scheduling in the special slot:   + Option 1: PDCCH is scheduled on the symbol right before the DL interruption   + Option 2: PDCCH is scheduled in the first OFDM symbol, and PDSCH with mapping type A is scheduled from the second OFDM symbol to the symbol right before the DL interruption. |
| R4-2014504 | China Telecom | Define test case for DL interruptions at UE switching between NR uplink carrier 1 and NR uplink carrier 2 in FDD+TDD inter-band uplink CA case. |
| R4-2014733 | CMCC | Proposal : The test case for TX switching between NR carrier #1(TDD 30kHz) and NR carrier#2 (TDD 30kHz) in SA scenario:  - Carrier#1 TDD UL/DL pattern is 3D1S4U, S = 10DL: 2GP: 2UL;  - Carrier#2 TDD UL/DL pattern is 1D1S2U, S = 10DL: 2GP: 2UL;  - SRS configuration:   * resourceMappingstartPosition: 0 * resourceMappingnrofSymbols: n2   - Tx switching between carrier 1 and carrier 2 happens immediately before SRS transmission in special slot   * DL interruption length shall not exceed the value defined in Table 8.2.2.2.10-1 depending on UE capability * The test verifies whether UE correctly receive the PDCCH scheduled on the symbol which is right before the DL interruption in special slot on carrier#1 amd 2nd special slot of every 8 slots on carrier#2, so that it sends ACK/NACK correctly. * No MRTD is set in the test. * The test case is only applicable to UE which supports pdcch-MonitoringAnyOccasions or pdcch-MonitoringAnyOccasionsWithSpanGap. |
| R4-2014734 | CMCC | Define test case for DL interruptions at UE switching between NR uplink carrier 1 and NR uplink carrier 2 in TDD+TDD inter-band uplink CA case. |
| R4-2015486 | Huawei, HiSilicon | Proposal 1: The test case for TX switching between NR carrier #1(FDD 15kHz) and NR carrier#2 (TDD 30kHz) in SA scenario:  - Carrier#2 TDD UL/DL pattern is 3D1S4U, S = 6DL: 4GP: 4UL;  - SRS configuration:   * resourceMappingstartPosition: 0 * resourceMappingnrofSymbols: n2   - Tx switching between carrier 1 and carrier 2 happens immediately before SRS transmission in special slot   * DL interruption length shall not exceed the value defined in Table 8.2.2.2.10-1 depending on UE capability * The test verifies whether UE correctly receive the PDCCH scheduled on the symbol which is right before the DL interruption in slot#1 on carrier#1, so that it sends ACK/NACK correctly. * No MRTD is set in the test. * The test case is only applicable to UE which supports pdcch-MonitoringAnyOccasions or pdcch-MonitoringAnyOccasionsWithSpanGap.   Proposal 2: Test case for DL Interruptions at UE switching between LTE 1Tx carrier and NR 2Tx carrier in inter-band ENDC can refer to NR SA test case, except:  - Carrier#2 TDD UL/DL pattern is 3D1S4U, S = 10DL: 2GP: 2UL;   * The test verifies whether UE correctly receive the PDCCH scheduled on the symbol which is right before the DL interruption in special slot on carrier#2, so that it sends ACK/NACK correctly. |
| R4-2015487 | Huawei, HiSilicon | Define test case for DL Interruptions at UE switching between LTE 1Tx carrier and NR 2Tx carrier in inter-band ENDC. |

## Open issues summary

### Sub-topic 2-1: Principle and general parameters for test case

**Issue 2-1-1: How to verify the symbol-level DL interruption in test**

* Proposals
  + Option 1(Huawei, CMCC): PDCCH is scheduled on the symbol right before the DL interruption. UE supports *pdcch-MonitoringAnyOccasions* or *pdcch*-*MonitoringAnyOccasionsWithSpanGap*.
  + Option 2(China Telecom): PDCCH is scheduled in the first OFDM symbol, and PDSCH with mapping type A is scheduled from the second OFDM symbol to the symbol right before the DL interruption.
* Recommended WF
  + Further discussion

**Issue 2-1-2: Whether MRTD is considered in test cases**

* Proposals
  + Option 1(China Telecom, CMCC, Huawei): No
* Recommended WF
  + No MRTD is set in the test.

**Issue 2-1-3: SRS configuration in the special slot**

* Proposals
  + Option 1(Huawei, China Telecom, CMCC): SRS configuration refers to SRSConf.1 in Table A.4.4.1.1.1-3 in TS 38.133 except that:

• resourceMappingstartPosition: 0

• resourceMappingnrofSymbols: n2

* Recommended WF
  + SRS configuration refers to SRSConf.1 in Table A.4.4.1.1.1-3 in TS 38.133 except that:

• resourceMappingstartPosition: 0

• resourceMappingnrofSymbols: n2


### Sub-topic 2-2: Specific parameters for DL Interruptions at UE switching between LTE 1Tx carrier and NR 2Tx carrier in inter-band ENDC

**Issue 2-2-1: TDD configuration**

* Proposals
  + Option 1 (Huawei): Carrier#2 TDD UL/DL pattern is 3D1S4U, S = 10DL: 2GP: 2UL
* Recommended WF
  + Is option 1 agreeable?

**Issue 2-2-2: Which symbol to be verified?**

* Proposals
  + Option 1:
    - symbol #4 or symbol#5 or symbol #8 on the special slot on NR TDD carrier depending on UE capability *uplinkTxSwitchingPeriod*
    - symbol level DL interruption can’t be verified in LTE



* Recommended WF
  + Is option 1 agreeable?

### Sub-topic 2-3: Specific parameters for DL interruptions at switching between two uplink carriers in FDD-TDD CA (SA)

**Issue 2-3-1: TDD configuration**

* Proposals
  + Option 1 (China Telecom): Carrier#2 TDD UL/DL pattern is 3D1S4U, S = 10DL: 2GP: 2UL
* Recommended WF
  + Is option 1 agreeable?

**Issue 2-3-2: Which symbol to be verified?**

* Proposals
  + Option 1(China Telecom):
    - For NR FDD carrier (Cell 1), this test verifies that the UE correctly receive the PDCCH scheduled on the symbol #8 or symbol #9 or symbol #10 in the second slot of every 4 slots (i.e., the slot overlapping with the special slot of the NR TDD carrier) depending on UE capability *uplinkTxSwitchingPeriod*
    - For NR TDD carrier (Cell 2), this test verifies that the UE correctly receive the PDCCH scheduled on the symbol #4 or symbol #5 or symbol #8 on the special slot depending on UE capability *uplinkTxSwitchingPeriod*
* Recommended WF
  + Is option 1 agreeable?

### Sub-topic 2-4: Specific parameters for DL interruptions at switching between two uplink carriers in TDD-TDD CA (SA)

**Issue 2-4-1: TDD configuration**

* Proposals
  + Option 1 (CMCC):


- Carrier#1 TDD UL/DL pattern is 3D1S4U, S = 10DL: 2GP: 2UL;

- Carrier#2 TDD UL/DL pattern is 1D1S2U, S = 10DL: 2GP: 2UL

* Recommended WF
  + Is option 1 agreeable?

**Issue 2-4-2: Which symbol to be verified?**

* Proposals
  + Option 1(CMCC):
    - For NR TDD PCell (Cell 1), this test verifies that the UE correctly receive the PDCCH scheduled on the symbol #4 or symbol #5 or symbol #8 on the special slot depending on UE capability uplinkTxSwitchingPeriod.
    - For NR TDD SCell (Cell 2), this test verifies that the UE correctly receive the PDCCH scheduled on the symbol #4 or symbol #5 or symbol #8 on the 2nd special slot of every 8 slots depending on UE capability uplinkTxSwitchingPeriod.



* Recommended WF
  + Is option 1 agreeable?

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MTK | **Issue 2-1-1: How to verify the symbol-level DL interruption in test**  We try to bring a new alternative (Option 3): Triggering an aperiodic CSI-RS L1-RSRP reporting with CSI-RS resources (with boosted power) on the OFDM symbol right before the interruption.  On Option 1, we share the same view as China Telecom that we should try to avoid testing this feature only on those UEs supporting some optional features in Rel-15.  On Option 2, in principle it is OK. But we need to be carefully in deciding the MCS according to the SNR level and the remaining REs. Otherwise, some UE may still pass the test by skipping more than the interrupted symbols. However, the length of interruption depending on both UE capability and the SCS’s of carriers. It may take a long time to conclude the MCS and SNR for different cases.  **Issue 2-1-2: Whether MRTD is considered in test cases**  Support Option 1, in which MRTD = 0us  **Issue 2-4-2: Which symbol to be verified?**  One question for clarification.  According to the figure provided in R4-2014733, when interruption occurs on the UL symbols of the victim cell. Is it the intention to test interruption to UL? |
| China Telecom | **Sub-topic 2-1: Principle and general parameters for test case**  Issue 2-1-1: How to verify the symbol-level DL interruption in test  Regarding the MCS and SNR for option 2, we can configure high SNR (e.g., 30 dB) and high code rate (e.g., MCS 28 in MCS table 1 with 64QAM and code rate of 0.93). Based on the current test setup, max 10 OFDM symbols can be used for PDSCH transmission (including data and DMRS REs). If 1 out of the 10 OFDM symbols is interrupted, data channel based on the remaining 9 symbols (with code rate > 1) cannot be correctly decoded. The situation is worse for PDSCH with less than 10 OFDM symbols.  The option 3 from MTK is also ok to us.  Issue 2-1-2: Whether MRTD is considered in test cases  OK with theRecommended WF.  Issue 2-1-3: SRS configuration in the special slot  OK with theRecommended WF.  **Sub-topic 2-2: Inter-band ENDC**  Issue 2-2-1: TDD configuration  OK with theRecommended WF. To reduce the spec impact, for 30kHz, ok to reuse the existing TDD pattern in 38.133.  Issue 2-2-2: Which symbol to be verified?  Can discuss together with Issue 2-1-1.  **Sub-topic 2-3: FDD-TDD CA (SA)**  **Issue 2-3-1: TDD configuration**  OK with theRecommended WF. To reduce the spec impact, for 30kHz, ok to reuse the existing TDD pattern in 38.133.  **Issue 2-3-2: Which symbol to be verified?**  Can discuss together with Issue 2-1-1.  **Sub-topic 2-4: TDD-TDD CA (SA)**  **Issue 2-4-1: TDD configuration**  OK with theRecommended WF. One more TDD pattern is needed for carrier 2.  **Issue 2-4-2: Which symbol to be verified?**  Can discuss together with Issue 2-1-1. |
| CMCC | **Issue 2-1-1: How to verify the symbol-level DL interruption in test**  In order to avoid that UE does not support *pdcch-MonitoringAnyOccasions* or *pdcch*-*MonitoringAnyOccasionsWithSpanGap,* we are fine to consider other options. Option 2 and option 3 are in principle OK.  **Issue 2-1-2: Whether MRTD is considered in test cases**  Support the recommended WF.  **Issue 2-1-3: SRS configuration in the special slot**  Support the recommended WF.  **Issue 2-2-1: TDD configuration**  OK to reuse existing TDD configuration  **Issue 2-2-2: Which symbol to be verified?**  OK with option 1  **Issue 2-3-1: TDD configuration**  OK with option 1  **Issue 2-3-2: Which symbol to be verified?**  OK with option 1  **Issue 2-4-1: TDD configuration**  Support the recommended WF  **Issue 2-4-2: Which symbol to be verified?**  To MTK: The DL interruption occurs in the DL symbols in NR TDD PCell or NR TDD SCell. We will not test the interruption to UL. |
| Huawei | **Issue 2-1-1: How to verify the symbol-level DL interruption in test**  For option2, it depends on MCS, if the MCS is low, the PDSCH allocated right before the interruption may be not impacted.  For the new option3 proposed by MTK, we are open to discuss it. We need time to further check the feasibility.  **Issue 2-1-2: Whether MRTD is considered in test cases**  Support the recommended WF.  **Issue 2-1-3: SRS configuration in the special slot**  Support the recommended WF.  **Issue 2-2-1: TDD configuration**  support option 1.  **Issue 2-2-2: Which symbol to be verified?**  support option1.  **Issue 2-3-1: TDD configuration**  Option 1 is ok.  **Issue 2-3-2: Which symbol to be verified?**  Option 1 is ok.  **Issue 2-4-1: TDD configuration**  Option 1 is ok.  **Issue 2-4-2: Which symbol to be verified?**  Option 1 is ok. |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014504  (China Telecom) | Huawei: depending on the outcome of the first issue. Besides the new text case shall be with change marks. |
| Company B |
|  |
| R4-2014734 (CMCC) | Huawei: depending on the outcome of the first issue. |
| Company B |
|  |
| R4-2015487 (Huawei, HiSilicon) | Huawei: depending on the outcome of the first issue. |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |