**3GPP TSG-RAN WG4 Meeting #97-eR4-2017258**

**E-Meeting, 02 November 2020 – 13 November 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **xx** | **rev** | **-** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on TC for 2-step RA type contention based RA in FR1 and FR2 NR cells for EN-DC |
|  |  |
| ***Source to WG:*** | NEC  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_2step\_RACH-Perf |  | ***Date:*** | 2020-10-23 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Addition of 2-step RA type test cases for contention based RA in EN-DC |
|  |  |
| ***Summary of change:*** | Test cases for 2-step RA type contention based RA for FR1 cells in EN-DC to test MsgB with fallbackRARTest cases for 2-step RA type contention based RA for FR2 cells in EN-DC to test MsgB with successRAR |
|  |  |
| ***Consequences if not approved:*** | 2-step RA type test cases will not be available in specification |
|  |  |
| ***Clauses affected:*** | A.4.3.2.2.1, A.4.3.2.2.3, A.5.3.2.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | R4-2015303 |

**------------------------------------Start of change 1------------------------------------------**

A.4.3.2.2 Random Access

A.4.3.2.2.1 4-step RA type contention based random access test in FR1 for PSCell in EN-DC

A.4.3.2.2.1.1 Test Purpose and Environment

The purpose of this test is to verify that the behavior of the random access procedure is according to the requirements and that the PRACH power settings and timing are within specified limits. This test will verify the requirements in clause 6.2.2.2 and clause 7.1.2 in an AWGN model.

**------------------------------------End of change 1------------------------------------------**

**------------------------------------Start of change 2------------------------------------------**

A.4.3.2.2.3 2-step RA type contention based random access test in FR1 for PSCell in EN-DC

A.4.3.2.2.3.1 Test Purpose and Environment

The purpose of this test is to verify that the behaviour of the random access procedure is according to the requirements and that the MsgA PRACH, MsgA PUSCH power settings and timing are within specified limits. This test will verify the requirements in clause 6.2.2.3 and clause 7.1.2 in an AWGN model.

For this test two cells are used, with the configuration of Cell 1 (E-UTRA PCell) specified in clause A.3.7.2.1 and Cell 2 configured as PSCell in FR1. Supported test parameters are shown in Table A.4.3.2.2.3.1-1. UE capable of EN-DC with PSCell in FR1 needs to be tested by using the parameters in Table A.4.3.2.2.3.1-2.

**Table A.4.3.2.2.3.1-1: Supported test configurations for 2-step RA type contention based random access test in FR1 for PSCell in EN-DC**

|  |  |
| --- | --- |
| **Config** | **Description** |
| 1 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 3 | LTE FDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| 4 | LTE TDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations depending on UE capability |

**Table A.4.3.2.2.3.1-2: General test parameters for 2-step RA type contention based random access test in FR1 for PSCell in EN-DC**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test-1** | **Comments** |
| SSB Configuration | Config 1,2 |  | SSB pattern 3 in FR1 | As defined in A.3.10 |
|  | Config 3,4 |  | SSB pattern 4 in FR1 |  |
|  |  |  |  |
|  |  |  |  |
| Duplex Mode for Cell 2 | Config 1,2 |  | FDD |  |
|  | Config 3,4 |  | TDD |
| TDD Configuration | Config 3,4 |  | TDDConf.2.1 |  |
| OCNG Pattern Note 1  |  | OCNG pattern 1 | As defined in A.3.2.1. |
| PDSCH parameters Note 3 ­ | Config 1,2 |  | SR.1.1 FDD | As defined in A.3.1.1. |
| Config 3,4 |  | SR.2.1 TDD |  |
| NR RF Channel Number |  | 1 |  |
| EPRE ratio of PSS to SSS | dB |  |  |
| EPRE ratio of PBCH\_DMRS to SSS | dB |  |  |
| EPRE ratio of PBCH to PBCH\_DMRS | dB |  |  |
| EPRE ratio of PDCCH\_DMRS to SSS | dB | 0 |  |
| EPRE ratio of PDCCH to PDCCH\_DMRS | dB |  |  |
| EPRE ratio of PDSCH\_DMRS to SSS | dB |  |  |
| EPRE ratio of PDSCH to PDSCH\_DMRS | dB |  |  |
| SSB with index 0 |  | dB | 3 | Power of SSB with index 0 is set to be above configured *msgA-RSRP-ThresholdSSB* |
|  |  | Config 1,2 | dBm/15kHz | -98 |  |
|  |  | Config 3,4 |  | -101 |  |
|  |  | dB | 3 |  |
|  | SS-RSRP Note 2 | dBm/ SCS | -95 |  |
| SSB with index 1 |  | dB | -17 | Power of SSB with index 1 is set to be below configured *msgA-RSRP-ThresholdSSB* |
|  |  | Config 1,2 | dBm/15kHz | -98  |  |
|  |  | Config 3,4 |  | -101 |  |
|  |  | dB | -17 |  |
|  | SS-RSRP Note 2 | dBm/ SCS | -115 |  |
| Io | Config 1,2 | dBm | -65.3/9.36MHz | For symbols without SSB  |
|  | Config 3,4 |  | -62.2/38.16MHz | index 1 |
| ss-PBCH-BlockPower | dBm/ SCS | -5 | As defined in clause 6.3.2 in TS 38.331 [2]. |
| Configured UE transmitted power () | dBm | 23 | As defined in clause 6.2.4 in TS 38.101-1. |
| MsgA Configuration |  | FR1 MsgA configuration 1 | As defined in A.3.19.2.1. |
| Propagation Condition  | - | AWGN |  |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols. The OCNG pattern is chosen during the test according to the presence of a DL reference measurement channel.Note 2: SS-RSRP, Es/Iot and Io levels have been derived from other parameters for information purpose. They are not settable parameters.Note 3: The DL PDSCH reference measurement channel is used in the test only when a downlink transmission dedicated to the UE under test is required. |

A.4.3.2.2.3.2 Test Requirements

Contention based random access is triggered by *not* explicitly assigning a random access preamble via dedicated signalling in the downlink.

A.4.3.2.2.3.2.1 MsgA Transmission

To test the UE behaviour specified in Clause 6.2.2.3.1.1 the System Simulator shall receive the MsgA with a preamble which belongs to one of the Random Access Preambles associated with the SSB with index 0, which has SS-RSRP above the configured *msgA-RSRP-ThresholdSSB*.

In addition, the power applied to all MsgA transmissions shall be in accordance with what is specified in Clause 6.2.2.3. The power of the first MsgA preamble transmission shall be -30 dBm with an accuracy specified in clause 6.3.4.2 of TS 38.101-1 [18]. The power of the first MsgA PUSCH transmission shall be [X] dBm with an accuracy specified in clause 6.3.4.2 of TS 38.101-1 [18]. The relative power applied to additional MsgA transmissions shall have an accuracy specified in clause 6.3.4.3 of TS 38.101-1 [18].

The transmit timing of all MsgA transmissions shall be within the accuracy specified in Clause 7.1.2.

A.4.3.2.2.3.2.2 MsgB Reception

To test the UE behaviour specified in Clause 6.2.2.3.1.2 the System Simulator shall transmit a MsgB with fallbackRAR containing a Random Access Preamble identifier corresponding to the transmitted Random Access Preamble after 5 preambles have been received by the System Simulator. In response to the first 4 preambles, the System Simulator shall transmit a MsgB *not* corresponding to the transmitted Random Access Preamble.

The UE may stop monitoring for MsgB(s) and shall transmit the msg3 if the MsgB with a fallbackRAR contains a Random Access Preamble identifier corresponding to the transmitted Random Access Preamble.

The UE shall again perform the Random Access Resource selection procedure specified in clause 5.1.2a in TS 38.321 [7], and transmit with the calculated MsgA PRACH and MsgA PUSCH transmission power when the backoff time expires if all received MsgB’s contain Random Access Preamble identifiers that do not match the transmitted Random Access Preamble.

In addition, the power applied to all MsgA transmissions shall be in accordance with what is specified in Clause 6.2.2.3. The power of the first preamble shall be -30 dBm with an accuracy specified in clause 6.3.4.2 of TS 38.101-1 [18]. The power of the first MsgA PUSCH transmission shall be [X] dBm with an accuracy specified in clause 6.3.4.2 of TS 38.101-1 [18]. The relative power applied to additional MsgA transmissions shall have an accuracy specified in clause 6.3.4.3 of TS 38.101-1 [18].

The transmit timing of all MsgA transmissions shall be within the accuracy specified in Clause 7.1.2.

A.4.3.2.2.3.2.3 No MsgB Reception

To test the UE behavior specified in clause 6.2.2.3.1.3 the System Simulator shall transmit a MsgB with fallbackRAR containing a successRAR message and a Random Access Preamble identifier corresponding to the transmitted Random Access Preamble after 5 preambles have been received by the System Simulator. The System Simulator shall *not* respond to the first 4 preambles.

The UE shall again perform the Random Access Resource selection procedure specified in clause 5.1.2a in TS 38.321 [7], and transmit with the calculated MsgA PRACH and MsgA PUSCH transmission power when the backoff time expires if no MsgB is received within the MsgB Response window.

In addition, the power applied to all MsgA transmissions shall be in accordance with what is specified in Clause 6.2.2.3. The power of the first preamble shall be -30 dBm with an accuracy specified in clause 6.3.4.2 of TS 38.101-1 [18]. The power of the first MsgA PUSCH transmission shall be [X] dBm with an accuracy specified in clause 6.3.4.2 of TS 38.101-1 [18]. The relative power applied to additional MsgA transmissions shall have an accuracy specified in clause 6.3.4.3 of TS 38.101-1 [18].

The transmit timing of all MsgA transmissions shall be within the accuracy specified in Clause 7.1.2.

**------------------------------------End of change 2------------------------------------------**

**------------------------------------Start of change 3------------------------------------------**

A.5.3.2.2.3 2-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC

A.5.3.2.2.3.1 Test Purpose and Environment

The purpose of this test is to verify that the behavior of the random access procedure is according to the requirements and that the MsgA power settings and timing are within specified limits. This test will verify the requirements in clause 6.2.2.3 and clause 7.1.2 in an AWGN model.

For this test two cells are used, with the configuration of Cell 1 (E-UTRA PCell) specified in clause A.3.7.2.1 and Cell 2 configured as PSCell or SCell in FR2. Supported test parameters are shown in Table A.5.3.2.2.3.1-1. UE capable of EN-DC with PSCell or SCell in FR2 needs to be tested by using the parameters in Table A.5.3.2.2.3.1-2 and Table A.5.3.2.2.3.1-3.

**Table A.5.3.2.2.3.1-1: Supported test configurations for 2-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC**

|  |  |
| --- | --- |
| **Config** | **Description** |
| 1 | LTE FDD, NR PSCell/SCell 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | LTE TDD, NR PSCell/SCell 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to be tested in one of the supported test configurations depending on UE capability |

**Table A.5.3.2.2.3.1-2: General test parameters for 2-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test-1** | **Comments** |
| SSB Configuration | Config 1,2 |  | SSB.1 FR2 | As defined in A.3.10 |
| Duplex Mode for Cell 2 | Config 1,2 |  | TDD |  |
| TDD Configuration | Config 1,2 |  | TDDConf.3.1 |  |
| BWchannel | Config 1 | MHz | 100: NRB,c = 24 |  |
| OCNG Pattern Note 1  |  | OP.3 | As defined in A.3.2.1. |
| PDSCH Reference Channel Note 2 | Config 1,2 |  | SR.3.1 TDD | As defined in A.3.1.1. |
| RMSI CORESET Reference Channel | Config 1,2 |  | CR.3.1 TDD | As defined in A.3.1.2 |
| NR RF Channel Number |  | 1 |  |
| EPRE ratio of PSS to SSS | dB | 0 |  |
| EPRE ratio of PBCH\_DMRS to SSS | dB |  |  |
| EPRE ratio of PBCH to PBCH\_DMRS | dB |  |  |
| EPRE ratio of PDCCH\_DMRS to SSS | dB |  |  |
| EPRE ratio of PDCCH to PDCCH\_DMRS | dB |  |  |
| EPRE ratio of PDSCH\_DMRS to SSS | dB |  |  |
| EPRE ratio of PDSCH to PDSCH\_DMRS | dB |  |  |
| ss-PBCH-BlockPower | dBm/ SCS | +20 +ΔUL | As defined in TS 38.331 [2].ΔUL is derived from the uplink calibration process Note 3 |
| Configured UE transmitted power () | dBm | maximum value configurable for certain power class | As defined in clause 6.2.4 in TS 38.101-2 [19] |
| MsgA Configuration |  | FR2 MsgA configuration 1 | As defined in A.3.19.3.1, with exceptions as defined below. |
| msgA-RSRP-ThresholdSSB | dBm | RSRP\_69 +ΔDL | RSRP\_69 corresponds to -88dBm. ΔDL is derived from the downlink calibration process Note 4 |
| msgA-PreambleReceivedTargetPower | dBm | -100 | As defined in TS 38.331 [2] |
| Note 1: OCNG shall be used such that a constant total transmitted power spectral density is achieved for all OFDM symbols. The OCNG pattern is chosen during the test according to the presence of a DL reference measurement channel.Note 2: The DL PDSCH reference measurement channel is used in the test only when a downlink transmission dedicated to the UE under test is required.Note 3: The ΔUL value is calculated as -ROUND(PMsgA0 -1), where PMsgA0 is the measured first MsgA PRACH power with -80.6dBm/SCS applied, *msgA-PreambleReceivedTargetPower* = -100dBm and *ss-PBCH-BlockPower* = 20dBm. These values are used during the uplink calibration process carried out before the test case is run, with the UE configured to send MsgA.Note 4: The ΔDL value is calculated as (RSRP\_REP – RSRP\_76), where RSRP\_REP is the SS-RSRP Reported value in Table 10.1.6.1-1 with -80.6dBm/SCS applied. These values are used during the downlink calibration process carried out before the test case is run, with the UE configured to report SS-RSRP. For a Reported value RSRP\_x, x is treated as a positive integer value. |

**Table A.5.3.2.2.3.1-3: OTA-related test parameters for 2-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC**

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test-1** | **Comments** |
| AoA setup |  | Setup 1 | As defined in A.3.15.1 |
| Assumption for UE beamsNote 2 |  | Rough |  |
| SSB with  | Es Note1 | dBm/SCS | -80.6 | Power of SSB with index 0 is set to be above configured *msgA-RSRP-ThresholdSSB* |
| index 0 | SSB\_RP | dBm/SCS | -80.6 |
|  | Es/IotBB | dB | 21.09 |  |
|  | Io | dBm/95.04 MHz | -56.01 | Io in symbols containing SSB index 0 |
| SSB with  | Es Note1 | dBm/SCS | -95.0 | Power of SSB with index 1 is set to be below configured *msgA-RSRP-ThresholdSSB* |
| index 1 | SSB\_RP | dBm/SCS | -95.0 |
|  | Es/IotBB | dB | 6.69 |  |
|  | Io | dBm/95.04 MHz | -70.41 | Io in symbols containing SSB index 1 |
| Propagation Condition  | - | AWGN |  |
| Note 1: No artificial noise is applied in this test.Note 2: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

A.5.3.2.2.3.2 Test Requirements

Contention based random access is triggered by *not* explicitly assigning a random access preamble via dedicated signalling in the downlink.

A.5.3.2.2.3.2.1 MsgA Transmission

To test the UE behaviour specified in Clause 6.2.2.3.1.1 the System Simulator shall receive the Random Access Preamble which belongs to one of the Random Access Preambles associated with the SSB with index 0, which has SS-RSRP above the configured *msgA-RSRP-ThresholdSSB*.

In addition, the power applied to all preambles shall be in accordance with what is specified in Clause 6.2.2.3. The power of the first preamble shall be 0.6 dBm to be received at TE with an accuracy specified in clause 6.3.4.2 of TS 38.101-2 [19]. The relative power applied to additional preambles shall have an accuracy specified in clause 6.3.4.3 of TS 38.101-2 [19].

The transmit timing of all MsgA PRACH and MsgA PUSCH transmissions shall be within the accuracy specified in Clause 7.1.2.

A.5.3.2.2.3.2.2 MsgB Reception

To test the UE behaviour specified in Clause 6.2.2.3.1.2 the System Simulator shall transmit a MsgB with successRAR containing a Random Access Preamble identifier corresponding to the transmitted Random Access Preamble after 5 preambles have been received by the System Simulator. In response to the first 2 preambles, the System Simulator shall transmit a MsgB *not* corresponding to the transmitted Random Access Preamble.

The UE may stop monitoring for MsgB(s) and shall transmit an ACK if the MsgB with a successRAR contains a Random Access Preamble identifier corresponding to the transmitted Random Access Preamble and if the Contention Resolution is successful.

The UE shall again perform the Random Access Resource selection procedure specified in clause 5.1.2a in TS38.321 [7], and transmit with the calculated MsgA PRACH and MsgA PUSCH transmission power when the backoff time expires if all received MsgBs contain Random Access Preamble identifiers that do not match the transmitted Random Access Preamble.

In addition, the power applied to all preambles shall be in accordance with what is specified in Clause 6.2.2.2. The power of the first preamble shall be 0.6 dBm to be received at TE with an accuracy specified in clause 6.3.4.2 of TS 38.101-2 [19]. The relative power applied to additional preambles shall have an accuracy specified in clause 6.3.4.3 of TS 38.101-2 [19].

The transmit timing of all MsgA transmissions shall be within the accuracy specified in Clause 7.1.2.

A.5.3.2.2.3.2.3 No MsgB Reception

To test the UE behaviour specified in clause 6.2.2.3.1.3 the System Simulator shall transmit a MsgB with successRAR containing a Random Access Preamble identifier corresponding to the transmitted Random Access Preamble after 3 preambles have been received by the System Simulator. The System Simulator shall *not* respond to the first 2 preambles.

The UE shall again perform the Random Access Resource selection procedure specified in clause 5.1.2a in TS38.321 [7], and transmit with the calculated MsgA PRACH and MsgA PUSCH transmission power when the backoff time expires if no MsgB is received within the RA Response window.

In addition, the power applied to all MsgA transmissions shall be in accordance with what is specified in Clause 6.2.2.3. The power of the first preamble shall be 0.6 dBm to be received at TE with an accuracy specified in clause 6.3.4.2 of TS 38.101-2 [19]. The relative power applied to additional preambles shall have an accuracy specified in clause 6.3.4.3 of TS 38.101-2 [19].

The transmit timing of all MsgA PRACH and MsgA PUSCH transmissions shall be within the accuracy specified in Clause 7.1.2.

**------------------------------------End of change 3------------------------------------------**