{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Cover","Parameters","FR1 PUSCH high reliability","FR1 PUSCH low latency","FR2 PUSCH high reliability","FR2 PUSCH low latency"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"FR1 PUSCH high reliability","index":2,"n_rows":18,"n_cols":29,"rows_kept":18,"cut":false,"hidden":false,"merged":[[10,6,13,6],[10,7,13,7],[10,9,11,9],[12,9,13,9],[6,9,7,9],[8,9,9,9],[2,6,5,6],[0,7,1,7],[2,7,5,7],[6,6,9,6],[6,7,9,7],[0,8,1,8],[0,9,1,9],[2,9,3,9],[4,9,5,9],[2,8,9,8],[6,2,9,2],[6,3,9,3],[6,4,9,4],[6,5,9,5],[2,0,9,0],[2,1,5,1],[6,1,9,1],[2,2,5,2],[2,3,5,3],[2,5,5,5],[2,4,5,4],[0,0,1,0],[0,5,1,5],[0,2,1,2],[0,1,1,1],[0,12,1,12],[0,13,0,14],[0,11,1,11],[0,10,1,10],[0,3,1,3],[0,6,1,6],[0,4,1,4],[0,27,0,28],[0,17,0,18],[0,19,0,20],[0,15,0,16],[0,21,0,22],[0,23,0,24],[0,25,0,26],[10,0,17,0],[14,5,17,5],[14,6,17,6],[14,7,17,7],[14,9,15,9],[16,9,17,9],[10,8,17,8],[14,1,17,1],[14,2,17,2],[14,3,17,3],[14,4,17,4],[10,2,13,2],[10,3,13,3],[10,4,13,4],[10,5,13,5],[10,1,13,1]]}
[" Test","Duplex mode","Aggregation factor "," waveform","MCS level","Tx/Rx","Propagation condition","DMRS","SCS","BW","PUSCH mapping type","38.104 req","38.141 req","Samsung",null,"DoCoMo",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 1.1","FDD","n2","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1","15kHz","5MHz","type A",{"$f":"DerivingPerfReq(N3:Y3)","v":-8.5},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-7.9},-11.3,-9.3000000000000007,null,null,-9,-7.5,-10,-7.5,-10.3,-8.3000000000000007,-10.9,-8.9,{"$f":"MAX(N3,P3,R3,T3,V3,X3)-MIN(N3,P3,R3,T3,V3,X3)","v":2.3000000000000007},1.8000000000000007,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3)","v":-10.3},-8.3000000000000007]
[null,null,null,null,null,null,null,null,null,null,"type B",{"$f":"DerivingPerfReq(N4:Y4)","v":-8.1999999999999993},-7.6,-11,-9,null,null,-9,-7.5,-9.8000000000000007,-7.3,-10.3,-8.3000000000000007,-10.9,-8.9,2,1.7000000000000002,-10.199999999999999,-8.1999999999999993]
[null,null,null,null,null,null,null,null,null,"10MHz","type A",-9.3000000000000007,-8.7000000000000011,-11.9,-9.9,null,null,-9.6,-8.1,-10.199999999999999,-7.7,-11.5,-9.5,-12.1,-10.1,2.5,2.3999999999999995,-11.06,-9.06]
[null,null,null,null,null,null,null,null,null,null,"type B",-9.8000000000000007,-9.2000000000000011,-11.8,-9.8000000000000007,null,null,-9.5,-8,-9.9,-7.4,-11.5,-9.5,-12.1,-10.1,2.5999999999999996,2.6999999999999993,-10.96,-8.9600000000000009]
[null,"TDD","n8","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1",null,"5MHz","type A",-8.1999999999999993,-7.6,null,null,null,null,-8.9,-7.4,-12.9,-10.4,-10.199999999999999,-8.4,-10.9,-8.9,{"$f":"MAX(N7,P7,R7,T7,V7,X7)-MIN(N7,P7,R7,T7,V7,X7)","v":4},3,-10.725,-8.7750000000000004]
[null,null,null,null,null,null,null,null,null,null,"type B",-8.1999999999999993,-7.6,null,null,null,null,-8.9,-7.4,-12.7,-10.199999999999999,-10.199999999999999,-8.4,-10.9,-8.9,3.7999999999999989,2.7999999999999989,-10.675000000000001,-8.7249999999999996]
[null,null,null,null,null,null,null,null,null,"10MHz","type A",-103,-103,null,null,null,null,-9.6,-8.1,-13.4,-10.9,-11.2,-9.1999999999999993,-12.4,-10.4,3.8000000000000007,2.8000000000000007,-11.65,-9.65]
[null,null,null,null,null,null,null,null,null,null,"type B",-10.1,-9.5,null,null,null,null,-9.6,-8,-13.2,-10.7,-11.2,-9.1999999999999993,-12.4,-10.4,3.5999999999999996,2.6999999999999993,-11.6,-9.5749999999999993]
["Test 1.2","FDD","n2","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1","30kHz","10MHz","type A",{"$f":"DerivingPerfReq(N11:Y11)","v":-8.1999999999999993},{"$f":"IF(L11>-100,L11+0.6,L11)","v":-7.6},-12.2,-10.199999999999999,null,null,-9.8000000000000007,-8.3000000000000007,-12.9,-10.4,-10.7,-8.6999999999999993,-9.6,-7.6,{"$f":"MAX(N11,P11,R11,T11,V11,X11)-MIN(N11,P11,R11,T11,V11,X11)","v":3.3000000000000007},{"$f":"MAX(O11,Q11,S11,U11,W11,Y11)-MIN(O11,Q11,S11,U11,W11,Y11)","v":2.8000000000000007},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11)","v":-11.04},{"$f":"AVERAGE(O11,Q11,S11,U11,W11,Y11)","v":-9.0399999999999991}]
[null,null,null,null,null,null,null,null,null,null,"type B",-8.1999999999999993,-7.6,-12.1,-10.1,null,null,-9.8000000000000007,-8.3000000000000007,-12.9,-10.4,-10.7,-8.6999999999999993,-9.6,-7.6,3.3000000000000007,2.8000000000000007,-11.02,-9.02]
[null,null,null,null,null,null,null,null,null,"40MHz","type A",-10.3,-9.7000000000000011,-13,-11,null,null,-10.1,-8.6,-13,-10.5,-11.5,-9.5,-10.8,-8.8000000000000007,2.9000000000000004,2.4000000000000004,-11.680000000000001,-9.6800000000000015]
[null,null,null,null,null,null,null,null,null,null,"type B",-10.199999999999999,-9.6,-12.9,-10.9,null,null,-10.1,-8.6,-12.8,-10.3,-11.5,-9.5,-10.8,-8.8000000000000007,2.8000000000000007,2.3000000000000007,-11.62,-9.6199999999999992]
[null,"TDD","n2","CP-OFDM","Table 3, MCS5","1T2R","TDLB100-400","DMRS 1+1",null,"10MHz","type A",{"$f":"DerivingPerfReq(N15:Y15)","v":-100},{"$f":"IF(L15>-100,L15+0.6,L15)","v":-100},null,null,null,null,-9.6,-8.1,null,null,null,null,null,null,{"$f":"MAX(N15,P15,R15,T15,V15,X15)-MIN(N15,P15,R15,T15,V15,X15)","v":0},{"$f":"MAX(O15,Q15,S15,U15,W15,Y15)-MIN(O15,Q15,S15,U15,W15,Y15)","v":0},{"$f":"AVERAGE(N15,P15,R15,T15,V15,X15)","v":-9.6},{"$f":"AVERAGE(O15,Q15,S15,U15,W15,Y15)","v":-8.1}]
[null,null,null,null,null,null,null,null,null,null,"type B",-100,-100,null,null,null,null,-9.5,-8,null,null,null,null,null,null,0,0,-9.5,-8]
[null,null,null,null,null,null,null,null,null,"40MHz","type A",-100,-100,null,null,null,null,-9.9,-8.4,null,null,null,null,null,null,0,0,-9.9,-8.4]
[null,null,null,null,null,null,null,null,null,null,"type B",-100,-100,null,null,null,null,-9.8000000000000007,-8.3000000000000007,null,null,null,null,null,null,0,0,-9.8000000000000007,-8.3000000000000007]

{"sheet":"FR1 PUSCH low latency","index":3,"n_rows":6,"n_cols":28,"rows_kept":6,"cut":false,"hidden":false,"merged":[[4,3,5,3],[4,2,5,2],[4,1,5,1],[4,0,5,0],[4,8,5,8],[4,7,5,7],[4,6,5,6],[4,5,5,5],[4,4,5,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[0,8,1,8],[2,8,3,8],[2,1,3,1],[2,0,3,0],[2,2,3,2],[2,3,3,3],[2,4,3,4],[0,26,0,27],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,24,0,25],[0,12,0,13],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,5,1,5],[0,6,1,6],[0,7,1,7]]}
[" Test","Symbol length"," waveform","Tx/Rx","PUSCH mapping type","MCS level","Propagation condition","DMRS","SCS","BW","38.104 req","38.141 req","Samsung",null,"DoCoMo",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 2.1","2os","CP-OFDM","1T2R","type B","Table 3, MCS10","TDLC300-100","DMRS 1+0","15kHz","5MHz",{"$f":"DerivingPerfReq(M3:X3)","v":0.6},{"$f":"IF(K3>-100,K3+0.6,K3)","v":1.2},-1.26,0.74,null,null,-1,0.5,-1.7,0.8,-1.5,0.5,-1.6,0.4,{"$f":"MAX(M3,O3,Q3,S3,U3,W3)-MIN(M3,O3,Q3,S3,U3,W3)","v":0.7},{"$f":"MAX(N3,P3,R3,T3,V3,X3)-MIN(N3,P3,R3,T3,V3,X3)","v":0.4},{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3)","v":-1.4120000000000001},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3)","v":0.58799999999999997}]
[null,null,null,null,null,null,null,null,null,"10MHz",{"$f":"DerivingPerfReq(M4:X4)","v":0.2},{"$f":"IF(K4>-100,K4+0.6,K4)","v":0.8},-1.71,0.28999999999999998,null,null,-1.5,0,-2.2999999999999998,0.2,-1.9,0.1,-1.7,0.3,{"$f":"MAX(M4,O4,Q4,S4,U4,W4)-MIN(M4,O4,Q4,S4,U4,W4)","v":0.79999999999999982},0.3,{"$f":"AVERAGE(M4,O4,Q4,S4,U4,W4)","v":-1.8219999999999998},0.17799999999999999]
["Test 2.2","2os","CP-OFDM","1T2R"," type B","Table 3, MCS10","TDLC300-100","DMRS 1+0","30kHz","10MHz",{"$f":"DerivingPerfReq(M5:X5)","v":0.4},{"$f":"IF(K5>-100,K5+0.6,K5)","v":1},-1.27,0.73,null,null,-1.2,0.3,-1.8,0.7,-2,0,-1.9,0.1,0.8,0.73,-1.6339999999999999,0.36599999999999999]
[null,null,null,null,null,null,null,null,null,"40MHz",{"$f":"DerivingPerfReq(M6:X6)","v":-0.1},{"$f":"IF(K6>-100,K6+0.6,K6)","v":0.5},-1.68,0.32,null,null,-1.3,0.2,-2.5,0,-2.8,-0.8,-2,0,1.4999999999999998,1.1200000000000001,-2.056,-5.6000000000000008E-2]

{"sheet":"FR2 PUSCH high reliability","index":4,"n_rows":18,"n_cols":29,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,10,1,10],[0,9,1,9],[0,7,1,7],[0,8,1,8],[0,6,1,6],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[14,0,17,0],[10,1,13,1],[10,2,13,2],[10,3,13,3],[10,4,13,4],[10,0,13,0],[2,0,5,0],[6,0,9,0],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,5,5,5],[2,6,5,6],[6,1,9,1],[6,2,9,2],[6,3,9,3],[6,4,9,4],[6,5,9,5],[6,6,9,6],[2,4,5,4],[10,5,13,5],[10,6,13,6],[10,8,13,8],[12,9,13,9],[14,1,17,1],[14,2,17,2],[14,3,17,3],[14,4,17,4],[14,5,17,5],[10,9,11,9],[14,6,17,6],[14,8,17,8],[14,9,15,9],[16,9,17,9],[2,7,9,7],[10,7,17,7],[8,9,9,9],[2,8,5,8],[6,8,9,8],[6,9,7,9],[2,9,3,9],[4,9,5,9]]}
[" Test","Duplex mode","Aggregation factor "," waveform","MCS level","Tx/Rx","PUSCH mapping type","SCS","BW","DMRS","Propagation condition","38.104 req","38.141 req","Samsung",null,"DoCoMo",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 3.1","TDD","n8","CP-OFDM","Table 3, MCS5","1T2R","type B","60KHz","50MHz","DMRS 1+1","TDLA30-75",{"$f":"DerivingPerfReq(N3:Y3)","v":-100},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-100},null,null,null,null,null,null,-9.4,-6.9,-12.4,-10.4,null,null,{"$f":"MAX(N3,P3,R3,T3,V3,X3)-MIN(N3,P3,R3,T3,V3,X3)","v":3},{"$f":"MAX(O3,Q3,S3,U3,W3,Y3)-MIN(O3,Q3,S3,U3,W3,Y3)","v":3.5},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3)","v":-10.9},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3)","v":-8.65}]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,-10.199999999999999,-7.7,-13.8,-11.8,null,null,3.6000000000000014,4.1000000000000005,-12,-9.75]
[null,null,null,null,null,null,null,null,null,"DMRS 1+0","TDLA30-75",{"$f":"DerivingPerfReq(N5:Y5)","v":-100},{"$f":"IF(L5>-100,L5+0.6,L5)","v":-100},null,null,null,null,null,null,-9.3000000000000007,-6.8,null,null,null,null,{"$f":"MAX(N5,P5,R5,T5,V5,X5)-MIN(N5,P5,R5,T5,V5,X5)","v":0},0,{"$f":"AVERAGE(N5,P5,R5,T5,V5,X5)","v":-9.3000000000000007},-6.8]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,-10.1,-7.6,null,null,null,null,0,0,-10.1,-7.6]
["Test 3.2","TDD","n8","CP-OFDM","Table 3, MCS5","1T2R","type B",null,"100MHz","DMRS 1+1","TDLA30-75",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,"DMRS 1+0","TDLA30-75",{"$f":"DerivingPerfReq(N9:Y9)","v":-100},{"$f":"IF(L9>-100,L9+0.6,L9)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(N9,P9,R9,T9,V9,X9)-MIN(N9,P9,R9,T9,V9,X9)","v":0},{"$f":"MAX(O9,Q9,S9,U9,W9,Y9)-MIN(O9,Q9,S9,U9,W9,Y9)","v":0},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(O9,Q9,S9,U9,W9,Y9)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["Test 3.3","TDD","n8","CP-OFDM","Table 3, MCS5","1T2R","type B","120KHz","50MHz","DMRS 1+1","TDLA30-75",-100,-100,null,null,null,null,null,null,-7.7,-5.2,-10.4,-8.4,null,null,2.7,3.2,-9.0500000000000007,-6.8000000000000007]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,-8.1999999999999993,-5.7,-12,-10,null,null,3.8000000000000007,4.3,-10.1,-7.85]
[null,null,null,null,null,null,null,null,null,"DMRS 1+0","TDLA30-75",-100,-100,null,null,null,null,null,null,-7.8,-5.3,null,null,null,null,0,0,-7.8,-5.3]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,-8.1999999999999993,-5.7,null,null,null,null,0,0,-8.1999999999999993,-5.7]
["Test 3.4","TDD","n8","CP-OFDM","Table 3, MCS5","1T2R","type B",null,"100MHz","DMRS 1+1","TDLA30-75",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,"DMRS 1+0","TDLA30-75",{"$f":"DerivingPerfReq(N17:Y17)","v":-100},{"$f":"IF(L17>-100,L17+0.6,L17)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(N17,P17,R17,T17,V17,X17)-MIN(N17,P17,R17,T17,V17,X17)","v":0},{"$f":"MAX(O17,Q17,S17,U17,W17,Y17)-MIN(O17,Q17,S17,U17,W17,Y17)","v":0},{"$f":"AVERAGE(N17,P17,R17,T17,V17,X17)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(O17,Q17,S17,U17,W17,Y17)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,"TDLA30-300",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]

{"sheet":"FR2 PUSCH low latency","index":5,"n_rows":34,"n_cols":28,"rows_kept":34,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,6,1,6],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[2,7,4,7],[0,24,0,25],[0,26,0,27],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,11,1,11],[2,1,5,1],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,5,5],[10,7,12,7],[6,1,9,1],[6,2,9,2],[6,3,9,3],[6,4,9,4],[6,5,9,5],[6,7,8,7],[10,1,13,1],[10,2,13,2],[10,3,13,3],[10,4,13,4],[10,5,13,5],[14,7,16,7],[18,1,21,1],[18,2,21,2],[18,3,21,3],[18,4,21,4],[18,5,21,5],[18,7,20,7],[14,1,17,1],[14,2,17,2],[14,3,17,3],[14,4,17,4],[14,5,17,5],[26,7,28,7],[22,1,25,1],[22,2,25,2],[22,3,25,3],[22,4,25,4],[22,5,25,5],[22,7,24,7],[30,4,33,4],[30,5,33,5],[26,1,29,1],[26,2,29,2],[26,3,29,3],[26,4,29,4],[26,5,29,5],[26,9,33,9],[2,0,9,0],[10,0,17,0],[18,0,25,0],[26,0,33,0],[30,7,32,7],[2,9,9,9],[2,8,9,8],[10,9,17,9],[10,8,17,8],[18,8,25,8],[18,9,25,9],[26,8,33,8],[30,1,33,1],[30,2,33,2],[30,3,33,3]]}
[" Test"," waveform","Tx/Rx","PUSCH mapping type","MCS level","Propagation condition","Symbol length","DMRS","SCS","BW","38.104 req","38.141 req","Samsung",null,"DoCoMo",null,"Intel",null,"Nokia",null,"Huawei",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Test 4.1","CP-OFDM","1T2R","type B","Table 3, MCS10","TDLC300-100","2os","DMRS 1+0","60kHz","50MHz",{"$f":"DerivingPerfReq(M3:X3)","v":-100},{"$f":"IF(K3>-100,K3+0.6,K3)","v":-100},null,null,null,null,null,null,-1.3,1.2,null,null,-1.6,0.4,{"$f":"MAX(M3,O3,Q3,S3,U3,W3)-MIN(M3,O3,Q3,S3,U3,W3)","v":0.30000000000000004},{"$f":"MAX(N3,P3,R3,T3,V3,X3)-MIN(N3,P3,R3,T3,V3,X3)","v":0.79999999999999993},{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3)","v":-1.4500000000000002},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3)","v":0.8}]
[null,null,null,null,null,null,"4os",null,null,null,null,null,null,null,null,null,null,null,-1.3,1.2]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M5:X5)","v":-100},{"$f":"IF(K5>-100,K5+0.6,K5)","v":-100},null,null,null,null,null,null,-1.5,1,null,null,null,null,{"$f":"MAX(M5,O5,Q5,S5,U5,W5)-MIN(M5,O5,Q5,S5,U5,W5)","v":0},0,{"$f":"AVERAGE(M5,O5,Q5,S5,U5,W5)","v":-1.5},1]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M6:X6)","v":-100},{"$f":"IF(K6>-100,K6+0.6,K6)","v":-100},null,null,null,null,null,null,-1.4,1.1000000000000001,null,null,null,null,0,0,-1.4,1.1000000000000001]
[null,"CP-OFDM","1T2R","type B","Table 3, MCS5","TDLC300-100","2os","DMRS 1+0",null,null,{"$f":"DerivingPerfReq(M7:X7)","v":-100},{"$f":"IF(K7>-100,K7+0.6,K7)","v":-100},null,null,null,null,null,null,-5.4,-2.9,null,null,null,null,{"$f":"MAX(M7,O7,Q7,S7,U7,W7)-MIN(M7,O7,Q7,S7,U7,W7)","v":0},{"$f":"MAX(N7,P7,R7,T7,V7,X7)-MIN(N7,P7,R7,T7,V7,X7)","v":0},{"$f":"AVERAGE(M7,O7,Q7,S7,U7,W7)","v":-5.4},{"$f":"AVERAGE(N7,P7,R7,T7,V7,X7)","v":-2.9}]
[null,null,null,null,null,null,"4os",null,null,null,null,null,null,null,null,null,null,null,-5.6,-3.1,null,null,-6.6,-4.5999999999999996]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M9:X9)","v":-100},{"$f":"IF(K9>-100,K9+0.6,K9)","v":-100},null,null,null,null,null,null,-5.5,-3,null,null,null,null,{"$f":"MAX(M9,O9,Q9,S9,U9,W9)-MIN(M9,O9,Q9,S9,U9,W9)","v":0},{"$f":"MAX(N9,P9,R9,T9,V9,X9)-MIN(N9,P9,R9,T9,V9,X9)","v":0},{"$f":"AVERAGE(M9,O9,Q9,S9,U9,W9)","v":-5.5},{"$f":"AVERAGE(N9,P9,R9,T9,V9,X9)","v":-3}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M10:X10)","v":-100},{"$f":"IF(K10>-100,K10+0.6,K10)","v":-100},null,null,null,null,null,null,-5.6,-3.1,-7.1,-5.0999999999999996,null,null,1.5,1.9999999999999996,-6.35,-4.0999999999999996]
["Test 4.2","CP-OFDM","1T2R","type B","Table 3, MCS10","TDLC300-100","2os","DMRS 1+0","60kHz","100MHz",{"$f":"DerivingPerfReq(M11:X11)","v":-100},{"$f":"IF(K11>-100,K11+0.6,K11)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M11,O11,Q11,S11,U11,W11)-MIN(M11,O11,Q11,S11,U11,W11)","v":0},{"$f":"MAX(N11,P11,R11,T11,V11,X11)-MIN(N11,P11,R11,T11,V11,X11)","v":0},{"$f":"AVERAGE(M11,O11,Q11,S11,U11,W11)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"4os"]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M13:X13)","v":-100},{"$f":"IF(K13>-100,K13+0.6,K13)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M13,O13,Q13,S13,U13,W13)-MIN(M13,O13,Q13,S13,U13,W13)","v":0},{"$f":"MAX(N13,P13,R13,T13,V13,X13)-MIN(N13,P13,R13,T13,V13,X13)","v":0},{"$f":"AVERAGE(M13,O13,Q13,S13,U13,W13)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N13,P13,R13,T13,V13,X13)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M14:X14)","v":-100},{"$f":"IF(K14>-100,K14+0.6,K14)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,"CP-OFDM","1T2R","type B","Table 3, MCS5","TDLC300-100","2os","DMRS 1+0",null,null,{"$f":"DerivingPerfReq(M15:X15)","v":-100},{"$f":"IF(K15>-100,K15+0.6,K15)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M15,O15,Q15,S15,U15,W15)-MIN(M15,O15,Q15,S15,U15,W15)","v":0},{"$f":"MAX(N15,P15,R15,T15,V15,X15)-MIN(N15,P15,R15,T15,V15,X15)","v":0},{"$f":"AVERAGE(M15,O15,Q15,S15,U15,W15)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N15,P15,R15,T15,V15,X15)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"4os"]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M17:X17)","v":-100},{"$f":"IF(K17>-100,K17+0.6,K17)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M17,O17,Q17,S17,U17,W17)-MIN(M17,O17,Q17,S17,U17,W17)","v":0},{"$f":"MAX(N17,P17,R17,T17,V17,X17)-MIN(N17,P17,R17,T17,V17,X17)","v":0},{"$f":"AVERAGE(M17,O17,Q17,S17,U17,W17)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N17,P17,R17,T17,V17,X17)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M18:X18)","v":-100},{"$f":"IF(K18>-100,K18+0.6,K18)","v":-100},null,null,null,null,null,null,null,null,-7.8,-5.8,null,null,0,0,-7.8,-5.8]
["Test 4.3","CP-OFDM","1T2R","type B","Table 3, MCS10","TDLC300-100","2os","DMRS 1+0","120kHz","50MHz",{"$f":"DerivingPerfReq(M19:X19)","v":-100},{"$f":"IF(K19>-100,K19+0.6,K19)","v":-100},null,null,null,null,null,null,-0.4,2.1,null,null,-1.5,0.5,{"$f":"MAX(M19,O19,Q19,S19,U19,W19)-MIN(M19,O19,Q19,S19,U19,W19)","v":1.1000000000000001},{"$f":"MAX(N19,P19,R19,T19,V19,X19)-MIN(N19,P19,R19,T19,V19,X19)","v":1.6},{"$f":"AVERAGE(M19,O19,Q19,S19,U19,W19)","v":-0.95},{"$f":"AVERAGE(N19,P19,R19,T19,V19,X19)","v":1.3}]
[null,null,null,null,null,null,"4os",null,null,null,null,null,null,null,null,null,null,null,-0.5,2]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M21:X21)","v":-100},{"$f":"IF(K21>-100,K21+0.6,K21)","v":-100},null,null,null,null,null,null,-0.7,1.8,null,null,null,null,{"$f":"MAX(M21,O21,Q21,S21,U21,W21)-MIN(M21,O21,Q21,S21,U21,W21)","v":0},{"$f":"MAX(N21,P21,R21,T21,V21,X21)-MIN(N21,P21,R21,T21,V21,X21)","v":0},{"$f":"AVERAGE(M21,O21,Q21,S21,U21,W21)","v":-0.7},{"$f":"AVERAGE(N21,P21,R21,T21,V21,X21)","v":1.8}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M22:X22)","v":-100},{"$f":"IF(K22>-100,K22+0.6,K22)","v":-100},null,null,null,null,null,null,-0.5,2,null,null,null,null,0,0,-0.5,2]
[null,"CP-OFDM","1T2R","type B","Table 3, MCS5","TDLC300-100","2os","DMRS 1+0",null,null,{"$f":"DerivingPerfReq(M23:X23)","v":-100},{"$f":"IF(K23>-100,K23+0.6,K23)","v":-100},null,null,null,null,null,null,-4.0999999999999996,-1.6,null,null,null,null,{"$f":"MAX(M23,O23,Q23,S23,U23,W23)-MIN(M23,O23,Q23,S23,U23,W23)","v":0},{"$f":"MAX(N23,P23,R23,T23,V23,X23)-MIN(N23,P23,R23,T23,V23,X23)","v":0},{"$f":"AVERAGE(M23,O23,Q23,S23,U23,W23)","v":-4.0999999999999996},{"$f":"AVERAGE(N23,P23,R23,T23,V23,X23)","v":-1.6}]
[null,null,null,null,null,null,"4os",null,null,null,null,null,null,null,null,null,null,null,-4.3,-1.8,null,null,-5.4,-3.4]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M25:X25)","v":-100},{"$f":"IF(K25>-100,K25+0.6,K25)","v":-100},null,null,null,null,null,null,-4.2,-1.7,null,null,null,null,{"$f":"MAX(M25,O25,Q25,S25,U25,W25)-MIN(M25,O25,Q25,S25,U25,W25)","v":0},{"$f":"MAX(N25,P25,R25,T25,V25,X25)-MIN(N25,P25,R25,T25,V25,X25)","v":0},{"$f":"AVERAGE(M25,O25,Q25,S25,U25,W25)","v":-4.2},{"$f":"AVERAGE(N25,P25,R25,T25,V25,X25)","v":-1.7}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M26:X26)","v":-100},{"$f":"IF(K26>-100,K26+0.6,K26)","v":-100},null,null,null,null,null,null,-4.2,-1.7,-7.1,-5.0999999999999996,null,null,2.8999999999999995,3.3999999999999995,-5.65,-3.4]
["Test 4.4","CP-OFDM","1T2R","type B","Table 3, MCS10","TDLC300-100","2os","DMRS 1+0","120kHz","100MHz",{"$f":"DerivingPerfReq(M27:X27)","v":-100},{"$f":"IF(K27>-100,K27+0.6,K27)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M27,O27,Q27,S27,U27,W27)-MIN(M27,O27,Q27,S27,U27,W27)","v":0},{"$f":"MAX(N27,P27,R27,T27,V27,X27)-MIN(N27,P27,R27,T27,V27,X27)","v":0},{"$f":"AVERAGE(M27,O27,Q27,S27,U27,W27)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N27,P27,R27,T27,V27,X27)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"4os"]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M29:X29)","v":-100},{"$f":"IF(K29>-100,K29+0.6,K29)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M29,O29,Q29,S29,U29,W29)-MIN(M29,O29,Q29,S29,U29,W29)","v":0},{"$f":"MAX(N29,P29,R29,T29,V29,X29)-MIN(N29,P29,R29,T29,V29,X29)","v":0},{"$f":"AVERAGE(M29,O29,Q29,S29,U29,W29)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N29,P29,R29,T29,V29,X29)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M30:X30)","v":-100},{"$f":"IF(K30>-100,K30+0.6,K30)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,"CP-OFDM","1T2R","type B","Table 3, MCS5","TDLC300-100","2os","DMRS 1+0",null,null,{"$f":"DerivingPerfReq(M31:X31)","v":-100},{"$f":"IF(K31>-100,K31+0.6,K31)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(M31,O31,Q31,S31,U31,W31)-MIN(M31,O31,Q31,S31,U31,W31)","v":0},{"$f":"MAX(N31,P31,R31,T31,V31,X31)-MIN(N31,P31,R31,T31,V31,X31)","v":0},{"$f":"AVERAGE(M31,O31,Q31,S31,U31,W31)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(N31,P31,R31,T31,V31,X31)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,"4os"]
[null,null,null,null,null,null,"7os",null,null,null,{"$f":"DerivingPerfReq(M33:X33)","v":-100},{"$f":"IF(K33>-100,K33+0.6,K33)","v":-100},null,null,null,null,null,null,null,null,-7.7,-5.7,null,null,{"$f":"MAX(M33,O33,Q33,S33,U33,W33)-MIN(M33,O33,Q33,S33,U33,W33)","v":0},{"$f":"MAX(N33,P33,R33,T33,V33,X33)-MIN(N33,P33,R33,T33,V33,X33)","v":0},{"$f":"AVERAGE(M33,O33,Q33,S33,U33,W33)","v":-7.7},{"$f":"AVERAGE(N33,P33,R33,T33,V33,X33)","v":-5.7}]
[null,null,null,null,null,null,"7os","DMRS 1+1",null,null,{"$f":"DerivingPerfReq(M34:X34)","v":-100},{"$f":"IF(K34>-100,K34+0.6,K34)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]