**3GPP TSG-RAN WG4 Meeting #97-e R4-2015919**

**Electronic Meeting, 02 November – 13 November 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **-1** | **CR** | **0548** | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to add NR intra-band FR1 in TS 38.101-1 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_CA\_R16\_Intra |  | ***Date:*** | 2020-11-16 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Adding approved NR Intra-band FR1 combinations |
|  |  |
| ***Summary of change:*** | Approved NR Intra-band FR1 combinations at RAN4 96-e:CA\_n48(A-B)CA\_n48(A-C)CA\_n66(2A)\_BCS1Approved NR Intra-band FR1 combinations at RAN4 97-e:CA\_n2(2A)CA\_n5(2A)CA\_n71(2A)CA\_n77(2A)\_BCS1 |
|  |  |
| ***Consequences if not approved:*** | Approved NR Intra-band FR1 combinations are not added |
|  |  |
| ***Clauses affected:*** | 5.5, 7.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-3 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---Start of changes---

### 5.5A.2 Configurations for intra-band non-contiguous CA

Table 5.5A.2-1: NR CA configurations and bandwidth combination sets defined for intra-band non-contiguous CA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | MaximumAggregated bandwidth(MHz) | Bandwidth combination set |
| CA\_n2(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n3(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n5(2A) | - | 5,10,15,20 | 5,10,15, 20 |  |  | 25 | 0 |
| CA\_n7(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n25(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n41(2A) | - | 40, 50, 60, 80, 100 | 40, 50, 60, 80, 100 |  |  | 180 | 0 |
| 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 190 | 1 |
| CA\_n48(2A) | - |  |  |  |  |  | 0 |
| 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 1402 |
| CA\_n48(3A) | - | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 |  | 1402 | 0 |
| CA\_n48(4A) | - | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 1352 | 0 |
| CA\_n66(2A) | - | 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 |  |  | 60 | 0 |
| 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  | 80 | 1 |
| CA\_n71(2A) | - | 5,10,15,20 | 5,10,15, 20 |  |  | 30 | 0 |
| CA\_n77(2A) | - | 20, 40, 80, 100 | 20, 40, 80, 100 |  |  | 200 | 0 |
| 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 1 |
| CA\_n78(2A) | - | 10, 20, 40, 50, 60, 80, 90, 100 | 10, 20, 40, 50, 60, 80, 90, 100 |  |  | 200 | 0 |
| 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |  | 200 | 1 |
| 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 200 | 2 |
| NOTE 1: Void.NOTE 2: Parameter value accounts for both, the maximum frequency range of band n48 (150 MHz), and the minimum frequency gaps in between NR non-contiguous component carriers. |

Table 5.5A.2-2: NR CA configurations and bandwidth combination sets defined for mixed intra-band contiguous and non-contiguous CA

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink CA configuration | CA Class | SCS(kHz) | 5MHz | 10MHz | 15MHz | 20MHz | 25 MHz | 30 MHz | 40MHz | 50MHz | 60MHz | 70MHz | 80MHz | 90 MHz | 100 MHz | Bandwidth combination set |
| CA\_n48(A-B) | CA\_n48B | A | 15 | Yes | Yes | Yes | Yes |  |  | Yes | Yes1 |  |  |  |  |  | 0 |
| 30 |  | Yes | Yes | Yes |  |  | Yes | Yes1 | Yes1 |  | Yes1 | Yes1 | Yes1 |
| 60 |  | Yes | Yes | Yes |  |  | Yes | Yes1 | Yes1 |  | Yes1 | Yes1 | Yes1 |
| B | See CA\_n48B bandwidth combination set 0 in Table 5.5A.1-1 |
| CA\_n48(A-C) | - | A | 15 | Yes | Yes | Yes | Yes |  |  | Yes | Yes1 |  |  |  |  |  | 0 |
| 30 |  | Yes | Yes | Yes |  |  | Yes | Yes1 | Yes1 |  | Yes1 | Yes1 | Yes1 |
| 60 |  | Yes | Yes | Yes |  |  | Yes | Yes1 | Yes1 |  | Yes1 | Yes1 | Yes1 |
| C | See CA\_n48C bandwidth combination set 0 in Table 5.5A.1-1 |
| NOTE 1: This UE channel bandwidth is applicable only to downlink |

### 5.5A.3 Configurations for inter-band CA

---Text omitted---

Table 7.3A.2.2-1: Intra-band non-contiguous CA with one uplink configuration for reference sensitivity

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS(kHz) | Aggregated channel bandwidth (PCC+SCC) | Wgap / [MHz] | UL PCC allocation | ΔRIBNC (dB) | Duplex mode |
| CA\_n2(2A) | 15 | 25RB+25RB | Wgap = 55.0 | 105 | 5.0 | FDD |
| Wgap = 30.0 | 25 | 0.0 |
| CA\_n3(2A) | 15 | 25RB+25RB | Wgap = 65.0 | 125 | 4.7 | FDD |
| Wgap = 45.0 | 255 | 0.0 |
| CA\_n5(2A) | 15 | 75RB + 25RB | Wgap = 5.0 | 55 | 6.3 | FDD |
| CA\_n7(2A) | 15 | 52RB+25RB | Wgap = 55 | 325 | 0.0 | FDD |
| Wgap = 30 | 505 | 0.0 |
| CA\_n25(2A) | 15 | 25RB+25RB | Wgap = 55.0 | 105 | 5.0 | FDD |
| Wgap = 30.0 | 25 | 0.0 |
| CA\_n41(2A) | N/A | NOTE 1 | NOTE 2 | NOTE 3 | 0.0 | TDD |
| CA\_n66(2A) | N/A | NOTE 1 | NOTE 2 | NOTE 3, NOTE 4 | 0.0 | FDD |
| CA\_n71(2A) | 15 | 25RB+25RB | Wgap = 25.0 | 5 | 4.0 | FDD |
| Wgap = 5.0 | 20 | 0.0 |
| 50RB+25RB | Wgap = 20.0 | 58 | 4.6 |
| Wgap = 5.0 | 208 | 2.3 |
| 75RB+50RB | Wgap = 10.0 | 59 | 22.2 |
| Wgap = 5.0 | 2010 | 5.2 |
| CA\_n77(2A) |  | NOTE 1 | NOTE 2 | NOTE 3 | 0.0 | TDD |
| CA\_n78(2A) |  | NOTE 1 | NOTE 2 | NOTE 3 | 0.0 | TDD |
| NOTE 1: All combinations of channel bandwidths defined in Table 5.5A.2-1.NOTE 2: All applicable sub-block gap sizes.NOTE 3: The PCC allocation is same as Transmission bandwidth configuration NRB as defined in Table 5.3.2-1. NOTE 4: The carrier center frequency of PCC in the DL operating band is configured closer to the UL operating band.NOTE 5: Refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission.NOTE 6: Wgap is the sub-block gap between the two sub-blocks.NOTE 7: The carrier centre frequency of SCC in the DL operating band is configured closer to the UL operating band.NOTE 8: Uplink resource block starts at RB postion [9] for SCS=15KHz.NOTE 9: Uplink resource block starts at RB postion [2] for SCS=15KHz.NOTE 10: Uplink resource block starts at RB postion [19] for SCS=15KHz. |

---End of changes---