3GPP TSG-RAN WG4 Meeting # 98-e R4-2100259

Electronic Meeting, 25th January – 5th February, 2021

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draftCR for Rel-17 NR inter band CA DC combinations for 2 bands DL with up to 2 bands UL within FR1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Verizon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R17\_2BDL\_xBUL | | | | |  | ***Date:*** | | | 2021-01-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Completion of NR CADC configuraions | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add NR CA configurations in Table 5.5A.3.1-1 and DC configurations in Table 5.5B.1-1 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The required NR CA and DC configuratons cannot be implmented in spec | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | Table 5.5A.3.1-1, Table 5.5B.1-1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | 38.521-3 ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

### 5.5A.3 Configurations for inter-band CA

Table 5.5A.3-1: Void

Table 5.5A.3-2: Void

Table 5.5A.3-3: Void

#### 5.5A.3.1 Configurations for inter-band CA (two bands)

Table 5.5A.3.1-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration | NR Band | Channel bandwidth (MHz) (NOTE 3) | | | | | | | | | | | | | Bandwidth combination set |
|  |  |  | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n1A-n3A | CA\_n1A-n3A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  |  |
| CA\_n1B-n3A | CA\_n1A-n3A | n1 | See CA\_n1B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  |  |
| CA\_n1A-n3(2A) | CA\_n1A-n3A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n3 | See CA\_n3(2A) bandwidth combination set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n1A-n7A | CA\_n1A-n7A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
| CA\_n1A-n7B | - | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n7 | See CA\_n7B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n1A-n8A | CA\_n1A-n8A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n1A-n28A | CA\_n1A-n28A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n1A-n40A | CA\_n1A-n40A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  |  |
| CA\_n1A-n41A | CA\_n1A-n41A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n1A-n77A | CA\_n1A-n77A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n1A-n78A | CA\_n1A-n78A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n1 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
|  |  | n1 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 2 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n1A-n78(2A) | CA\_n1A-n78A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n1 | 2 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 1 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n1A-n78C | CA\_n1A-n78A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n1A-n79A | CA\_n1A-n79A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n1A-n79C | CA\_n1A-n79A | n1 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n79 | See CA\_n79C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n2A-n5A | CA\_n2A-n5A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n2A-n48A | CA\_n2A-n48A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | 5 | 10 | 15 | 20 |  |  | 40 | 501 | 601 |  | 801 | 901 | 1001 |  |
| CA\_n2A-n48B | CA\_n2A-n48A  CA\_n48B | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n2A-n48C | CA\_n2A-n48A  CA\_n48C | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n2A-n48(2A) | CA\_n2A-n48A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n2A-n48(A-C) | CA\_n2A-n48A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48(A-C) Bandwidth Combination Set 0 in Table 5.5A.2-2 | | | | | | | | | | | | |  |
| CA\_n2A-n66A | - | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n2A-n66A | CA\_n2A-n66A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n2A-n66B | CA\_n2A-n66A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | See CA\_n66B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n2A-n77A | CA\_n2A-n77A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n2A-n77(2A) | CA\_n2A-n77A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n2A-n77C | CA\_n2A-n77A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n2A-n78A | CA\_n2A-n78A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n2A-n78(2A) | CA\_n2A-n78A | n2 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n3A-n7A | CA\_n3A-n7A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
| CA\_n3A-n7A | - | n3 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
| CA\_n3A-n7B | - | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n7 | See CA\_n7B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n3A-n8A | CA\_n3A-n8A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n3A-n28A | CA\_n3A-n28A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n3A-n38A | CA\_n3A-n38A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n38 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n3A-n40A | CA\_n3A-n40A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  |  |
| CA\_n3A-n41A | CA\_n3A-n41A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 1 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  |  |  |  |  |
| CA\_n3A-n41C | CA\_n3A-n41A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n3A-n41(2A) | CA\_n3A-n41A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n3A-n77A | CA\_n3A-n77A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n3A-n77(2A) | CA\_n77(2A)  CA\_n3A-n77A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n3A-n78A | CA\_n3A-n78A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n3A-n78C | CA\_n3A-n78A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n3A-n78(2A) | CA\_n78(2A) | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n3A-n79A | CA\_n3A-n79A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n3A-n79C | CA\_n3A-n79A | n3 | 5 | 10 | 15 | 20 | 25 | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n79 | See CA\_n79C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n5A-n7A | - | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
| CA\_n5A-n7B | - | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n7 | See CA\_n7B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n5A-n25A | CA\_n5A-n25A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n5A-n25(2A) | CA\_n5A-n25A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n5A-n48A | CA\_n5A-n48A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | 5 | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n5A-n48(2A) | CA\_n5A-n48A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_48(2A) in Table 5.5A.2-1 in 38.101-1 | | | | | | | | | | | | |  |
| CA\_n5A-n48B | CA\_n5A-n48A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48C in Table 5.5A.1-1 in 38.101-1 | | | | | | | | | | | | |  |
| CA\_n5A-n48C | CA\_n5A-n48A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48C in Table 5.5A.1-1 in 38.101-1 | | | | | | | | | | | | |  |
| CA\_n5A-n66A | CA\_n5A-n66A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n5A-n66(2A) | CA\_n5A-n66A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n5A-n77A | CA\_n5A-n77A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n5A-n77(2A) | CA\_n5A-n77A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n5A-n77C | CA\_n5A-n77A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n5A-n78A | CA\_n5A-n78A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n5A-n78(2A) | CA\_n5A-n78A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n5A-n78C | CA\_n5A-n78A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n5A-n79A | CA\_n5A-n79A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n5A-n79C | CA\_n5A-n79A | n5 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n79 | See CA\_n79C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n7A-n25A | CA\_n7A-n25A | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n7A-n25(2A) | CA\_n7A-n25A | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n7(2A)-n25A | CA\_n7A-n25A | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n7 | See CA\_n7(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n7(2A)-n25(2A) | CA\_n7A-n25A | n7 | See CA\_n7(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n7A-n28A | CA\_n7A-n28A | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 0 |
|  |  | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n7B-n28A | - | n7 | See CA\_n7B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n7A-n66A | CA\_n7A-n66A | n7 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 |  | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
|  |  | n7 | 5 | 10 | 15 | 20 | 25 | 60 | 40 |  |  |  |  |  |  | 1 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 60 | 40 |  |  |  |  |  |  |  |
| CA\_n7A-n66(2A) | CA\_n7A-n66A | n7 | 5 | 10 | 15 | 20 | 25 | 60 | 40 |  |  |  |  |  |  | 0 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n7(2A)-n66 | CA\_n7A-n66A | n7 | See CA\_n7(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 60 | 40 |  |  |  |  |  |  |  |
| CA\_n7(2A)-n66(2A) | CA\_n7A-n66A | n7 | See CA\_n7(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n7A-n78A | CA\_n7A-n78A | n7 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n7A-n78(2A) | CA\_n7A-n78A | n7 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n7(2A)-n78A | CA\_n7A-n78A | n7 | See CA\_n7(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n7(2A)-n78(2A) | CA\_n7A-n78A | n7 | See CA\_n7(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n8A-n28A | - | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n28 | 5 | 10 | 15 | 20 |  | 30 |  |  |  |  |  |  |  |  |
| CA\_n8A-n39A | CA\_n8A-n39A | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n39 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n8A-n40A | CA\_n8A-n40A | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  |  |
| CA\_n8A-n41A | CA\_n8A-n41A | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  |  |  |  |  |
| CA\_n8A-n75A | - | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n75 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n8A-n78A | CA\_n8A-n78A | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n8A-n78(2A) | CA\_n8A-n78A | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n8A-n79A | CA\_n8A-n79A | n8 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n79 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n20A-n28A | CA\_n20A-n28A | n20 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  |  | n20 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  |  | n28 | 5 | 10 | 15 | 20 |  | 30 |  |  |  |  |  |  |  |  |
| CA\_n20A-n75A | - | n20 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n75 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n20A-n78A | CA\_n20A-n78A | n20 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n25A-n38A | CA\_n25A-n38A | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n38 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n25(2A)-n38A | CA\_n25A-n38A | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n38 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n25A-n41A | CA\_n25A-n41A | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n25(2A)-n41A | CA\_n25A-n41A | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n25A-n41C | CA\_n25A-n41A  CA\_n41C | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 1 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n25A-n41(2A) | CA\_n25A-n41A | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25A-n48A | - | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | 5 | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n25A-n48(2A) | - | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25A-n48C | - | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n48 | See CA\_n48C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n25A-n66A | CA\_n25A-n66A | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  | 30 | 40 |  |  |  |  |  |  |  |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n25A-n66(2A) | CA\_n25A-n66A | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25(2A)-n66A | CA\_n25A-n66A | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n66 |  | 10 | 15 | 20 |  | 30 | 40 |  |  |  |  |  |  |  |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n66 |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| CA\_n25(2A)-n66(2A) | CA\_n25A-n66A | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25A-n71A | CA\_n25A-n71A | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n25A-n71(2A) | - | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n71 | See CA\_n71(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25A-n77A | CA\_n25A-n77A | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n25A-n78A | CA\_n25A-n78A | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n25A-n78(2A) | CA\_n25A-n78A | n25 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25(2A)-n78A | CA\_n25A-n78A | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n78 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n25(2A)-n78(2A) | CA\_n25A-n78A | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n25 | See CA\_n25(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n25A-n46A | - | n25 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n46 |  |  |  | 20 |  |  | 40 |  | 60 |  | 80 |  |  |  |
| CA\_n28A-n40A | CA\_n28A-n40A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  |  |
| CA\_n28A-n41A | CA\_n28A-n41A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n41 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n28A-n50A | CA\_n28A-n50A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n50 | 5 | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 801 |  |  |  |
| CA\_n28A-n75A | - | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n75 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n28A-n75A | - | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n75 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 |  |  |  |  |  |  |
| CA\_n28A-n77A | CA\_n28A-n77A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n28A-n77(2A) | CA\_n77(2A)  CA\_n28A-n77A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n28A-n78A | CA\_n28A-n78A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n28 | 5 | 10 | 15 | 20 |  | 30 |  |  |  |  |  |  |  | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n28A-n78(2A) | CA\_n78(2A)  CA\_n28A-n78A | n28 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n29A-n66A | - | n29 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
|  |  | n29 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n29A-n66B | - | n29 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | See CA\_n66B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n29A-n66(2A) | - | n29 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n29 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n29A-n70A | - | n29 | 5 | 10 |  |  |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n70 | 5 | 10 | 15 | 201 | 251 |  |  |  |  |  |  |  |  |  |
| CA\_n38A-n66A | CA\_n38A-n66A | n38 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  | 30 | 40 |  |  |  |  |  |  |  |
|  |  | n38 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n38A-n66(2A) | CA\_n38A-n66A | n38 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n38A-n78A | CA\_n38A-n78A | n38 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n38 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n38A-n78(2A) | CA\_n38A-n78A | n38 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n38 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 1 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n28A-n79A | CA\_n28A-n79A | n28 | 5 | 10 | 15 | 20 |  | 30 |  |  |  |  |  |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n34A-n79A | CA\_n34A-n79A | n34 | 5 | 10 | 15 |  |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n39A-n40A | CA\_n39A-n40A | n39 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  |  |
| CA\_n39A-n41A | CA\_n39A-n41A | n39 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n39A-n41C | CA\_n39A-n41A | n39 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n39A-n41(2A) | CA\_n39A-n41A | n39 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n39A-n79A | CA\_n39A-n79A | n39 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n40A-n41A | CA\_n40A-n41A | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  | 0 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  |  |  |  |  |
| CA\_n40A-n41C | CA\_n41C  CA\_n40A-n41A | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n40 | Refer to CA\_n41C Bandwidth combination set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n40A-n78A | CA\_n40A-n78A | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n40A-n78(2A) | CA\_n40A-n78A | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n40A-n79A | CA\_n40A-n79A | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 |  |  | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
|  |  | n40 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n41A-n50A | CA\_n41A-n50A | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n50 | 5 | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 801 |  |  |  |
| CA\_n41A-n66A | CA\_n41A-n66A | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n41(2A)-n66A | - | n41 | See CA\_n41(2A) Bandwidth Combination Set 1 inTable 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n41C-n66A | - | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n41C-n66A | CA\_n41C  CA\_n41A-n66A | n41 | See CA\_n41C Bandwidth Combination Set 1 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n41A-n71A | CA\_n41A-n71A | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n41A-n71B | - | n41 |  | 10 | 15 | 20 |  | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n71 | See CA\_n71B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n41A-n71(2A) | - | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n71 | See CA\_n71(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n41C-n71A | CA\_n41C  CA\_n41A-n71A | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 1 in Table 5.5A.1-1 | | | | | | | | | | | | | 1 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n41(2A)-n71A | - | n41 | See CA\_n41(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n41(2A)-n71B | - | n41 | See CA\_n41(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n71 | See CA\_n71B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n41C-n71B | - | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n71 | See CA\_n71B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n41A-n77A | CA\_n41A-n77A | n41 |  | 10 | 15 | 20 |  | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n41(2A)-n77A | CA\_n41A-n77A | n41 | See CA\_n41(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 in TS 38.101-1 | | | | | | | | | | | | | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n41C-n77A | CA\_n41A-n77A  CA\_n41C | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 in TS 38.101-1 | | | | | | | | | | | | | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n41A-n77(2A) | CA\_n41A-n77A | n41 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 0 |
|  |  | n77 |  | 10 | 15 | 20 |  | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n41A-n78A | CA\_n41A-n78A | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 |  | 100 | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n41A-n78(2A) | - | n41 |  | 10 | 15 | 50 |  | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n71 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 in TS 38.101-1 | | | | | | | | | | | | |  |
| CA\_n41A-n78A | CA\_n41A-n78A | n41 |  | 10 | 15 | 20 |  | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n41A-n79A | CA\_n41A-n79A | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
|  |  | n41 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  |  |  |  | 1 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n41C-n79A | CA\_n41A-n79A  CA\_n41C | n41 | See CA\_n41C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n46A-n48A | CA\_n46A-n48A | n46 |  |  |  | 20 |  |  | 40 |  | 60 |  | 80 |  |  | 0 |
|  |  | n48 |  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n46B-n48A | CA\_n46A-n48A | n46 | See CA\_n46B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n48 |  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n46C-n48A | CA\_n46A-n48A | n46 | See CA\_n46C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n48 |  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n46D-n48A | CA\_n46A-n48A | n46 | See CA\_n46D Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n48 |  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n46E-n48A | CA\_n46A-n48A | n46 | See CA\_n46E Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n48 |  |  |  | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n46A-n66A | - | n46 |  |  |  | 20 |  |  | 40 |  | 60 |  | 80 |  |  | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  |  |
| CA\_n48A-n66A | CA\_n48A-n66A | n48 | 5 | 10 | 15 | 20 |  |  | 40 | 501 | 601 |  | 801 | 901 | 1001 | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n48B-n66A | CA\_n48A-n66A | n48 | See CA\_n48B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  | CA\_n48B | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n48C-n66A | CA\_n48A-n66A | n48 | See CA\_n48C Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  | CA\_n48C | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n48(2A)-n66A | CA\_n48A-n66A | n48 | See CA\_n48(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n48(A-C)-n66A | CA\_n48A-n66A | n48 | See CA\_n48(A-C) Bandwidth Combination Set 0 in Table 5.5A.2-2 | | | | | | | | | | | | | 0 |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  |  |
| CA\_n50A-n78A | CA\_n50A-n78A | n50 | 5 | 10 | 15 | 20 |  | 30 | 40 | 50 | 60 |  | 801 |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n66A-n70A | - | n66 | 5 | 10 | 15 | 20 | 25 |  |  |  |  |  |  |  |  | 0 |
|  |  | n70 | 5 | 10 | 15 | 201 | 251 |  |  |  |  |  |  |  |  |  |
| CA\_n66B-n70A | - | n66 | See CA\_n66B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n70 | 5 | 10 | 15 | 201 | 251 |  |  |  |  |  |  |  |  |  |
| CA\_n66(2A)-n70A | - | n66 | See CA\_n66(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n70 | 5 | 10 | 15 | 201 | 251 |  |  |  |  |  |  |  |  |  |
| CA\_n66A-n71A | CA\_n66A-n71A | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n66A-n71(2A) | - | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  | 0 |
|  |  | n71 | See CA\_n71(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n66(2A)-n71A | CA\_n66A-n71A | n66 | See CA\_n66(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n66B-n71A | CA\_n66A-n71A | n66 | See CA\_n66B Bandwidth Combination Set 0 in Table 5.5A.1-1 | | | | | | | | | | | | | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n66A-n77A | CA\_n66A-n77A | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n66(2A)-n77A | CA\_n66A-n77A | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n66A-n77(2A) | CA\_n66A-n77A | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n66A-n77(2A) | CA\_n66A-n77A  CA\_n77(2A) | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n66(2A)-n77(2A) | CA\_n66A-n77A  CA\_n77(2A) | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n66A-n77C | CA\_n66A-n77A | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n77 | See CA\_n77C Bandwidth Combination Set 1 in Table 5.5A.1-1 | | | | | | | | | | | | |  |
| CA\_n66A-n78A | CA\_n66A-n78A | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n66 | 5 | 10 | 15 | 20 | 25 | 30 | 40 |  |  |  |  |  |  | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n66A-n78(2A) | CA\_n66A-n78A | n66 | 5 | 10 | 15 | 20 |  | 30 | 40 |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n66 | 5 | 10 | 15 | 20 |  |  | 40 |  |  |  |  |  |  | 1 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n66(2A)-n78A | CA\_n66A-n78A | n66 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 1 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n66(2A)-n78(2A) | CA\_n66A-n78A | n66 | See CA\_n66(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n66 | See CA\_n66(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n70A-n71A | CA\_n70A-n71A | n70 | 5 | 10 | 15 | 201 | 251 |  |  |  |  |  |  |  |  | 0 |
|  |  | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n71A-n77A | CA\_n71A-n77A | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n77 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n71A-n78A | CA\_n71A-n78A | n71 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 |  |
| CA\_n71A-n78(2A) | CA\_n71A-n78A | n71 |  | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n75A-n78A | - | n75 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n75A-n78(2A) | - | n75 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | |  |
| CA\_n76A-n78A | - | n76 | 5 |  |  |  |  |  |  |  |  |  |  |  |  | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n77A-n78A2 |  | n77 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 |  |
| CA\_n77A-n79A | CA\_n77A-n79A | n77 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n78A-n79A | CA\_n78A-n79A | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
|  |  | n78 |  | 10 | 15 | 20 | 25 | 30 | 40 | 50 | 60 |  | 80 | 90 | 100 | 1 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n78(2A)-n79A | CA\_n78A-n79A | n78 | See CA\_n78(2A) Bandwidth Combination Set 1 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n79 |  |  |  |  |  |  | 40 | 50 | 60 |  | 80 |  | 100 |  |
| CA\_n78A-n92A | CA\_n78A-n92A | n78 |  | 10 | 15 | 20 |  |  | 40 | 50 | 60 |  | 80 | 90 | 100 | 0 |
|  |  | n92 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| CA\_n78(2A)-n92A | CA\_n78A-n92A | n78 | See CA\_n78(2A) Bandwidth Combination Set 0 in Table 5.5A.2-1 | | | | | | | | | | | | | 0 |
|  |  | n92 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: This UE channel bandwidth is applicable only to downlink.  NOTE 2: The minimum requirements for intra-band contiguous or non-contiguous CA apply.  NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.  NOTE 4: This UE channel bandwidth is optional in this release of the specification.  NOTE 5: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.  NOTE 6: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration | | | | | | | | | | | | | | | | |

## 5.5B Configurations for DC

For an NR DC configuration specified in 5.5B.1-1, the bandwidth combination sets for the corresponding NR CA configuration in 5.5A.3,i.e.,dual uplink inter-band carrier aggregation with uplink assigned to two NR bands, are applicable to Dual Connectivity.

Table 5.5B.1-1: Inter-band NR DC configurations (two bands)

| NR DC  configuration | Uplink NR DC  configuration |
| --- | --- |
| DC\_n2A-n5A | DC\_n2A-n5A |
| DC\_n2A-n48A | DC\_n2A-n48A |
| DC\_n2A-n48B | DC\_n2A-n48A |
| DC\_n2A-n48C | DC\_n2A-n48A |
| DC\_n2A-n48(2A) | DC\_n2A-n48A |
| DC\_n2A-n48(A-C) | DC\_n2A-n48A |
| DC\_n2A-n66A | DC\_n2A-n66A |
| DC\_n2A-n66B | DC\_n2A-n66A |
| DC\_n2A-n77A | DC\_n2A-n77A |
| DC\_n2A-n77(2A) | DC\_n2A-n77A |
| DC\_n2A-n77C | DC\_n2A-n77A |
| DC\_n3A-n77A | DC\_n3A-n77A |
| DC\_n5A-n48A | DC\_n5A-n48A |
| DC\_n5A-n48(2A) | DC\_n5A-n48A |
| DC\_n5A-n48B | DC\_n5A-n48A |
| DC\_n5A-n48C | DC\_n5A-n48A |
| DC\_n5A-n66A | DC\_n5A-n66A |
| DC\_n5A-n66(2A) | DC\_n5A-n66A |
| DC\_n5A-n77A | DC\_n5A-n77A |
| DC\_n5A-n77(2A) | DC\_n5A-n77A |
| DC\_n5A-n77C | DC\_n5A-n77A |
| DC\_n28A-n77A | DC\_n28A-n77A |
| DC\_n46A-n48A | DC\_n46A-n48A |
| DC\_n46B-n48A | DC\_n46A-n48A |
| DC\_n46C-n48A | DC\_n46A-n48A |
| DC\_n46D-n48A | DC\_n46A-n48A |
| DC\_n46E-n48A | DC\_n46A-n48A |
| DC\_n48A-n66A | DC\_n48A-n66A |
| DC\_n48(2A)-n66A | DC\_n48A-n66A |
| DC\_n48B-n66A | DC\_n48A-n66A |
| DC\_n48C-n66A | DC\_n48A-n66A |
| DC\_n48(A-C)-n66A) | DC\_n48A-n66A |
| DC\_n66A-n77A | DC\_n66A-n77A |
| DC\_n66A-n77(2A) | DC\_n66A-n77A |
| DC\_n66(2A)-n77(2A) | DC\_n66A-n77A |
| DC\_n66A-n77C | DC\_n66A-n77A |